Attaching to ia_video_ingestion
[36mia_video_ingestion    |[0m [setupvars.sh] OpenVINO environment initialized
[36mia_video_ingestion    |[0m /EIS/fpga_env.sh: line 30: /opt/altera/aocl-pro-rte/aclrte-linux64/init_opencl.sh: No such file or directory
[36mia_video_ingestion    |[0m [setupvars.sh] OpenVINO environment initialized
[36mia_video_ingestion    |[0m I0505 13:08:47.096662      18 init.go:32] initializing configuration manager...
[36mia_video_ingestion    |[0m I0505 13:08:47.096764      18 util.go:30] Waiting for Port: 2379 on hostname: localhost 
[36mia_video_ingestion    |[0m I0505 13:08:47.098459      18 util.go:34] Port: 2379 on hostname: localhost is up.
[36mia_video_ingestion    |[0m I0505 13:08:47.101837      18 cgo.go:40] Register user callback
[36mia_video_ingestion    |[0m I0505 13:08:47.101860      18 cgo.go:138] Register the key: /VideoIngestion/config for watch key
[36mia_video_ingestion    |[0m I0505 13:08:47.101871      18 EtcdClient.go:153] Watching on key: /VideoIngestion/config
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  WARN:get_config_value:138: JSON does not contain key: queue_size
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  INFO:VideoIngestion:131: "queue_size" key missing, so using default queue size:                     10
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  WARN:get_config_value:138: JSON does not contain key: udfs
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  INFO:VideoIngestion:157: "udfs" key doesn't exist, so udf output queue is same as                 udf input queue!!
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  INFO:GstreamerIngestor:59: cvt_pipeline initialized
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  INFO:GstreamerIngestor:71: Pipeline: pylonsrc imageformat=yuv422 exposureGigE=3250 interpacketdelay=1500 ! video/x-raw,format=YUY2 ! videoconvert ! video/x-raw,format=BGR ! appsink name="sink"
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  WARN:get_config_value:138: JSON does not contain key: poll_interval
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  INFO:GstreamerIngestor:84: Poll interval: 0.000000
[36mia_video_ingestion    |[0m 
[36mia_video_ingestion    |[0m (process:18): GLib-CRITICAL **: 13:08:47.102: g_path_get_basename: assertion 'file_name != NULL' failed
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  WARN:get_config_value:138: JSON does not contain key: zmq_connect_retries
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  WARN:get_config_value:138: JSON does not contain key: camera1_stream
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  INFO:start:205: Publisher thread started...
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  WARN:start:322: Start attempted after stop or after start
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  INFO:start:209: Started udf manager
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  INFO:start:215: Ingestor thread started...
[36mia_video_ingestion    |[0m [Tue May  5 13:08:47 2020]  INFO:run:150: Gstreamer ingestor thread started
[36mia_video_ingestion    |[0m 0:00:01.196368439 [331m   18[00m 0x7febbc0024d0 [37m[00m [00m            pylonsrc gstpylonsrc.c:2381:pylonc_print_camera_info:<pylonsrc0>[00m Status: Using camera "acA2040-120um" (serial number: , id: 0).
[36mia_video_ingestion    |[0m [Tue May  5 13:08:48 2020] ERROR:bus_call:189: Gst Bus Error: Failed to initialise the camera
[36mia_video_ingestion    |[0m [Tue May  5 13:08:48 2020]  INFO:run:153: Gstreamer ingestor thread stopped
