# (C) 2001-2018 Intel Corporation. All rights reserved.
# Your use of Intel Corporation's design tools, logic functions and other 
# software and tools, and its AMPP partner logic functions, and any output 
# files from any of the foregoing (including device programming or simulation 
# files), and any associated documentation or information are expressly subject 
# to the terms and conditions of the Intel Program License Subscription 
# Agreement, Intel FPGA IP License Agreement, or other applicable 
# license agreement, including, without limitation, that your use is for the 
# sole purpose of programming logic devices manufactured by Intel and sold by 
# Intel or its authorized distributors.  Please refer to the applicable 
# agreement for further details.


# The clock output is 250MHz
if {[get_collection_size [get_clocks altera_int_osc_clk -nowarn]] == 0} {
	create_clock -name altera_int_osc_clk -period 4.000 [get_nodes {*|intosc|oscillator_dut~oscillator_clock}]
}