Intel® Driver & Support Assistant

Detailed Report

Last scan: 6/15/2022 7:34 PM

Computer

|  |  |
| --- | --- |
| Intel® Client Systems NUC |  |
| System Manufacturer | Intel® Client Systems |
| System Model | NUC8i7HVK |
| System Type | Mobile |
| Motherboard Manufacturer | Intel Corporation |
| Motherboard Product | NUC8i7HVB |
| Version | J68196-602 |
| BIOS Version | HNKBLi70.86A.0067.2021.0528.1339 |
| Date | 5/28/2021 |
| SMBIOS Version | 3.1 |
| Secure Boot | Off |

Operating System

|  |  |
| --- | --- |
| Microsoft Windows 11 Pro (64-bit) |  |
| Release | 2009 |
| Version | 21H2 |
| OS Build | 10.0.22000 |
| Build Branch | co\_release |
| Locale | English (United States) |
| Windows Directory | C:\WINDOWS |
| System Directory | C:\WINDOWS\system32 |
| .NET Framework Versions | 2.0.50727.4927, 3.0.30729.4926,3.5.30729.4926, 4.0.0.0, 4.8.04161 |

|  |  |
| --- | --- |
| Installed Internet Browsers | Mozilla Firefox, Mozilla Firefox, Internet Explorer11.1.22000.0, Microsoft Edge |

Processor

|  |  |
| --- | --- |
| Intel® Core™ i7-8809G CPU @ 3.10GHz |  |
| Device Details |  |
| Manufacturer | GenuineIntel |
| Description | Intel64 Family 6 Model 158 Stepping 9 |
| Architecture | x64 |
| # of Cores | 4 |
| # of Threads | 8 |
| Processor Base Frequency | 3096 MHz |
| Current Voltage | 1.6 |
| Level 2 Cache | 1024 Kb |
| Level 3 Cache | 8192 Kb |
| Processor Id | 0x906E9 |
| Availability | Running at full power |

Chipset

|  |
| --- |
| Intel® 100 Series/C230 Series Chipset Family |
| Device Details |

Graphics

|  |
| --- |
| Intel® HD Graphics 630 |
| Device Details |
| Adapter Compatibility | Intel Corporation |
| Video Processor | Intel® HD Graphics Family |
| Resolution | 1920 x 1080 |

|  |  |
| --- | --- |
| Bits Per Pixel | 32 |
| Number of Colors | 4294967296 |
| Refresh Rate - Current | 59 Hz |
| Refresh Rate - Maximum | 0 Hz |
| Provider | Intel Corporation |
| Version | 30.0.101.1660 |
| Date | 3/18/2022 |
| Adapter DAC Type | Internal |
| Adapter RAM | 1.00 GB |
| Availability | Running at full power |
| Status | This device is working properly. |
| Location | PCI bus 0, device 2, function 0 |
| Device Id | PCI\VEN\_8086&DEV\_591B&SUBSYS\_20738086&REV\_04\3&11583659&0&10 |
| Radeon RX Vega M GH Graphics |
| Device Details |
| Adapter Compatibility | Advanced Micro Devices, Inc. |
| Video Processor | AMD Radeon Graphics Processor (0x694C) |
| Resolution | 1920 x 1080 |
| Bits Per Pixel | 32 |
| Number of Colors | 4294967296 |

|  |  |
| --- | --- |
| Refresh Rate - Current | 59 Hz |
| Refresh Rate - Maximum | 60 Hz |
| Refresh Rate - Minimum | 50 Hz |
| Provider | Advanced Micro Devices, Inc. |
| Version | 30.0.13037.4001 |
| Date | 12/3/2021 |
| Adapter DAC Type | Internal DAC(400MHz) |
| Adapter RAM | 4.00 GB |
| Availability | Running at full power |
| Status | This device is working properly. |
| Location | PCI bus 1, device 0, function 0 |
| Device Id | PCI\VEN\_1002&DEV\_694C&SUBSYS\_20738086&REV\_C0\4&2BF2E4F6&0&0008 |

Audio

|  |
| --- |
| AMD High Definition Audio Device |
| Device Details |
| Provider | Advanced Micro Devices |
| Name | AtihdWT6.sys |
| Version | 10.0.1.21 |
| Date | 7/13/2021 |
| Device Id | HDAUDIO\FUNC\_01&VEN\_1002&DEV\_AA01&SUBSYS\_00AA0100&REV\_1007\5&11002998&0&00 |
| Intel® Display Audio |
| Device Details |

Networking and I/O

|  |  |
| --- | --- |
| Provider | Intel® Corporation |
| Name | IntcDAud.sys |
| Version | 10.27.0.12 |
| Date | 11/21/2021 |
| Device Id | HDAUDIO\FUNC\_01&VEN\_8086&DEV\_280B&SUBSYS\_80860101&REV\_1000\4&DD712FD&0&02 |
| Realtek High Definition Audio |
| Device Details |
| Provider | Realtek Semiconductor Corp. |
| Name | RTKVHD64.sys |
| Version | 6.0.9275.1 |
| Date | 12/1/2021 |
| Device Id | HDAUDIO\FUNC\_01&VEN\_10EC&DEV\_0700&SUBSYS\_80862073&REV\_1000\4&DD712FD&0&00 |

|  |
| --- |
| Intel® I210 Gigabit Network Connection |
| Device Details |
| Manufacturer | Intel |
| Availability | Running at full power |
| Status | This device is working properly. |
| Installed | True |
| MACAddress | 54:B2:03:98:39:2C |
| Service Name | e1rexpress |
| Provider | Intel |
| Version | 13.0.14.0 |
| Date | 2/24/2022 |

|  |  |
| --- | --- |
| Device Id | PCI\VEN\_8086&DEV\_157B&SUBSYS\_00008086&REV\_03\4&1D2C348D&0&00E1 |
| Revision | 03 |
| Intel® Dual Band Wireless-AC 8265 |
| Device Details |
| Manufacturer | Intel Corporation |
| Availability | Running at full power |
| Status | This device is working properly. |
| Installed | True |
| MACAddress | B8:9A:2A:26:3B:6C |
| Service Name | Netwtw06 |
| Provider | Intel |
| Version | 20.70.21.2 |
| Date | 1/10/2021 |
| Device Id | PCI\VEN\_8086&DEV\_24FD&SUBSYS\_10108086&REV\_78\4&1A9424EB&0&00E2 |
| Revision | 78 |
| Intel® Ethernet Connection (2) I219-LM |
| Device Details |
| Manufacturer | Intel |
| Availability | Running at full power |
| Status | This device is working properly. |
| Installed | True |
| MACAddress | 54:B2:03:98:39:2B |
| Service Name | e1dexpress |
| Provider | Intel |

|  |  |
| --- | --- |
| Version | 12.19.2.45 |
| Date | 1/30/2022 |
| Device Id | PCI\VEN\_8086&DEV\_15B7&SUBSYS\_00008086&REV\_31\3&11583659&0&FE |
| Revision | 31 |

Memory

|  |  |
| --- | --- |
| 16 GB |  |
| Device Details |  |
| Physical Memory - Total | 16 GB |
| Physical Memory - Available | 14.13 GB |
| Virtual Memory - Total | 18.35 GB |
| Virtual Memory - Available | 15.48 GB |
| Page File | C:\pagefile.sys |
| Page File Space | 2.38 GB |

Storage

|  |
| --- |
| Seagate Backup+ Hub BK SCSI Disk Device |
| Device Details |  |
| Capacity | 7452.03 GB |
| Version | D781 |
| Serial Number | NA9R8QB0 |
| Partitions | 1 |
| Provider | Microsoft |
| Version | 10.0.22000.1 |
| Date | 6/21/2006 |
| Device Id | SCSI\DISK&VEN\_SEAGATE&PROD\_BACKUP+\_HUB\_BK\8&3F64D0D&0&000000 |
| Device Path | \\.\PHYSICALDRIVE3 |
| E: |  |

|  |  |
| --- | --- |
| File System | NTFS |
| Compressed | False |
| Capacity | 7451.91 GB |
| Free Space | 6970.46 GB |
| CT1000P5SSD8 |  |
| Device Details |  |
| Capacity | 931.51 GB |
| Version | P4CR311 |
| Serial Number | 0000\_0000\_0000\_0001\_00A0\_7520\_289E\_558F. |
| Partitions | 3 |
| Provider | Microsoft |
| Version | 10.0.22000.1 |
| Date | 6/21/2006 |
| Device Id | SCSI\DISK&VEN\_NVME&PROD\_CT1000P5SSD8\5&2F1FA7B9&0&000000 |
| Device Path | \\.\PHYSICALDRIVE1 |
| C: |  |
| File System | NTFS |
| Compressed | False |
| Capacity | 930.81 GB |
| Free Space | 388.26 GB |
| CT1000P5SSD8 |  |
| Device Details |  |
| Capacity | 931.51 GB |
| Version | P4CR311 |
| Serial Number | 0000\_0000\_0000\_0001\_00A0\_7520\_2B18\_D59B. |
| Partitions | 1 |

|  |  |
| --- | --- |
| Provider | Microsoft |
| Version | 10.0.22000.1 |
| Date | 6/21/2006 |
| Device Id | SCSI\DISK&VEN\_NVME&PROD\_CT1000P5SSD8\5&214C1270&0&000000 |
| Device Path | \\.\PHYSICALDRIVE0 |
| D: |  |
| File System | NTFS |
| Compressed | False |
| Capacity | 931.51 GB |
| Free Space | 895.57 GB |
| Seagate Backup+ Desk SCSI Disk Device |
| Device Details |  |
| Capacity | 4657.52 GB |
| Version | 040B |
| Serial Number | NA7EX2LL |
| Partitions | 1 |
| Provider | Microsoft |
| Version | 10.0.22000.1 |
| Date | 6/21/2006 |
| Device Id | SCSI\DISK&VEN\_SEAGATE&PROD\_BACKUP+ DESK\7&27E0E161&0&000000 |
| Device Path | \\.\PHYSICALDRIVE2 |
| X: |  |
| File System | NTFS |
| Compressed | False |
| Capacity | 4657.40 GB |
| Free Space | 1711.48 GB |