<?xml version="1.0" ?>
<ipxact:component xmlns:altera="http://www.altera.com/XMLSchema/IPXact2014/extensions" xmlns:ipxact="http://www.accellera.org/XMLSchema/IPXACT/1685-2014">
  <ipxact:vendor>Intel Corporation</ipxact:vendor>
  <ipxact:library>pcie</ipxact:library>
  <ipxact:name>pcie_s10_hip_avmm_bridge_0</ipxact:name>
  <ipxact:version>20.0.0</ipxact:version>
  <ipxact:busInterfaces>
    <ipxact:busInterface>
      <ipxact:name>refclk</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="clock" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="clock" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>refclk</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>100000000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>coreclkout_hip</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="clock" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="clock" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>coreclkout_hip</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:master></ipxact:master>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedDirectClock" type="string">
          <ipxact:name>associatedDirectClock</ipxact:name>
          <ipxact:displayName>Associated direct clock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>125000000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clockRateKnown" type="bit">
          <ipxact:name>clockRateKnown</ipxact:name>
          <ipxact:displayName>Clock rate known</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>npor</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>npor</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>npor</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>pin_perst</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>pin_perst</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>app_nreset_status</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="reset" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="reset" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>reset_n</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>app_nreset_status</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:master></ipxact:master>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value>coreclkout_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedDirectReset" type="string">
          <ipxact:name>associatedDirectReset</ipxact:name>
          <ipxact:displayName>Associated direct reset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedResetSinks" type="string">
          <ipxact:name>associatedResetSinks</ipxact:name>
          <ipxact:displayName>Associated reset sinks</ipxact:displayName>
          <ipxact:value>none</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="synchronousEdges" type="string">
          <ipxact:name>synchronousEdges</ipxact:name>
          <ipxact:displayName>Synchronous edges</ipxact:displayName>
          <ipxact:value>BOTH</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>ninit_done</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>ninit_done</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>ninit_done</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>txs</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>address</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txs_address_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>chipselect</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txs_chipselect_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>byteenable</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txs_byteenable_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>readdata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txs_readdata_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>writedata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txs_writedata_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>read</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txs_read_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>write</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txs_write_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>burstcount</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txs_burstcount_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>readdatavalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txs_readdatavalid_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>waitrequest</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txs_waitrequest_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="addressAlignment" type="string">
          <ipxact:name>addressAlignment</ipxact:name>
          <ipxact:displayName>Slave addressing</ipxact:displayName>
          <ipxact:value>DYNAMIC</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressGroup" type="int">
          <ipxact:name>addressGroup</ipxact:name>
          <ipxact:displayName>Address group</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressSpan" type="string">
          <ipxact:name>addressSpan</ipxact:name>
          <ipxact:displayName>Address span</ipxact:displayName>
          <ipxact:value>18446744073709551616</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressUnits" type="string">
          <ipxact:name>addressUnits</ipxact:name>
          <ipxact:displayName>Address units</ipxact:displayName>
          <ipxact:value>SYMBOLS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="alwaysBurstMaxBurst" type="bit">
          <ipxact:name>alwaysBurstMaxBurst</ipxact:name>
          <ipxact:displayName>Always burst maximum burst</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value>coreclkout_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>Associated reset</ipxact:displayName>
          <ipxact:value>app_nreset_status</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bitsPerSymbol" type="int">
          <ipxact:name>bitsPerSymbol</ipxact:name>
          <ipxact:displayName>Bits per symbol</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bridgedAddressOffset" type="string">
          <ipxact:name>bridgedAddressOffset</ipxact:name>
          <ipxact:displayName>Bridged Address Offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bridgesToMaster" type="string">
          <ipxact:name>bridgesToMaster</ipxact:name>
          <ipxact:displayName>Bridges to master</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstOnBurstBoundariesOnly" type="bit">
          <ipxact:name>burstOnBurstBoundariesOnly</ipxact:name>
          <ipxact:displayName>Burst on burst boundaries only</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstcountUnits" type="string">
          <ipxact:name>burstcountUnits</ipxact:name>
          <ipxact:displayName>Burstcount units</ipxact:displayName>
          <ipxact:value>WORDS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="constantBurstBehavior" type="bit">
          <ipxact:name>constantBurstBehavior</ipxact:name>
          <ipxact:displayName>Constant burst behavior</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="explicitAddressSpan" type="string">
          <ipxact:name>explicitAddressSpan</ipxact:name>
          <ipxact:displayName>Explicit address span</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="holdTime" type="int">
          <ipxact:name>holdTime</ipxact:name>
          <ipxact:displayName>Hold</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="interleaveBursts" type="bit">
          <ipxact:name>interleaveBursts</ipxact:name>
          <ipxact:displayName>Interleave bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isBigEndian" type="bit">
          <ipxact:name>isBigEndian</ipxact:name>
          <ipxact:displayName>Big endian</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isFlash" type="bit">
          <ipxact:name>isFlash</ipxact:name>
          <ipxact:displayName>Flash memory</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isMemoryDevice" type="bit">
          <ipxact:name>isMemoryDevice</ipxact:name>
          <ipxact:displayName>Memory device</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isNonVolatileStorage" type="bit">
          <ipxact:name>isNonVolatileStorage</ipxact:name>
          <ipxact:displayName>Non-volatile storage</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="linewrapBursts" type="bit">
          <ipxact:name>linewrapBursts</ipxact:name>
          <ipxact:displayName>Linewrap bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingReadTransactions" type="int">
          <ipxact:name>maximumPendingReadTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending read transactions</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingWriteTransactions" type="int">
          <ipxact:name>maximumPendingWriteTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending write transactions</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumReadLatency" type="int">
          <ipxact:name>minimumReadLatency</ipxact:name>
          <ipxact:displayName>minimumReadLatency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumResponseLatency" type="int">
          <ipxact:name>minimumResponseLatency</ipxact:name>
          <ipxact:displayName>Minimum response latency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumUninterruptedRunLength" type="int">
          <ipxact:name>minimumUninterruptedRunLength</ipxact:name>
          <ipxact:displayName>Minimum uninterrupted run length</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="printableDevice" type="bit">
          <ipxact:name>printableDevice</ipxact:name>
          <ipxact:displayName>Can receive stdout/stderr</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readLatency" type="int">
          <ipxact:name>readLatency</ipxact:name>
          <ipxact:displayName>Read latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readWaitStates" type="int">
          <ipxact:name>readWaitStates</ipxact:name>
          <ipxact:displayName>Read wait states</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readWaitTime" type="int">
          <ipxact:name>readWaitTime</ipxact:name>
          <ipxact:displayName>Read wait</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerIncomingSignals" type="bit">
          <ipxact:name>registerIncomingSignals</ipxact:name>
          <ipxact:displayName>Register incoming signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerOutgoingSignals" type="bit">
          <ipxact:name>registerOutgoingSignals</ipxact:name>
          <ipxact:displayName>Register outgoing signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="setupTime" type="int">
          <ipxact:name>setupTime</ipxact:name>
          <ipxact:displayName>Setup</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="timingUnits" type="string">
          <ipxact:name>timingUnits</ipxact:name>
          <ipxact:displayName>Timing units</ipxact:displayName>
          <ipxact:value>Cycles</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="transparentBridge" type="bit">
          <ipxact:name>transparentBridge</ipxact:name>
          <ipxact:displayName>Transparent bridge</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="waitrequestAllowance" type="int">
          <ipxact:name>waitrequestAllowance</ipxact:name>
          <ipxact:displayName>Waitrequest allowance</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="wellBehavedWaitrequest" type="bit">
          <ipxact:name>wellBehavedWaitrequest</ipxact:name>
          <ipxact:displayName>Well-behaved waitrequest</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeLatency" type="int">
          <ipxact:name>writeLatency</ipxact:name>
          <ipxact:displayName>Write latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeWaitStates" type="int">
          <ipxact:name>writeWaitStates</ipxact:name>
          <ipxact:displayName>Write wait states</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeWaitTime" type="int">
          <ipxact:name>writeWaitTime</ipxact:name>
          <ipxact:displayName>Write wait</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="embeddedsw.configuration.isFlash" type="string">
              <ipxact:name>embeddedsw.configuration.isFlash</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="embeddedsw.configuration.isMemoryDevice" type="string">
              <ipxact:name>embeddedsw.configuration.isMemoryDevice</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="embeddedsw.configuration.isNonVolatileStorage" type="string">
              <ipxact:name>embeddedsw.configuration.isNonVolatileStorage</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="embeddedsw.configuration.isPrintableDevice" type="string">
              <ipxact:name>embeddedsw.configuration.isPrintableDevice</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rxm_bar0</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>address</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar0_address_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>byteenable</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar0_byteenable_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>readdata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar0_readdata_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>writedata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar0_writedata_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>read</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar0_read_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>write</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar0_write_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>readdatavalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar0_readdatavalid_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>waitrequest</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar0_waitrequest_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:master></ipxact:master>
      <ipxact:parameters>
        <ipxact:parameter parameterId="adaptsTo" type="string">
          <ipxact:name>adaptsTo</ipxact:name>
          <ipxact:displayName>Adapts to</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressGroup" type="int">
          <ipxact:name>addressGroup</ipxact:name>
          <ipxact:displayName>Address group</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressUnits" type="string">
          <ipxact:name>addressUnits</ipxact:name>
          <ipxact:displayName>Address units</ipxact:displayName>
          <ipxact:value>SYMBOLS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="alwaysBurstMaxBurst" type="bit">
          <ipxact:name>alwaysBurstMaxBurst</ipxact:name>
          <ipxact:displayName>Always burst maximum burst</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value>coreclkout_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>Associated reset</ipxact:displayName>
          <ipxact:value>app_nreset_status</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bitsPerSymbol" type="int">
          <ipxact:name>bitsPerSymbol</ipxact:name>
          <ipxact:displayName>Bits per symbol</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstOnBurstBoundariesOnly" type="bit">
          <ipxact:name>burstOnBurstBoundariesOnly</ipxact:name>
          <ipxact:displayName>Burst on burst boundaries only</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstcountUnits" type="string">
          <ipxact:name>burstcountUnits</ipxact:name>
          <ipxact:displayName>Burstcount units</ipxact:displayName>
          <ipxact:value>WORDS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="constantBurstBehavior" type="bit">
          <ipxact:name>constantBurstBehavior</ipxact:name>
          <ipxact:displayName>Constant burst behavior</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dBSBigEndian" type="bit">
          <ipxact:name>dBSBigEndian</ipxact:name>
          <ipxact:displayName>dBS big endian</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="doStreamReads" type="bit">
          <ipxact:name>doStreamReads</ipxact:name>
          <ipxact:displayName>Use flow control for read transfers</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="doStreamWrites" type="bit">
          <ipxact:name>doStreamWrites</ipxact:name>
          <ipxact:displayName>Use flow control for write transfers</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="holdTime" type="int">
          <ipxact:name>holdTime</ipxact:name>
          <ipxact:displayName>Hold</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="interleaveBursts" type="bit">
          <ipxact:name>interleaveBursts</ipxact:name>
          <ipxact:displayName>Interleave bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isAsynchronous" type="bit">
          <ipxact:name>isAsynchronous</ipxact:name>
          <ipxact:displayName>Is asynchronous</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isBigEndian" type="bit">
          <ipxact:name>isBigEndian</ipxact:name>
          <ipxact:displayName>Is big endian</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isReadable" type="bit">
          <ipxact:name>isReadable</ipxact:name>
          <ipxact:displayName>Is readable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isWriteable" type="bit">
          <ipxact:name>isWriteable</ipxact:name>
          <ipxact:displayName>Is writeable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="linewrapBursts" type="bit">
          <ipxact:name>linewrapBursts</ipxact:name>
          <ipxact:displayName>Linewrap bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maxAddressWidth" type="int">
          <ipxact:name>maxAddressWidth</ipxact:name>
          <ipxact:displayName>Maximum address width</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingReadTransactions" type="int">
          <ipxact:name>maximumPendingReadTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending read transactions</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingWriteTransactions" type="int">
          <ipxact:name>maximumPendingWriteTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending write transactions</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumReadLatency" type="int">
          <ipxact:name>minimumReadLatency</ipxact:name>
          <ipxact:displayName>minimumReadLatency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumResponseLatency" type="int">
          <ipxact:name>minimumResponseLatency</ipxact:name>
          <ipxact:displayName>Minimum response latency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readLatency" type="int">
          <ipxact:name>readLatency</ipxact:name>
          <ipxact:displayName>Read latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readWaitTime" type="int">
          <ipxact:name>readWaitTime</ipxact:name>
          <ipxact:displayName>Read wait</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerIncomingSignals" type="bit">
          <ipxact:name>registerIncomingSignals</ipxact:name>
          <ipxact:displayName>Register incoming signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerOutgoingSignals" type="bit">
          <ipxact:name>registerOutgoingSignals</ipxact:name>
          <ipxact:displayName>Register outgoing signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="setupTime" type="int">
          <ipxact:name>setupTime</ipxact:name>
          <ipxact:displayName>Setup</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="timingUnits" type="string">
          <ipxact:name>timingUnits</ipxact:name>
          <ipxact:displayName>Timing units</ipxact:displayName>
          <ipxact:value>Cycles</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="waitrequestAllowance" type="int">
          <ipxact:name>waitrequestAllowance</ipxact:name>
          <ipxact:displayName>Waitrequest allowance</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeWaitTime" type="int">
          <ipxact:name>writeWaitTime</ipxact:name>
          <ipxact:displayName>Write wait</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rxm_bar2</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>address</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar2_address_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>byteenable</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar2_byteenable_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>readdata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar2_readdata_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>writedata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar2_writedata_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>read</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar2_read_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>write</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar2_write_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>burstcount</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar2_burstcount_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>readdatavalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar2_readdatavalid_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>waitrequest</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar2_waitrequest_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:master></ipxact:master>
      <ipxact:parameters>
        <ipxact:parameter parameterId="adaptsTo" type="string">
          <ipxact:name>adaptsTo</ipxact:name>
          <ipxact:displayName>Adapts to</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressGroup" type="int">
          <ipxact:name>addressGroup</ipxact:name>
          <ipxact:displayName>Address group</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressUnits" type="string">
          <ipxact:name>addressUnits</ipxact:name>
          <ipxact:displayName>Address units</ipxact:displayName>
          <ipxact:value>SYMBOLS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="alwaysBurstMaxBurst" type="bit">
          <ipxact:name>alwaysBurstMaxBurst</ipxact:name>
          <ipxact:displayName>Always burst maximum burst</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value>coreclkout_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>Associated reset</ipxact:displayName>
          <ipxact:value>app_nreset_status</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bitsPerSymbol" type="int">
          <ipxact:name>bitsPerSymbol</ipxact:name>
          <ipxact:displayName>Bits per symbol</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstOnBurstBoundariesOnly" type="bit">
          <ipxact:name>burstOnBurstBoundariesOnly</ipxact:name>
          <ipxact:displayName>Burst on burst boundaries only</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstcountUnits" type="string">
          <ipxact:name>burstcountUnits</ipxact:name>
          <ipxact:displayName>Burstcount units</ipxact:displayName>
          <ipxact:value>WORDS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="constantBurstBehavior" type="bit">
          <ipxact:name>constantBurstBehavior</ipxact:name>
          <ipxact:displayName>Constant burst behavior</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dBSBigEndian" type="bit">
          <ipxact:name>dBSBigEndian</ipxact:name>
          <ipxact:displayName>dBS big endian</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="doStreamReads" type="bit">
          <ipxact:name>doStreamReads</ipxact:name>
          <ipxact:displayName>Use flow control for read transfers</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="doStreamWrites" type="bit">
          <ipxact:name>doStreamWrites</ipxact:name>
          <ipxact:displayName>Use flow control for write transfers</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="holdTime" type="int">
          <ipxact:name>holdTime</ipxact:name>
          <ipxact:displayName>Hold</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="interleaveBursts" type="bit">
          <ipxact:name>interleaveBursts</ipxact:name>
          <ipxact:displayName>Interleave bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isAsynchronous" type="bit">
          <ipxact:name>isAsynchronous</ipxact:name>
          <ipxact:displayName>Is asynchronous</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isBigEndian" type="bit">
          <ipxact:name>isBigEndian</ipxact:name>
          <ipxact:displayName>Is big endian</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isReadable" type="bit">
          <ipxact:name>isReadable</ipxact:name>
          <ipxact:displayName>Is readable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isWriteable" type="bit">
          <ipxact:name>isWriteable</ipxact:name>
          <ipxact:displayName>Is writeable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="linewrapBursts" type="bit">
          <ipxact:name>linewrapBursts</ipxact:name>
          <ipxact:displayName>Linewrap bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maxAddressWidth" type="int">
          <ipxact:name>maxAddressWidth</ipxact:name>
          <ipxact:displayName>Maximum address width</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingReadTransactions" type="int">
          <ipxact:name>maximumPendingReadTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending read transactions</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingWriteTransactions" type="int">
          <ipxact:name>maximumPendingWriteTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending write transactions</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumReadLatency" type="int">
          <ipxact:name>minimumReadLatency</ipxact:name>
          <ipxact:displayName>minimumReadLatency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumResponseLatency" type="int">
          <ipxact:name>minimumResponseLatency</ipxact:name>
          <ipxact:displayName>Minimum response latency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readLatency" type="int">
          <ipxact:name>readLatency</ipxact:name>
          <ipxact:displayName>Read latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readWaitTime" type="int">
          <ipxact:name>readWaitTime</ipxact:name>
          <ipxact:displayName>Read wait</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerIncomingSignals" type="bit">
          <ipxact:name>registerIncomingSignals</ipxact:name>
          <ipxact:displayName>Register incoming signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerOutgoingSignals" type="bit">
          <ipxact:name>registerOutgoingSignals</ipxact:name>
          <ipxact:displayName>Register outgoing signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="setupTime" type="int">
          <ipxact:name>setupTime</ipxact:name>
          <ipxact:displayName>Setup</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="timingUnits" type="string">
          <ipxact:name>timingUnits</ipxact:name>
          <ipxact:displayName>Timing units</ipxact:displayName>
          <ipxact:value>Cycles</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="waitrequestAllowance" type="int">
          <ipxact:name>waitrequestAllowance</ipxact:name>
          <ipxact:displayName>Waitrequest allowance</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeWaitTime" type="int">
          <ipxact:name>writeWaitTime</ipxact:name>
          <ipxact:displayName>Write wait</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rxm_bar4</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>address</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar4_address_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>byteenable</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar4_byteenable_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>readdata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar4_readdata_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>writedata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar4_writedata_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>read</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar4_read_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>write</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar4_write_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>burstcount</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar4_burstcount_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>readdatavalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar4_readdatavalid_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>waitrequest</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_bar4_waitrequest_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:master></ipxact:master>
      <ipxact:parameters>
        <ipxact:parameter parameterId="adaptsTo" type="string">
          <ipxact:name>adaptsTo</ipxact:name>
          <ipxact:displayName>Adapts to</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressGroup" type="int">
          <ipxact:name>addressGroup</ipxact:name>
          <ipxact:displayName>Address group</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressUnits" type="string">
          <ipxact:name>addressUnits</ipxact:name>
          <ipxact:displayName>Address units</ipxact:displayName>
          <ipxact:value>SYMBOLS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="alwaysBurstMaxBurst" type="bit">
          <ipxact:name>alwaysBurstMaxBurst</ipxact:name>
          <ipxact:displayName>Always burst maximum burst</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value>coreclkout_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>Associated reset</ipxact:displayName>
          <ipxact:value>app_nreset_status</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bitsPerSymbol" type="int">
          <ipxact:name>bitsPerSymbol</ipxact:name>
          <ipxact:displayName>Bits per symbol</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstOnBurstBoundariesOnly" type="bit">
          <ipxact:name>burstOnBurstBoundariesOnly</ipxact:name>
          <ipxact:displayName>Burst on burst boundaries only</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstcountUnits" type="string">
          <ipxact:name>burstcountUnits</ipxact:name>
          <ipxact:displayName>Burstcount units</ipxact:displayName>
          <ipxact:value>WORDS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="constantBurstBehavior" type="bit">
          <ipxact:name>constantBurstBehavior</ipxact:name>
          <ipxact:displayName>Constant burst behavior</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dBSBigEndian" type="bit">
          <ipxact:name>dBSBigEndian</ipxact:name>
          <ipxact:displayName>dBS big endian</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="doStreamReads" type="bit">
          <ipxact:name>doStreamReads</ipxact:name>
          <ipxact:displayName>Use flow control for read transfers</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="doStreamWrites" type="bit">
          <ipxact:name>doStreamWrites</ipxact:name>
          <ipxact:displayName>Use flow control for write transfers</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="holdTime" type="int">
          <ipxact:name>holdTime</ipxact:name>
          <ipxact:displayName>Hold</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="interleaveBursts" type="bit">
          <ipxact:name>interleaveBursts</ipxact:name>
          <ipxact:displayName>Interleave bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isAsynchronous" type="bit">
          <ipxact:name>isAsynchronous</ipxact:name>
          <ipxact:displayName>Is asynchronous</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isBigEndian" type="bit">
          <ipxact:name>isBigEndian</ipxact:name>
          <ipxact:displayName>Is big endian</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isReadable" type="bit">
          <ipxact:name>isReadable</ipxact:name>
          <ipxact:displayName>Is readable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isWriteable" type="bit">
          <ipxact:name>isWriteable</ipxact:name>
          <ipxact:displayName>Is writeable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="linewrapBursts" type="bit">
          <ipxact:name>linewrapBursts</ipxact:name>
          <ipxact:displayName>Linewrap bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maxAddressWidth" type="int">
          <ipxact:name>maxAddressWidth</ipxact:name>
          <ipxact:displayName>Maximum address width</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingReadTransactions" type="int">
          <ipxact:name>maximumPendingReadTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending read transactions</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingWriteTransactions" type="int">
          <ipxact:name>maximumPendingWriteTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending write transactions</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumReadLatency" type="int">
          <ipxact:name>minimumReadLatency</ipxact:name>
          <ipxact:displayName>minimumReadLatency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumResponseLatency" type="int">
          <ipxact:name>minimumResponseLatency</ipxact:name>
          <ipxact:displayName>Minimum response latency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readLatency" type="int">
          <ipxact:name>readLatency</ipxact:name>
          <ipxact:displayName>Read latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readWaitTime" type="int">
          <ipxact:name>readWaitTime</ipxact:name>
          <ipxact:displayName>Read wait</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerIncomingSignals" type="bit">
          <ipxact:name>registerIncomingSignals</ipxact:name>
          <ipxact:displayName>Register incoming signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerOutgoingSignals" type="bit">
          <ipxact:name>registerOutgoingSignals</ipxact:name>
          <ipxact:displayName>Register outgoing signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="setupTime" type="int">
          <ipxact:name>setupTime</ipxact:name>
          <ipxact:displayName>Setup</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="timingUnits" type="string">
          <ipxact:name>timingUnits</ipxact:name>
          <ipxact:displayName>Timing units</ipxact:displayName>
          <ipxact:value>Cycles</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="waitrequestAllowance" type="int">
          <ipxact:name>waitrequestAllowance</ipxact:name>
          <ipxact:displayName>Waitrequest allowance</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeWaitTime" type="int">
          <ipxact:name>writeWaitTime</ipxact:name>
          <ipxact:displayName>Write wait</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rxm_irq</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="interrupt" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="interrupt" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>irq</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxm_irq_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:master></ipxact:master>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedAddressablePoint" type="string">
          <ipxact:name>associatedAddressablePoint</ipxact:name>
          <ipxact:displayName>Associated addressable interface</ipxact:displayName>
          <ipxact:value>pcie.rxm_bar0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>Associated reset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="irqMap" type="string">
          <ipxact:name>irqMap</ipxact:name>
          <ipxact:displayName>IRQ Map</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="irqScheme" type="string">
          <ipxact:name>irqScheme</ipxact:name>
          <ipxact:displayName>Interrupt scheme</ipxact:displayName>
          <ipxact:value>INDIVIDUAL_REQUESTS</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>cra</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>chipselect</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>cra_chipselect_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>address</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>cra_address_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>byteenable</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>cra_byteenable_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>read</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>cra_read_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>readdata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>cra_readdata_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>write</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>cra_write_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>writedata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>cra_writedata_i</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>waitrequest</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>cra_waitrequest_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>readdatavalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>cra_readdatavalid_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="addressAlignment" type="string">
          <ipxact:name>addressAlignment</ipxact:name>
          <ipxact:displayName>Slave addressing</ipxact:displayName>
          <ipxact:value>DYNAMIC</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressGroup" type="int">
          <ipxact:name>addressGroup</ipxact:name>
          <ipxact:displayName>Address group</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressSpan" type="string">
          <ipxact:name>addressSpan</ipxact:name>
          <ipxact:displayName>Address span</ipxact:displayName>
          <ipxact:value>32768</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressUnits" type="string">
          <ipxact:name>addressUnits</ipxact:name>
          <ipxact:displayName>Address units</ipxact:displayName>
          <ipxact:value>SYMBOLS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="alwaysBurstMaxBurst" type="bit">
          <ipxact:name>alwaysBurstMaxBurst</ipxact:name>
          <ipxact:displayName>Always burst maximum burst</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value>coreclkout_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>Associated reset</ipxact:displayName>
          <ipxact:value>app_nreset_status</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bitsPerSymbol" type="int">
          <ipxact:name>bitsPerSymbol</ipxact:name>
          <ipxact:displayName>Bits per symbol</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bridgedAddressOffset" type="string">
          <ipxact:name>bridgedAddressOffset</ipxact:name>
          <ipxact:displayName>Bridged Address Offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bridgesToMaster" type="string">
          <ipxact:name>bridgesToMaster</ipxact:name>
          <ipxact:displayName>Bridges to master</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstOnBurstBoundariesOnly" type="bit">
          <ipxact:name>burstOnBurstBoundariesOnly</ipxact:name>
          <ipxact:displayName>Burst on burst boundaries only</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstcountUnits" type="string">
          <ipxact:name>burstcountUnits</ipxact:name>
          <ipxact:displayName>Burstcount units</ipxact:displayName>
          <ipxact:value>WORDS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="constantBurstBehavior" type="bit">
          <ipxact:name>constantBurstBehavior</ipxact:name>
          <ipxact:displayName>Constant burst behavior</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="explicitAddressSpan" type="string">
          <ipxact:name>explicitAddressSpan</ipxact:name>
          <ipxact:displayName>Explicit address span</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="holdTime" type="int">
          <ipxact:name>holdTime</ipxact:name>
          <ipxact:displayName>Hold</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="interleaveBursts" type="bit">
          <ipxact:name>interleaveBursts</ipxact:name>
          <ipxact:displayName>Interleave bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isBigEndian" type="bit">
          <ipxact:name>isBigEndian</ipxact:name>
          <ipxact:displayName>Big endian</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isFlash" type="bit">
          <ipxact:name>isFlash</ipxact:name>
          <ipxact:displayName>Flash memory</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isMemoryDevice" type="bit">
          <ipxact:name>isMemoryDevice</ipxact:name>
          <ipxact:displayName>Memory device</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isNonVolatileStorage" type="bit">
          <ipxact:name>isNonVolatileStorage</ipxact:name>
          <ipxact:displayName>Non-volatile storage</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="linewrapBursts" type="bit">
          <ipxact:name>linewrapBursts</ipxact:name>
          <ipxact:displayName>Linewrap bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingReadTransactions" type="int">
          <ipxact:name>maximumPendingReadTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending read transactions</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingWriteTransactions" type="int">
          <ipxact:name>maximumPendingWriteTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending write transactions</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumReadLatency" type="int">
          <ipxact:name>minimumReadLatency</ipxact:name>
          <ipxact:displayName>minimumReadLatency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumResponseLatency" type="int">
          <ipxact:name>minimumResponseLatency</ipxact:name>
          <ipxact:displayName>Minimum response latency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumUninterruptedRunLength" type="int">
          <ipxact:name>minimumUninterruptedRunLength</ipxact:name>
          <ipxact:displayName>Minimum uninterrupted run length</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="printableDevice" type="bit">
          <ipxact:name>printableDevice</ipxact:name>
          <ipxact:displayName>Can receive stdout/stderr</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readLatency" type="int">
          <ipxact:name>readLatency</ipxact:name>
          <ipxact:displayName>Read latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readWaitStates" type="int">
          <ipxact:name>readWaitStates</ipxact:name>
          <ipxact:displayName>Read wait states</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readWaitTime" type="int">
          <ipxact:name>readWaitTime</ipxact:name>
          <ipxact:displayName>Read wait</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerIncomingSignals" type="bit">
          <ipxact:name>registerIncomingSignals</ipxact:name>
          <ipxact:displayName>Register incoming signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerOutgoingSignals" type="bit">
          <ipxact:name>registerOutgoingSignals</ipxact:name>
          <ipxact:displayName>Register outgoing signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="setupTime" type="int">
          <ipxact:name>setupTime</ipxact:name>
          <ipxact:displayName>Setup</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="timingUnits" type="string">
          <ipxact:name>timingUnits</ipxact:name>
          <ipxact:displayName>Timing units</ipxact:displayName>
          <ipxact:value>Cycles</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="transparentBridge" type="bit">
          <ipxact:name>transparentBridge</ipxact:name>
          <ipxact:displayName>Transparent bridge</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="waitrequestAllowance" type="int">
          <ipxact:name>waitrequestAllowance</ipxact:name>
          <ipxact:displayName>Waitrequest allowance</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="wellBehavedWaitrequest" type="bit">
          <ipxact:name>wellBehavedWaitrequest</ipxact:name>
          <ipxact:displayName>Well-behaved waitrequest</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeLatency" type="int">
          <ipxact:name>writeLatency</ipxact:name>
          <ipxact:displayName>Write latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeWaitStates" type="int">
          <ipxact:name>writeWaitStates</ipxact:name>
          <ipxact:displayName>Write wait states</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeWaitTime" type="int">
          <ipxact:name>writeWaitTime</ipxact:name>
          <ipxact:displayName>Write wait</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="embeddedsw.configuration.isFlash" type="string">
              <ipxact:name>embeddedsw.configuration.isFlash</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="embeddedsw.configuration.isMemoryDevice" type="string">
              <ipxact:name>embeddedsw.configuration.isMemoryDevice</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="embeddedsw.configuration.isNonVolatileStorage" type="string">
              <ipxact:name>embeddedsw.configuration.isNonVolatileStorage</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="embeddedsw.configuration.isPrintableDevice" type="string">
              <ipxact:name>embeddedsw.configuration.isPrintableDevice</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>cra_irq</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="interrupt" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="interrupt" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>irq</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>cra_irq_o</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedAddressablePoint" type="string">
          <ipxact:name>associatedAddressablePoint</ipxact:name>
          <ipxact:displayName>Associated addressable interface</ipxact:displayName>
          <ipxact:value>pcie.cra</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>Associated reset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bridgedReceiverOffset" type="longint">
          <ipxact:name>bridgedReceiverOffset</ipxact:name>
          <ipxact:displayName>Bridged receiver offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bridgesToReceiver" type="string">
          <ipxact:name>bridgesToReceiver</ipxact:name>
          <ipxact:displayName>Bridges to receiver</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="irqScheme" type="string">
          <ipxact:name>irqScheme</ipxact:name>
          <ipxact:displayName>Interrupt scheme</ipxact:displayName>
          <ipxact:value>NONE</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>hip_ctrl</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>simu_mode_pipe</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>simu_mode_pipe</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>test_in</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>test_in</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>hip_pipe</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>sim_pipe_pclk_in</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>sim_pipe_pclk_in</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>sim_pipe_rate</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>sim_pipe_rate</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>sim_ltssmstate</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>sim_ltssmstate</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>txdata0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txdata0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>txdatak0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txdatak0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>txcompl0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txcompl0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>txelecidle0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txelecidle0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>txdetectrx0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txdetectrx0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>powerdown0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>powerdown0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>txmargin0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txmargin0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>txdeemph0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txdeemph0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>txswing0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txswing0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>txsynchd0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txsynchd0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>txblkst0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txblkst0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>txdataskip0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>txdataskip0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rate0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rate0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rxpolarity0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxpolarity0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>currentrxpreset0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>currentrxpreset0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>currentcoeff0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>currentcoeff0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rxeqeval0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxeqeval0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rxeqinprogress0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxeqinprogress0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>invalidreq0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>invalidreq0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rxdata0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxdata0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rxdatak0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxdatak0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>phystatus0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>phystatus0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rxvalid0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxvalid0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rxstatus0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxstatus0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rxelecidle0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxelecidle0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rxsynchd0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxsynchd0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rxblkst0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxblkst0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rxdataskip0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rxdataskip0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>dirfeedback0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>dirfeedback0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>sim_pipe_mask_tx_pll_lock</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>sim_pipe_mask_tx_pll_lock</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>hip_serial</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_in0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_in0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>tx_out0</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_out0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
  </ipxact:busInterfaces>
  <ipxact:model>
    <ipxact:views>
      <ipxact:view>
        <ipxact:name>QUARTUS_SYNTH</ipxact:name>
        <ipxact:envIdentifier>:quartus.altera.com:</ipxact:envIdentifier>
        <ipxact:componentInstantiationRef>QUARTUS_SYNTH</ipxact:componentInstantiationRef>
      </ipxact:view>
    </ipxact:views>
    <ipxact:instantiations>
      <ipxact:componentInstantiation>
        <ipxact:name>QUARTUS_SYNTH</ipxact:name>
        <ipxact:moduleName>altera_pcie_s10_hip_avmm_bridge</ipxact:moduleName>
        <ipxact:fileSetRef>
          <ipxact:localName>QUARTUS_SYNTH</ipxact:localName>
        </ipxact:fileSetRef>
      </ipxact:componentInstantiation>
    </ipxact:instantiations>
    <ipxact:ports>
      <ipxact:port>
        <ipxact:name>refclk</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>coreclkout_hip</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>npor</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>pin_perst</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>app_nreset_status</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>ninit_done</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txs_address_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txs_chipselect_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txs_byteenable_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>7</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txs_readdata_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txs_writedata_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txs_read_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txs_write_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txs_burstcount_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>6</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txs_readdatavalid_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txs_waitrequest_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar0_address_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar0_byteenable_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>7</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar0_readdata_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar0_writedata_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar0_read_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar0_write_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar0_readdatavalid_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar0_waitrequest_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar2_address_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar2_byteenable_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>7</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar2_readdata_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar2_writedata_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar2_read_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar2_write_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar2_burstcount_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>6</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar2_readdatavalid_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar2_waitrequest_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar4_address_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar4_byteenable_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>7</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar4_readdata_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar4_writedata_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>63</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar4_read_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar4_write_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar4_burstcount_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>6</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar4_readdatavalid_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_bar4_waitrequest_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxm_irq_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>15</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>cra_chipselect_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>cra_address_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>14</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>cra_byteenable_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>3</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>cra_read_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>cra_readdata_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>31</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>cra_write_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>cra_writedata_i</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>31</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>cra_waitrequest_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>cra_readdatavalid_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>cra_irq_o</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>simu_mode_pipe</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>test_in</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>66</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>sim_pipe_pclk_in</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>sim_pipe_rate</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>1</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>sim_ltssmstate</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>5</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txdata0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>31</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txdatak0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>3</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txcompl0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txelecidle0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txdetectrx0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>powerdown0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>1</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txmargin0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>2</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txdeemph0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txswing0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txsynchd0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>1</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txblkst0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>txdataskip0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rate0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>1</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxpolarity0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>currentrxpreset0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>2</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>currentcoeff0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>17</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxeqeval0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxeqinprogress0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>invalidreq0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxdata0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>31</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxdatak0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>3</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>phystatus0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxvalid0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxstatus0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>2</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxelecidle0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxsynchd0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>1</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxblkst0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rxdataskip0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>dirfeedback0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>5</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>sim_pipe_mask_tx_pll_lock</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_in0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_out0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
    </ipxact:ports>
  </ipxact:model>
  <ipxact:vendorExtensions>
    <altera:entity_info>
      <ipxact:vendor>Intel Corporation</ipxact:vendor>
      <ipxact:library>pcie</ipxact:library>
      <ipxact:name>altera_pcie_s10_hip_avmm_bridge</ipxact:name>
      <ipxact:version>20.0.0</ipxact:version>
    </altera:entity_info>
    <altera:altera_module_parameters>
      <ipxact:parameters>
        <ipxact:parameter parameterId="interface_type_hwtcl" type="string">
          <ipxact:name>interface_type_hwtcl</ipxact:name>
          <ipxact:displayName>Application interface type</ipxact:displayName>
          <ipxact:value>Avalon-MM</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device_die_types" type="string">
          <ipxact:name>device_die_types</ipxact:name>
          <ipxact:displayName>device_die_types</ipxact:displayName>
          <ipxact:value>HSSI_CRETE2E,HSSI_CRETE3,MAIN_ND4H,UIB_HBM</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device_die_revisions" type="string">
          <ipxact:name>device_die_revisions</ipxact:name>
          <ipxact:displayName>device_die_revisions</ipxact:displayName>
          <ipxact:value>HSSI_CRETE2E_REVB,HSSI_CRETE3_REVA,MAIN_ND4H_REVB,UIB_HBM_REVB</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="app_interface_width_hwtcl" type="string">
          <ipxact:name>app_interface_width_hwtcl</ipxact:name>
          <ipxact:displayName>Application interface width</ipxact:displayName>
          <ipxact:value>64-bit</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="app_interface_freq_hwtcl" type="string">
          <ipxact:name>app_interface_freq_hwtcl</ipxact:name>
          <ipxact:displayName>Application interface frequency</ipxact:displayName>
          <ipxact:value>125 MHz</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="wrala_hwtcl" type="string">
          <ipxact:name>wrala_hwtcl</ipxact:name>
          <ipxact:displayName>Hard IP Mode</ipxact:displayName>
          <ipxact:value>Gen3x1, Interface - 64 bit, 125 MHz</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="wrala_integer_hwtcl" type="int">
          <ipxact:name>wrala_integer_hwtcl</ipxact:name>
          <ipxact:displayName>Hard IP Mode Integer</ipxact:displayName>
          <ipxact:value>14</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="select_design_example_hwtcl" type="string">
          <ipxact:name>select_design_example_hwtcl</ipxact:name>
          <ipxact:displayName>Select design</ipxact:displayName>
          <ipxact:value>PIO</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="crete_type" type="int">
          <ipxact:name>crete_type</ipxact:name>
          <ipxact:displayName>crete_type</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_rp_ep_mode_hwtcl" type="string">
          <ipxact:name>virtual_rp_ep_mode_hwtcl</ipxact:name>
          <ipxact:displayName>Port type</ipxact:displayName>
          <ipxact:value>Native Endpoint</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_rp_ep_mode_integer_hwtcl" type="int">
          <ipxact:name>virtual_rp_ep_mode_integer_hwtcl</ipxact:name>
          <ipxact:displayName>virtual_rp_ep_mode_integer_hwtcl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_ep_native_hwtcl" type="string">
          <ipxact:name>virtual_ep_native_hwtcl</ipxact:name>
          <ipxact:displayName>virtual_ep_native_hwtcl</ipxact:displayName>
          <ipxact:value>Native</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_link_width_hwtcl" type="string">
          <ipxact:name>virtual_link_width_hwtcl</ipxact:name>
          <ipxact:displayName>Number of lanes</ipxact:displayName>
          <ipxact:value>x1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_link_width_integer_hwtcl" type="int">
          <ipxact:name>virtual_link_width_integer_hwtcl</ipxact:name>
          <ipxact:displayName>virtual_link_width_integer_hwtcl</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_link_rate_hwtcl" type="string">
          <ipxact:name>virtual_link_rate_hwtcl</ipxact:name>
          <ipxact:displayName>Lane rate</ipxact:displayName>
          <ipxact:value>Gen3 (8.0 Gbps)</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_link_rate_integer_hwtcl" type="int">
          <ipxact:name>virtual_link_rate_integer_hwtcl</ipxact:name>
          <ipxact:displayName>virtual_link_rate_integer_hwtcl</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_txeq_mode_hwtcl" type="string">
          <ipxact:name>virtual_txeq_mode_hwtcl</ipxact:name>
          <ipxact:displayName>virtual_txeq_mode_hwtcl</ipxact:displayName>
          <ipxact:value>gen3_cr2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="interface_type_integer_hwtcl" type="int">
          <ipxact:name>interface_type_integer_hwtcl</ipxact:name>
          <ipxact:displayName>interface_type_integer_hwtcl</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_rx_buffer_limit_ports_hwtcl" type="int">
          <ipxact:name>enable_rx_buffer_limit_ports_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Rx Buffer Limit Ports </ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_np_buffer_limit_bypass_hwtcl" type="int">
          <ipxact:name>rx_np_buffer_limit_bypass_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Non-Posted Rx Buffer Limit Bypass</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_p_buffer_limit_bypass_hwtcl" type="int">
          <ipxact:name>rx_p_buffer_limit_bypass_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Posted Rx Buffer Limit Bypass</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_cpl_buffer_limit_bypass_hwtcl" type="int">
          <ipxact:name>rx_cpl_buffer_limit_bypass_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Completion Rx Buffer Limit Bypass</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar0_type_integer_hwtcl" type="int">
          <ipxact:name>pf0_bar0_type_integer_hwtcl</ipxact:name>
          <ipxact:displayName>pf0_bar0_type_integer_hwtcl</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar1_type_integer_hwtcl" type="int">
          <ipxact:name>pf0_bar1_type_integer_hwtcl</ipxact:name>
          <ipxact:displayName>pf0_bar1_type_integer_hwtcl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar2_type_integer_hwtcl" type="int">
          <ipxact:name>pf0_bar2_type_integer_hwtcl</ipxact:name>
          <ipxact:displayName>pf0_bar2_type_integer_hwtcl</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar3_type_integer_hwtcl" type="int">
          <ipxact:name>pf0_bar3_type_integer_hwtcl</ipxact:name>
          <ipxact:displayName>pf0_bar3_type_integer_hwtcl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar4_type_integer_hwtcl" type="int">
          <ipxact:name>pf0_bar4_type_integer_hwtcl</ipxact:name>
          <ipxact:displayName>pf0_bar4_type_integer_hwtcl</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar5_type_integer_hwtcl" type="int">
          <ipxact:name>pf0_bar5_type_integer_hwtcl</ipxact:name>
          <ipxact:displayName>pf0_bar5_type_integer_hwtcl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar0_type_gui_hwtcl" type="string">
          <ipxact:name>pf0_bar0_type_gui_hwtcl</ipxact:name>
          <ipxact:displayName>Type</ipxact:displayName>
          <ipxact:value>32-bit non-prefetchable memory</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar0_type_hwtcl" type="string">
          <ipxact:name>pf0_bar0_type_hwtcl</ipxact:name>
          <ipxact:displayName>pf0_bar0_type_hwtcl</ipxact:displayName>
          <ipxact:value>32-bit non-prefetchable memory</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar0_address_width_hwtcl" type="int">
          <ipxact:name>pf0_bar0_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar0_address_width_mask_hwtcl" type="int">
          <ipxact:name>pf0_bar0_address_width_mask_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar0_enable_rxm_burst_hwtcl" type="int">
          <ipxact:name>pf0_bar0_enable_rxm_burst_hwtcl</ipxact:name>
          <ipxact:displayName>Enable burst capability for Avalon-MM BAR0 Master port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar1_type_hwtcl" type="string">
          <ipxact:name>pf0_bar1_type_hwtcl</ipxact:name>
          <ipxact:displayName>Type</ipxact:displayName>
          <ipxact:value>Disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar1_address_width_hwtcl" type="int">
          <ipxact:name>pf0_bar1_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar1_address_width_mask_hwtcl" type="int">
          <ipxact:name>pf0_bar1_address_width_mask_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar1_enable_rxm_burst_hwtcl" type="int">
          <ipxact:name>pf0_bar1_enable_rxm_burst_hwtcl</ipxact:name>
          <ipxact:displayName>Enable burst capability for RXM Avalon-MM BAR1 Master port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar2_type_hwtcl" type="string">
          <ipxact:name>pf0_bar2_type_hwtcl</ipxact:name>
          <ipxact:displayName>Type</ipxact:displayName>
          <ipxact:value>64-bit prefetchable memory</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar2_address_width_hwtcl" type="int">
          <ipxact:name>pf0_bar2_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar2_address_width_mask_hwtcl" type="int">
          <ipxact:name>pf0_bar2_address_width_mask_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar2_enable_rxm_burst_hwtcl" type="int">
          <ipxact:name>pf0_bar2_enable_rxm_burst_hwtcl</ipxact:name>
          <ipxact:displayName>Enable burst capability for RXM Avalon-MM BAR2 Master port</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar3_type_hwtcl" type="string">
          <ipxact:name>pf0_bar3_type_hwtcl</ipxact:name>
          <ipxact:displayName>Type</ipxact:displayName>
          <ipxact:value>Disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar3_address_width_hwtcl" type="int">
          <ipxact:name>pf0_bar3_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar3_address_width_mask_hwtcl" type="int">
          <ipxact:name>pf0_bar3_address_width_mask_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>28</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar3_enable_rxm_burst_hwtcl" type="int">
          <ipxact:name>pf0_bar3_enable_rxm_burst_hwtcl</ipxact:name>
          <ipxact:displayName>Enable burst capability for RXM Avalon-MM BAR3 Master port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar4_type_hwtcl" type="string">
          <ipxact:name>pf0_bar4_type_hwtcl</ipxact:name>
          <ipxact:displayName>Type</ipxact:displayName>
          <ipxact:value>64-bit prefetchable memory</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar4_address_width_hwtcl" type="int">
          <ipxact:name>pf0_bar4_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar4_address_width_mask_hwtcl" type="int">
          <ipxact:name>pf0_bar4_address_width_mask_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar4_enable_rxm_burst_hwtcl" type="int">
          <ipxact:name>pf0_bar4_enable_rxm_burst_hwtcl</ipxact:name>
          <ipxact:displayName>Enable burst capability for RXM Avalon-MM BAR4 Master port</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar5_type_hwtcl" type="string">
          <ipxact:name>pf0_bar5_type_hwtcl</ipxact:name>
          <ipxact:displayName>Type</ipxact:displayName>
          <ipxact:value>Disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar5_address_width_hwtcl" type="int">
          <ipxact:name>pf0_bar5_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar5_address_width_mask_hwtcl" type="int">
          <ipxact:name>pf0_bar5_address_width_mask_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>28</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar5_enable_rxm_burst_hwtcl" type="int">
          <ipxact:name>pf0_bar5_enable_rxm_burst_hwtcl</ipxact:name>
          <ipxact:displayName>Enable burst capability for RXM Avalon-MM BAR5 Master port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="force_address_width_hwtcl" type="int">
          <ipxact:name>force_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>force_address_width_hwtcl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_expansion_base_address_register_hwtcl" type="int">
          <ipxact:name>pf0_expansion_base_address_register_hwtcl</ipxact:name>
          <ipxact:displayName>Size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_rom_bar_enabled_hwtcl" type="string">
          <ipxact:name>pf0_rom_bar_enabled_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Expansion ROM</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_auto_lane_flip_ctrl_en_hwtcl" type="string">
          <ipxact:name>pf0_auto_lane_flip_ctrl_en_hwtcl</ipxact:name>
          <ipxact:displayName>Enable auto lane reversal</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_loopback_enable_hwtcl" type="int">
          <ipxact:name>pf0_loopback_enable_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Loopback Master</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="avmm_addr_width_hwtcl" type="int">
          <ipxact:name>avmm_addr_width_hwtcl</ipxact:name>
          <ipxact:displayName>Avalon-MM address width</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="avmm_number_of_tags_hwtcl" type="int">
          <ipxact:name>avmm_number_of_tags_hwtcl</ipxact:name>
          <ipxact:displayName>Avalon-MM number of tags</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dma_enabled_hwtcl" type="int">
          <ipxact:name>dma_enabled_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Avalon-MM DMA.</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dma_controller_enabled_hwtcl" type="int">
          <ipxact:name>dma_controller_enabled_hwtcl</ipxact:name>
          <ipxact:displayName>Instantiate internal descriptor controller</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_cra_slave_port_hwtcl" type="int">
          <ipxact:name>enable_cra_slave_port_hwtcl</ipxact:name>
          <ipxact:displayName>Enable control register access (CRA) Avalon-MM slave port</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_advanced_interrupt_hwtcl" type="int">
          <ipxact:name>enable_advanced_interrupt_hwtcl</ipxact:name>
          <ipxact:displayName>Export MSI/MSI-X conduit interfaces</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_hip_status_for_avmm_hwtcl" type="int">
          <ipxact:name>enable_hip_status_for_avmm_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Hard IP Status Bus when using the Avalon-MM interface</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="txs_enabled_hwtcl" type="int">
          <ipxact:name>txs_enabled_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Avalon-MM Slave interface with individual byte access. (TXS).</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="user_txs_address_width_hwtcl" type="int">
          <ipxact:name>user_txs_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>Address width of accessible PCIe memory space(TXS)</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hptxs_enabled_hwtcl" type="int">
          <ipxact:name>hptxs_enabled_hwtcl</ipxact:name>
          <ipxact:displayName>Enable High Performance bursting Avalon-MM Slave interface (HPTXS).</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hptxs_enabled_mapping_hwtcl" type="int">
          <ipxact:name>hptxs_enabled_mapping_hwtcl</ipxact:name>
          <ipxact:displayName>Enable mapping (HPTXS)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="user_hptxs_address_width_hwtcl" type="int">
          <ipxact:name>user_hptxs_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>Address width of accessible PCIe memory space (HPTXS)</ipxact:displayName>
          <ipxact:value>25</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hptxs_address_translation_table_address_width_hwtcl" type="int">
          <ipxact:name>hptxs_address_translation_table_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>Number of address pages (HPTXS)</ipxact:displayName>
          <ipxact:value>9</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hptxs_address_translation_window_address_width_hwtcl" type="int">
          <ipxact:name>hptxs_address_translation_window_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>Size of address pages (HPTXS)</ipxact:displayName>
          <ipxact:value>16</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="txs_address_width_hwtcl" type="int">
          <ipxact:name>txs_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>txs_address_width_hwtcl</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="txs_data_width_hwtcl" type="int">
          <ipxact:name>txs_data_width_hwtcl</ipxact:name>
          <ipxact:displayName>txs_data_width_hwtcl</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hptxs_address_width_hwtcl" type="int">
          <ipxact:name>hptxs_address_width_hwtcl</ipxact:name>
          <ipxact:displayName>hptxs_address_width_hwtcl</ipxact:displayName>
          <ipxact:value>25</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_64adapter_hwtcl" type="int">
          <ipxact:name>enable_64adapter_hwtcl</ipxact:name>
          <ipxact:displayName>enable_64adapter_hwtcl</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_plladapter_hwtcl" type="int">
          <ipxact:name>enable_plladapter_hwtcl</ipxact:name>
          <ipxact:displayName>enable_plladapter_hwtcl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cg_impl_cra_av_slave_port_hwtcl" type="int">
          <ipxact:name>cg_impl_cra_av_slave_port_hwtcl</ipxact:name>
          <ipxact:displayName>Enable control register access (CRA) Avalon-MM slave port</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cg_enable_a2p_interrupt_hwtcl" type="int">
          <ipxact:name>cg_enable_a2p_interrupt_hwtcl</ipxact:name>
          <ipxact:displayName>Enable PCIe interrupt at power-on</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="user_txs_addr_width_hwtcl" type="int">
          <ipxact:name>user_txs_addr_width_hwtcl</ipxact:name>
          <ipxact:displayName>Address width of accessible PCIe memory space</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cg_a2p_addr_map_num_entries_hwtcl" type="int">
          <ipxact:name>cg_a2p_addr_map_num_entries_hwtcl</ipxact:name>
          <ipxact:displayName>Number of address pages</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cg_a2p_addr_map_pass_thru_bits_hwtcl" type="int">
          <ipxact:name>cg_a2p_addr_map_pass_thru_bits_hwtcl</ipxact:name>
          <ipxact:displayName>Size of address pages</ipxact:displayName>
          <ipxact:value>12</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dma_instantiate_controller_hwtcl" type="int">
          <ipxact:name>dma_instantiate_controller_hwtcl</ipxact:name>
          <ipxact:displayName>dma_instantiate_controller_hwtcl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_width_integer_rxm0_hwtcl" type="int">
          <ipxact:name>data_width_integer_rxm0_hwtcl</ipxact:name>
          <ipxact:displayName>data_width_integer_rxm0_hwtcl</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_byte_width_integer_rxm0_hwtcl" type="int">
          <ipxact:name>data_byte_width_integer_rxm0_hwtcl</ipxact:name>
          <ipxact:displayName>data_byte_width_integer_rxm0_hwtcl</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_burstcount_integer_rxm0_hwtcl" type="int">
          <ipxact:name>data_burstcount_integer_rxm0_hwtcl</ipxact:name>
          <ipxact:displayName>data_burstcount_integer_rxm0_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_width_integer_rxm1_hwtcl" type="int">
          <ipxact:name>data_width_integer_rxm1_hwtcl</ipxact:name>
          <ipxact:displayName>data_width_integer_rxm1_hwtcl</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_byte_width_integer_rxm1_hwtcl" type="int">
          <ipxact:name>data_byte_width_integer_rxm1_hwtcl</ipxact:name>
          <ipxact:displayName>data_byte_width_integer_rxm1_hwtcl</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_burstcount_integer_rxm1_hwtcl" type="int">
          <ipxact:name>data_burstcount_integer_rxm1_hwtcl</ipxact:name>
          <ipxact:displayName>data_burstcount_integer_rxm1_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_width_integer_rxm2_hwtcl" type="int">
          <ipxact:name>data_width_integer_rxm2_hwtcl</ipxact:name>
          <ipxact:displayName>data_width_integer_rxm2_hwtcl</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_byte_width_integer_rxm2_hwtcl" type="int">
          <ipxact:name>data_byte_width_integer_rxm2_hwtcl</ipxact:name>
          <ipxact:displayName>data_byte_width_integer_rxm2_hwtcl</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_burstcount_integer_rxm2_hwtcl" type="int">
          <ipxact:name>data_burstcount_integer_rxm2_hwtcl</ipxact:name>
          <ipxact:displayName>data_burstcount_integer_rxm2_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_width_integer_rxm3_hwtcl" type="int">
          <ipxact:name>data_width_integer_rxm3_hwtcl</ipxact:name>
          <ipxact:displayName>data_width_integer_rxm3_hwtcl</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_byte_width_integer_rxm3_hwtcl" type="int">
          <ipxact:name>data_byte_width_integer_rxm3_hwtcl</ipxact:name>
          <ipxact:displayName>data_byte_width_integer_rxm3_hwtcl</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_burstcount_integer_rxm3_hwtcl" type="int">
          <ipxact:name>data_burstcount_integer_rxm3_hwtcl</ipxact:name>
          <ipxact:displayName>data_burstcount_integer_rxm3_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_width_integer_rxm4_hwtcl" type="int">
          <ipxact:name>data_width_integer_rxm4_hwtcl</ipxact:name>
          <ipxact:displayName>data_width_integer_rxm4_hwtcl</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_byte_width_integer_rxm4_hwtcl" type="int">
          <ipxact:name>data_byte_width_integer_rxm4_hwtcl</ipxact:name>
          <ipxact:displayName>data_byte_width_integer_rxm4_hwtcl</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_burstcount_integer_rxm4_hwtcl" type="int">
          <ipxact:name>data_burstcount_integer_rxm4_hwtcl</ipxact:name>
          <ipxact:displayName>data_burstcount_integer_rxm4_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_width_integer_rxm5_hwtcl" type="int">
          <ipxact:name>data_width_integer_rxm5_hwtcl</ipxact:name>
          <ipxact:displayName>data_width_integer_rxm5_hwtcl</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_byte_width_integer_rxm5_hwtcl" type="int">
          <ipxact:name>data_byte_width_integer_rxm5_hwtcl</ipxact:name>
          <ipxact:displayName>data_byte_width_integer_rxm5_hwtcl</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_burstcount_integer_rxm5_hwtcl" type="int">
          <ipxact:name>data_burstcount_integer_rxm5_hwtcl</ipxact:name>
          <ipxact:displayName>data_burstcount_integer_rxm5_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_maxpayload_size_hwtcl" type="string">
          <ipxact:name>virtual_maxpayload_size_hwtcl</ipxact:name>
          <ipxact:displayName>Maximum payload size supported</ipxact:displayName>
          <ipxact:value>512</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_ext_tag_supp_hwtcl" type="int">
          <ipxact:name>pf0_pcie_cap_ext_tag_supp_hwtcl</ipxact:name>
          <ipxact:displayName>Support Extended Tag Field</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_flr_cap_hwtcl" type="string">
          <ipxact:name>pf0_pcie_cap_flr_cap_hwtcl</ipxact:name>
          <ipxact:displayName>Function level reset</ipxact:displayName>
          <ipxact:value>Disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_user_vsec_cap_enable_hwtcl" type="int">
          <ipxact:name>virtual_pf0_user_vsec_cap_enable_hwtcl</ipxact:name>
          <ipxact:displayName>Vendor Specific Extended Capability</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_port_num_hwtcl" type="int">
          <ipxact:name>pf0_pcie_cap_port_num_hwtcl</ipxact:name>
          <ipxact:displayName>Link port number(Root Port only)</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_slot_clk_config_hwtcl" type="int">
          <ipxact:name>pf0_pcie_cap_slot_clk_config_hwtcl</ipxact:name>
          <ipxact:displayName>Slot clock configuration</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msi_multiple_msg_cap_hwtcl" type="string">
          <ipxact:name>pf0_pci_msi_multiple_msg_cap_hwtcl</ipxact:name>
          <ipxact:displayName>Number of MSI messages requested</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msi_64_bit_addr_cap_hwtcl" type="int">
          <ipxact:name>pf0_pci_msi_64_bit_addr_cap_hwtcl</ipxact:name>
          <ipxact:displayName>MSI 64-bit address capable</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_msix_enable_hwtcl" type="int">
          <ipxact:name>virtual_pf0_msix_enable_hwtcl</ipxact:name>
          <ipxact:displayName>Implement MSI-X</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_table_size_hwtcl" type="int">
          <ipxact:name>pf0_pci_msix_table_size_hwtcl</ipxact:name>
          <ipxact:displayName>Table size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_table_offset_hwtcl" type="longint">
          <ipxact:name>pf0_pci_msix_table_offset_hwtcl</ipxact:name>
          <ipxact:displayName>Table offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_bir_hwtcl" type="int">
          <ipxact:name>pf0_pci_msix_bir_hwtcl</ipxact:name>
          <ipxact:displayName>Table BAR indicator</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_pba_offset_hwtcl" type="longint">
          <ipxact:name>pf0_pci_msix_pba_offset_hwtcl</ipxact:name>
          <ipxact:displayName>Pending bit array (PBA) offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_pba_hwtcl" type="int">
          <ipxact:name>pf0_pci_msix_pba_hwtcl</ipxact:name>
          <ipxact:displayName>PBA BAR indicator</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_slot_imp_hwtcl" type="int">
          <ipxact:name>pf0_pcie_slot_imp_hwtcl</ipxact:name>
          <ipxact:displayName>Use Slot Power registers (Root Port only)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_slot_power_limit_value_hwtcl" type="int">
          <ipxact:name>pf0_pcie_cap_slot_power_limit_value_hwtcl</ipxact:name>
          <ipxact:displayName>Slot power scale</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_slot_power_limit_scale_hwtcl" type="int">
          <ipxact:name>pf0_pcie_cap_slot_power_limit_scale_hwtcl</ipxact:name>
          <ipxact:displayName>Slot power limit</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_phy_slot_num_hwtcl" type="int">
          <ipxact:name>pf0_pcie_cap_phy_slot_num_hwtcl</ipxact:name>
          <ipxact:displayName>Slot number</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_ep_l0s_accpt_latency_hwtcl" type="int">
          <ipxact:name>pf0_pcie_cap_ep_l0s_accpt_latency_hwtcl</ipxact:name>
          <ipxact:displayName>Endpoint L0s acceptable latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_ep_l1_accpt_latency_hwtcl" type="int">
          <ipxact:name>pf0_pcie_cap_ep_l1_accpt_latency_hwtcl</ipxact:name>
          <ipxact:displayName>Endpoint L1s acceptable latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_user_id_hwtcl" type="int">
          <ipxact:name>cvp_user_id_hwtcl</ipxact:name>
          <ipxact:displayName>User ID register from the Vendor Specific Extended Capability</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hip_reconfig_hwtcl" type="int">
          <ipxact:name>hip_reconfig_hwtcl</ipxact:name>
          <ipxact:displayName>Enable HIP dynamic reconfiguration of PCIe read-only registers</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="xcvr_reconfig_hwtcl" type="int">
          <ipxact:name>xcvr_reconfig_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Transceiver dynamic reconfiguration</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="xcvr_adme_hwtcl" type="int">
          <ipxact:name>xcvr_adme_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Native PHY, ATXPLL and fPLL ADME for Transceiver Toolkit</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pcie_link_inspector_hwtcl" type="int">
          <ipxact:name>pcie_link_inspector_hwtcl</ipxact:name>
          <ipxact:displayName>Enable PCIe Link Inspector</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pcie_link_inspector_avmm_hwtcl" type="int">
          <ipxact:name>pcie_link_inspector_avmm_hwtcl</ipxact:name>
          <ipxact:displayName>Enable PCIe Link Inspector AVMM Interface</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_sel_deemphasis_hwtcl" type="string">
          <ipxact:name>pf0_pcie_cap_sel_deemphasis_hwtcl</ipxact:name>
          <ipxact:displayName>Gen 2 TX de-emphasis</ipxact:displayName>
          <ipxact:value>6dB</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="anlg_voltage" type="string">
          <ipxact:name>anlg_voltage</ipxact:name>
          <ipxact:displayName>VCCR/VCCT supply voltage for the transceiver</ipxact:displayName>
          <ipxact:value>1_0V</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_phase23_txpreset_hwtcl" type="string">
          <ipxact:name>virtual_phase23_txpreset_hwtcl</ipxact:name>
          <ipxact:displayName>Requested equalization far-end TX preset</ipxact:displayName>
          <ipxact:value>Preset 8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_eq_eieos_cnt_hwtcl" type="int">
          <ipxact:name>pf0_eq_eieos_cnt_hwtcl</ipxact:name>
          <ipxact:displayName>Disable resetting EIEOS interval count during EQ master phase</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_g_delay_added_hwtcl" type="int">
          <ipxact:name>hrc_rstctl_timer_g_delay_added_hwtcl</ipxact:name>
          <ipxact:displayName>Enable delayed reset release</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ceb_extend_pcie_hwtcl" type="int">
          <ipxact:name>ceb_extend_pcie_hwtcl</ipxact:name>
          <ipxact:displayName>Use PCI Express extended space</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_vendor_id_hwtcl" type="int">
          <ipxact:name>pf0_pci_type0_vendor_id_hwtcl</ipxact:name>
          <ipxact:displayName>Vendor ID</ipxact:displayName>
          <ipxact:value>4466</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_device_id_hwtcl" type="int">
          <ipxact:name>pf0_pci_type0_device_id_hwtcl</ipxact:name>
          <ipxact:displayName>Device ID</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_revision_id_hwtcl" type="int">
          <ipxact:name>pf0_revision_id_hwtcl</ipxact:name>
          <ipxact:displayName>Revision ID</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_class_code_hwtcl" type="int">
          <ipxact:name>pf0_class_code_hwtcl</ipxact:name>
          <ipxact:displayName>Class code</ipxact:displayName>
          <ipxact:value>16711680</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_base_class_code_hwtcl" type="int">
          <ipxact:name>pf0_base_class_code_hwtcl</ipxact:name>
          <ipxact:displayName>Base Class code</ipxact:displayName>
          <ipxact:value>255</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_subclass_code_hwtcl" type="int">
          <ipxact:name>pf0_subclass_code_hwtcl</ipxact:name>
          <ipxact:displayName>Sub Class code</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_program_interface_hwtcl" type="int">
          <ipxact:name>pf0_program_interface_hwtcl</ipxact:name>
          <ipxact:displayName>Program Interface code</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_subsys_vendor_id_hwtcl" type="int">
          <ipxact:name>pf0_subsys_vendor_id_hwtcl</ipxact:name>
          <ipxact:displayName>Subsystem Vendor ID</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_subsys_dev_id_hwtcl" type="int">
          <ipxact:name>pf0_subsys_dev_id_hwtcl</ipxact:name>
          <ipxact:displayName>Subsystem Device ID</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pll_refclk_freq_hwtcl" type="string">
          <ipxact:name>pll_refclk_freq_hwtcl</ipxact:name>
          <ipxact:displayName>Reference clock frequency</ipxact:displayName>
          <ipxact:value>100 MHz</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_width_integer_hwtcl" type="int">
          <ipxact:name>data_width_integer_hwtcl</ipxact:name>
          <ipxact:displayName>data_width_integer_hwtcl</ipxact:displayName>
          <ipxact:value>256</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_clk_mhz_integer_hwtcl" type="int">
          <ipxact:name>pld_clk_mhz_integer_hwtcl</ipxact:name>
          <ipxact:displayName>pld_clk_mhz_integer_hwtcl</ipxact:displayName>
          <ipxact:value>125</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="apps_type_hwtcl" type="int">
          <ipxact:name>apps_type_hwtcl</ipxact:name>
          <ipxact:displayName>Set apps_type_hwtcl BFM driver value</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bfm_drive_interface_clk_hwtcl" type="int">
          <ipxact:name>bfm_drive_interface_clk_hwtcl</ipxact:name>
          <ipxact:displayName>bfm_drive_interface_clk_hwtcl</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bfm_drive_interface_npor_hwtcl" type="int">
          <ipxact:name>bfm_drive_interface_npor_hwtcl</ipxact:name>
          <ipxact:displayName>bfm_drive_interface_npor_hwtcl</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bfm_drive_interface_pipe_hwtcl" type="int">
          <ipxact:name>bfm_drive_interface_pipe_hwtcl</ipxact:name>
          <ipxact:displayName>bfm_drive_interface_pipe_hwtcl</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bfm_drive_interface_control_hwtcl" type="int">
          <ipxact:name>bfm_drive_interface_control_hwtcl</ipxact:name>
          <ipxact:displayName>bfm_drive_interface_control_hwtcl</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="serial_sim_hwtcl" type="int">
          <ipxact:name>serial_sim_hwtcl</ipxact:name>
          <ipxact:displayName>serial_sim_hwtcl</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_pipe32_phyip_ser_driver_hwtcl" type="int">
          <ipxact:name>enable_pipe32_phyip_ser_driver_hwtcl</ipxact:name>
          <ipxact:displayName>enable_pipe32_phyip_ser_driver_hwtcl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="use_rpbfm_pro" type="int">
          <ipxact:name>use_rpbfm_pro</ipxact:name>
          <ipxact:displayName>use_rpbfm_pro</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="use_pll_lock_hwtcl" type="int">
          <ipxact:name>use_pll_lock_hwtcl</ipxact:name>
          <ipxact:displayName>use_pll_lock_hwtcl</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_test_out_hwtcl" type="int">
          <ipxact:name>enable_test_out_hwtcl</ipxact:name>
          <ipxact:displayName>enable_test_out_hwtcl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_pld_warm_rst_rdy_hwtcl" type="int">
          <ipxact:name>enable_pld_warm_rst_rdy_hwtcl</ipxact:name>
          <ipxact:displayName>enable_pld_warm_rst_rdy_hwtcl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_avst_deskew_hwtcl" type="int">
          <ipxact:name>enable_avst_deskew_hwtcl</ipxact:name>
          <ipxact:displayName>Enable Deskew logic for Gen3x16</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="eios_workaround_enable_hwtcl" type="int">
          <ipxact:name>eios_workaround_enable_hwtcl</ipxact:name>
          <ipxact:displayName>eios_workaround_enable_hwtcl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_pcie_cv_fix" type="int">
          <ipxact:name>enable_pcie_cv_fix</ipxact:name>
          <ipxact:displayName>enable_pcie_cv_fix</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_jtag0" type="int">
          <ipxact:name>cvp_jtag0</ipxact:name>
          <ipxact:displayName>cvp_jtag0</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_jtag1" type="int">
          <ipxact:name>cvp_jtag1</ipxact:name>
          <ipxact:displayName>cvp_jtag1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_jtag2" type="int">
          <ipxact:name>cvp_jtag2</ipxact:name>
          <ipxact:displayName>cvp_jtag2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_jtag3" type="int">
          <ipxact:name>cvp_jtag3</ipxact:name>
          <ipxact:displayName>cvp_jtag3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_cardbus_cis_pointer" type="int">
          <ipxact:name>pf0_cardbus_cis_pointer</ipxact:name>
          <ipxact:displayName>pf0_cardbus_cis_pointer</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_mask_radm_2" type="int">
          <ipxact:name>pf0_mask_radm_2</ipxact:name>
          <ipxact:displayName>pf0_mask_radm_2</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_ser_num_reg_1_dw" type="int">
          <ipxact:name>pf0_sn_ser_num_reg_1_dw</ipxact:name>
          <ipxact:displayName>pf0_sn_ser_num_reg_1_dw</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_ser_num_reg_2_dw" type="int">
          <ipxact:name>pf0_sn_ser_num_reg_2_dw</ipxact:name>
          <ipxact:displayName>pf0_sn_ser_num_reg_2_dw</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_sup_page_size" type="int">
          <ipxact:name>pf0_sriov_sup_page_size</ipxact:name>
          <ipxact:displayName>pf0_sriov_sup_page_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar0_mask" type="int">
          <ipxact:name>pf0_sriov_vf_bar0_mask</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar0_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar1_mask" type="int">
          <ipxact:name>pf0_sriov_vf_bar1_mask</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar1_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar2_mask" type="int">
          <ipxact:name>pf0_sriov_vf_bar2_mask</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar2_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar3_mask" type="int">
          <ipxact:name>pf0_sriov_vf_bar3_mask</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar3_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar4_mask" type="int">
          <ipxact:name>pf0_sriov_vf_bar4_mask</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar4_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar5_mask" type="int">
          <ipxact:name>pf0_sriov_vf_bar5_mask</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar5_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_cardbus_cis_pointer" type="int">
          <ipxact:name>pf1_cardbus_cis_pointer</ipxact:name>
          <ipxact:displayName>pf1_cardbus_cis_pointer</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_ser_num_reg_1_dw" type="int">
          <ipxact:name>pf1_sn_ser_num_reg_1_dw</ipxact:name>
          <ipxact:displayName>pf1_sn_ser_num_reg_1_dw</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_ser_num_reg_2_dw" type="int">
          <ipxact:name>pf1_sn_ser_num_reg_2_dw</ipxact:name>
          <ipxact:displayName>pf1_sn_ser_num_reg_2_dw</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_sup_page_size" type="int">
          <ipxact:name>pf1_sriov_sup_page_size</ipxact:name>
          <ipxact:displayName>pf1_sriov_sup_page_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar0_mask" type="int">
          <ipxact:name>pf1_sriov_vf_bar0_mask</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar0_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar1_mask" type="int">
          <ipxact:name>pf1_sriov_vf_bar1_mask</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar1_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar2_mask" type="int">
          <ipxact:name>pf1_sriov_vf_bar2_mask</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar2_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar3_mask" type="int">
          <ipxact:name>pf1_sriov_vf_bar3_mask</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar3_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar4_mask" type="int">
          <ipxact:name>pf1_sriov_vf_bar4_mask</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar4_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar5_mask" type="int">
          <ipxact:name>pf1_sriov_vf_bar5_mask</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar5_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_cardbus_cis_pointer" type="int">
          <ipxact:name>pf2_cardbus_cis_pointer</ipxact:name>
          <ipxact:displayName>pf2_cardbus_cis_pointer</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_ser_num_reg_1_dw" type="int">
          <ipxact:name>pf2_sn_ser_num_reg_1_dw</ipxact:name>
          <ipxact:displayName>pf2_sn_ser_num_reg_1_dw</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_ser_num_reg_2_dw" type="int">
          <ipxact:name>pf2_sn_ser_num_reg_2_dw</ipxact:name>
          <ipxact:displayName>pf2_sn_ser_num_reg_2_dw</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_sup_page_size" type="int">
          <ipxact:name>pf2_sriov_sup_page_size</ipxact:name>
          <ipxact:displayName>pf2_sriov_sup_page_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_cardbus_cis_pointer" type="int">
          <ipxact:name>pf3_cardbus_cis_pointer</ipxact:name>
          <ipxact:displayName>pf3_cardbus_cis_pointer</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_ser_num_reg_1_dw" type="int">
          <ipxact:name>pf3_sn_ser_num_reg_1_dw</ipxact:name>
          <ipxact:displayName>pf3_sn_ser_num_reg_1_dw</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_ser_num_reg_2_dw" type="int">
          <ipxact:name>pf3_sn_ser_num_reg_2_dw</ipxact:name>
          <ipxact:displayName>pf3_sn_ser_num_reg_2_dw</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_sup_page_size" type="int">
          <ipxact:name>pf3_sriov_sup_page_size</ipxact:name>
          <ipxact:displayName>pf3_sriov_sup_page_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="test_in_hi" type="int">
          <ipxact:name>test_in_hi</ipxact:name>
          <ipxact:displayName>test_in_hi</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="test_in_lo" type="int">
          <ipxact:name>test_in_lo</ipxact:name>
          <ipxact:displayName>test_in_lo</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="slave_address_map_0_hwtcl" type="int">
          <ipxact:name>slave_address_map_0_hwtcl</ipxact:name>
          <ipxact:displayName>slave_address_map_0_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="slave_address_map_1_hwtcl" type="int">
          <ipxact:name>slave_address_map_1_hwtcl</ipxact:name>
          <ipxact:displayName>slave_address_map_1_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="slave_address_map_2_hwtcl" type="int">
          <ipxact:name>slave_address_map_2_hwtcl</ipxact:name>
          <ipxact:displayName>slave_address_map_2_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="slave_address_map_3_hwtcl" type="int">
          <ipxact:name>slave_address_map_3_hwtcl</ipxact:name>
          <ipxact:displayName>slave_address_map_3_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="slave_address_map_4_hwtcl" type="int">
          <ipxact:name>slave_address_map_4_hwtcl</ipxact:name>
          <ipxact:displayName>slave_address_map_4_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="slave_address_map_5_hwtcl" type="int">
          <ipxact:name>slave_address_map_5_hwtcl</ipxact:name>
          <ipxact:displayName>slave_address_map_5_hwtcl</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device_family" type="string">
          <ipxact:name>device_family</ipxact:name>
          <ipxact:displayName>device_family</ipxact:displayName>
          <ipxact:value>Stratix 10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="base_device" type="string">
          <ipxact:name>base_device</ipxact:name>
          <ipxact:displayName>base_device</ipxact:displayName>
          <ipxact:value>ND4H</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="part_trait_device" type="string">
          <ipxact:name>part_trait_device</ipxact:name>
          <ipxact:displayName>part_trait_device</ipxact:displayName>
          <ipxact:value>1SM16BEU2F55E2VG</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="design_environment" type="string">
          <ipxact:name>design_environment</ipxact:name>
          <ipxact:displayName>design_environment</ipxact:displayName>
          <ipxact:value>NATIVE</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device" type="string">
          <ipxact:name>device</ipxact:name>
          <ipxact:displayName>device</ipxact:displayName>
          <ipxact:value>1SM16BEU2F55E2VG</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_example_design_qii_hwtcl" type="int">
          <ipxact:name>enable_example_design_qii_hwtcl</ipxact:name>
          <ipxact:displayName>Generate a Quartus Project that includes the example design</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_example_design_sim_rp_hwtcl" type="int">
          <ipxact:name>enable_example_design_sim_rp_hwtcl</ipxact:name>
          <ipxact:displayName>Simulation</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_example_design_sim_hwtcl" type="int">
          <ipxact:name>enable_example_design_sim_hwtcl</ipxact:name>
          <ipxact:displayName>Simulation</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="select_example_design_sim_BFM_hwtcl" type="string">
          <ipxact:name>select_example_design_sim_BFM_hwtcl</ipxact:name>
          <ipxact:displayName>Select simulation Root Complex BFM</ipxact:displayName>
          <ipxact:value>Intel FPGA BFM</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_example_design_synth_hwtcl" type="int">
          <ipxact:name>enable_example_design_synth_hwtcl</ipxact:name>
          <ipxact:displayName>Synthesis</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_example_design_synth_rp_hwtcl" type="int">
          <ipxact:name>enable_example_design_synth_rp_hwtcl</ipxact:name>
          <ipxact:displayName>Synthesis</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_example_design_tb_hwtcl" type="int">
          <ipxact:name>enable_example_design_tb_hwtcl</ipxact:name>
          <ipxact:displayName>Generate the example design testbench</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="select_design_example_rtl_lang_hwtcl" type="string">
          <ipxact:name>select_design_example_rtl_lang_hwtcl</ipxact:name>
          <ipxact:displayName>Generated file format</ipxact:displayName>
          <ipxact:value>Verilog</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="targeted_devkit_hwtcl" type="string">
          <ipxact:name>targeted_devkit_hwtcl</ipxact:name>
          <ipxact:displayName>Select board</ipxact:displayName>
          <ipxact:value>NONE</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="chosen_devkit_hwtcl" type="string">
          <ipxact:name>chosen_devkit_hwtcl</ipxact:name>
          <ipxact:displayName>Current development kit:</ipxact:displayName>
          <ipxact:value>NONE</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="chosen_devkit_opn_hwtcl" type="string">
          <ipxact:name>chosen_devkit_opn_hwtcl</ipxact:name>
          <ipxact:displayName>chosen_devkit_opn_hwtcl</ipxact:displayName>
          <ipxact:value>1SM16BEU2F55E2VG</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="adp_bypass" type="string">
          <ipxact:name>adp_bypass</ipxact:name>
          <ipxact:displayName>adp_bypass</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="aux_cfg_vf_en" type="string">
          <ipxact:name>aux_cfg_vf_en</ipxact:name>
          <ipxact:displayName>aux_cfg_vf_en</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="aux_warm_reset_ctl" type="string">
          <ipxact:name>aux_warm_reset_ctl</ipxact:name>
          <ipxact:displayName>aux_warm_reset_ctl</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_blk_crs_en" type="string">
          <ipxact:name>cfg_blk_crs_en</ipxact:name>
          <ipxact:displayName>cfg_blk_crs_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_dbi_pf0_table_size" type="int">
          <ipxact:name>cfg_dbi_pf0_table_size</ipxact:name>
          <ipxact:displayName>cfg_dbi_pf0_table_size</ipxact:displayName>
          <ipxact:value>262</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_dbi_pf1_start_addr" type="int">
          <ipxact:name>cfg_dbi_pf1_start_addr</ipxact:name>
          <ipxact:displayName>cfg_dbi_pf1_start_addr</ipxact:displayName>
          <ipxact:value>320</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_dbi_pf1_tablesize" type="int">
          <ipxact:name>cfg_dbi_pf1_tablesize</ipxact:name>
          <ipxact:displayName>cfg_dbi_pf1_tablesize</ipxact:displayName>
          <ipxact:value>172</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_g3_pset_coeff_0" type="int">
          <ipxact:name>cfg_g3_pset_coeff_0</ipxact:name>
          <ipxact:displayName>cfg_g3_pset_coeff_0</ipxact:displayName>
          <ipxact:value>64320</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_g3_pset_coeff_1" type="int">
          <ipxact:name>cfg_g3_pset_coeff_1</ipxact:name>
          <ipxact:displayName>cfg_g3_pset_coeff_1</ipxact:displayName>
          <ipxact:value>44160</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_g3_pset_coeff_10" type="int">
          <ipxact:name>cfg_g3_pset_coeff_10</ipxact:name>
          <ipxact:displayName>cfg_g3_pset_coeff_10</ipxact:displayName>
          <ipxact:value>84480</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_g3_pset_coeff_2" type="int">
          <ipxact:name>cfg_g3_pset_coeff_2</ipxact:name>
          <ipxact:displayName>cfg_g3_pset_coeff_2</ipxact:displayName>
          <ipxact:value>52224</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_g3_pset_coeff_3" type="int">
          <ipxact:name>cfg_g3_pset_coeff_3</ipxact:name>
          <ipxact:displayName>cfg_g3_pset_coeff_3</ipxact:displayName>
          <ipxact:value>36096</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_g3_pset_coeff_4" type="int">
          <ipxact:name>cfg_g3_pset_coeff_4</ipxact:name>
          <ipxact:displayName>cfg_g3_pset_coeff_4</ipxact:displayName>
          <ipxact:value>3840</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_g3_pset_coeff_5" type="int">
          <ipxact:name>cfg_g3_pset_coeff_5</ipxact:name>
          <ipxact:displayName>cfg_g3_pset_coeff_5</ipxact:displayName>
          <ipxact:value>3462</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_g3_pset_coeff_6" type="int">
          <ipxact:name>cfg_g3_pset_coeff_6</ipxact:name>
          <ipxact:displayName>cfg_g3_pset_coeff_6</ipxact:displayName>
          <ipxact:value>3336</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_g3_pset_coeff_7" type="int">
          <ipxact:name>cfg_g3_pset_coeff_7</ipxact:name>
          <ipxact:displayName>cfg_g3_pset_coeff_7</ipxact:displayName>
          <ipxact:value>51846</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_g3_pset_coeff_8" type="int">
          <ipxact:name>cfg_g3_pset_coeff_8</ipxact:name>
          <ipxact:displayName>cfg_g3_pset_coeff_8</ipxact:displayName>
          <ipxact:value>35592</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_g3_pset_coeff_9" type="int">
          <ipxact:name>cfg_g3_pset_coeff_9</ipxact:name>
          <ipxact:displayName>cfg_g3_pset_coeff_9</ipxact:displayName>
          <ipxact:value>3210</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_vf_num_pf0" type="int">
          <ipxact:name>cfg_vf_num_pf0</ipxact:name>
          <ipxact:displayName>cfg_vf_num_pf0</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_vf_num_pf1" type="int">
          <ipxact:name>cfg_vf_num_pf1</ipxact:name>
          <ipxact:displayName>cfg_vf_num_pf1</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_vf_table_size" type="int">
          <ipxact:name>cfg_vf_table_size</ipxact:name>
          <ipxact:displayName>cfg_vf_table_size</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clkmod_gen3_hclk_div_sel" type="string">
          <ipxact:name>clkmod_gen3_hclk_div_sel</ipxact:name>
          <ipxact:displayName>clkmod_gen3_hclk_div_sel</ipxact:displayName>
          <ipxact:value>hclk_div2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clkmod_gen3_hclk_source_sel" type="string">
          <ipxact:name>clkmod_gen3_hclk_source_sel</ipxact:name>
          <ipxact:displayName>clkmod_gen3_hclk_source_sel</ipxact:displayName>
          <ipxact:value>hclk_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clkmod_hip_clk_dis" type="string">
          <ipxact:name>clkmod_hip_clk_dis</ipxact:name>
          <ipxact:displayName>clkmod_hip_clk_dis</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clkmod_pclk_sel" type="string">
          <ipxact:name>clkmod_pclk_sel</ipxact:name>
          <ipxact:displayName>clkmod_pclk_sel</ipxact:displayName>
          <ipxact:value>pclk_ch0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clkmod_pld_clk_out_sel" type="string">
          <ipxact:name>clkmod_pld_clk_out_sel</ipxact:name>
          <ipxact:displayName>clkmod_pld_clk_out_sel</ipxact:displayName>
          <ipxact:value>div4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clkmod_pld_clk_out_sel_2x" type="string">
          <ipxact:name>clkmod_pld_clk_out_sel_2x</ipxact:name>
          <ipxact:displayName>clkmod_pld_clk_out_sel_2x</ipxact:displayName>
          <ipxact:value>aib2x_div4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clock_ctl_rsvd_3" type="string">
          <ipxact:name>clock_ctl_rsvd_3</ipxact:name>
          <ipxact:displayName>clock_ctl_rsvd_3</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clock_ctl_rsvd_5" type="string">
          <ipxact:name>clock_ctl_rsvd_5</ipxact:name>
          <ipxact:displayName>clock_ctl_rsvd_5</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clrhip_not_rst_sticky" type="string">
          <ipxact:name>clrhip_not_rst_sticky</ipxact:name>
          <ipxact:displayName>clrhip_not_rst_sticky</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="crs_override" type="string">
          <ipxact:name>crs_override</ipxact:name>
          <ipxact:displayName>crs_override</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="crs_override_value" type="string">
          <ipxact:name>crs_override_value</ipxact:name>
          <ipxact:displayName>crs_override_value</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_blocking_dis" type="string">
          <ipxact:name>cvp_blocking_dis</ipxact:name>
          <ipxact:displayName>cvp_blocking_dis</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_clk_sel" type="string">
          <ipxact:name>cvp_clk_sel</ipxact:name>
          <ipxact:displayName>cvp_clk_sel</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_data_compressed" type="string">
          <ipxact:name>cvp_data_compressed</ipxact:name>
          <ipxact:displayName>cvp_data_compressed</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_data_encrypted" type="string">
          <ipxact:name>cvp_data_encrypted</ipxact:name>
          <ipxact:displayName>cvp_data_encrypted</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_extra" type="string">
          <ipxact:name>cvp_extra</ipxact:name>
          <ipxact:displayName>cvp_extra</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_hard_reset_bypass" type="string">
          <ipxact:name>cvp_hard_reset_bypass</ipxact:name>
          <ipxact:displayName>cvp_hard_reset_bypass</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_hip_clk_sel_default" type="string">
          <ipxact:name>cvp_hip_clk_sel_default</ipxact:name>
          <ipxact:displayName>cvp_hip_clk_sel_default</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_intf_reset_ctl" type="int">
          <ipxact:name>cvp_intf_reset_ctl</ipxact:name>
          <ipxact:displayName>cvp_intf_reset_ctl</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_irq_en" type="string">
          <ipxact:name>cvp_irq_en</ipxact:name>
          <ipxact:displayName>cvp_irq_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_mode_default" type="string">
          <ipxact:name>cvp_mode_default</ipxact:name>
          <ipxact:displayName>cvp_mode_default</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_mode_gating_dis" type="string">
          <ipxact:name>cvp_mode_gating_dis</ipxact:name>
          <ipxact:displayName>cvp_mode_gating_dis</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_rate_sel" type="string">
          <ipxact:name>cvp_rate_sel</ipxact:name>
          <ipxact:displayName>cvp_rate_sel</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_user_id" type="int">
          <ipxact:name>cvp_user_id</ipxact:name>
          <ipxact:displayName>cvp_user_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_vsec_id" type="int">
          <ipxact:name>cvp_vsec_id</ipxact:name>
          <ipxact:displayName>cvp_vsec_id</ipxact:displayName>
          <ipxact:value>4466</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_vsec_rev" type="int">
          <ipxact:name>cvp_vsec_rev</ipxact:name>
          <ipxact:displayName>cvp_vsec_rev</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_warm_rst_ready_force_bit0" type="string">
          <ipxact:name>cvp_warm_rst_ready_force_bit0</ipxact:name>
          <ipxact:displayName>cvp_warm_rst_ready_force_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_warm_rst_ready_force_bit1" type="string">
          <ipxact:name>cvp_warm_rst_ready_force_bit1</ipxact:name>
          <ipxact:displayName>cvp_warm_rst_ready_force_bit1</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_warm_rst_req_ena" type="string">
          <ipxact:name>cvp_warm_rst_req_ena</ipxact:name>
          <ipxact:displayName>cvp_warm_rst_req_ena</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cvp_write_mask_ctl" type="int">
          <ipxact:name>cvp_write_mask_ctl</ipxact:name>
          <ipxact:displayName>cvp_write_mask_ctl</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device_type" type="string">
          <ipxact:name>device_type</ipxact:name>
          <ipxact:displayName>device_type</ipxact:displayName>
          <ipxact:value>dev_nep</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ecc_chk_val" type="string">
          <ipxact:name>ecc_chk_val</ipxact:name>
          <ipxact:displayName>ecc_chk_val</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ecc_gen_val" type="string">
          <ipxact:name>ecc_gen_val</ipxact:name>
          <ipxact:displayName>ecc_gen_val</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="eco_flops" type="int">
          <ipxact:name>eco_flops</ipxact:name>
          <ipxact:displayName>eco_flops</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="eqctrl_adp_ctle" type="string">
          <ipxact:name>eqctrl_adp_ctle</ipxact:name>
          <ipxact:displayName>eqctrl_adp_ctle</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="eqctrl_ctle_val" type="string">
          <ipxact:name>eqctrl_ctle_val</ipxact:name>
          <ipxact:displayName>eqctrl_ctle_val</ipxact:displayName>
          <ipxact:value>ctle_val_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="eqctrl_dir_mode_en" type="string">
          <ipxact:name>eqctrl_dir_mode_en</ipxact:name>
          <ipxact:displayName>eqctrl_dir_mode_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="eqctrl_fom_mode_en" type="string">
          <ipxact:name>eqctrl_fom_mode_en</ipxact:name>
          <ipxact:displayName>eqctrl_fom_mode_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="eqctrl_legacy_mode_en" type="string">
          <ipxact:name>eqctrl_legacy_mode_en</ipxact:name>
          <ipxact:displayName>eqctrl_legacy_mode_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="eqctrl_num_fom_cycles" type="int">
          <ipxact:name>eqctrl_num_fom_cycles</ipxact:name>
          <ipxact:displayName>eqctrl_num_fom_cycles</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="eqctrl_use_dsp_rxpreset" type="string">
          <ipxact:name>eqctrl_use_dsp_rxpreset</ipxact:name>
          <ipxact:displayName>eqctrl_use_dsp_rxpreset</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="func_mode" type="string">
          <ipxact:name>func_mode</ipxact:name>
          <ipxact:displayName>func_mode</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gpio_irq" type="int">
          <ipxact:name>gpio_irq</ipxact:name>
          <ipxact:displayName>gpio_irq</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hip_pcs_chnl_en" type="int">
          <ipxact:name>hip_pcs_chnl_en</ipxact:name>
          <ipxact:displayName>hip_pcs_chnl_en</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_chnl_cal_done_active" type="string">
          <ipxact:name>hrc_chnl_cal_done_active</ipxact:name>
          <ipxact:displayName>hrc_chnl_cal_done_active</ipxact:displayName>
          <ipxact:value>chnl_cal_done_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_chnl_en" type="int">
          <ipxact:name>hrc_chnl_en</ipxact:name>
          <ipxact:displayName>hrc_chnl_en</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_chnl_txpll_master_cgb_rst_en" type="int">
          <ipxact:name>hrc_chnl_txpll_master_cgb_rst_en</ipxact:name>
          <ipxact:displayName>hrc_chnl_txpll_master_cgb_rst_en</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_chnl_txpll_rst_en" type="int">
          <ipxact:name>hrc_chnl_txpll_rst_en</ipxact:name>
          <ipxact:displayName>hrc_chnl_txpll_rst_en</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_en_pcs_fifo_err" type="string">
          <ipxact:name>hrc_en_pcs_fifo_err</ipxact:name>
          <ipxact:displayName>hrc_en_pcs_fifo_err</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_force_inactive_rst" type="string">
          <ipxact:name>hrc_force_inactive_rst</ipxact:name>
          <ipxact:displayName>hrc_force_inactive_rst</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_fref_clk_active" type="string">
          <ipxact:name>hrc_fref_clk_active</ipxact:name>
          <ipxact:displayName>hrc_fref_clk_active</ipxact:displayName>
          <ipxact:value>fref_clk_sel_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_mask_tx_pll_lock_active" type="string">
          <ipxact:name>hrc_mask_tx_pll_lock_active</ipxact:name>
          <ipxact:displayName>hrc_mask_tx_pll_lock_active</ipxact:displayName>
          <ipxact:value>mask_tx_pll_lock_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_pll_cal_done_active" type="string">
          <ipxact:name>hrc_pll_cal_done_active</ipxact:name>
          <ipxact:displayName>hrc_pll_cal_done_active</ipxact:displayName>
          <ipxact:value>pll_cal_done_12</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_pll_perst_en" type="string">
          <ipxact:name>hrc_pll_perst_en</ipxact:name>
          <ipxact:displayName>hrc_pll_perst_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_pma_perst_en" type="string">
          <ipxact:name>hrc_pma_perst_en</ipxact:name>
          <ipxact:displayName>hrc_pma_perst_en</ipxact:displayName>
          <ipxact:value>level</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_1ms" type="int">
          <ipxact:name>hrc_rstctl_1ms</ipxact:name>
          <ipxact:displayName>hrc_rstctl_1ms</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_1us" type="int">
          <ipxact:name>hrc_rstctl_1us</ipxact:name>
          <ipxact:displayName>hrc_rstctl_1us</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_type_a" type="string">
          <ipxact:name>hrc_rstctl_timer_type_a</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_type_a</ipxact:displayName>
          <ipxact:value>fref_cyc_a</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_type_f" type="string">
          <ipxact:name>hrc_rstctl_timer_type_f</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_type_f</ipxact:displayName>
          <ipxact:value>fref_cyc_f</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_type_g" type="string">
          <ipxact:name>hrc_rstctl_timer_type_g</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_type_g</ipxact:displayName>
          <ipxact:value>fref_cyc_g</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_type_h" type="string">
          <ipxact:name>hrc_rstctl_timer_type_h</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_type_h</ipxact:displayName>
          <ipxact:value>fref_cyc_h</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_type_i" type="string">
          <ipxact:name>hrc_rstctl_timer_type_i</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_type_i</ipxact:displayName>
          <ipxact:value>fref_cyc_i</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_type_j" type="string">
          <ipxact:name>hrc_rstctl_timer_type_j</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_type_j</ipxact:displayName>
          <ipxact:value>fref_cyc_j</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_value_a" type="int">
          <ipxact:name>hrc_rstctl_timer_value_a</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_value_a</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_value_f" type="int">
          <ipxact:name>hrc_rstctl_timer_value_f</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_value_f</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_value_g" type="int">
          <ipxact:name>hrc_rstctl_timer_value_g</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_value_g</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_value_h" type="int">
          <ipxact:name>hrc_rstctl_timer_value_h</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_value_h</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_value_i" type="int">
          <ipxact:name>hrc_rstctl_timer_value_i</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_value_i</ipxact:displayName>
          <ipxact:value>20</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rstctl_timer_value_j" type="int">
          <ipxact:name>hrc_rstctl_timer_value_j</ipxact:name>
          <ipxact:displayName>hrc_rstctl_timer_value_j</ipxact:displayName>
          <ipxact:value>20</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rx_pcs_rst_n_active" type="string">
          <ipxact:name>hrc_rx_pcs_rst_n_active</ipxact:name>
          <ipxact:displayName>hrc_rx_pcs_rst_n_active</ipxact:displayName>
          <ipxact:value>rx_pcs_rst_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rx_pll_lock_active" type="string">
          <ipxact:name>hrc_rx_pll_lock_active</ipxact:name>
          <ipxact:displayName>hrc_rx_pll_lock_active</ipxact:displayName>
          <ipxact:value>rx_pll_lock_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rx_pma_rstb_active" type="string">
          <ipxact:name>hrc_rx_pma_rstb_active</ipxact:name>
          <ipxact:displayName>hrc_rx_pma_rstb_active</ipxact:displayName>
          <ipxact:value>rx_pma_rstb_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_soft_rstctrl_clr" type="string">
          <ipxact:name>hrc_soft_rstctrl_clr</ipxact:name>
          <ipxact:displayName>hrc_soft_rstctrl_clr</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_soft_rstctrl_en" type="string">
          <ipxact:name>hrc_soft_rstctrl_en</ipxact:name>
          <ipxact:displayName>hrc_soft_rstctrl_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_tx_lc_pll_rstb_active" type="string">
          <ipxact:name>hrc_tx_lc_pll_rstb_active</ipxact:name>
          <ipxact:displayName>hrc_tx_lc_pll_rstb_active</ipxact:displayName>
          <ipxact:value>tx_lc_pll_rstb_12</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_tx_lcff_pll_lock_active" type="string">
          <ipxact:name>hrc_tx_lcff_pll_lock_active</ipxact:name>
          <ipxact:displayName>hrc_tx_lcff_pll_lock_active</ipxact:displayName>
          <ipxact:value>tx_lcff_pll_lock_12</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_tx_pcs_rst_n_active" type="string">
          <ipxact:name>hrc_tx_pcs_rst_n_active</ipxact:name>
          <ipxact:displayName>hrc_tx_pcs_rst_n_active</ipxact:displayName>
          <ipxact:value>tx_pcs_rst_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="irq_misc_ctrl" type="int">
          <ipxact:name>irq_misc_ctrl</ipxact:name>
          <ipxact:displayName>irq_misc_ctrl</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="k_phy_misc_ctrl_rsvd_0_5" type="int">
          <ipxact:name>k_phy_misc_ctrl_rsvd_0_5</ipxact:name>
          <ipxact:displayName>k_phy_misc_ctrl_rsvd_0_5</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="k_phy_misc_ctrl_rsvd_13_15" type="int">
          <ipxact:name>k_phy_misc_ctrl_rsvd_13_15</ipxact:name>
          <ipxact:displayName>k_phy_misc_ctrl_rsvd_13_15</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_ack_n_fts" type="int">
          <ipxact:name>pf0_ack_n_fts</ipxact:name>
          <ipxact:displayName>pf0_ack_n_fts</ipxact:displayName>
          <ipxact:value>255</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_adv_err_int_msg_num" type="int">
          <ipxact:name>pf0_adv_err_int_msg_num</ipxact:name>
          <ipxact:displayName>pf0_adv_err_int_msg_num</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_aer_cap_aer_ext_cap_hdr_off_addr_byte2" type="int">
          <ipxact:name>pf0_aer_cap_aer_ext_cap_hdr_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_aer_cap_aer_ext_cap_hdr_off_addr_byte2</ipxact:displayName>
          <ipxact:value>258</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_aer_cap_aer_ext_cap_hdr_off_addr_byte3" type="int">
          <ipxact:name>pf0_aer_cap_aer_ext_cap_hdr_off_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_aer_cap_aer_ext_cap_hdr_off_addr_byte3</ipxact:displayName>
          <ipxact:value>259</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_aer_cap_root_err_status_off_addr_byte0" type="int">
          <ipxact:name>pf0_aer_cap_root_err_status_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_aer_cap_root_err_status_off_addr_byte0</ipxact:displayName>
          <ipxact:value>304</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_aer_cap_version" type="int">
          <ipxact:name>pf0_aer_cap_version</ipxact:name>
          <ipxact:displayName>pf0_aer_cap_version</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_aer_next_offset" type="int">
          <ipxact:name>pf0_aer_next_offset</ipxact:name>
          <ipxact:displayName>pf0_aer_next_offset</ipxact:displayName>
          <ipxact:value>328</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_ari_cap_ari_base_addr_byte2" type="int">
          <ipxact:name>pf0_ari_cap_ari_base_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_ari_cap_ari_base_addr_byte2</ipxact:displayName>
          <ipxact:value>378</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_ari_cap_ari_base_addr_byte3" type="int">
          <ipxact:name>pf0_ari_cap_ari_base_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_ari_cap_ari_base_addr_byte3</ipxact:displayName>
          <ipxact:value>379</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_ari_cap_version" type="int">
          <ipxact:name>pf0_ari_cap_version</ipxact:name>
          <ipxact:displayName>pf0_ari_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_ari_next_offset" type="int">
          <ipxact:name>pf0_ari_next_offset</ipxact:name>
          <ipxact:displayName>pf0_ari_next_offset</ipxact:displayName>
          <ipxact:value>392</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_ats_cap_ats_cap_hdr_reg_addr_byte2" type="int">
          <ipxact:name>pf0_ats_cap_ats_cap_hdr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_ats_cap_ats_cap_hdr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>646</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_ats_cap_ats_cap_hdr_reg_addr_byte3" type="int">
          <ipxact:name>pf0_ats_cap_ats_cap_hdr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_ats_cap_ats_cap_hdr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>647</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_ats_cap_ats_capabilities_ctrl_reg_addr_byte0" type="int">
          <ipxact:name>pf0_ats_cap_ats_capabilities_ctrl_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_ats_cap_ats_capabilities_ctrl_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>648</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_ats_cap_version" type="int">
          <ipxact:name>pf0_ats_cap_version</ipxact:name>
          <ipxact:displayName>pf0_ats_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_ats_capabilities_ctrl_reg_rsvdp_7" type="string">
          <ipxact:name>pf0_ats_capabilities_ctrl_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf0_ats_capabilities_ctrl_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_ats_next_offset" type="int">
          <ipxact:name>pf0_ats_next_offset</ipxact:name>
          <ipxact:displayName>pf0_ats_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_auto_lane_flip_ctrl_en" type="string">
          <ipxact:name>pf0_auto_lane_flip_ctrl_en</ipxact:name>
          <ipxact:displayName>pf0_auto_lane_flip_ctrl_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_aux_clk_freq" type="int">
          <ipxact:name>pf0_aux_clk_freq</ipxact:name>
          <ipxact:displayName>pf0_aux_clk_freq</ipxact:displayName>
          <ipxact:value>500</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_aux_clk_freq_off_rsvdp_10" type="int">
          <ipxact:name>pf0_aux_clk_freq_off_rsvdp_10</ipxact:name>
          <ipxact:displayName>pf0_aux_clk_freq_off_rsvdp_10</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_aux_curr" type="int">
          <ipxact:name>pf0_aux_curr</ipxact:name>
          <ipxact:displayName>pf0_aux_curr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar0_mem_io" type="string">
          <ipxact:name>pf0_bar0_mem_io</ipxact:name>
          <ipxact:displayName>pf0_bar0_mem_io</ipxact:displayName>
          <ipxact:value>pf0_bar0_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar0_prefetch" type="string">
          <ipxact:name>pf0_bar0_prefetch</ipxact:name>
          <ipxact:displayName>pf0_bar0_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar0_start" type="int">
          <ipxact:name>pf0_bar0_start</ipxact:name>
          <ipxact:displayName>pf0_bar0_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar0_type" type="string">
          <ipxact:name>pf0_bar0_type</ipxact:name>
          <ipxact:displayName>pf0_bar0_type</ipxact:displayName>
          <ipxact:value>pf0_bar0_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar1_mem_io" type="string">
          <ipxact:name>pf0_bar1_mem_io</ipxact:name>
          <ipxact:displayName>pf0_bar1_mem_io</ipxact:displayName>
          <ipxact:value>pf0_bar1_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar1_prefetch" type="string">
          <ipxact:name>pf0_bar1_prefetch</ipxact:name>
          <ipxact:displayName>pf0_bar1_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar1_start" type="int">
          <ipxact:name>pf0_bar1_start</ipxact:name>
          <ipxact:displayName>pf0_bar1_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar1_type" type="string">
          <ipxact:name>pf0_bar1_type</ipxact:name>
          <ipxact:displayName>pf0_bar1_type</ipxact:displayName>
          <ipxact:value>pf0_bar1_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar2_mem_io" type="string">
          <ipxact:name>pf0_bar2_mem_io</ipxact:name>
          <ipxact:displayName>pf0_bar2_mem_io</ipxact:displayName>
          <ipxact:value>pf0_bar2_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar2_prefetch" type="string">
          <ipxact:name>pf0_bar2_prefetch</ipxact:name>
          <ipxact:displayName>pf0_bar2_prefetch</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar2_start" type="int">
          <ipxact:name>pf0_bar2_start</ipxact:name>
          <ipxact:displayName>pf0_bar2_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar2_type" type="string">
          <ipxact:name>pf0_bar2_type</ipxact:name>
          <ipxact:displayName>pf0_bar2_type</ipxact:displayName>
          <ipxact:value>pf0_bar2_mem64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar3_mem_io" type="string">
          <ipxact:name>pf0_bar3_mem_io</ipxact:name>
          <ipxact:displayName>pf0_bar3_mem_io</ipxact:displayName>
          <ipxact:value>pf0_bar3_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar3_prefetch" type="string">
          <ipxact:name>pf0_bar3_prefetch</ipxact:name>
          <ipxact:displayName>pf0_bar3_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar3_start" type="int">
          <ipxact:name>pf0_bar3_start</ipxact:name>
          <ipxact:displayName>pf0_bar3_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar3_type" type="string">
          <ipxact:name>pf0_bar3_type</ipxact:name>
          <ipxact:displayName>pf0_bar3_type</ipxact:displayName>
          <ipxact:value>pf0_bar3_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar4_mem_io" type="string">
          <ipxact:name>pf0_bar4_mem_io</ipxact:name>
          <ipxact:displayName>pf0_bar4_mem_io</ipxact:displayName>
          <ipxact:value>pf0_bar4_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar4_prefetch" type="string">
          <ipxact:name>pf0_bar4_prefetch</ipxact:name>
          <ipxact:displayName>pf0_bar4_prefetch</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar4_start" type="int">
          <ipxact:name>pf0_bar4_start</ipxact:name>
          <ipxact:displayName>pf0_bar4_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar4_type" type="string">
          <ipxact:name>pf0_bar4_type</ipxact:name>
          <ipxact:displayName>pf0_bar4_type</ipxact:displayName>
          <ipxact:value>pf0_bar4_mem64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar5_mem_io" type="string">
          <ipxact:name>pf0_bar5_mem_io</ipxact:name>
          <ipxact:displayName>pf0_bar5_mem_io</ipxact:displayName>
          <ipxact:value>pf0_bar5_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar5_prefetch" type="string">
          <ipxact:name>pf0_bar5_prefetch</ipxact:name>
          <ipxact:displayName>pf0_bar5_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar5_start" type="int">
          <ipxact:name>pf0_bar5_start</ipxact:name>
          <ipxact:displayName>pf0_bar5_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_bar5_type" type="string">
          <ipxact:name>pf0_bar5_type</ipxact:name>
          <ipxact:displayName>pf0_bar5_type</ipxact:displayName>
          <ipxact:value>pf0_bar5_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_base_class_code" type="int">
          <ipxact:name>pf0_base_class_code</ipxact:name>
          <ipxact:displayName>pf0_base_class_code</ipxact:displayName>
          <ipxact:value>255</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_cap_id_nxt_ptr_reg_rsvdp_20" type="string">
          <ipxact:name>pf0_cap_id_nxt_ptr_reg_rsvdp_20</ipxact:name>
          <ipxact:displayName>pf0_cap_id_nxt_ptr_reg_rsvdp_20</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_cap_pointer" type="int">
          <ipxact:name>pf0_cap_pointer</ipxact:name>
          <ipxact:displayName>pf0_cap_pointer</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_common_clk_n_fts" type="int">
          <ipxact:name>pf0_common_clk_n_fts</ipxact:name>
          <ipxact:displayName>pf0_common_clk_n_fts</ipxact:displayName>
          <ipxact:value>255</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_con_status_reg_rsvdp_2" type="string">
          <ipxact:name>pf0_con_status_reg_rsvdp_2</ipxact:name>
          <ipxact:displayName>pf0_con_status_reg_rsvdp_2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_con_status_reg_rsvdp_4" type="int">
          <ipxact:name>pf0_con_status_reg_rsvdp_4</ipxact:name>
          <ipxact:displayName>pf0_con_status_reg_rsvdp_4</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_config_phy_tx_change" type="string">
          <ipxact:name>pf0_config_phy_tx_change</ipxact:name>
          <ipxact:displayName>pf0_config_phy_tx_change</ipxact:displayName>
          <ipxact:value>pf0_full_swing</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_config_tx_comp_rx" type="string">
          <ipxact:name>pf0_config_tx_comp_rx</ipxact:name>
          <ipxact:displayName>pf0_config_tx_comp_rx</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_cross_link_active" type="string">
          <ipxact:name>pf0_cross_link_active</ipxact:name>
          <ipxact:displayName>pf0_cross_link_active</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_cross_link_en" type="string">
          <ipxact:name>pf0_cross_link_en</ipxact:name>
          <ipxact:displayName>pf0_cross_link_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_d1_support" type="string">
          <ipxact:name>pf0_d1_support</ipxact:name>
          <ipxact:displayName>pf0_d1_support</ipxact:displayName>
          <ipxact:value>pf0_d1_not_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_d2_support" type="string">
          <ipxact:name>pf0_d2_support</ipxact:name>
          <ipxact:displayName>pf0_d2_support</ipxact:displayName>
          <ipxact:value>pf0_d2_not_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_0" type="int">
          <ipxact:name>pf0_dbi_reserved_0</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_0</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_1" type="int">
          <ipxact:name>pf0_dbi_reserved_1</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_10" type="int">
          <ipxact:name>pf0_dbi_reserved_10</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_10</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_11" type="int">
          <ipxact:name>pf0_dbi_reserved_11</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_11</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_12" type="int">
          <ipxact:name>pf0_dbi_reserved_12</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_13" type="int">
          <ipxact:name>pf0_dbi_reserved_13</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_13</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_14" type="int">
          <ipxact:name>pf0_dbi_reserved_14</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_14</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_15" type="int">
          <ipxact:name>pf0_dbi_reserved_15</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_15</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_16" type="int">
          <ipxact:name>pf0_dbi_reserved_16</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_16</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_17" type="int">
          <ipxact:name>pf0_dbi_reserved_17</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_17</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_18" type="int">
          <ipxact:name>pf0_dbi_reserved_18</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_18</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_19" type="int">
          <ipxact:name>pf0_dbi_reserved_19</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_19</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_2" type="int">
          <ipxact:name>pf0_dbi_reserved_2</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_20" type="int">
          <ipxact:name>pf0_dbi_reserved_20</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_20</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_21" type="int">
          <ipxact:name>pf0_dbi_reserved_21</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_21</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_22" type="int">
          <ipxact:name>pf0_dbi_reserved_22</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_22</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_23" type="int">
          <ipxact:name>pf0_dbi_reserved_23</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_23</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_24" type="int">
          <ipxact:name>pf0_dbi_reserved_24</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_24</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_25" type="int">
          <ipxact:name>pf0_dbi_reserved_25</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_25</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_26" type="int">
          <ipxact:name>pf0_dbi_reserved_26</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_26</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_27" type="int">
          <ipxact:name>pf0_dbi_reserved_27</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_27</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_28" type="int">
          <ipxact:name>pf0_dbi_reserved_28</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_28</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_29" type="int">
          <ipxact:name>pf0_dbi_reserved_29</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_29</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_3" type="int">
          <ipxact:name>pf0_dbi_reserved_3</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_30" type="int">
          <ipxact:name>pf0_dbi_reserved_30</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_30</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_31" type="int">
          <ipxact:name>pf0_dbi_reserved_31</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_31</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_32" type="int">
          <ipxact:name>pf0_dbi_reserved_32</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_32</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_33" type="int">
          <ipxact:name>pf0_dbi_reserved_33</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_33</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_34" type="int">
          <ipxact:name>pf0_dbi_reserved_34</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_34</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_35" type="int">
          <ipxact:name>pf0_dbi_reserved_35</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_35</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_36" type="int">
          <ipxact:name>pf0_dbi_reserved_36</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_36</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_37" type="int">
          <ipxact:name>pf0_dbi_reserved_37</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_37</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_38" type="int">
          <ipxact:name>pf0_dbi_reserved_38</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_38</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_39" type="int">
          <ipxact:name>pf0_dbi_reserved_39</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_39</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_4" type="int">
          <ipxact:name>pf0_dbi_reserved_4</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_4</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_40" type="int">
          <ipxact:name>pf0_dbi_reserved_40</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_40</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_41" type="int">
          <ipxact:name>pf0_dbi_reserved_41</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_41</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_42" type="int">
          <ipxact:name>pf0_dbi_reserved_42</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_42</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_43" type="int">
          <ipxact:name>pf0_dbi_reserved_43</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_43</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_44" type="int">
          <ipxact:name>pf0_dbi_reserved_44</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_44</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_45" type="int">
          <ipxact:name>pf0_dbi_reserved_45</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_45</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_46" type="int">
          <ipxact:name>pf0_dbi_reserved_46</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_46</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_47" type="int">
          <ipxact:name>pf0_dbi_reserved_47</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_47</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_48" type="int">
          <ipxact:name>pf0_dbi_reserved_48</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_48</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_49" type="int">
          <ipxact:name>pf0_dbi_reserved_49</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_49</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_5" type="int">
          <ipxact:name>pf0_dbi_reserved_5</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_5</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_50" type="int">
          <ipxact:name>pf0_dbi_reserved_50</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_50</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_51" type="int">
          <ipxact:name>pf0_dbi_reserved_51</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_51</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_52" type="int">
          <ipxact:name>pf0_dbi_reserved_52</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_52</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_53" type="int">
          <ipxact:name>pf0_dbi_reserved_53</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_53</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_54" type="int">
          <ipxact:name>pf0_dbi_reserved_54</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_54</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_55" type="int">
          <ipxact:name>pf0_dbi_reserved_55</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_55</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_56" type="int">
          <ipxact:name>pf0_dbi_reserved_56</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_56</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_57" type="int">
          <ipxact:name>pf0_dbi_reserved_57</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_57</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_6" type="int">
          <ipxact:name>pf0_dbi_reserved_6</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_6</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_7" type="int">
          <ipxact:name>pf0_dbi_reserved_7</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_7</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_8" type="int">
          <ipxact:name>pf0_dbi_reserved_8</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_8</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_reserved_9" type="int">
          <ipxact:name>pf0_dbi_reserved_9</ipxact:name>
          <ipxact:displayName>pf0_dbi_reserved_9</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dbi_ro_wr_en" type="string">
          <ipxact:name>pf0_dbi_ro_wr_en</ipxact:name>
          <ipxact:displayName>pf0_dbi_ro_wr_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_device_capabilities_reg_rsvdp_12" type="int">
          <ipxact:name>pf0_device_capabilities_reg_rsvdp_12</ipxact:name>
          <ipxact:displayName>pf0_device_capabilities_reg_rsvdp_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_device_capabilities_reg_rsvdp_16" type="int">
          <ipxact:name>pf0_device_capabilities_reg_rsvdp_16</ipxact:name>
          <ipxact:displayName>pf0_device_capabilities_reg_rsvdp_16</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_device_capabilities_reg_rsvdp_29" type="int">
          <ipxact:name>pf0_device_capabilities_reg_rsvdp_29</ipxact:name>
          <ipxact:displayName>pf0_device_capabilities_reg_rsvdp_29</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_direct_speed_change" type="string">
          <ipxact:name>pf0_direct_speed_change</ipxact:name>
          <ipxact:displayName>pf0_direct_speed_change</ipxact:displayName>
          <ipxact:value>pf0_auto_speed_chg</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_disable_fc_wd_timer" type="string">
          <ipxact:name>pf0_disable_fc_wd_timer</ipxact:name>
          <ipxact:displayName>pf0_disable_fc_wd_timer</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_disable_scrambler_gen_3" type="string">
          <ipxact:name>pf0_disable_scrambler_gen_3</ipxact:name>
          <ipxact:displayName>pf0_disable_scrambler_gen_3</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dll_link_en" type="string">
          <ipxact:name>pf0_dll_link_en</ipxact:name>
          <ipxact:displayName>pf0_dll_link_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsi" type="string">
          <ipxact:name>pf0_dsi</ipxact:name>
          <ipxact:displayName>pf0_dsi</ipxact:displayName>
          <ipxact:value>pf0_not_required</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint0" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint0</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint0</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint1" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint1</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint10" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint10</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint10</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint11" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint11</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint11</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint12" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint12</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint13" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint13</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint13</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint14" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint14</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint14</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint15" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint15</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint15</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint2" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint2</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint3" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint3</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint4" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint4</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint4</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint5" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint5</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint5</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint6" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint6</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint6</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint7" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint7</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint7</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint8" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint8</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint8</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_rx_preset_hint9" type="int">
          <ipxact:name>pf0_dsp_rx_preset_hint9</ipxact:name>
          <ipxact:displayName>pf0_dsp_rx_preset_hint9</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset0" type="int">
          <ipxact:name>pf0_dsp_tx_preset0</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset0</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset1" type="int">
          <ipxact:name>pf0_dsp_tx_preset1</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset10" type="int">
          <ipxact:name>pf0_dsp_tx_preset10</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset10</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset11" type="int">
          <ipxact:name>pf0_dsp_tx_preset11</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset11</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset12" type="int">
          <ipxact:name>pf0_dsp_tx_preset12</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset13" type="int">
          <ipxact:name>pf0_dsp_tx_preset13</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset13</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset14" type="int">
          <ipxact:name>pf0_dsp_tx_preset14</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset14</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset15" type="int">
          <ipxact:name>pf0_dsp_tx_preset15</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset15</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset2" type="int">
          <ipxact:name>pf0_dsp_tx_preset2</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset3" type="int">
          <ipxact:name>pf0_dsp_tx_preset3</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset4" type="int">
          <ipxact:name>pf0_dsp_tx_preset4</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset4</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset5" type="int">
          <ipxact:name>pf0_dsp_tx_preset5</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset5</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset6" type="int">
          <ipxact:name>pf0_dsp_tx_preset6</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset6</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset7" type="int">
          <ipxact:name>pf0_dsp_tx_preset7</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset7</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset8" type="int">
          <ipxact:name>pf0_dsp_tx_preset8</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset8</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_dsp_tx_preset9" type="int">
          <ipxact:name>pf0_dsp_tx_preset9</ipxact:name>
          <ipxact:displayName>pf0_dsp_tx_preset9</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_eidle_timer" type="int">
          <ipxact:name>pf0_eidle_timer</ipxact:name>
          <ipxact:displayName>pf0_eidle_timer</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_eq_eieos_cnt" type="string">
          <ipxact:name>pf0_eq_eieos_cnt</ipxact:name>
          <ipxact:displayName>pf0_eq_eieos_cnt</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_eq_phase_2_3" type="string">
          <ipxact:name>pf0_eq_phase_2_3</ipxact:name>
          <ipxact:displayName>pf0_eq_phase_2_3</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_eq_redo" type="string">
          <ipxact:name>pf0_eq_redo</ipxact:name>
          <ipxact:displayName>pf0_eq_redo</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_exp_rom_bar_mask_reg_rsvdp_1" type="int">
          <ipxact:name>pf0_exp_rom_bar_mask_reg_rsvdp_1</ipxact:name>
          <ipxact:displayName>pf0_exp_rom_bar_mask_reg_rsvdp_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_exp_rom_base_addr_reg_rsvdp_1" type="int">
          <ipxact:name>pf0_exp_rom_base_addr_reg_rsvdp_1</ipxact:name>
          <ipxact:displayName>pf0_exp_rom_base_addr_reg_rsvdp_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_fast_link_mode" type="string">
          <ipxact:name>pf0_fast_link_mode</ipxact:name>
          <ipxact:displayName>pf0_fast_link_mode</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_fast_training_seq" type="int">
          <ipxact:name>pf0_fast_training_seq</ipxact:name>
          <ipxact:displayName>pf0_fast_training_seq</ipxact:displayName>
          <ipxact:value>255</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_forward_user_vsec" type="string">
          <ipxact:name>pf0_forward_user_vsec</ipxact:name>
          <ipxact:displayName>pf0_forward_user_vsec</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen1_ei_inference" type="string">
          <ipxact:name>pf0_gen1_ei_inference</ipxact:name>
          <ipxact:displayName>pf0_gen1_ei_inference</ipxact:displayName>
          <ipxact:value>pf0_use_rx_eidle</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen2_ctrl_off_rsvdp_22" type="int">
          <ipxact:name>pf0_gen2_ctrl_off_rsvdp_22</ipxact:name>
          <ipxact:displayName>pf0_gen2_ctrl_off_rsvdp_22</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_dc_balance_disable" type="string">
          <ipxact:name>pf0_gen3_dc_balance_disable</ipxact:name>
          <ipxact:displayName>pf0_gen3_dc_balance_disable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_dllp_xmt_delay_disable" type="string">
          <ipxact:name>pf0_gen3_dllp_xmt_delay_disable</ipxact:name>
          <ipxact:displayName>pf0_gen3_dllp_xmt_delay_disable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_control_off_rsvdp_26" type="int">
          <ipxact:name>pf0_gen3_eq_control_off_rsvdp_26</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_control_off_rsvdp_26</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_control_off_rsvdp_6" type="int">
          <ipxact:name>pf0_gen3_eq_control_off_rsvdp_6</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_control_off_rsvdp_6</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_eval_2ms_disable" type="string">
          <ipxact:name>pf0_gen3_eq_eval_2ms_disable</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_eval_2ms_disable</ipxact:displayName>
          <ipxact:value>pf0_abort</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_fb_mode" type="string">
          <ipxact:name>pf0_gen3_eq_fb_mode</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_fb_mode</ipxact:displayName>
          <ipxact:value>pf0_dir_chg</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_fb_mode_dir_change_off_rsvdp_18" type="int">
          <ipxact:name>pf0_gen3_eq_fb_mode_dir_change_off_rsvdp_18</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_fb_mode_dir_change_off_rsvdp_18</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_fmdc_max_post_cusror_delta" type="int">
          <ipxact:name>pf0_gen3_eq_fmdc_max_post_cusror_delta</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_fmdc_max_post_cusror_delta</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_fmdc_max_pre_cusror_delta" type="int">
          <ipxact:name>pf0_gen3_eq_fmdc_max_pre_cusror_delta</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_fmdc_max_pre_cusror_delta</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_fmdc_n_evals" type="int">
          <ipxact:name>pf0_gen3_eq_fmdc_n_evals</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_fmdc_n_evals</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_fmdc_t_min_phase23" type="int">
          <ipxact:name>pf0_gen3_eq_fmdc_t_min_phase23</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_fmdc_t_min_phase23</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_fom_inc_initial_eval" type="string">
          <ipxact:name>pf0_gen3_eq_fom_inc_initial_eval</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_fom_inc_initial_eval</ipxact:displayName>
          <ipxact:value>pf0_ignore_init_fom</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_local_fs" type="int">
          <ipxact:name>pf0_gen3_eq_local_fs</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_local_fs</ipxact:displayName>
          <ipxact:value>60</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_local_fs_lf_off_rsvdp_12" type="int">
          <ipxact:name>pf0_gen3_eq_local_fs_lf_off_rsvdp_12</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_local_fs_lf_off_rsvdp_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_local_lf" type="int">
          <ipxact:name>pf0_gen3_eq_local_lf</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_local_lf</ipxact:displayName>
          <ipxact:value>20</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_phase23_exit_mode" type="string">
          <ipxact:name>pf0_gen3_eq_phase23_exit_mode</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_phase23_exit_mode</ipxact:displayName>
          <ipxact:value>pf0_next_rec_speed</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_pset_req_as_coef" type="string">
          <ipxact:name>pf0_gen3_eq_pset_req_as_coef</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_pset_req_as_coef</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_eq_pset_req_vec" type="int">
          <ipxact:name>pf0_gen3_eq_pset_req_vec</ipxact:name>
          <ipxact:displayName>pf0_gen3_eq_pset_req_vec</ipxact:displayName>
          <ipxact:value>256</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_equalization_disable" type="string">
          <ipxact:name>pf0_gen3_equalization_disable</ipxact:name>
          <ipxact:displayName>pf0_gen3_equalization_disable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_related_off_rsvdp_1" type="int">
          <ipxact:name>pf0_gen3_related_off_rsvdp_1</ipxact:name>
          <ipxact:displayName>pf0_gen3_related_off_rsvdp_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_related_off_rsvdp_13" type="int">
          <ipxact:name>pf0_gen3_related_off_rsvdp_13</ipxact:name>
          <ipxact:displayName>pf0_gen3_related_off_rsvdp_13</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_related_off_rsvdp_19" type="int">
          <ipxact:name>pf0_gen3_related_off_rsvdp_19</ipxact:name>
          <ipxact:displayName>pf0_gen3_related_off_rsvdp_19</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_gen3_zrxdc_noncompl" type="string">
          <ipxact:name>pf0_gen3_zrxdc_noncompl</ipxact:name>
          <ipxact:displayName>pf0_gen3_zrxdc_noncompl</ipxact:displayName>
          <ipxact:value>pf0_compliant</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_global_inval_spprtd" type="string">
          <ipxact:name>pf0_global_inval_spprtd</ipxact:name>
          <ipxact:displayName>pf0_global_inval_spprtd</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_header_type" type="int">
          <ipxact:name>pf0_header_type</ipxact:name>
          <ipxact:displayName>pf0_header_type</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_int_pin" type="string">
          <ipxact:name>pf0_int_pin</ipxact:name>
          <ipxact:displayName>pf0_int_pin</ipxact:displayName>
          <ipxact:value>pf0_inta</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_invalidate_q_depth" type="int">
          <ipxact:name>pf0_invalidate_q_depth</ipxact:name>
          <ipxact:displayName>pf0_invalidate_q_depth</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control01_reg_rsvdp_15" type="string">
          <ipxact:name>pf0_lane_equalization_control01_reg_rsvdp_15</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control01_reg_rsvdp_15</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control01_reg_rsvdp_23" type="string">
          <ipxact:name>pf0_lane_equalization_control01_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control01_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control01_reg_rsvdp_31" type="string">
          <ipxact:name>pf0_lane_equalization_control01_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control01_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control01_reg_rsvdp_7" type="string">
          <ipxact:name>pf0_lane_equalization_control01_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control01_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1011_reg_rsvdp_15" type="string">
          <ipxact:name>pf0_lane_equalization_control1011_reg_rsvdp_15</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1011_reg_rsvdp_15</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1011_reg_rsvdp_23" type="string">
          <ipxact:name>pf0_lane_equalization_control1011_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1011_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1011_reg_rsvdp_31" type="string">
          <ipxact:name>pf0_lane_equalization_control1011_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1011_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1011_reg_rsvdp_7" type="string">
          <ipxact:name>pf0_lane_equalization_control1011_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1011_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1213_reg_rsvdp_15" type="string">
          <ipxact:name>pf0_lane_equalization_control1213_reg_rsvdp_15</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1213_reg_rsvdp_15</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1213_reg_rsvdp_23" type="string">
          <ipxact:name>pf0_lane_equalization_control1213_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1213_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1213_reg_rsvdp_31" type="string">
          <ipxact:name>pf0_lane_equalization_control1213_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1213_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1213_reg_rsvdp_7" type="string">
          <ipxact:name>pf0_lane_equalization_control1213_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1213_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1415_reg_rsvdp_15" type="string">
          <ipxact:name>pf0_lane_equalization_control1415_reg_rsvdp_15</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1415_reg_rsvdp_15</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1415_reg_rsvdp_23" type="string">
          <ipxact:name>pf0_lane_equalization_control1415_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1415_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1415_reg_rsvdp_31" type="string">
          <ipxact:name>pf0_lane_equalization_control1415_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1415_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control1415_reg_rsvdp_7" type="string">
          <ipxact:name>pf0_lane_equalization_control1415_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control1415_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control23_reg_rsvdp_15" type="string">
          <ipxact:name>pf0_lane_equalization_control23_reg_rsvdp_15</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control23_reg_rsvdp_15</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control23_reg_rsvdp_23" type="string">
          <ipxact:name>pf0_lane_equalization_control23_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control23_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control23_reg_rsvdp_31" type="string">
          <ipxact:name>pf0_lane_equalization_control23_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control23_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control23_reg_rsvdp_7" type="string">
          <ipxact:name>pf0_lane_equalization_control23_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control23_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control45_reg_rsvdp_15" type="string">
          <ipxact:name>pf0_lane_equalization_control45_reg_rsvdp_15</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control45_reg_rsvdp_15</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control45_reg_rsvdp_23" type="string">
          <ipxact:name>pf0_lane_equalization_control45_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control45_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control45_reg_rsvdp_31" type="string">
          <ipxact:name>pf0_lane_equalization_control45_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control45_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control45_reg_rsvdp_7" type="string">
          <ipxact:name>pf0_lane_equalization_control45_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control45_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control67_reg_rsvdp_15" type="string">
          <ipxact:name>pf0_lane_equalization_control67_reg_rsvdp_15</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control67_reg_rsvdp_15</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control67_reg_rsvdp_23" type="string">
          <ipxact:name>pf0_lane_equalization_control67_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control67_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control67_reg_rsvdp_31" type="string">
          <ipxact:name>pf0_lane_equalization_control67_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control67_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control67_reg_rsvdp_7" type="string">
          <ipxact:name>pf0_lane_equalization_control67_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control67_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control89_reg_rsvdp_15" type="string">
          <ipxact:name>pf0_lane_equalization_control89_reg_rsvdp_15</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control89_reg_rsvdp_15</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control89_reg_rsvdp_23" type="string">
          <ipxact:name>pf0_lane_equalization_control89_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control89_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control89_reg_rsvdp_31" type="string">
          <ipxact:name>pf0_lane_equalization_control89_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control89_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_lane_equalization_control89_reg_rsvdp_7" type="string">
          <ipxact:name>pf0_lane_equalization_control89_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf0_lane_equalization_control89_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_link_capabilities_reg_rsvdp_23" type="string">
          <ipxact:name>pf0_link_capabilities_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf0_link_capabilities_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_link_capable" type="string">
          <ipxact:name>pf0_link_capable</ipxact:name>
          <ipxact:displayName>pf0_link_capable</ipxact:displayName>
          <ipxact:value>pf0_conn_x1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_link_control_link_status_reg_rsvdp_12" type="int">
          <ipxact:name>pf0_link_control_link_status_reg_rsvdp_12</ipxact:name>
          <ipxact:displayName>pf0_link_control_link_status_reg_rsvdp_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_link_control_link_status_reg_rsvdp_2" type="string">
          <ipxact:name>pf0_link_control_link_status_reg_rsvdp_2</ipxact:name>
          <ipxact:displayName>pf0_link_control_link_status_reg_rsvdp_2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_link_control_link_status_reg_rsvdp_25" type="int">
          <ipxact:name>pf0_link_control_link_status_reg_rsvdp_25</ipxact:name>
          <ipxact:displayName>pf0_link_control_link_status_reg_rsvdp_25</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_link_control_link_status_reg_rsvdp_9" type="string">
          <ipxact:name>pf0_link_control_link_status_reg_rsvdp_9</ipxact:name>
          <ipxact:displayName>pf0_link_control_link_status_reg_rsvdp_9</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_link_disable" type="string">
          <ipxact:name>pf0_link_disable</ipxact:name>
          <ipxact:displayName>pf0_link_disable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_link_num" type="int">
          <ipxact:name>pf0_link_num</ipxact:name>
          <ipxact:displayName>pf0_link_num</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_loopback_enable" type="string">
          <ipxact:name>pf0_loopback_enable</ipxact:name>
          <ipxact:displayName>pf0_loopback_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_mask_radm_1" type="int">
          <ipxact:name>pf0_mask_radm_1</ipxact:name>
          <ipxact:displayName>pf0_mask_radm_1</ipxact:displayName>
          <ipxact:value>8200</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_max_func_num" type="string">
          <ipxact:name>pf0_max_func_num</ipxact:name>
          <ipxact:displayName>pf0_max_func_num</ipxact:displayName>
          <ipxact:value>pf0_one_function</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_misc_control_1_off_rsvdp_1" type="int">
          <ipxact:name>pf0_misc_control_1_off_rsvdp_1</ipxact:name>
          <ipxact:displayName>pf0_misc_control_1_off_rsvdp_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1" type="int">
          <ipxact:name>pf0_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>81</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2" type="int">
          <ipxact:name>pf0_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>82</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_msix_pba_offset_reg_addr_byte0" type="int">
          <ipxact:name>pf0_msix_cap_msix_pba_offset_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_msix_pba_offset_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>184</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_msix_pba_offset_reg_addr_byte1" type="int">
          <ipxact:name>pf0_msix_cap_msix_pba_offset_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_msix_pba_offset_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>185</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_msix_pba_offset_reg_addr_byte2" type="int">
          <ipxact:name>pf0_msix_cap_msix_pba_offset_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_msix_pba_offset_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>186</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_msix_pba_offset_reg_addr_byte3" type="int">
          <ipxact:name>pf0_msix_cap_msix_pba_offset_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_msix_pba_offset_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>187</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_msix_table_offset_reg_addr_byte0" type="int">
          <ipxact:name>pf0_msix_cap_msix_table_offset_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_msix_table_offset_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>180</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_msix_table_offset_reg_addr_byte1" type="int">
          <ipxact:name>pf0_msix_cap_msix_table_offset_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_msix_table_offset_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>181</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_msix_table_offset_reg_addr_byte2" type="int">
          <ipxact:name>pf0_msix_cap_msix_table_offset_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_msix_table_offset_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>182</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_msix_table_offset_reg_addr_byte3" type="int">
          <ipxact:name>pf0_msix_cap_msix_table_offset_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_msix_table_offset_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>183</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1" type="int">
          <ipxact:name>pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>177</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2" type="int">
          <ipxact:name>pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>178</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3" type="int">
          <ipxact:name>pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>179</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2" type="int">
          <ipxact:name>pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2</ipxact:displayName>
          <ipxact:value>2097330</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3" type="int">
          <ipxact:name>pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3</ipxact:displayName>
          <ipxact:value>2097331</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_multi_func" type="string">
          <ipxact:name>pf0_multi_func</ipxact:name>
          <ipxact:displayName>pf0_multi_func</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_no_soft_rst" type="string">
          <ipxact:name>pf0_no_soft_rst</ipxact:name>
          <ipxact:displayName>pf0_no_soft_rst</ipxact:displayName>
          <ipxact:value>pf0_internally_reset</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_num_of_lanes" type="int">
          <ipxact:name>pf0_num_of_lanes</ipxact:name>
          <ipxact:displayName>pf0_num_of_lanes</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_page_aligned_req" type="string">
          <ipxact:name>pf0_page_aligned_req</ipxact:name>
          <ipxact:displayName>pf0_page_aligned_req</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msi_64_bit_addr_cap" type="string">
          <ipxact:name>pf0_pci_msi_64_bit_addr_cap</ipxact:name>
          <ipxact:displayName>pf0_pci_msi_64_bit_addr_cap</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msi_cap_next_offset" type="int">
          <ipxact:name>pf0_pci_msi_cap_next_offset</ipxact:name>
          <ipxact:displayName>pf0_pci_msi_cap_next_offset</ipxact:displayName>
          <ipxact:value>112</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msi_enable" type="string">
          <ipxact:name>pf0_pci_msi_enable</ipxact:name>
          <ipxact:displayName>pf0_pci_msi_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msi_multiple_msg_cap" type="string">
          <ipxact:name>pf0_pci_msi_multiple_msg_cap</ipxact:name>
          <ipxact:displayName>pf0_pci_msi_multiple_msg_cap</ipxact:displayName>
          <ipxact:value>pf0_msi_vec_4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msi_multiple_msg_en" type="int">
          <ipxact:name>pf0_pci_msi_multiple_msg_en</ipxact:name>
          <ipxact:displayName>pf0_pci_msi_multiple_msg_en</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_bir" type="int">
          <ipxact:name>pf0_pci_msix_bir</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_bir</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_cap_id_next_ctrl_reg_rsvdp_27" type="int">
          <ipxact:name>pf0_pci_msix_cap_id_next_ctrl_reg_rsvdp_27</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_cap_id_next_ctrl_reg_rsvdp_27</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2" type="int">
          <ipxact:name>pf0_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_cap_next_offset" type="int">
          <ipxact:name>pf0_pci_msix_cap_next_offset</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_cap_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_enable" type="string">
          <ipxact:name>pf0_pci_msix_enable</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_enable_vfcomm_cs2" type="string">
          <ipxact:name>pf0_pci_msix_enable_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_enable_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_function_mask" type="string">
          <ipxact:name>pf0_pci_msix_function_mask</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_function_mask</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_function_mask_vfcomm_cs2" type="string">
          <ipxact:name>pf0_pci_msix_function_mask_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_function_mask_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_pba" type="int">
          <ipxact:name>pf0_pci_msix_pba</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_pba</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_pba_offset" type="int">
          <ipxact:name>pf0_pci_msix_pba_offset</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_pba_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_table_offset" type="int">
          <ipxact:name>pf0_pci_msix_table_offset</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_table_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_table_size" type="int">
          <ipxact:name>pf0_pci_msix_table_size</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_table_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_msix_table_size_vfcomm_cs2" type="int">
          <ipxact:name>pf0_pci_msix_table_size_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_pci_msix_table_size_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar0_enabled" type="string">
          <ipxact:name>pf0_pci_type0_bar0_enabled</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar0_enabled</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar0_mask_31_1" type="int">
          <ipxact:name>pf0_pci_type0_bar0_mask_31_1</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar0_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar1_dummy_mask_7_1" type="int">
          <ipxact:name>pf0_pci_type0_bar1_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar1_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar1_enabled" type="string">
          <ipxact:name>pf0_pci_type0_bar1_enabled</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar1_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf0_pci_type0_bar1_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar1_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar1_mask_31_1" type="int">
          <ipxact:name>pf0_pci_type0_bar1_mask_31_1</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar1_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar2_enabled" type="string">
          <ipxact:name>pf0_pci_type0_bar2_enabled</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar2_enabled</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar2_mask_31_1" type="int">
          <ipxact:name>pf0_pci_type0_bar2_mask_31_1</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar2_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar3_dummy_mask_7_1" type="int">
          <ipxact:name>pf0_pci_type0_bar3_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar3_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar3_enabled" type="string">
          <ipxact:name>pf0_pci_type0_bar3_enabled</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar3_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf0_pci_type0_bar3_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar3_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar3_mask_31_1" type="int">
          <ipxact:name>pf0_pci_type0_bar3_mask_31_1</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar3_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar4_enabled" type="string">
          <ipxact:name>pf0_pci_type0_bar4_enabled</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar4_enabled</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar4_mask_31_1" type="int">
          <ipxact:name>pf0_pci_type0_bar4_mask_31_1</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar4_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar5_dummy_mask_7_1" type="int">
          <ipxact:name>pf0_pci_type0_bar5_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar5_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar5_enabled" type="string">
          <ipxact:name>pf0_pci_type0_bar5_enabled</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar5_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf0_pci_type0_bar5_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar5_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_bar5_mask_31_1" type="int">
          <ipxact:name>pf0_pci_type0_bar5_mask_31_1</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_bar5_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_device_id" type="int">
          <ipxact:name>pf0_pci_type0_device_id</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_device_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pci_type0_vendor_id" type="int">
          <ipxact:name>pf0_pci_type0_vendor_id</ipxact:name>
          <ipxact:displayName>pf0_pci_type0_vendor_id</ipxact:displayName>
          <ipxact:value>4466</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_active_state_link_pm_control" type="string">
          <ipxact:name>pf0_pcie_cap_active_state_link_pm_control</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_active_state_link_pm_control</ipxact:displayName>
          <ipxact:value>pf0_aspm_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_active_state_link_pm_support" type="string">
          <ipxact:name>pf0_pcie_cap_active_state_link_pm_support</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_active_state_link_pm_support</ipxact:displayName>
          <ipxact:value>pf0_no_aspm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_aspm_opt_compliance" type="string">
          <ipxact:name>pf0_pcie_cap_aspm_opt_compliance</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_aspm_opt_compliance</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_attention_indicator" type="string">
          <ipxact:name>pf0_pcie_cap_attention_indicator</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_attention_indicator</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_attention_indicator_button" type="string">
          <ipxact:name>pf0_pcie_cap_attention_indicator_button</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_attention_indicator_button</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_aux_power_pm_en" type="string">
          <ipxact:name>pf0_pcie_cap_aux_power_pm_en</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_aux_power_pm_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_clock_power_man" type="string">
          <ipxact:name>pf0_pcie_cap_clock_power_man</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_clock_power_man</ipxact:displayName>
          <ipxact:value>pf0_refclk_remove_not_ok</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_common_clk_config" type="string">
          <ipxact:name>pf0_pcie_cap_common_clk_config</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_common_clk_config</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_crs_sw_visibility" type="string">
          <ipxact:name>pf0_pcie_cap_crs_sw_visibility</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_crs_sw_visibility</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_device_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf0_pcie_cap_device_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_device_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>116</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_device_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf0_pcie_cap_device_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_device_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>117</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_device_capabilities_reg_addr_byte2" type="int">
          <ipxact:name>pf0_pcie_cap_device_capabilities_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_device_capabilities_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>118</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_device_control_device_status_addr_byte1" type="int">
          <ipxact:name>pf0_pcie_cap_device_control_device_status_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_device_control_device_status_addr_byte1</ipxact:displayName>
          <ipxact:value>121</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_dll_active" type="string">
          <ipxact:name>pf0_pcie_cap_dll_active</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_dll_active</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_dll_active_rep_cap" type="string">
          <ipxact:name>pf0_pcie_cap_dll_active_rep_cap</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_dll_active_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_electromech_interlock" type="string">
          <ipxact:name>pf0_pcie_cap_electromech_interlock</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_electromech_interlock</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_en_clk_power_man" type="string">
          <ipxact:name>pf0_pcie_cap_en_clk_power_man</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_en_clk_power_man</ipxact:displayName>
          <ipxact:value>pf0_clkreq_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_en_no_snoop" type="string">
          <ipxact:name>pf0_pcie_cap_en_no_snoop</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_en_no_snoop</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_enter_compliance" type="string">
          <ipxact:name>pf0_pcie_cap_enter_compliance</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_enter_compliance</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_ep_l0s_accpt_latency" type="int">
          <ipxact:name>pf0_pcie_cap_ep_l0s_accpt_latency</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_ep_l0s_accpt_latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_ep_l1_accpt_latency" type="int">
          <ipxact:name>pf0_pcie_cap_ep_l1_accpt_latency</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_ep_l1_accpt_latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_ext_tag_en" type="string">
          <ipxact:name>pf0_pcie_cap_ext_tag_en</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_ext_tag_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_ext_tag_supp" type="string">
          <ipxact:name>pf0_pcie_cap_ext_tag_supp</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_ext_tag_supp</ipxact:displayName>
          <ipxact:value>pf0_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_extended_synch" type="string">
          <ipxact:name>pf0_pcie_cap_extended_synch</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_extended_synch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_flr_cap" type="string">
          <ipxact:name>pf0_pcie_cap_flr_cap</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_flr_cap</ipxact:displayName>
          <ipxact:value>pf0_not_capable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_hot_plug_capable" type="string">
          <ipxact:name>pf0_pcie_cap_hot_plug_capable</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_hot_plug_capable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_hot_plug_surprise" type="string">
          <ipxact:name>pf0_pcie_cap_hot_plug_surprise</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_hot_plug_surprise</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_hw_auto_speed_disable" type="string">
          <ipxact:name>pf0_pcie_cap_hw_auto_speed_disable</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_hw_auto_speed_disable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd" type="string">
          <ipxact:name>pf0_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31" type="string">
          <ipxact:name>pf0_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_initiate_flr" type="string">
          <ipxact:name>pf0_pcie_cap_initiate_flr</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_initiate_flr</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_l0s_exit_latency_commclk_dis" type="int">
          <ipxact:name>pf0_pcie_cap_l0s_exit_latency_commclk_dis</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_l0s_exit_latency_commclk_dis</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_l0s_exit_latency_commclk_ena_cs2" type="int">
          <ipxact:name>pf0_pcie_cap_l0s_exit_latency_commclk_ena_cs2</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_l0s_exit_latency_commclk_ena_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_l1_exit_latency_commclk_dis" type="int">
          <ipxact:name>pf0_pcie_cap_l1_exit_latency_commclk_dis</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_l1_exit_latency_commclk_dis</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_l1_exit_latency_commclk_ena_cs2" type="int">
          <ipxact:name>pf0_pcie_cap_l1_exit_latency_commclk_ena_cs2</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_l1_exit_latency_commclk_ena_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_auto_bw_int_en" type="string">
          <ipxact:name>pf0_pcie_cap_link_auto_bw_int_en</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_auto_bw_int_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_auto_bw_status" type="string">
          <ipxact:name>pf0_pcie_cap_link_auto_bw_status</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_auto_bw_status</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_bw_man_int_en" type="string">
          <ipxact:name>pf0_pcie_cap_link_bw_man_int_en</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_bw_man_int_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_bw_man_status" type="string">
          <ipxact:name>pf0_pcie_cap_link_bw_man_status</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_bw_man_status</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_bw_not_cap" type="string">
          <ipxact:name>pf0_pcie_cap_link_bw_not_cap</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_bw_not_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf0_pcie_cap_link_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>124</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf0_pcie_cap_link_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>125</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_capabilities_reg_addr_byte2" type="int">
          <ipxact:name>pf0_pcie_cap_link_capabilities_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_capabilities_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>126</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_capabilities_reg_addr_byte3" type="int">
          <ipxact:name>pf0_pcie_cap_link_capabilities_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_capabilities_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_control2_link_status2_reg_addr_byte0" type="int">
          <ipxact:name>pf0_pcie_cap_link_control2_link_status2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_control2_link_status2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12583072</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_control_link_status_reg_addr_byte0" type="int">
          <ipxact:name>pf0_pcie_cap_link_control_link_status_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_control_link_status_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4194432</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_control_link_status_reg_addr_byte1" type="int">
          <ipxact:name>pf0_pcie_cap_link_control_link_status_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_control_link_status_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4194433</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_control_link_status_reg_addr_byte2" type="int">
          <ipxact:name>pf0_pcie_cap_link_control_link_status_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_control_link_status_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4194434</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_disable" type="string">
          <ipxact:name>pf0_pcie_cap_link_disable</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_disable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_link_training" type="string">
          <ipxact:name>pf0_pcie_cap_link_training</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_link_training</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_max_link_speed" type="string">
          <ipxact:name>pf0_pcie_cap_max_link_speed</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_max_link_speed</ipxact:displayName>
          <ipxact:value>pf0_max_8gts</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_max_link_width" type="string">
          <ipxact:name>pf0_pcie_cap_max_link_width</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_max_link_width</ipxact:displayName>
          <ipxact:value>pf0_x1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_max_payload_size" type="string">
          <ipxact:name>pf0_pcie_cap_max_payload_size</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_max_payload_size</ipxact:displayName>
          <ipxact:value>pf0_payload_512</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_max_read_req_size" type="int">
          <ipxact:name>pf0_pcie_cap_max_read_req_size</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_max_read_req_size</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_mrl_sensor" type="string">
          <ipxact:name>pf0_pcie_cap_mrl_sensor</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_mrl_sensor</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_nego_link_width" type="string">
          <ipxact:name>pf0_pcie_cap_nego_link_width</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_nego_link_width</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_next_ptr" type="int">
          <ipxact:name>pf0_pcie_cap_next_ptr</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_next_ptr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_no_cmd_cpl_support" type="string">
          <ipxact:name>pf0_pcie_cap_no_cmd_cpl_support</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_no_cmd_cpl_support</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1" type="int">
          <ipxact:name>pf0_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>113</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3" type="int">
          <ipxact:name>pf0_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>115</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_phantom_func_en" type="string">
          <ipxact:name>pf0_pcie_cap_phantom_func_en</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_phantom_func_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_phantom_func_support" type="int">
          <ipxact:name>pf0_pcie_cap_phantom_func_support</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_phantom_func_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_phy_slot_num" type="int">
          <ipxact:name>pf0_pcie_cap_phy_slot_num</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_phy_slot_num</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_port_num" type="int">
          <ipxact:name>pf0_pcie_cap_port_num</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_port_num</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_power_controller" type="string">
          <ipxact:name>pf0_pcie_cap_power_controller</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_power_controller</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_power_indicator" type="string">
          <ipxact:name>pf0_pcie_cap_power_indicator</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_power_indicator</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_rcb" type="string">
          <ipxact:name>pf0_pcie_cap_rcb</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_rcb</ipxact:displayName>
          <ipxact:value>pf0_rcb_64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_retrain_link" type="string">
          <ipxact:name>pf0_pcie_cap_retrain_link</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_retrain_link</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_role_based_err_report" type="string">
          <ipxact:name>pf0_pcie_cap_role_based_err_report</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_role_based_err_report</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_root_control_root_capabilities_reg_addr_byte2" type="int">
          <ipxact:name>pf0_pcie_cap_root_control_root_capabilities_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_root_control_root_capabilities_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>142</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_sel_deemphasis" type="string">
          <ipxact:name>pf0_pcie_cap_sel_deemphasis</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_sel_deemphasis</ipxact:displayName>
          <ipxact:value>pf0_minus_6db</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_shadow_link_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf0_pcie_cap_shadow_link_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_shadow_link_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097276</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_shadow_link_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf0_pcie_cap_shadow_link_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_shadow_link_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097277</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_slot_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf0_pcie_cap_slot_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_slot_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>132</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_slot_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf0_pcie_cap_slot_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_slot_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>133</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_slot_capabilities_reg_addr_byte2" type="int">
          <ipxact:name>pf0_pcie_cap_slot_capabilities_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_slot_capabilities_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>134</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_slot_capabilities_reg_addr_byte3" type="int">
          <ipxact:name>pf0_pcie_cap_slot_capabilities_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_slot_capabilities_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>135</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_slot_clk_config" type="string">
          <ipxact:name>pf0_pcie_cap_slot_clk_config</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_slot_clk_config</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_slot_power_limit_scale" type="int">
          <ipxact:name>pf0_pcie_cap_slot_power_limit_scale</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_slot_power_limit_scale</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_slot_power_limit_value" type="int">
          <ipxact:name>pf0_pcie_cap_slot_power_limit_value</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_slot_power_limit_value</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_surprise_down_err_rep_cap" type="string">
          <ipxact:name>pf0_pcie_cap_surprise_down_err_rep_cap</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_surprise_down_err_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_target_link_speed" type="string">
          <ipxact:name>pf0_pcie_cap_target_link_speed</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_target_link_speed</ipxact:displayName>
          <ipxact:value>pf0_trgt_gen3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_tx_margin" type="string">
          <ipxact:name>pf0_pcie_cap_tx_margin</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_tx_margin</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_int_msg_num" type="int">
          <ipxact:name>pf0_pcie_int_msg_num</ipxact:name>
          <ipxact:displayName>pf0_pcie_int_msg_num</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_slot_imp" type="string">
          <ipxact:name>pf0_pcie_slot_imp</ipxact:name>
          <ipxact:displayName>pf0_pcie_slot_imp</ipxact:displayName>
          <ipxact:value>pf0_not_implemented</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pipe_loopback" type="string">
          <ipxact:name>pf0_pipe_loopback</ipxact:name>
          <ipxact:displayName>pf0_pipe_loopback</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pipe_loopback_control_off_rsvdp_27" type="int">
          <ipxact:name>pf0_pipe_loopback_control_off_rsvdp_27</ipxact:name>
          <ipxact:displayName>pf0_pipe_loopback_control_off_rsvdp_27</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pm_cap_cap_id_nxt_ptr_reg_addr_byte1" type="int">
          <ipxact:name>pf0_pm_cap_cap_id_nxt_ptr_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_pm_cap_cap_id_nxt_ptr_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>65</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pm_cap_cap_id_nxt_ptr_reg_addr_byte2" type="int">
          <ipxact:name>pf0_pm_cap_cap_id_nxt_ptr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_pm_cap_cap_id_nxt_ptr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>66</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pm_cap_cap_id_nxt_ptr_reg_addr_byte3" type="int">
          <ipxact:name>pf0_pm_cap_cap_id_nxt_ptr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_pm_cap_cap_id_nxt_ptr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>67</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pm_cap_con_status_reg_addr_byte0" type="int">
          <ipxact:name>pf0_pm_cap_con_status_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_pm_cap_con_status_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>68</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pm_next_pointer" type="int">
          <ipxact:name>pf0_pm_next_pointer</ipxact:name>
          <ipxact:displayName>pf0_pm_next_pointer</ipxact:displayName>
          <ipxact:value>80</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pm_spec_ver" type="int">
          <ipxact:name>pf0_pm_spec_ver</ipxact:name>
          <ipxact:displayName>pf0_pm_spec_ver</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pme_clk" type="string">
          <ipxact:name>pf0_pme_clk</ipxact:name>
          <ipxact:displayName>pf0_pme_clk</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pme_support" type="int">
          <ipxact:name>pf0_pme_support</ipxact:name>
          <ipxact:displayName>pf0_pme_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_link_ctrl_off_rsvdp_4" type="string">
          <ipxact:name>pf0_port_link_ctrl_off_rsvdp_4</ipxact:name>
          <ipxact:displayName>pf0_port_link_ctrl_off_rsvdp_4</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_ack_f_aspm_ctrl_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_ack_f_aspm_ctrl_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_ack_f_aspm_ctrl_off_addr_byte1</ipxact:displayName>
          <ipxact:value>1805</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_ack_f_aspm_ctrl_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_ack_f_aspm_ctrl_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_ack_f_aspm_ctrl_off_addr_byte2</ipxact:displayName>
          <ipxact:value>1806</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_aux_clk_freq_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_aux_clk_freq_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_aux_clk_freq_off_addr_byte0</ipxact:displayName>
          <ipxact:value>2880</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_aux_clk_freq_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_aux_clk_freq_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_aux_clk_freq_off_addr_byte1</ipxact:displayName>
          <ipxact:value>2881</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_filter_mask_2_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_filter_mask_2_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_filter_mask_2_off_addr_byte0</ipxact:displayName>
          <ipxact:value>1824</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_filter_mask_2_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_filter_mask_2_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_filter_mask_2_off_addr_byte1</ipxact:displayName>
          <ipxact:value>1825</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_filter_mask_2_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_filter_mask_2_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_filter_mask_2_off_addr_byte2</ipxact:displayName>
          <ipxact:value>1826</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_filter_mask_2_off_addr_byte3" type="int">
          <ipxact:name>pf0_port_logic_filter_mask_2_off_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_port_logic_filter_mask_2_off_addr_byte3</ipxact:displayName>
          <ipxact:value>1827</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen2_ctrl_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_gen2_ctrl_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen2_ctrl_off_addr_byte0</ipxact:displayName>
          <ipxact:value>2060</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen2_ctrl_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_gen2_ctrl_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen2_ctrl_off_addr_byte1</ipxact:displayName>
          <ipxact:value>2061</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen2_ctrl_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_gen2_ctrl_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen2_ctrl_off_addr_byte2</ipxact:displayName>
          <ipxact:value>4196366</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_eq_control_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_gen3_eq_control_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_eq_control_off_addr_byte0</ipxact:displayName>
          <ipxact:value>2216</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_eq_control_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_gen3_eq_control_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_eq_control_off_addr_byte1</ipxact:displayName>
          <ipxact:value>2217</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_eq_control_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_gen3_eq_control_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_eq_control_off_addr_byte2</ipxact:displayName>
          <ipxact:value>2218</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_eq_control_off_addr_byte3" type="int">
          <ipxact:name>pf0_port_logic_gen3_eq_control_off_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_eq_control_off_addr_byte3</ipxact:displayName>
          <ipxact:value>2219</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_eq_fb_mode_dir_change_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_gen3_eq_fb_mode_dir_change_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_eq_fb_mode_dir_change_off_addr_byte0</ipxact:displayName>
          <ipxact:value>2220</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_eq_fb_mode_dir_change_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_gen3_eq_fb_mode_dir_change_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_eq_fb_mode_dir_change_off_addr_byte1</ipxact:displayName>
          <ipxact:value>2221</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_eq_fb_mode_dir_change_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_gen3_eq_fb_mode_dir_change_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_eq_fb_mode_dir_change_off_addr_byte2</ipxact:displayName>
          <ipxact:value>2222</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_eq_local_fs_lf_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_gen3_eq_local_fs_lf_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_eq_local_fs_lf_off_addr_byte0</ipxact:displayName>
          <ipxact:value>2196</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_eq_local_fs_lf_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_gen3_eq_local_fs_lf_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_eq_local_fs_lf_off_addr_byte1</ipxact:displayName>
          <ipxact:value>2197</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_related_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_gen3_related_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_related_off_addr_byte0</ipxact:displayName>
          <ipxact:value>2192</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_related_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_gen3_related_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_related_off_addr_byte1</ipxact:displayName>
          <ipxact:value>2193</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_gen3_related_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_gen3_related_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_gen3_related_off_addr_byte2</ipxact:displayName>
          <ipxact:value>2194</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_misc_control_1_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_misc_control_1_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_misc_control_1_off_addr_byte0</ipxact:displayName>
          <ipxact:value>2236</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_pipe_loopback_control_off_addr_byte3" type="int">
          <ipxact:name>pf0_port_logic_pipe_loopback_control_off_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_port_logic_pipe_loopback_control_off_addr_byte3</ipxact:displayName>
          <ipxact:value>2235</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_port_force_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_port_force_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_port_force_off_addr_byte0</ipxact:displayName>
          <ipxact:value>1800</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_port_link_ctrl_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_port_link_ctrl_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_port_link_ctrl_off_addr_byte0</ipxact:displayName>
          <ipxact:value>1808</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_port_link_ctrl_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_port_link_ctrl_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_port_link_ctrl_off_addr_byte2</ipxact:displayName>
          <ipxact:value>1810</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_queue_status_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_queue_status_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_queue_status_off_addr_byte2</ipxact:displayName>
          <ipxact:value>1854</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_queue_status_off_addr_byte3" type="int">
          <ipxact:name>pf0_port_logic_queue_status_off_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_port_logic_queue_status_off_addr_byte3</ipxact:displayName>
          <ipxact:value>1855</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_symbol_timer_filter_1_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_symbol_timer_filter_1_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_symbol_timer_filter_1_off_addr_byte0</ipxact:displayName>
          <ipxact:value>1820</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_symbol_timer_filter_1_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_symbol_timer_filter_1_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_symbol_timer_filter_1_off_addr_byte1</ipxact:displayName>
          <ipxact:value>1821</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_symbol_timer_filter_1_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_symbol_timer_filter_1_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_symbol_timer_filter_1_off_addr_byte2</ipxact:displayName>
          <ipxact:value>1822</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_symbol_timer_filter_1_off_addr_byte3" type="int">
          <ipxact:name>pf0_port_logic_symbol_timer_filter_1_off_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_port_logic_symbol_timer_filter_1_off_addr_byte3</ipxact:displayName>
          <ipxact:value>1823</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_timer_ctrl_max_func_num_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_timer_ctrl_max_func_num_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_timer_ctrl_max_func_num_off_addr_byte0</ipxact:displayName>
          <ipxact:value>1816</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_vc0_cpl_rx_q_ctrl_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_vc0_cpl_rx_q_ctrl_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_vc0_cpl_rx_q_ctrl_off_addr_byte0</ipxact:displayName>
          <ipxact:value>1872</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_vc0_cpl_rx_q_ctrl_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_vc0_cpl_rx_q_ctrl_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_vc0_cpl_rx_q_ctrl_off_addr_byte1</ipxact:displayName>
          <ipxact:value>1873</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_vc0_cpl_rx_q_ctrl_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_vc0_cpl_rx_q_ctrl_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_vc0_cpl_rx_q_ctrl_off_addr_byte2</ipxact:displayName>
          <ipxact:value>1874</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_vc0_np_rx_q_ctrl_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_vc0_np_rx_q_ctrl_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_vc0_np_rx_q_ctrl_off_addr_byte0</ipxact:displayName>
          <ipxact:value>1868</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_vc0_np_rx_q_ctrl_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_vc0_np_rx_q_ctrl_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_vc0_np_rx_q_ctrl_off_addr_byte1</ipxact:displayName>
          <ipxact:value>1869</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_vc0_np_rx_q_ctrl_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_vc0_np_rx_q_ctrl_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_vc0_np_rx_q_ctrl_off_addr_byte2</ipxact:displayName>
          <ipxact:value>1870</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_vc0_p_rx_q_ctrl_off_addr_byte0" type="int">
          <ipxact:name>pf0_port_logic_vc0_p_rx_q_ctrl_off_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_port_logic_vc0_p_rx_q_ctrl_off_addr_byte0</ipxact:displayName>
          <ipxact:value>1864</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_vc0_p_rx_q_ctrl_off_addr_byte1" type="int">
          <ipxact:name>pf0_port_logic_vc0_p_rx_q_ctrl_off_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_port_logic_vc0_p_rx_q_ctrl_off_addr_byte1</ipxact:displayName>
          <ipxact:value>1865</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_port_logic_vc0_p_rx_q_ctrl_off_addr_byte2" type="int">
          <ipxact:name>pf0_port_logic_vc0_p_rx_q_ctrl_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_port_logic_vc0_p_rx_q_ctrl_off_addr_byte2</ipxact:displayName>
          <ipxact:value>1866</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_power_state" type="int">
          <ipxact:name>pf0_power_state</ipxact:name>
          <ipxact:displayName>pf0_power_state</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pre_det_lane" type="string">
          <ipxact:name>pf0_pre_det_lane</ipxact:name>
          <ipxact:displayName>pf0_pre_det_lane</ipxact:displayName>
          <ipxact:value>pf0_det_all_lanes</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_program_interface" type="int">
          <ipxact:name>pf0_program_interface</ipxact:name>
          <ipxact:displayName>pf0_program_interface</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_queue_status_off_rsvdp_29" type="int">
          <ipxact:name>pf0_queue_status_off_rsvdp_29</ipxact:name>
          <ipxact:displayName>pf0_queue_status_off_rsvdp_29</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved4" type="string">
          <ipxact:name>pf0_reserved4</ipxact:name>
          <ipxact:displayName>pf0_reserved4</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved6" type="string">
          <ipxact:name>pf0_reserved6</ipxact:name>
          <ipxact:displayName>pf0_reserved6</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved8" type="string">
          <ipxact:name>pf0_reserved8</ipxact:name>
          <ipxact:displayName>pf0_reserved8</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_0_addr" type="int">
          <ipxact:name>pf0_reserved_0_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_0_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_10_addr" type="int">
          <ipxact:name>pf0_reserved_10_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_10_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_11_addr" type="int">
          <ipxact:name>pf0_reserved_11_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_11_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_12_addr" type="int">
          <ipxact:name>pf0_reserved_12_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_12_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_13_addr" type="int">
          <ipxact:name>pf0_reserved_13_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_13_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_14_addr" type="int">
          <ipxact:name>pf0_reserved_14_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_14_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_15_addr" type="int">
          <ipxact:name>pf0_reserved_15_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_15_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_16_addr" type="int">
          <ipxact:name>pf0_reserved_16_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_16_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_17_addr" type="int">
          <ipxact:name>pf0_reserved_17_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_17_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_18_addr" type="int">
          <ipxact:name>pf0_reserved_18_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_18_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_19_addr" type="int">
          <ipxact:name>pf0_reserved_19_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_19_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_1_addr" type="int">
          <ipxact:name>pf0_reserved_1_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_1_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_20_addr" type="int">
          <ipxact:name>pf0_reserved_20_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_20_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_21_addr" type="int">
          <ipxact:name>pf0_reserved_21_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_21_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_22_addr" type="int">
          <ipxact:name>pf0_reserved_22_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_22_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_23_addr" type="int">
          <ipxact:name>pf0_reserved_23_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_23_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_24_addr" type="int">
          <ipxact:name>pf0_reserved_24_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_24_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_25_addr" type="int">
          <ipxact:name>pf0_reserved_25_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_25_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_26_addr" type="int">
          <ipxact:name>pf0_reserved_26_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_26_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_27_addr" type="int">
          <ipxact:name>pf0_reserved_27_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_27_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_28_addr" type="int">
          <ipxact:name>pf0_reserved_28_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_28_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_29_addr" type="int">
          <ipxact:name>pf0_reserved_29_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_29_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_2_addr" type="int">
          <ipxact:name>pf0_reserved_2_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_2_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_30_addr" type="int">
          <ipxact:name>pf0_reserved_30_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_30_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_31_addr" type="int">
          <ipxact:name>pf0_reserved_31_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_31_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_32_addr" type="int">
          <ipxact:name>pf0_reserved_32_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_32_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_33_addr" type="int">
          <ipxact:name>pf0_reserved_33_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_33_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_34_addr" type="int">
          <ipxact:name>pf0_reserved_34_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_34_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_35_addr" type="int">
          <ipxact:name>pf0_reserved_35_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_35_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_36_addr" type="int">
          <ipxact:name>pf0_reserved_36_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_36_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_37_addr" type="int">
          <ipxact:name>pf0_reserved_37_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_37_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_38_addr" type="int">
          <ipxact:name>pf0_reserved_38_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_38_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_39_addr" type="int">
          <ipxact:name>pf0_reserved_39_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_39_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_3_addr" type="int">
          <ipxact:name>pf0_reserved_3_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_3_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_40_addr" type="int">
          <ipxact:name>pf0_reserved_40_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_40_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_41_addr" type="int">
          <ipxact:name>pf0_reserved_41_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_41_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_42_addr" type="int">
          <ipxact:name>pf0_reserved_42_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_42_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_43_addr" type="int">
          <ipxact:name>pf0_reserved_43_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_43_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_44_addr" type="int">
          <ipxact:name>pf0_reserved_44_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_44_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_45_addr" type="int">
          <ipxact:name>pf0_reserved_45_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_45_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_46_addr" type="int">
          <ipxact:name>pf0_reserved_46_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_46_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_47_addr" type="int">
          <ipxact:name>pf0_reserved_47_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_47_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_48_addr" type="int">
          <ipxact:name>pf0_reserved_48_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_48_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_49_addr" type="int">
          <ipxact:name>pf0_reserved_49_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_49_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_4_addr" type="int">
          <ipxact:name>pf0_reserved_4_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_4_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_50_addr" type="int">
          <ipxact:name>pf0_reserved_50_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_50_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_51_addr" type="int">
          <ipxact:name>pf0_reserved_51_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_51_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_52_addr" type="int">
          <ipxact:name>pf0_reserved_52_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_52_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_53_addr" type="int">
          <ipxact:name>pf0_reserved_53_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_53_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_54_addr" type="int">
          <ipxact:name>pf0_reserved_54_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_54_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_55_addr" type="int">
          <ipxact:name>pf0_reserved_55_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_55_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_56_addr" type="int">
          <ipxact:name>pf0_reserved_56_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_56_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_57_addr" type="int">
          <ipxact:name>pf0_reserved_57_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_57_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_5_addr" type="int">
          <ipxact:name>pf0_reserved_5_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_5_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_6_addr" type="int">
          <ipxact:name>pf0_reserved_6_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_6_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_7_addr" type="int">
          <ipxact:name>pf0_reserved_7_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_7_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_8_addr" type="int">
          <ipxact:name>pf0_reserved_8_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_8_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reserved_9_addr" type="int">
          <ipxact:name>pf0_reserved_9_addr</ipxact:name>
          <ipxact:displayName>pf0_reserved_9_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_reset_assert" type="string">
          <ipxact:name>pf0_reset_assert</ipxact:name>
          <ipxact:displayName>pf0_reset_assert</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_revision_id" type="int">
          <ipxact:name>pf0_revision_id</ipxact:name>
          <ipxact:displayName>pf0_revision_id</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_rom_bar_enable" type="string">
          <ipxact:name>pf0_rom_bar_enable</ipxact:name>
          <ipxact:displayName>pf0_rom_bar_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_rom_bar_enabled" type="string">
          <ipxact:name>pf0_rom_bar_enabled</ipxact:name>
          <ipxact:displayName>pf0_rom_bar_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_rom_mask" type="int">
          <ipxact:name>pf0_rom_mask</ipxact:name>
          <ipxact:displayName>pf0_rom_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_root_control_root_capabilities_reg_rsvdp_17" type="int">
          <ipxact:name>pf0_root_control_root_capabilities_reg_rsvdp_17</ipxact:name>
          <ipxact:displayName>pf0_root_control_root_capabilities_reg_rsvdp_17</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_root_err_status_off_rsvdp_7" type="int">
          <ipxact:name>pf0_root_err_status_off_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf0_root_err_status_off_rsvdp_7</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_rp_exp_rom_bar_mask_reg_rp_rom_rsvdp_1" type="int">
          <ipxact:name>pf0_rp_exp_rom_bar_mask_reg_rp_rom_rsvdp_1</ipxact:name>
          <ipxact:displayName>pf0_rp_exp_rom_bar_mask_reg_rp_rom_rsvdp_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_rp_rom_bar_enabled" type="string">
          <ipxact:name>pf0_rp_rom_bar_enabled</ipxact:name>
          <ipxact:displayName>pf0_rp_rom_bar_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_rp_rom_mask" type="int">
          <ipxact:name>pf0_rp_rom_mask</ipxact:name>
          <ipxact:displayName>pf0_rp_rom_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_rxeq_ph01_en" type="string">
          <ipxact:name>pf0_rxeq_ph01_en</ipxact:name>
          <ipxact:displayName>pf0_rxeq_ph01_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_rxstatus_value" type="int">
          <ipxact:name>pf0_rxstatus_value</ipxact:name>
          <ipxact:displayName>pf0_rxstatus_value</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_scramble_disable" type="string">
          <ipxact:name>pf0_scramble_disable</ipxact:name>
          <ipxact:displayName>pf0_scramble_disable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sel_deemphasis" type="string">
          <ipxact:name>pf0_sel_deemphasis</ipxact:name>
          <ipxact:displayName>pf0_sel_deemphasis</ipxact:displayName>
          <ipxact:value>pf0_minus_3db_ctl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_shadow_link_capabilities_reg_shadow_rsvdp_23" type="string">
          <ipxact:name>pf0_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf0_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_shadow_pcie_cap_active_state_link_pm_support" type="int">
          <ipxact:name>pf0_shadow_pcie_cap_active_state_link_pm_support</ipxact:name>
          <ipxact:displayName>pf0_shadow_pcie_cap_active_state_link_pm_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_shadow_pcie_cap_aspm_opt_compliance" type="string">
          <ipxact:name>pf0_shadow_pcie_cap_aspm_opt_compliance</ipxact:name>
          <ipxact:displayName>pf0_shadow_pcie_cap_aspm_opt_compliance</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_shadow_pcie_cap_clock_power_man" type="string">
          <ipxact:name>pf0_shadow_pcie_cap_clock_power_man</ipxact:name>
          <ipxact:displayName>pf0_shadow_pcie_cap_clock_power_man</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_shadow_pcie_cap_dll_active_rep_cap" type="string">
          <ipxact:name>pf0_shadow_pcie_cap_dll_active_rep_cap</ipxact:name>
          <ipxact:displayName>pf0_shadow_pcie_cap_dll_active_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_shadow_pcie_cap_link_bw_not_cap" type="string">
          <ipxact:name>pf0_shadow_pcie_cap_link_bw_not_cap</ipxact:name>
          <ipxact:displayName>pf0_shadow_pcie_cap_link_bw_not_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_shadow_pcie_cap_max_link_width" type="int">
          <ipxact:name>pf0_shadow_pcie_cap_max_link_width</ipxact:name>
          <ipxact:displayName>pf0_shadow_pcie_cap_max_link_width</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_shadow_pcie_cap_surprise_down_err_rep_cap" type="string">
          <ipxact:name>pf0_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:name>
          <ipxact:displayName>pf0_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_shadow_sriov_vf_stride_ari_cs2" type="int">
          <ipxact:name>pf0_shadow_sriov_vf_stride_ari_cs2</ipxact:name>
          <ipxact:displayName>pf0_shadow_sriov_vf_stride_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_skp_int_val" type="int">
          <ipxact:name>pf0_skp_int_val</ipxact:name>
          <ipxact:displayName>pf0_skp_int_val</ipxact:displayName>
          <ipxact:value>640</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_cap_ser_num_reg_dw_1_addr_byte0" type="int">
          <ipxact:name>pf0_sn_cap_ser_num_reg_dw_1_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sn_cap_ser_num_reg_dw_1_addr_byte0</ipxact:displayName>
          <ipxact:value>364</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_cap_ser_num_reg_dw_1_addr_byte1" type="int">
          <ipxact:name>pf0_sn_cap_ser_num_reg_dw_1_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sn_cap_ser_num_reg_dw_1_addr_byte1</ipxact:displayName>
          <ipxact:value>365</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_cap_ser_num_reg_dw_1_addr_byte2" type="int">
          <ipxact:name>pf0_sn_cap_ser_num_reg_dw_1_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sn_cap_ser_num_reg_dw_1_addr_byte2</ipxact:displayName>
          <ipxact:value>366</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_cap_ser_num_reg_dw_1_addr_byte3" type="int">
          <ipxact:name>pf0_sn_cap_ser_num_reg_dw_1_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sn_cap_ser_num_reg_dw_1_addr_byte3</ipxact:displayName>
          <ipxact:value>367</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_cap_ser_num_reg_dw_2_addr_byte0" type="int">
          <ipxact:name>pf0_sn_cap_ser_num_reg_dw_2_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sn_cap_ser_num_reg_dw_2_addr_byte0</ipxact:displayName>
          <ipxact:value>368</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_cap_ser_num_reg_dw_2_addr_byte1" type="int">
          <ipxact:name>pf0_sn_cap_ser_num_reg_dw_2_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sn_cap_ser_num_reg_dw_2_addr_byte1</ipxact:displayName>
          <ipxact:value>369</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_cap_ser_num_reg_dw_2_addr_byte2" type="int">
          <ipxact:name>pf0_sn_cap_ser_num_reg_dw_2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sn_cap_ser_num_reg_dw_2_addr_byte2</ipxact:displayName>
          <ipxact:value>370</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_cap_ser_num_reg_dw_2_addr_byte3" type="int">
          <ipxact:name>pf0_sn_cap_ser_num_reg_dw_2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sn_cap_ser_num_reg_dw_2_addr_byte3</ipxact:displayName>
          <ipxact:value>371</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_cap_sn_base_addr_byte2" type="int">
          <ipxact:name>pf0_sn_cap_sn_base_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sn_cap_sn_base_addr_byte2</ipxact:displayName>
          <ipxact:value>362</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_cap_sn_base_addr_byte3" type="int">
          <ipxact:name>pf0_sn_cap_sn_base_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sn_cap_sn_base_addr_byte3</ipxact:displayName>
          <ipxact:value>363</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_cap_version" type="int">
          <ipxact:name>pf0_sn_cap_version</ipxact:name>
          <ipxact:displayName>pf0_sn_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sn_next_offset" type="int">
          <ipxact:name>pf0_sn_next_offset</ipxact:name>
          <ipxact:displayName>pf0_sn_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control01_reg_addr_byte0" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control01_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control01_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>404</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control01_reg_addr_byte1" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control01_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control01_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>405</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control01_reg_addr_byte2" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control01_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control01_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>406</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control01_reg_addr_byte3" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control01_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control01_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>407</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte0" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>424</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte1" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>425</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte2" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>426</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte3" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1011_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>427</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte0" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>428</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte1" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>429</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte2" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>430</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte3" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1213_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>431</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte0" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>432</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte1" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>433</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte2" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>434</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte3" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control1415_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>435</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control23_reg_addr_byte0" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control23_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control23_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>408</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control23_reg_addr_byte1" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control23_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control23_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>409</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control23_reg_addr_byte2" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control23_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control23_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>410</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control23_reg_addr_byte3" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control23_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control23_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>411</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control45_reg_addr_byte0" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control45_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control45_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>412</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control45_reg_addr_byte1" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control45_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control45_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>413</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control45_reg_addr_byte2" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control45_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control45_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>414</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control45_reg_addr_byte3" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control45_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control45_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>415</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control67_reg_addr_byte0" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control67_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control67_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>416</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control67_reg_addr_byte1" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control67_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control67_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>417</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control67_reg_addr_byte2" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control67_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control67_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>418</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control67_reg_addr_byte3" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control67_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control67_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>419</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control89_reg_addr_byte0" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control89_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control89_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>420</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control89_reg_addr_byte1" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control89_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control89_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>421</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control89_reg_addr_byte2" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control89_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control89_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>422</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_lane_equalization_control89_reg_addr_byte3" type="int">
          <ipxact:name>pf0_spcie_cap_lane_equalization_control89_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_lane_equalization_control89_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>423</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_spcie_cap_header_reg_addr_byte2" type="int">
          <ipxact:name>pf0_spcie_cap_spcie_cap_header_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_spcie_cap_header_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>394</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_spcie_cap_header_reg_addr_byte3" type="int">
          <ipxact:name>pf0_spcie_cap_spcie_cap_header_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_spcie_cap_header_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>395</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_cap_version" type="int">
          <ipxact:name>pf0_spcie_cap_version</ipxact:name>
          <ipxact:displayName>pf0_spcie_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_spcie_next_offset" type="int">
          <ipxact:name>pf0_spcie_next_offset</ipxact:name>
          <ipxact:displayName>pf0_spcie_next_offset</ipxact:displayName>
          <ipxact:value>2944</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_sriov_initial_vfs_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_sriov_initial_vfs_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_sriov_initial_vfs_addr_byte0</ipxact:displayName>
          <ipxact:value>2097604</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_sriov_initial_vfs_addr_byte1" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_sriov_initial_vfs_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_sriov_initial_vfs_addr_byte1</ipxact:displayName>
          <ipxact:value>2097605</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0</ipxact:displayName>
          <ipxact:value>2097612</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1</ipxact:displayName>
          <ipxact:value>2097613</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2</ipxact:displayName>
          <ipxact:value>2097614</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3</ipxact:displayName>
          <ipxact:value>2097615</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097628</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte1" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097629</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte2" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097630</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte3" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar0_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097631</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097632</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte1" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097633</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte2" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097634</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte3" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar1_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097635</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097636</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte1" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097637</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte2" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097638</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte3" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar2_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097639</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097640</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte1" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097641</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte2" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097642</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte3" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar3_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097643</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097644</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte1" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097645</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte2" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097646</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte3" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar4_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097647</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097648</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte1" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097649</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte2" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097650</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte3" type="int">
          <ipxact:name>pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_shadow_vf_bar5_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097651</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sriov_bar1_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_sriov_bar1_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sriov_bar1_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097632</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sriov_bar3_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_sriov_bar3_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sriov_bar3_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097640</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sriov_bar5_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_sriov_bar5_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sriov_bar5_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097648</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sriov_base_reg_addr_byte2" type="int">
          <ipxact:name>pf0_sriov_cap_sriov_base_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sriov_base_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>442</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sriov_base_reg_addr_byte3" type="int">
          <ipxact:name>pf0_sriov_cap_sriov_base_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sriov_base_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>443</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sriov_initial_vfs_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_sriov_initial_vfs_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sriov_initial_vfs_addr_byte0</ipxact:displayName>
          <ipxact:value>452</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sriov_initial_vfs_addr_byte1" type="int">
          <ipxact:name>pf0_sriov_cap_sriov_initial_vfs_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sriov_initial_vfs_addr_byte1</ipxact:displayName>
          <ipxact:value>453</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sriov_vf_offset_position_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_sriov_vf_offset_position_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sriov_vf_offset_position_addr_byte0</ipxact:displayName>
          <ipxact:value>460</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sriov_vf_offset_position_addr_byte1" type="int">
          <ipxact:name>pf0_sriov_cap_sriov_vf_offset_position_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sriov_vf_offset_position_addr_byte1</ipxact:displayName>
          <ipxact:value>461</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sriov_vf_offset_position_addr_byte2" type="int">
          <ipxact:name>pf0_sriov_cap_sriov_vf_offset_position_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sriov_vf_offset_position_addr_byte2</ipxact:displayName>
          <ipxact:value>462</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sriov_vf_offset_position_addr_byte3" type="int">
          <ipxact:name>pf0_sriov_cap_sriov_vf_offset_position_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sriov_vf_offset_position_addr_byte3</ipxact:displayName>
          <ipxact:value>463</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sup_page_sizes_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_sup_page_sizes_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sup_page_sizes_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>468</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sup_page_sizes_reg_addr_byte1" type="int">
          <ipxact:name>pf0_sriov_cap_sup_page_sizes_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sup_page_sizes_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>469</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sup_page_sizes_reg_addr_byte2" type="int">
          <ipxact:name>pf0_sriov_cap_sup_page_sizes_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sup_page_sizes_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>470</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_sup_page_sizes_reg_addr_byte3" type="int">
          <ipxact:name>pf0_sriov_cap_sup_page_sizes_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_sup_page_sizes_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>471</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_version" type="int">
          <ipxact:name>pf0_sriov_cap_version</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_vf_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_vf_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_vf_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>476</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_vf_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_vf_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_vf_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>480</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_vf_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_vf_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_vf_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>484</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_vf_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_vf_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_vf_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>488</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_vf_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_vf_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_vf_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>492</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_vf_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf0_sriov_cap_vf_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_vf_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>496</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_vf_device_id_reg_addr_byte2" type="int">
          <ipxact:name>pf0_sriov_cap_vf_device_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_vf_device_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>466</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_cap_vf_device_id_reg_addr_byte3" type="int">
          <ipxact:name>pf0_sriov_cap_vf_device_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_sriov_cap_vf_device_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>467</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_initial_vfs_ari_cs2" type="int">
          <ipxact:name>pf0_sriov_initial_vfs_ari_cs2</ipxact:name>
          <ipxact:displayName>pf0_sriov_initial_vfs_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_initial_vfs_nonari" type="int">
          <ipxact:name>pf0_sriov_initial_vfs_nonari</ipxact:name>
          <ipxact:displayName>pf0_sriov_initial_vfs_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_next_offset" type="int">
          <ipxact:name>pf0_sriov_next_offset</ipxact:name>
          <ipxact:displayName>pf0_sriov_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar0_prefetch" type="string">
          <ipxact:name>pf0_sriov_vf_bar0_prefetch</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar0_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar0_start" type="int">
          <ipxact:name>pf0_sriov_vf_bar0_start</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar0_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar0_type" type="string">
          <ipxact:name>pf0_sriov_vf_bar0_type</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar0_type</ipxact:displayName>
          <ipxact:value>pf0_sriov_vf_bar0_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar1_dummy_mask_7_1" type="int">
          <ipxact:name>pf0_sriov_vf_bar1_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar1_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar1_enabled" type="string">
          <ipxact:name>pf0_sriov_vf_bar1_enabled</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar1_prefetch" type="string">
          <ipxact:name>pf0_sriov_vf_bar1_prefetch</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar1_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar1_start" type="int">
          <ipxact:name>pf0_sriov_vf_bar1_start</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar1_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar1_type" type="string">
          <ipxact:name>pf0_sriov_vf_bar1_type</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar1_type</ipxact:displayName>
          <ipxact:value>pf0_sriov_vf_bar1_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar2_prefetch" type="string">
          <ipxact:name>pf0_sriov_vf_bar2_prefetch</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar2_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar2_start" type="int">
          <ipxact:name>pf0_sriov_vf_bar2_start</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar2_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar2_type" type="string">
          <ipxact:name>pf0_sriov_vf_bar2_type</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar2_type</ipxact:displayName>
          <ipxact:value>pf0_sriov_vf_bar2_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar3_dummy_mask_7_1" type="int">
          <ipxact:name>pf0_sriov_vf_bar3_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar3_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar3_enabled" type="string">
          <ipxact:name>pf0_sriov_vf_bar3_enabled</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar3_prefetch" type="string">
          <ipxact:name>pf0_sriov_vf_bar3_prefetch</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar3_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar3_start" type="int">
          <ipxact:name>pf0_sriov_vf_bar3_start</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar3_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar3_type" type="string">
          <ipxact:name>pf0_sriov_vf_bar3_type</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar3_type</ipxact:displayName>
          <ipxact:value>pf0_sriov_vf_bar3_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar4_prefetch" type="string">
          <ipxact:name>pf0_sriov_vf_bar4_prefetch</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar4_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar4_start" type="int">
          <ipxact:name>pf0_sriov_vf_bar4_start</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar4_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar4_type" type="string">
          <ipxact:name>pf0_sriov_vf_bar4_type</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar4_type</ipxact:displayName>
          <ipxact:value>pf0_sriov_vf_bar4_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar5_dummy_mask_7_1" type="int">
          <ipxact:name>pf0_sriov_vf_bar5_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar5_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar5_enabled" type="string">
          <ipxact:name>pf0_sriov_vf_bar5_enabled</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar5_prefetch" type="string">
          <ipxact:name>pf0_sriov_vf_bar5_prefetch</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar5_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar5_start" type="int">
          <ipxact:name>pf0_sriov_vf_bar5_start</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar5_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_bar5_type" type="string">
          <ipxact:name>pf0_sriov_vf_bar5_type</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_bar5_type</ipxact:displayName>
          <ipxact:value>pf0_sriov_vf_bar5_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_device_id" type="int">
          <ipxact:name>pf0_sriov_vf_device_id</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_device_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_offset_ari_cs2" type="int">
          <ipxact:name>pf0_sriov_vf_offset_ari_cs2</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_offset_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_offset_nonari" type="int">
          <ipxact:name>pf0_sriov_vf_offset_nonari</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_offset_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_sriov_vf_stride_nonari" type="int">
          <ipxact:name>pf0_sriov_vf_stride_nonari</ipxact:name>
          <ipxact:displayName>pf0_sriov_vf_stride_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_subclass_code" type="int">
          <ipxact:name>pf0_subclass_code</ipxact:name>
          <ipxact:displayName>pf0_subclass_code</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_subsys_dev_id" type="int">
          <ipxact:name>pf0_subsys_dev_id</ipxact:name>
          <ipxact:displayName>pf0_subsys_dev_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_subsys_vendor_id" type="int">
          <ipxact:name>pf0_subsys_vendor_id</ipxact:name>
          <ipxact:displayName>pf0_subsys_vendor_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_timer_mod_flow_control" type="int">
          <ipxact:name>pf0_timer_mod_flow_control</ipxact:name>
          <ipxact:displayName>pf0_timer_mod_flow_control</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_timer_mod_flow_control_en" type="string">
          <ipxact:name>pf0_timer_mod_flow_control_en</ipxact:name>
          <ipxact:displayName>pf0_timer_mod_flow_control_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_cap_tph_ext_cap_hdr_reg_addr_byte2" type="int">
          <ipxact:name>pf0_tph_cap_tph_ext_cap_hdr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_tph_cap_tph_ext_cap_hdr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>506</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_cap_tph_ext_cap_hdr_reg_addr_byte3" type="int">
          <ipxact:name>pf0_tph_cap_tph_ext_cap_hdr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_tph_cap_tph_ext_cap_hdr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>507</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_cap_tph_req_cap_reg_addr_byte0" type="int">
          <ipxact:name>pf0_tph_cap_tph_req_cap_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_tph_cap_tph_req_cap_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>508</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_cap_tph_req_cap_reg_addr_byte1" type="int">
          <ipxact:name>pf0_tph_cap_tph_req_cap_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_tph_cap_tph_req_cap_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>509</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_cap_tph_req_cap_reg_addr_byte2" type="int">
          <ipxact:name>pf0_tph_cap_tph_req_cap_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_tph_cap_tph_req_cap_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>510</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_cap_tph_req_cap_reg_addr_byte3" type="int">
          <ipxact:name>pf0_tph_cap_tph_req_cap_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_tph_cap_tph_req_cap_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>511</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0" type="int">
          <ipxact:name>pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0</ipxact:displayName>
          <ipxact:value>2097660</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1" type="int">
          <ipxact:name>pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1</ipxact:displayName>
          <ipxact:value>2097661</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2" type="int">
          <ipxact:name>pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2</ipxact:displayName>
          <ipxact:value>2097662</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3" type="int">
          <ipxact:name>pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3</ipxact:displayName>
          <ipxact:value>2097663</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_int_vec" type="string">
          <ipxact:name>pf0_tph_req_cap_int_vec</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_int_vec</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_int_vec_vfcomm_cs2" type="string">
          <ipxact:name>pf0_tph_req_cap_int_vec_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_int_vec_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_reg_rsvdp_11" type="int">
          <ipxact:name>pf0_tph_req_cap_reg_rsvdp_11</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_reg_rsvdp_11</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_reg_rsvdp_27" type="int">
          <ipxact:name>pf0_tph_req_cap_reg_rsvdp_27</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_reg_rsvdp_27</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_reg_rsvdp_3" type="int">
          <ipxact:name>pf0_tph_req_cap_reg_rsvdp_3</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_reg_rsvdp_3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2" type="int">
          <ipxact:name>pf0_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2" type="int">
          <ipxact:name>pf0_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2" type="int">
          <ipxact:name>pf0_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_st_table_loc_0" type="string">
          <ipxact:name>pf0_tph_req_cap_st_table_loc_0</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_st_table_loc_0</ipxact:displayName>
          <ipxact:value>pf0_not_in_tph_struct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_st_table_loc_0_vfcomm_cs2" type="string">
          <ipxact:name>pf0_tph_req_cap_st_table_loc_0_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_st_table_loc_0_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>pf0_in_tph_struct_vf</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_st_table_loc_1" type="string">
          <ipxact:name>pf0_tph_req_cap_st_table_loc_1</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_st_table_loc_1</ipxact:displayName>
          <ipxact:value>pf0_in_msix_table</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_st_table_loc_1_vfcomm_cs2" type="string">
          <ipxact:name>pf0_tph_req_cap_st_table_loc_1_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_st_table_loc_1_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>pf0_in_msix_table_vf</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_st_table_size" type="int">
          <ipxact:name>pf0_tph_req_cap_st_table_size</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_st_table_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_st_table_size_vfcomm_cs2" type="int">
          <ipxact:name>pf0_tph_req_cap_st_table_size_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_st_table_size_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_cap_ver" type="int">
          <ipxact:name>pf0_tph_req_cap_ver</ipxact:name>
          <ipxact:displayName>pf0_tph_req_cap_ver</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_device_spec" type="string">
          <ipxact:name>pf0_tph_req_device_spec</ipxact:name>
          <ipxact:displayName>pf0_tph_req_device_spec</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_device_spec_vfcomm_cs2" type="string">
          <ipxact:name>pf0_tph_req_device_spec_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_tph_req_device_spec_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_extended_tph" type="string">
          <ipxact:name>pf0_tph_req_extended_tph</ipxact:name>
          <ipxact:displayName>pf0_tph_req_extended_tph</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_extended_tph_vfcomm_cs2" type="string">
          <ipxact:name>pf0_tph_req_extended_tph_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_tph_req_extended_tph_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_next_ptr" type="int">
          <ipxact:name>pf0_tph_req_next_ptr</ipxact:name>
          <ipxact:displayName>pf0_tph_req_next_ptr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_no_st_mode" type="string">
          <ipxact:name>pf0_tph_req_no_st_mode</ipxact:name>
          <ipxact:displayName>pf0_tph_req_no_st_mode</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_tph_req_no_st_mode_vfcomm_cs2" type="string">
          <ipxact:name>pf0_tph_req_no_st_mode_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf0_tph_req_no_st_mode_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar0_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar0_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar0_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097168</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar0_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_bar0_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar0_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097169</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar0_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_bar0_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar0_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097170</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar0_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_bar0_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar0_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097171</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>16</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar1_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar1_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar1_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097172</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar1_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar1_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar1_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097172</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar1_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_bar1_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar1_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097173</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar1_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_bar1_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar1_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097174</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar1_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_bar1_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar1_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097175</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>20</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar2_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar2_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar2_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097176</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar2_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_bar2_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar2_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097177</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar2_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_bar2_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar2_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097178</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar2_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_bar2_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar2_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097179</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>24</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar3_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar3_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar3_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097180</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar3_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar3_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar3_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097180</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar3_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_bar3_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar3_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097181</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar3_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_bar3_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar3_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097182</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar3_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_bar3_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar3_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097183</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>28</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar4_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar4_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar4_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097184</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar4_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_bar4_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar4_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097185</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar4_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_bar4_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar4_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097186</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar4_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_bar4_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar4_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097187</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar5_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar5_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar5_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097188</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar5_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar5_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar5_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097188</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar5_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_bar5_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar5_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097189</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar5_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_bar5_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar5_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097190</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar5_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_bar5_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar5_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097191</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>36</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>14</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>40</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>41</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>42</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_cardbus_cis_ptr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>43</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_class_code_revision_id_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_class_code_revision_id_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_class_code_revision_id_addr_byte0</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_class_code_revision_id_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_class_code_revision_id_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_class_code_revision_id_addr_byte1</ipxact:displayName>
          <ipxact:value>9</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_class_code_revision_id_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_class_code_revision_id_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_class_code_revision_id_addr_byte2</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_class_code_revision_id_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_class_code_revision_id_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_class_code_revision_id_addr_byte3</ipxact:displayName>
          <ipxact:value>11</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_device_id_vendor_id_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_device_id_vendor_id_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_device_id_vendor_id_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_device_id_vendor_id_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_device_id_vendor_id_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_device_id_vendor_id_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_device_id_vendor_id_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_device_id_vendor_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_device_id_vendor_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_device_id_vendor_id_reg_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_device_id_vendor_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_device_id_vendor_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097200</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097201</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097202</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_exp_rom_bar_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097203</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_exp_rom_base_addr_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_exp_rom_base_addr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_exp_rom_base_addr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>48</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>61</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_pci_cap_ptr_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_pci_cap_ptr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_pci_cap_ptr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>52</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2097208</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2097209</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2097210</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_rp_exp_rom_bar_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2097211</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0" type="int">
          <ipxact:name>pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>44</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1" type="int">
          <ipxact:name>pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>45</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2" type="int">
          <ipxact:name>pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>46</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3" type="int">
          <ipxact:name>pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>47</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint0" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint0</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint0</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint1" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint1</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint1</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint10" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint10</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint10</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint11" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint11</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint11</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint12" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint12</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint12</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint13" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint13</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint13</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint14" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint14</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint14</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint15" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint15</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint15</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint2" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint2</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint2</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint3" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint3</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint3</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint4" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint4</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint4</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint5" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint5</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint5</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint6" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint6</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint6</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint7" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint7</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint7</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint8" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint8</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint8</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_rx_preset_hint9" type="int">
          <ipxact:name>pf0_usp_rx_preset_hint9</ipxact:name>
          <ipxact:displayName>pf0_usp_rx_preset_hint9</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset0" type="int">
          <ipxact:name>pf0_usp_tx_preset0</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset0</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset1" type="int">
          <ipxact:name>pf0_usp_tx_preset1</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset1</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset10" type="int">
          <ipxact:name>pf0_usp_tx_preset10</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset10</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset11" type="int">
          <ipxact:name>pf0_usp_tx_preset11</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset11</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset12" type="int">
          <ipxact:name>pf0_usp_tx_preset12</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset12</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset13" type="int">
          <ipxact:name>pf0_usp_tx_preset13</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset13</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset14" type="int">
          <ipxact:name>pf0_usp_tx_preset14</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset14</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset15" type="int">
          <ipxact:name>pf0_usp_tx_preset15</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset15</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset2" type="int">
          <ipxact:name>pf0_usp_tx_preset2</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset2</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset3" type="int">
          <ipxact:name>pf0_usp_tx_preset3</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset3</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset4" type="int">
          <ipxact:name>pf0_usp_tx_preset4</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset4</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset5" type="int">
          <ipxact:name>pf0_usp_tx_preset5</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset5</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset6" type="int">
          <ipxact:name>pf0_usp_tx_preset6</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset6</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset7" type="int">
          <ipxact:name>pf0_usp_tx_preset7</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset7</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset8" type="int">
          <ipxact:name>pf0_usp_tx_preset8</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset8</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_usp_tx_preset9" type="int">
          <ipxact:name>pf0_usp_tx_preset9</ipxact:name>
          <ipxact:displayName>pf0_usp_tx_preset9</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc0_cpl_data_credit" type="int">
          <ipxact:name>pf0_vc0_cpl_data_credit</ipxact:name>
          <ipxact:displayName>pf0_vc0_cpl_data_credit</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc0_cpl_header_credit" type="int">
          <ipxact:name>pf0_vc0_cpl_header_credit</ipxact:name>
          <ipxact:displayName>pf0_vc0_cpl_header_credit</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc0_cpl_tlp_q_mode" type="int">
          <ipxact:name>pf0_vc0_cpl_tlp_q_mode</ipxact:name>
          <ipxact:displayName>pf0_vc0_cpl_tlp_q_mode</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc0_np_data_credit" type="int">
          <ipxact:name>pf0_vc0_np_data_credit</ipxact:name>
          <ipxact:displayName>pf0_vc0_np_data_credit</ipxact:displayName>
          <ipxact:value>230</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc0_np_header_credit" type="int">
          <ipxact:name>pf0_vc0_np_header_credit</ipxact:name>
          <ipxact:displayName>pf0_vc0_np_header_credit</ipxact:displayName>
          <ipxact:value>115</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc0_np_tlp_q_mode" type="int">
          <ipxact:name>pf0_vc0_np_tlp_q_mode</ipxact:name>
          <ipxact:displayName>pf0_vc0_np_tlp_q_mode</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc0_p_data_credit" type="int">
          <ipxact:name>pf0_vc0_p_data_credit</ipxact:name>
          <ipxact:displayName>pf0_vc0_p_data_credit</ipxact:displayName>
          <ipxact:value>750</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc0_p_header_credit" type="int">
          <ipxact:name>pf0_vc0_p_header_credit</ipxact:name>
          <ipxact:displayName>pf0_vc0_p_header_credit</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc0_p_tlp_q_mode" type="int">
          <ipxact:name>pf0_vc0_p_tlp_q_mode</ipxact:name>
          <ipxact:displayName>pf0_vc0_p_tlp_q_mode</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc_cap_vc_base_addr_byte2" type="int">
          <ipxact:name>pf0_vc_cap_vc_base_addr_byte2</ipxact:name>
          <ipxact:displayName>pf0_vc_cap_vc_base_addr_byte2</ipxact:displayName>
          <ipxact:value>330</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc_cap_vc_base_addr_byte3" type="int">
          <ipxact:name>pf0_vc_cap_vc_base_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_vc_cap_vc_base_addr_byte3</ipxact:displayName>
          <ipxact:value>331</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc_cap_version" type="int">
          <ipxact:name>pf0_vc_cap_version</ipxact:name>
          <ipxact:displayName>pf0_vc_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vc_next_offset" type="int">
          <ipxact:name>pf0_vc_next_offset</ipxact:name>
          <ipxact:displayName>pf0_vc_next_offset</ipxact:displayName>
          <ipxact:value>392</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vendor_specific_dllp_req" type="string">
          <ipxact:name>pf0_vendor_specific_dllp_req</ipxact:name>
          <ipxact:displayName>pf0_vendor_specific_dllp_req</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vf_bar0_reg_rsvdp_0" type="string">
          <ipxact:name>pf0_vf_bar0_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf0_vf_bar0_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vf_bar1_reg_rsvdp_0" type="string">
          <ipxact:name>pf0_vf_bar1_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf0_vf_bar1_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vf_bar2_reg_rsvdp_0" type="string">
          <ipxact:name>pf0_vf_bar2_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf0_vf_bar2_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vf_bar3_reg_rsvdp_0" type="string">
          <ipxact:name>pf0_vf_bar3_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf0_vf_bar3_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vf_bar4_reg_rsvdp_0" type="string">
          <ipxact:name>pf0_vf_bar4_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf0_vf_bar4_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vf_bar5_reg_rsvdp_0" type="string">
          <ipxact:name>pf0_vf_bar5_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf0_vf_bar5_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_vf_forward_user_vsec" type="string">
          <ipxact:name>pf0_vf_forward_user_vsec</ipxact:name>
          <ipxact:displayName>pf0_vf_forward_user_vsec</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_aer_cap_aer_ext_cap_hdr_off_addr_byte2" type="int">
          <ipxact:name>pf1_aer_cap_aer_ext_cap_hdr_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_aer_cap_aer_ext_cap_hdr_off_addr_byte2</ipxact:displayName>
          <ipxact:value>4354</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_aer_cap_aer_ext_cap_hdr_off_addr_byte3" type="int">
          <ipxact:name>pf1_aer_cap_aer_ext_cap_hdr_off_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_aer_cap_aer_ext_cap_hdr_off_addr_byte3</ipxact:displayName>
          <ipxact:value>4355</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_aer_cap_version" type="int">
          <ipxact:name>pf1_aer_cap_version</ipxact:name>
          <ipxact:displayName>pf1_aer_cap_version</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_aer_next_offset" type="int">
          <ipxact:name>pf1_aer_next_offset</ipxact:name>
          <ipxact:displayName>pf1_aer_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_ari_cap_ari_base_addr_byte2" type="int">
          <ipxact:name>pf1_ari_cap_ari_base_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_ari_cap_ari_base_addr_byte2</ipxact:displayName>
          <ipxact:value>4474</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_ari_cap_ari_base_addr_byte3" type="int">
          <ipxact:name>pf1_ari_cap_ari_base_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_ari_cap_ari_base_addr_byte3</ipxact:displayName>
          <ipxact:value>4475</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_ari_cap_version" type="int">
          <ipxact:name>pf1_ari_cap_version</ipxact:name>
          <ipxact:displayName>pf1_ari_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_ari_next_offset" type="int">
          <ipxact:name>pf1_ari_next_offset</ipxact:name>
          <ipxact:displayName>pf1_ari_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_ats_cap_ats_cap_hdr_reg_addr_byte2" type="int">
          <ipxact:name>pf1_ats_cap_ats_cap_hdr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_ats_cap_ats_cap_hdr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4742</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_ats_cap_ats_cap_hdr_reg_addr_byte3" type="int">
          <ipxact:name>pf1_ats_cap_ats_cap_hdr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_ats_cap_ats_cap_hdr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4743</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_ats_cap_ats_capabilities_ctrl_reg_addr_byte0" type="int">
          <ipxact:name>pf1_ats_cap_ats_capabilities_ctrl_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_ats_cap_ats_capabilities_ctrl_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4744</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_ats_cap_version" type="int">
          <ipxact:name>pf1_ats_cap_version</ipxact:name>
          <ipxact:displayName>pf1_ats_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_ats_capabilities_ctrl_reg_rsvdp_7" type="string">
          <ipxact:name>pf1_ats_capabilities_ctrl_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf1_ats_capabilities_ctrl_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_ats_next_offset" type="int">
          <ipxact:name>pf1_ats_next_offset</ipxact:name>
          <ipxact:displayName>pf1_ats_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_aux_curr" type="int">
          <ipxact:name>pf1_aux_curr</ipxact:name>
          <ipxact:displayName>pf1_aux_curr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar0_mem_io" type="string">
          <ipxact:name>pf1_bar0_mem_io</ipxact:name>
          <ipxact:displayName>pf1_bar0_mem_io</ipxact:displayName>
          <ipxact:value>pf1_bar0_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar0_prefetch" type="string">
          <ipxact:name>pf1_bar0_prefetch</ipxact:name>
          <ipxact:displayName>pf1_bar0_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar0_start" type="int">
          <ipxact:name>pf1_bar0_start</ipxact:name>
          <ipxact:displayName>pf1_bar0_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar0_type" type="string">
          <ipxact:name>pf1_bar0_type</ipxact:name>
          <ipxact:displayName>pf1_bar0_type</ipxact:displayName>
          <ipxact:value>pf1_bar0_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar1_mem_io" type="string">
          <ipxact:name>pf1_bar1_mem_io</ipxact:name>
          <ipxact:displayName>pf1_bar1_mem_io</ipxact:displayName>
          <ipxact:value>pf1_bar1_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar1_prefetch" type="string">
          <ipxact:name>pf1_bar1_prefetch</ipxact:name>
          <ipxact:displayName>pf1_bar1_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar1_start" type="int">
          <ipxact:name>pf1_bar1_start</ipxact:name>
          <ipxact:displayName>pf1_bar1_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar1_type" type="string">
          <ipxact:name>pf1_bar1_type</ipxact:name>
          <ipxact:displayName>pf1_bar1_type</ipxact:displayName>
          <ipxact:value>pf1_bar1_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar2_mem_io" type="string">
          <ipxact:name>pf1_bar2_mem_io</ipxact:name>
          <ipxact:displayName>pf1_bar2_mem_io</ipxact:displayName>
          <ipxact:value>pf1_bar2_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar2_prefetch" type="string">
          <ipxact:name>pf1_bar2_prefetch</ipxact:name>
          <ipxact:displayName>pf1_bar2_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar2_start" type="int">
          <ipxact:name>pf1_bar2_start</ipxact:name>
          <ipxact:displayName>pf1_bar2_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar2_type" type="string">
          <ipxact:name>pf1_bar2_type</ipxact:name>
          <ipxact:displayName>pf1_bar2_type</ipxact:displayName>
          <ipxact:value>pf1_bar2_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar3_mem_io" type="string">
          <ipxact:name>pf1_bar3_mem_io</ipxact:name>
          <ipxact:displayName>pf1_bar3_mem_io</ipxact:displayName>
          <ipxact:value>pf1_bar3_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar3_prefetch" type="string">
          <ipxact:name>pf1_bar3_prefetch</ipxact:name>
          <ipxact:displayName>pf1_bar3_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar3_start" type="int">
          <ipxact:name>pf1_bar3_start</ipxact:name>
          <ipxact:displayName>pf1_bar3_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar3_type" type="string">
          <ipxact:name>pf1_bar3_type</ipxact:name>
          <ipxact:displayName>pf1_bar3_type</ipxact:displayName>
          <ipxact:value>pf1_bar3_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar4_mem_io" type="string">
          <ipxact:name>pf1_bar4_mem_io</ipxact:name>
          <ipxact:displayName>pf1_bar4_mem_io</ipxact:displayName>
          <ipxact:value>pf1_bar4_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar4_prefetch" type="string">
          <ipxact:name>pf1_bar4_prefetch</ipxact:name>
          <ipxact:displayName>pf1_bar4_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar4_start" type="int">
          <ipxact:name>pf1_bar4_start</ipxact:name>
          <ipxact:displayName>pf1_bar4_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar4_type" type="string">
          <ipxact:name>pf1_bar4_type</ipxact:name>
          <ipxact:displayName>pf1_bar4_type</ipxact:displayName>
          <ipxact:value>pf1_bar4_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar5_mem_io" type="string">
          <ipxact:name>pf1_bar5_mem_io</ipxact:name>
          <ipxact:displayName>pf1_bar5_mem_io</ipxact:displayName>
          <ipxact:value>pf1_bar5_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar5_prefetch" type="string">
          <ipxact:name>pf1_bar5_prefetch</ipxact:name>
          <ipxact:displayName>pf1_bar5_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar5_start" type="int">
          <ipxact:name>pf1_bar5_start</ipxact:name>
          <ipxact:displayName>pf1_bar5_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_bar5_type" type="string">
          <ipxact:name>pf1_bar5_type</ipxact:name>
          <ipxact:displayName>pf1_bar5_type</ipxact:displayName>
          <ipxact:value>pf1_bar5_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_base_class_code" type="int">
          <ipxact:name>pf1_base_class_code</ipxact:name>
          <ipxact:displayName>pf1_base_class_code</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_cap_id_nxt_ptr_reg_rsvdp_20" type="string">
          <ipxact:name>pf1_cap_id_nxt_ptr_reg_rsvdp_20</ipxact:name>
          <ipxact:displayName>pf1_cap_id_nxt_ptr_reg_rsvdp_20</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_cap_pointer" type="int">
          <ipxact:name>pf1_cap_pointer</ipxact:name>
          <ipxact:displayName>pf1_cap_pointer</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_con_status_reg_rsvdp_2" type="string">
          <ipxact:name>pf1_con_status_reg_rsvdp_2</ipxact:name>
          <ipxact:displayName>pf1_con_status_reg_rsvdp_2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_con_status_reg_rsvdp_4" type="int">
          <ipxact:name>pf1_con_status_reg_rsvdp_4</ipxact:name>
          <ipxact:displayName>pf1_con_status_reg_rsvdp_4</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_d1_support" type="string">
          <ipxact:name>pf1_d1_support</ipxact:name>
          <ipxact:displayName>pf1_d1_support</ipxact:displayName>
          <ipxact:value>pf1_d1_not_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_d2_support" type="string">
          <ipxact:name>pf1_d2_support</ipxact:name>
          <ipxact:displayName>pf1_d2_support</ipxact:displayName>
          <ipxact:value>pf1_d2_not_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_0" type="int">
          <ipxact:name>pf1_dbi_reserved_0</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_0</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_1" type="int">
          <ipxact:name>pf1_dbi_reserved_1</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_10" type="int">
          <ipxact:name>pf1_dbi_reserved_10</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_10</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_11" type="int">
          <ipxact:name>pf1_dbi_reserved_11</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_11</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_12" type="int">
          <ipxact:name>pf1_dbi_reserved_12</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_13" type="int">
          <ipxact:name>pf1_dbi_reserved_13</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_13</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_14" type="int">
          <ipxact:name>pf1_dbi_reserved_14</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_14</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_15" type="int">
          <ipxact:name>pf1_dbi_reserved_15</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_15</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_16" type="int">
          <ipxact:name>pf1_dbi_reserved_16</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_16</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_17" type="int">
          <ipxact:name>pf1_dbi_reserved_17</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_17</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_18" type="int">
          <ipxact:name>pf1_dbi_reserved_18</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_18</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_19" type="int">
          <ipxact:name>pf1_dbi_reserved_19</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_19</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_2" type="int">
          <ipxact:name>pf1_dbi_reserved_2</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_3" type="int">
          <ipxact:name>pf1_dbi_reserved_3</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_4" type="int">
          <ipxact:name>pf1_dbi_reserved_4</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_4</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_5" type="int">
          <ipxact:name>pf1_dbi_reserved_5</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_5</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_6" type="int">
          <ipxact:name>pf1_dbi_reserved_6</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_6</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_7" type="int">
          <ipxact:name>pf1_dbi_reserved_7</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_7</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_8" type="int">
          <ipxact:name>pf1_dbi_reserved_8</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_8</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dbi_reserved_9" type="int">
          <ipxact:name>pf1_dbi_reserved_9</ipxact:name>
          <ipxact:displayName>pf1_dbi_reserved_9</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_device_capabilities_reg_rsvdp_12" type="int">
          <ipxact:name>pf1_device_capabilities_reg_rsvdp_12</ipxact:name>
          <ipxact:displayName>pf1_device_capabilities_reg_rsvdp_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_device_capabilities_reg_rsvdp_16" type="int">
          <ipxact:name>pf1_device_capabilities_reg_rsvdp_16</ipxact:name>
          <ipxact:displayName>pf1_device_capabilities_reg_rsvdp_16</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_device_capabilities_reg_rsvdp_29" type="int">
          <ipxact:name>pf1_device_capabilities_reg_rsvdp_29</ipxact:name>
          <ipxact:displayName>pf1_device_capabilities_reg_rsvdp_29</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_dsi" type="string">
          <ipxact:name>pf1_dsi</ipxact:name>
          <ipxact:displayName>pf1_dsi</ipxact:displayName>
          <ipxact:value>pf1_not_required</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_exp_rom_bar_mask_reg_rsvdp_1" type="int">
          <ipxact:name>pf1_exp_rom_bar_mask_reg_rsvdp_1</ipxact:name>
          <ipxact:displayName>pf1_exp_rom_bar_mask_reg_rsvdp_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_exp_rom_base_addr_reg_rsvdp_1" type="int">
          <ipxact:name>pf1_exp_rom_base_addr_reg_rsvdp_1</ipxact:name>
          <ipxact:displayName>pf1_exp_rom_base_addr_reg_rsvdp_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_forward_user_vsec" type="string">
          <ipxact:name>pf1_forward_user_vsec</ipxact:name>
          <ipxact:displayName>pf1_forward_user_vsec</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_global_inval_spprtd" type="string">
          <ipxact:name>pf1_global_inval_spprtd</ipxact:name>
          <ipxact:displayName>pf1_global_inval_spprtd</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_header_type" type="int">
          <ipxact:name>pf1_header_type</ipxact:name>
          <ipxact:displayName>pf1_header_type</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_int_pin" type="string">
          <ipxact:name>pf1_int_pin</ipxact:name>
          <ipxact:displayName>pf1_int_pin</ipxact:displayName>
          <ipxact:value>pf1_no_int</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_invalidate_q_depth" type="int">
          <ipxact:name>pf1_invalidate_q_depth</ipxact:name>
          <ipxact:displayName>pf1_invalidate_q_depth</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_link_capabilities_reg_rsvdp_23" type="string">
          <ipxact:name>pf1_link_capabilities_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf1_link_capabilities_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_link_control_link_status_reg_rsvdp_12" type="int">
          <ipxact:name>pf1_link_control_link_status_reg_rsvdp_12</ipxact:name>
          <ipxact:displayName>pf1_link_control_link_status_reg_rsvdp_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_link_control_link_status_reg_rsvdp_2" type="string">
          <ipxact:name>pf1_link_control_link_status_reg_rsvdp_2</ipxact:name>
          <ipxact:displayName>pf1_link_control_link_status_reg_rsvdp_2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_link_control_link_status_reg_rsvdp_25" type="int">
          <ipxact:name>pf1_link_control_link_status_reg_rsvdp_25</ipxact:name>
          <ipxact:displayName>pf1_link_control_link_status_reg_rsvdp_25</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_link_control_link_status_reg_rsvdp_9" type="string">
          <ipxact:name>pf1_link_control_link_status_reg_rsvdp_9</ipxact:name>
          <ipxact:displayName>pf1_link_control_link_status_reg_rsvdp_9</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1" type="int">
          <ipxact:name>pf1_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4177</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2" type="int">
          <ipxact:name>pf1_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4178</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_msix_pba_offset_reg_addr_byte0" type="int">
          <ipxact:name>pf1_msix_cap_msix_pba_offset_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_msix_pba_offset_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4280</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_msix_pba_offset_reg_addr_byte1" type="int">
          <ipxact:name>pf1_msix_cap_msix_pba_offset_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_msix_pba_offset_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4281</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_msix_pba_offset_reg_addr_byte2" type="int">
          <ipxact:name>pf1_msix_cap_msix_pba_offset_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_msix_pba_offset_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4282</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_msix_pba_offset_reg_addr_byte3" type="int">
          <ipxact:name>pf1_msix_cap_msix_pba_offset_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_msix_pba_offset_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4283</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_msix_table_offset_reg_addr_byte0" type="int">
          <ipxact:name>pf1_msix_cap_msix_table_offset_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_msix_table_offset_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4276</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_msix_table_offset_reg_addr_byte1" type="int">
          <ipxact:name>pf1_msix_cap_msix_table_offset_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_msix_table_offset_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4277</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_msix_table_offset_reg_addr_byte2" type="int">
          <ipxact:name>pf1_msix_cap_msix_table_offset_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_msix_table_offset_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4278</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_msix_table_offset_reg_addr_byte3" type="int">
          <ipxact:name>pf1_msix_cap_msix_table_offset_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_msix_table_offset_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4279</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1" type="int">
          <ipxact:name>pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4273</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2" type="int">
          <ipxact:name>pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4274</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3" type="int">
          <ipxact:name>pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4275</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2" type="int">
          <ipxact:name>pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2</ipxact:displayName>
          <ipxact:value>2101426</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3" type="int">
          <ipxact:name>pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3</ipxact:displayName>
          <ipxact:value>2101427</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_multi_func" type="string">
          <ipxact:name>pf1_multi_func</ipxact:name>
          <ipxact:displayName>pf1_multi_func</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_no_soft_rst" type="string">
          <ipxact:name>pf1_no_soft_rst</ipxact:name>
          <ipxact:displayName>pf1_no_soft_rst</ipxact:displayName>
          <ipxact:value>pf1_internally_reset</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_page_aligned_req" type="string">
          <ipxact:name>pf1_page_aligned_req</ipxact:name>
          <ipxact:displayName>pf1_page_aligned_req</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msi_64_bit_addr_cap" type="string">
          <ipxact:name>pf1_pci_msi_64_bit_addr_cap</ipxact:name>
          <ipxact:displayName>pf1_pci_msi_64_bit_addr_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msi_cap_next_offset" type="int">
          <ipxact:name>pf1_pci_msi_cap_next_offset</ipxact:name>
          <ipxact:displayName>pf1_pci_msi_cap_next_offset</ipxact:displayName>
          <ipxact:value>112</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msi_enable" type="string">
          <ipxact:name>pf1_pci_msi_enable</ipxact:name>
          <ipxact:displayName>pf1_pci_msi_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msi_multiple_msg_cap" type="string">
          <ipxact:name>pf1_pci_msi_multiple_msg_cap</ipxact:name>
          <ipxact:displayName>pf1_pci_msi_multiple_msg_cap</ipxact:displayName>
          <ipxact:value>pf1_msi_vec_1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msi_multiple_msg_en" type="int">
          <ipxact:name>pf1_pci_msi_multiple_msg_en</ipxact:name>
          <ipxact:displayName>pf1_pci_msi_multiple_msg_en</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_bir" type="int">
          <ipxact:name>pf1_pci_msix_bir</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_bir</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_cap_id_next_ctrl_reg_rsvdp_27" type="int">
          <ipxact:name>pf1_pci_msix_cap_id_next_ctrl_reg_rsvdp_27</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_cap_id_next_ctrl_reg_rsvdp_27</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2" type="int">
          <ipxact:name>pf1_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_cap_next_offset" type="int">
          <ipxact:name>pf1_pci_msix_cap_next_offset</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_cap_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_enable" type="string">
          <ipxact:name>pf1_pci_msix_enable</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_enable_vfcomm_cs2" type="string">
          <ipxact:name>pf1_pci_msix_enable_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_enable_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_function_mask" type="string">
          <ipxact:name>pf1_pci_msix_function_mask</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_function_mask</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_function_mask_vfcomm_cs2" type="string">
          <ipxact:name>pf1_pci_msix_function_mask_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_function_mask_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_pba" type="int">
          <ipxact:name>pf1_pci_msix_pba</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_pba</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_pba_offset" type="int">
          <ipxact:name>pf1_pci_msix_pba_offset</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_pba_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_table_offset" type="int">
          <ipxact:name>pf1_pci_msix_table_offset</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_table_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_table_size" type="int">
          <ipxact:name>pf1_pci_msix_table_size</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_table_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_msix_table_size_vfcomm_cs2" type="int">
          <ipxact:name>pf1_pci_msix_table_size_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_pci_msix_table_size_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar0_enabled" type="string">
          <ipxact:name>pf1_pci_type0_bar0_enabled</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar0_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar0_mask_31_1" type="int">
          <ipxact:name>pf1_pci_type0_bar0_mask_31_1</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar0_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar1_dummy_mask_7_1" type="int">
          <ipxact:name>pf1_pci_type0_bar1_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar1_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar1_enabled" type="string">
          <ipxact:name>pf1_pci_type0_bar1_enabled</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar1_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf1_pci_type0_bar1_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar1_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar1_mask_31_1" type="int">
          <ipxact:name>pf1_pci_type0_bar1_mask_31_1</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar1_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar2_enabled" type="string">
          <ipxact:name>pf1_pci_type0_bar2_enabled</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar2_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar2_mask_31_1" type="int">
          <ipxact:name>pf1_pci_type0_bar2_mask_31_1</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar2_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar3_dummy_mask_7_1" type="int">
          <ipxact:name>pf1_pci_type0_bar3_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar3_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar3_enabled" type="string">
          <ipxact:name>pf1_pci_type0_bar3_enabled</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar3_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf1_pci_type0_bar3_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar3_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar3_mask_31_1" type="int">
          <ipxact:name>pf1_pci_type0_bar3_mask_31_1</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar3_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar4_enabled" type="string">
          <ipxact:name>pf1_pci_type0_bar4_enabled</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar4_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar4_mask_31_1" type="int">
          <ipxact:name>pf1_pci_type0_bar4_mask_31_1</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar4_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar5_dummy_mask_7_1" type="int">
          <ipxact:name>pf1_pci_type0_bar5_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar5_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar5_enabled" type="string">
          <ipxact:name>pf1_pci_type0_bar5_enabled</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar5_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf1_pci_type0_bar5_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar5_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_bar5_mask_31_1" type="int">
          <ipxact:name>pf1_pci_type0_bar5_mask_31_1</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_bar5_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_device_id" type="int">
          <ipxact:name>pf1_pci_type0_device_id</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_device_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pci_type0_vendor_id" type="int">
          <ipxact:name>pf1_pci_type0_vendor_id</ipxact:name>
          <ipxact:displayName>pf1_pci_type0_vendor_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_active_state_link_pm_control" type="string">
          <ipxact:name>pf1_pcie_cap_active_state_link_pm_control</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_active_state_link_pm_control</ipxact:displayName>
          <ipxact:value>pf1_aspm_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_active_state_link_pm_support" type="string">
          <ipxact:name>pf1_pcie_cap_active_state_link_pm_support</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_active_state_link_pm_support</ipxact:displayName>
          <ipxact:value>pf1_no_aspm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_aspm_opt_compliance" type="string">
          <ipxact:name>pf1_pcie_cap_aspm_opt_compliance</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_aspm_opt_compliance</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_aux_power_pm_en" type="string">
          <ipxact:name>pf1_pcie_cap_aux_power_pm_en</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_aux_power_pm_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_clock_power_man" type="string">
          <ipxact:name>pf1_pcie_cap_clock_power_man</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_clock_power_man</ipxact:displayName>
          <ipxact:value>pf1_refclk_remove_not_ok</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_common_clk_config" type="string">
          <ipxact:name>pf1_pcie_cap_common_clk_config</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_common_clk_config</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_device_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf1_pcie_cap_device_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_device_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4212</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_device_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf1_pcie_cap_device_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_device_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4213</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_device_capabilities_reg_addr_byte2" type="int">
          <ipxact:name>pf1_pcie_cap_device_capabilities_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_device_capabilities_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4214</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_device_control_device_status_addr_byte1" type="int">
          <ipxact:name>pf1_pcie_cap_device_control_device_status_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_device_control_device_status_addr_byte1</ipxact:displayName>
          <ipxact:value>4217</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_dll_active" type="string">
          <ipxact:name>pf1_pcie_cap_dll_active</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_dll_active</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_dll_active_rep_cap" type="string">
          <ipxact:name>pf1_pcie_cap_dll_active_rep_cap</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_dll_active_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_en_clk_power_man" type="string">
          <ipxact:name>pf1_pcie_cap_en_clk_power_man</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_en_clk_power_man</ipxact:displayName>
          <ipxact:value>pf1_clkreq_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_en_no_snoop" type="string">
          <ipxact:name>pf1_pcie_cap_en_no_snoop</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_en_no_snoop</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_enter_compliance" type="string">
          <ipxact:name>pf1_pcie_cap_enter_compliance</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_enter_compliance</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_ep_l0s_accpt_latency" type="int">
          <ipxact:name>pf1_pcie_cap_ep_l0s_accpt_latency</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_ep_l0s_accpt_latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_ep_l1_accpt_latency" type="int">
          <ipxact:name>pf1_pcie_cap_ep_l1_accpt_latency</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_ep_l1_accpt_latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_ext_tag_en" type="string">
          <ipxact:name>pf1_pcie_cap_ext_tag_en</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_ext_tag_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_ext_tag_supp" type="string">
          <ipxact:name>pf1_pcie_cap_ext_tag_supp</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_ext_tag_supp</ipxact:displayName>
          <ipxact:value>pf1_not_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_extended_synch" type="string">
          <ipxact:name>pf1_pcie_cap_extended_synch</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_extended_synch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_flr_cap" type="string">
          <ipxact:name>pf1_pcie_cap_flr_cap</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_flr_cap</ipxact:displayName>
          <ipxact:value>pf1_not_capable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_hw_auto_speed_disable" type="string">
          <ipxact:name>pf1_pcie_cap_hw_auto_speed_disable</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_hw_auto_speed_disable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd" type="string">
          <ipxact:name>pf1_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31" type="string">
          <ipxact:name>pf1_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_initiate_flr" type="string">
          <ipxact:name>pf1_pcie_cap_initiate_flr</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_initiate_flr</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_l0s_exit_latency_commclk_dis" type="int">
          <ipxact:name>pf1_pcie_cap_l0s_exit_latency_commclk_dis</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_l0s_exit_latency_commclk_dis</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_l0s_exit_latency_commclk_ena_cs2" type="int">
          <ipxact:name>pf1_pcie_cap_l0s_exit_latency_commclk_ena_cs2</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_l0s_exit_latency_commclk_ena_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_l1_exit_latency_commclk_dis" type="int">
          <ipxact:name>pf1_pcie_cap_l1_exit_latency_commclk_dis</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_l1_exit_latency_commclk_dis</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_l1_exit_latency_commclk_ena_cs2" type="int">
          <ipxact:name>pf1_pcie_cap_l1_exit_latency_commclk_ena_cs2</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_l1_exit_latency_commclk_ena_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_auto_bw_int_en" type="string">
          <ipxact:name>pf1_pcie_cap_link_auto_bw_int_en</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_auto_bw_int_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_auto_bw_status" type="string">
          <ipxact:name>pf1_pcie_cap_link_auto_bw_status</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_auto_bw_status</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_bw_man_int_en" type="string">
          <ipxact:name>pf1_pcie_cap_link_bw_man_int_en</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_bw_man_int_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_bw_man_status" type="string">
          <ipxact:name>pf1_pcie_cap_link_bw_man_status</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_bw_man_status</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_bw_not_cap" type="string">
          <ipxact:name>pf1_pcie_cap_link_bw_not_cap</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_bw_not_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf1_pcie_cap_link_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4220</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf1_pcie_cap_link_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4221</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_capabilities_reg_addr_byte2" type="int">
          <ipxact:name>pf1_pcie_cap_link_capabilities_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_capabilities_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4222</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_capabilities_reg_addr_byte3" type="int">
          <ipxact:name>pf1_pcie_cap_link_capabilities_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_capabilities_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4223</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_control2_link_status2_reg_addr_byte0" type="int">
          <ipxact:name>pf1_pcie_cap_link_control2_link_status2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_control2_link_status2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12587168</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_control_link_status_reg_addr_byte0" type="int">
          <ipxact:name>pf1_pcie_cap_link_control_link_status_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_control_link_status_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4198528</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_control_link_status_reg_addr_byte1" type="int">
          <ipxact:name>pf1_pcie_cap_link_control_link_status_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_control_link_status_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4198529</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_control_link_status_reg_addr_byte2" type="int">
          <ipxact:name>pf1_pcie_cap_link_control_link_status_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_control_link_status_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4198530</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_disable" type="string">
          <ipxact:name>pf1_pcie_cap_link_disable</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_disable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_link_training" type="string">
          <ipxact:name>pf1_pcie_cap_link_training</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_link_training</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_max_link_speed" type="string">
          <ipxact:name>pf1_pcie_cap_max_link_speed</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_max_link_speed</ipxact:displayName>
          <ipxact:value>pf1_max_8gts</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_max_link_width" type="string">
          <ipxact:name>pf1_pcie_cap_max_link_width</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_max_link_width</ipxact:displayName>
          <ipxact:value>pf1_x1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_max_payload_size" type="string">
          <ipxact:name>pf1_pcie_cap_max_payload_size</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_max_payload_size</ipxact:displayName>
          <ipxact:value>pf1_payload_512</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_max_read_req_size" type="int">
          <ipxact:name>pf1_pcie_cap_max_read_req_size</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_max_read_req_size</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_nego_link_width" type="string">
          <ipxact:name>pf1_pcie_cap_nego_link_width</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_nego_link_width</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_next_ptr" type="int">
          <ipxact:name>pf1_pcie_cap_next_ptr</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_next_ptr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1" type="int">
          <ipxact:name>pf1_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4209</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3" type="int">
          <ipxact:name>pf1_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4211</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_phantom_func_en" type="string">
          <ipxact:name>pf1_pcie_cap_phantom_func_en</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_phantom_func_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_phantom_func_support" type="int">
          <ipxact:name>pf1_pcie_cap_phantom_func_support</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_phantom_func_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_port_num" type="int">
          <ipxact:name>pf1_pcie_cap_port_num</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_port_num</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_rcb" type="string">
          <ipxact:name>pf1_pcie_cap_rcb</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_rcb</ipxact:displayName>
          <ipxact:value>pf1_rcb_64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_retrain_link" type="string">
          <ipxact:name>pf1_pcie_cap_retrain_link</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_retrain_link</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_role_based_err_report" type="string">
          <ipxact:name>pf1_pcie_cap_role_based_err_report</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_role_based_err_report</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_sel_deemphasis" type="string">
          <ipxact:name>pf1_pcie_cap_sel_deemphasis</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_sel_deemphasis</ipxact:displayName>
          <ipxact:value>pf1_minus_6db</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_shadow_link_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf1_pcie_cap_shadow_link_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_shadow_link_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101372</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_shadow_link_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf1_pcie_cap_shadow_link_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_shadow_link_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101373</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_slot_clk_config" type="string">
          <ipxact:name>pf1_pcie_cap_slot_clk_config</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_slot_clk_config</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_surprise_down_err_rep_cap" type="string">
          <ipxact:name>pf1_pcie_cap_surprise_down_err_rep_cap</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_surprise_down_err_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_target_link_speed" type="string">
          <ipxact:name>pf1_pcie_cap_target_link_speed</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_target_link_speed</ipxact:displayName>
          <ipxact:value>pf1_trgt_gen3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_tx_margin" type="string">
          <ipxact:name>pf1_pcie_cap_tx_margin</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_tx_margin</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_int_msg_num" type="int">
          <ipxact:name>pf1_pcie_int_msg_num</ipxact:name>
          <ipxact:displayName>pf1_pcie_int_msg_num</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_slot_imp" type="string">
          <ipxact:name>pf1_pcie_slot_imp</ipxact:name>
          <ipxact:displayName>pf1_pcie_slot_imp</ipxact:displayName>
          <ipxact:value>pf1_not_implemented</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pm_cap_cap_id_nxt_ptr_reg_addr_byte1" type="int">
          <ipxact:name>pf1_pm_cap_cap_id_nxt_ptr_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_pm_cap_cap_id_nxt_ptr_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4161</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pm_cap_cap_id_nxt_ptr_reg_addr_byte2" type="int">
          <ipxact:name>pf1_pm_cap_cap_id_nxt_ptr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_pm_cap_cap_id_nxt_ptr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4162</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pm_cap_cap_id_nxt_ptr_reg_addr_byte3" type="int">
          <ipxact:name>pf1_pm_cap_cap_id_nxt_ptr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_pm_cap_cap_id_nxt_ptr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4163</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pm_cap_con_status_reg_addr_byte0" type="int">
          <ipxact:name>pf1_pm_cap_con_status_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_pm_cap_con_status_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4164</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pm_next_pointer" type="int">
          <ipxact:name>pf1_pm_next_pointer</ipxact:name>
          <ipxact:displayName>pf1_pm_next_pointer</ipxact:displayName>
          <ipxact:value>80</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pm_spec_ver" type="int">
          <ipxact:name>pf1_pm_spec_ver</ipxact:name>
          <ipxact:displayName>pf1_pm_spec_ver</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pme_clk" type="string">
          <ipxact:name>pf1_pme_clk</ipxact:name>
          <ipxact:displayName>pf1_pme_clk</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pme_support" type="int">
          <ipxact:name>pf1_pme_support</ipxact:name>
          <ipxact:displayName>pf1_pme_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_power_state" type="int">
          <ipxact:name>pf1_power_state</ipxact:name>
          <ipxact:displayName>pf1_power_state</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_program_interface" type="int">
          <ipxact:name>pf1_program_interface</ipxact:name>
          <ipxact:displayName>pf1_program_interface</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_0_addr" type="int">
          <ipxact:name>pf1_reserved_0_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_0_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_10_addr" type="int">
          <ipxact:name>pf1_reserved_10_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_10_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_11_addr" type="int">
          <ipxact:name>pf1_reserved_11_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_11_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_12_addr" type="int">
          <ipxact:name>pf1_reserved_12_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_12_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_13_addr" type="int">
          <ipxact:name>pf1_reserved_13_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_13_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_14_addr" type="int">
          <ipxact:name>pf1_reserved_14_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_14_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_15_addr" type="int">
          <ipxact:name>pf1_reserved_15_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_15_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_16_addr" type="int">
          <ipxact:name>pf1_reserved_16_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_16_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_17_addr" type="int">
          <ipxact:name>pf1_reserved_17_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_17_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_18_addr" type="int">
          <ipxact:name>pf1_reserved_18_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_18_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_19_addr" type="int">
          <ipxact:name>pf1_reserved_19_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_19_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_1_addr" type="int">
          <ipxact:name>pf1_reserved_1_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_1_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_2_addr" type="int">
          <ipxact:name>pf1_reserved_2_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_2_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_3_addr" type="int">
          <ipxact:name>pf1_reserved_3_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_3_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_4_addr" type="int">
          <ipxact:name>pf1_reserved_4_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_4_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_5_addr" type="int">
          <ipxact:name>pf1_reserved_5_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_5_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_6_addr" type="int">
          <ipxact:name>pf1_reserved_6_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_6_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_7_addr" type="int">
          <ipxact:name>pf1_reserved_7_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_7_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_8_addr" type="int">
          <ipxact:name>pf1_reserved_8_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_8_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_reserved_9_addr" type="int">
          <ipxact:name>pf1_reserved_9_addr</ipxact:name>
          <ipxact:displayName>pf1_reserved_9_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_revision_id" type="int">
          <ipxact:name>pf1_revision_id</ipxact:name>
          <ipxact:displayName>pf1_revision_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_rom_bar_enable" type="string">
          <ipxact:name>pf1_rom_bar_enable</ipxact:name>
          <ipxact:displayName>pf1_rom_bar_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_rom_bar_enabled" type="string">
          <ipxact:name>pf1_rom_bar_enabled</ipxact:name>
          <ipxact:displayName>pf1_rom_bar_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_rom_mask" type="int">
          <ipxact:name>pf1_rom_mask</ipxact:name>
          <ipxact:displayName>pf1_rom_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_shadow_link_capabilities_reg_shadow_rsvdp_23" type="string">
          <ipxact:name>pf1_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf1_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_shadow_pcie_cap_active_state_link_pm_support" type="int">
          <ipxact:name>pf1_shadow_pcie_cap_active_state_link_pm_support</ipxact:name>
          <ipxact:displayName>pf1_shadow_pcie_cap_active_state_link_pm_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_shadow_pcie_cap_aspm_opt_compliance" type="string">
          <ipxact:name>pf1_shadow_pcie_cap_aspm_opt_compliance</ipxact:name>
          <ipxact:displayName>pf1_shadow_pcie_cap_aspm_opt_compliance</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_shadow_pcie_cap_clock_power_man" type="string">
          <ipxact:name>pf1_shadow_pcie_cap_clock_power_man</ipxact:name>
          <ipxact:displayName>pf1_shadow_pcie_cap_clock_power_man</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_shadow_pcie_cap_dll_active_rep_cap" type="string">
          <ipxact:name>pf1_shadow_pcie_cap_dll_active_rep_cap</ipxact:name>
          <ipxact:displayName>pf1_shadow_pcie_cap_dll_active_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_shadow_pcie_cap_link_bw_not_cap" type="string">
          <ipxact:name>pf1_shadow_pcie_cap_link_bw_not_cap</ipxact:name>
          <ipxact:displayName>pf1_shadow_pcie_cap_link_bw_not_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_shadow_pcie_cap_max_link_width" type="int">
          <ipxact:name>pf1_shadow_pcie_cap_max_link_width</ipxact:name>
          <ipxact:displayName>pf1_shadow_pcie_cap_max_link_width</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_shadow_pcie_cap_surprise_down_err_rep_cap" type="string">
          <ipxact:name>pf1_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:name>
          <ipxact:displayName>pf1_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_shadow_sriov_vf_stride_ari_cs2" type="int">
          <ipxact:name>pf1_shadow_sriov_vf_stride_ari_cs2</ipxact:name>
          <ipxact:displayName>pf1_shadow_sriov_vf_stride_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_cap_ser_num_reg_dw_1_addr_byte0" type="int">
          <ipxact:name>pf1_sn_cap_ser_num_reg_dw_1_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sn_cap_ser_num_reg_dw_1_addr_byte0</ipxact:displayName>
          <ipxact:value>4460</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_cap_ser_num_reg_dw_1_addr_byte1" type="int">
          <ipxact:name>pf1_sn_cap_ser_num_reg_dw_1_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sn_cap_ser_num_reg_dw_1_addr_byte1</ipxact:displayName>
          <ipxact:value>4461</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_cap_ser_num_reg_dw_1_addr_byte2" type="int">
          <ipxact:name>pf1_sn_cap_ser_num_reg_dw_1_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sn_cap_ser_num_reg_dw_1_addr_byte2</ipxact:displayName>
          <ipxact:value>4462</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_cap_ser_num_reg_dw_1_addr_byte3" type="int">
          <ipxact:name>pf1_sn_cap_ser_num_reg_dw_1_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sn_cap_ser_num_reg_dw_1_addr_byte3</ipxact:displayName>
          <ipxact:value>4463</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_cap_ser_num_reg_dw_2_addr_byte0" type="int">
          <ipxact:name>pf1_sn_cap_ser_num_reg_dw_2_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sn_cap_ser_num_reg_dw_2_addr_byte0</ipxact:displayName>
          <ipxact:value>4464</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_cap_ser_num_reg_dw_2_addr_byte1" type="int">
          <ipxact:name>pf1_sn_cap_ser_num_reg_dw_2_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sn_cap_ser_num_reg_dw_2_addr_byte1</ipxact:displayName>
          <ipxact:value>4465</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_cap_ser_num_reg_dw_2_addr_byte2" type="int">
          <ipxact:name>pf1_sn_cap_ser_num_reg_dw_2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sn_cap_ser_num_reg_dw_2_addr_byte2</ipxact:displayName>
          <ipxact:value>4466</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_cap_ser_num_reg_dw_2_addr_byte3" type="int">
          <ipxact:name>pf1_sn_cap_ser_num_reg_dw_2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sn_cap_ser_num_reg_dw_2_addr_byte3</ipxact:displayName>
          <ipxact:value>4467</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_cap_sn_base_addr_byte2" type="int">
          <ipxact:name>pf1_sn_cap_sn_base_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sn_cap_sn_base_addr_byte2</ipxact:displayName>
          <ipxact:value>4458</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_cap_sn_base_addr_byte3" type="int">
          <ipxact:name>pf1_sn_cap_sn_base_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sn_cap_sn_base_addr_byte3</ipxact:displayName>
          <ipxact:value>4459</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_cap_version" type="int">
          <ipxact:name>pf1_sn_cap_version</ipxact:name>
          <ipxact:displayName>pf1_sn_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sn_next_offset" type="int">
          <ipxact:name>pf1_sn_next_offset</ipxact:name>
          <ipxact:displayName>pf1_sn_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_sriov_initial_vfs_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_sriov_initial_vfs_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_sriov_initial_vfs_addr_byte0</ipxact:displayName>
          <ipxact:value>2101700</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_sriov_initial_vfs_addr_byte1" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_sriov_initial_vfs_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_sriov_initial_vfs_addr_byte1</ipxact:displayName>
          <ipxact:value>2101701</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0</ipxact:displayName>
          <ipxact:value>2101708</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1</ipxact:displayName>
          <ipxact:value>2101709</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2</ipxact:displayName>
          <ipxact:value>2101710</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3</ipxact:displayName>
          <ipxact:value>2101711</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101724</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte1" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101725</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte2" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101726</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte3" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar0_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101727</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101728</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte1" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101729</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte2" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101730</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte3" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar1_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101731</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101732</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte1" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101733</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte2" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101734</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte3" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar2_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101735</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101736</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte1" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101737</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte2" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101738</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte3" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar3_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101739</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101740</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte1" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101741</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte2" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101742</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte3" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar4_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101743</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101744</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte1" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101745</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte2" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101746</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte3" type="int">
          <ipxact:name>pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_shadow_vf_bar5_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101747</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sriov_bar1_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_sriov_bar1_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sriov_bar1_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101728</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sriov_bar3_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_sriov_bar3_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sriov_bar3_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101736</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sriov_bar5_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_sriov_bar5_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sriov_bar5_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101744</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sriov_base_reg_addr_byte2" type="int">
          <ipxact:name>pf1_sriov_cap_sriov_base_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sriov_base_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4538</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sriov_base_reg_addr_byte3" type="int">
          <ipxact:name>pf1_sriov_cap_sriov_base_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sriov_base_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4539</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sriov_initial_vfs_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_sriov_initial_vfs_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sriov_initial_vfs_addr_byte0</ipxact:displayName>
          <ipxact:value>4548</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sriov_initial_vfs_addr_byte1" type="int">
          <ipxact:name>pf1_sriov_cap_sriov_initial_vfs_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sriov_initial_vfs_addr_byte1</ipxact:displayName>
          <ipxact:value>4549</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sriov_vf_offset_position_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_sriov_vf_offset_position_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sriov_vf_offset_position_addr_byte0</ipxact:displayName>
          <ipxact:value>4556</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sriov_vf_offset_position_addr_byte1" type="int">
          <ipxact:name>pf1_sriov_cap_sriov_vf_offset_position_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sriov_vf_offset_position_addr_byte1</ipxact:displayName>
          <ipxact:value>4557</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sriov_vf_offset_position_addr_byte2" type="int">
          <ipxact:name>pf1_sriov_cap_sriov_vf_offset_position_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sriov_vf_offset_position_addr_byte2</ipxact:displayName>
          <ipxact:value>4558</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sriov_vf_offset_position_addr_byte3" type="int">
          <ipxact:name>pf1_sriov_cap_sriov_vf_offset_position_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sriov_vf_offset_position_addr_byte3</ipxact:displayName>
          <ipxact:value>4559</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sup_page_sizes_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_sup_page_sizes_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sup_page_sizes_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4564</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sup_page_sizes_reg_addr_byte1" type="int">
          <ipxact:name>pf1_sriov_cap_sup_page_sizes_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sup_page_sizes_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4565</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sup_page_sizes_reg_addr_byte2" type="int">
          <ipxact:name>pf1_sriov_cap_sup_page_sizes_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sup_page_sizes_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4566</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_sup_page_sizes_reg_addr_byte3" type="int">
          <ipxact:name>pf1_sriov_cap_sup_page_sizes_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_sup_page_sizes_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4567</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_version" type="int">
          <ipxact:name>pf1_sriov_cap_version</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_vf_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_vf_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_vf_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4572</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_vf_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_vf_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_vf_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4576</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_vf_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_vf_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_vf_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4580</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_vf_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_vf_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_vf_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4584</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_vf_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_vf_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_vf_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4588</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_vf_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf1_sriov_cap_vf_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_vf_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4592</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_vf_device_id_reg_addr_byte2" type="int">
          <ipxact:name>pf1_sriov_cap_vf_device_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_vf_device_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4562</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_cap_vf_device_id_reg_addr_byte3" type="int">
          <ipxact:name>pf1_sriov_cap_vf_device_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_sriov_cap_vf_device_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4563</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_initial_vfs_ari_cs2" type="int">
          <ipxact:name>pf1_sriov_initial_vfs_ari_cs2</ipxact:name>
          <ipxact:displayName>pf1_sriov_initial_vfs_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_initial_vfs_nonari" type="int">
          <ipxact:name>pf1_sriov_initial_vfs_nonari</ipxact:name>
          <ipxact:displayName>pf1_sriov_initial_vfs_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_next_offset" type="int">
          <ipxact:name>pf1_sriov_next_offset</ipxact:name>
          <ipxact:displayName>pf1_sriov_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar0_prefetch" type="string">
          <ipxact:name>pf1_sriov_vf_bar0_prefetch</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar0_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar0_start" type="int">
          <ipxact:name>pf1_sriov_vf_bar0_start</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar0_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar0_type" type="string">
          <ipxact:name>pf1_sriov_vf_bar0_type</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar0_type</ipxact:displayName>
          <ipxact:value>pf1_sriov_vf_bar0_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar1_dummy_mask_7_1" type="int">
          <ipxact:name>pf1_sriov_vf_bar1_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar1_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar1_enabled" type="string">
          <ipxact:name>pf1_sriov_vf_bar1_enabled</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar1_prefetch" type="string">
          <ipxact:name>pf1_sriov_vf_bar1_prefetch</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar1_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar1_start" type="int">
          <ipxact:name>pf1_sriov_vf_bar1_start</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar1_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar1_type" type="string">
          <ipxact:name>pf1_sriov_vf_bar1_type</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar1_type</ipxact:displayName>
          <ipxact:value>pf1_sriov_vf_bar1_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar2_prefetch" type="string">
          <ipxact:name>pf1_sriov_vf_bar2_prefetch</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar2_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar2_start" type="int">
          <ipxact:name>pf1_sriov_vf_bar2_start</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar2_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar2_type" type="string">
          <ipxact:name>pf1_sriov_vf_bar2_type</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar2_type</ipxact:displayName>
          <ipxact:value>pf1_sriov_vf_bar2_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar3_dummy_mask_7_1" type="int">
          <ipxact:name>pf1_sriov_vf_bar3_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar3_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar3_enabled" type="string">
          <ipxact:name>pf1_sriov_vf_bar3_enabled</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar3_prefetch" type="string">
          <ipxact:name>pf1_sriov_vf_bar3_prefetch</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar3_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar3_start" type="int">
          <ipxact:name>pf1_sriov_vf_bar3_start</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar3_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar3_type" type="string">
          <ipxact:name>pf1_sriov_vf_bar3_type</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar3_type</ipxact:displayName>
          <ipxact:value>pf1_sriov_vf_bar3_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar4_prefetch" type="string">
          <ipxact:name>pf1_sriov_vf_bar4_prefetch</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar4_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar4_start" type="int">
          <ipxact:name>pf1_sriov_vf_bar4_start</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar4_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar4_type" type="string">
          <ipxact:name>pf1_sriov_vf_bar4_type</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar4_type</ipxact:displayName>
          <ipxact:value>pf1_sriov_vf_bar4_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar5_dummy_mask_7_1" type="int">
          <ipxact:name>pf1_sriov_vf_bar5_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar5_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar5_enabled" type="string">
          <ipxact:name>pf1_sriov_vf_bar5_enabled</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar5_prefetch" type="string">
          <ipxact:name>pf1_sriov_vf_bar5_prefetch</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar5_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar5_start" type="int">
          <ipxact:name>pf1_sriov_vf_bar5_start</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar5_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_bar5_type" type="string">
          <ipxact:name>pf1_sriov_vf_bar5_type</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_bar5_type</ipxact:displayName>
          <ipxact:value>pf1_sriov_vf_bar5_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_device_id" type="int">
          <ipxact:name>pf1_sriov_vf_device_id</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_device_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_offset_ari_cs2" type="int">
          <ipxact:name>pf1_sriov_vf_offset_ari_cs2</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_offset_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_offset_position_nonari" type="int">
          <ipxact:name>pf1_sriov_vf_offset_position_nonari</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_offset_position_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_sriov_vf_stride_nonari" type="int">
          <ipxact:name>pf1_sriov_vf_stride_nonari</ipxact:name>
          <ipxact:displayName>pf1_sriov_vf_stride_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_subclass_code" type="int">
          <ipxact:name>pf1_subclass_code</ipxact:name>
          <ipxact:displayName>pf1_subclass_code</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_subsys_dev_id" type="int">
          <ipxact:name>pf1_subsys_dev_id</ipxact:name>
          <ipxact:displayName>pf1_subsys_dev_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_subsys_vendor_id" type="int">
          <ipxact:name>pf1_subsys_vendor_id</ipxact:name>
          <ipxact:displayName>pf1_subsys_vendor_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_cap_tph_ext_cap_hdr_reg_addr_byte2" type="int">
          <ipxact:name>pf1_tph_cap_tph_ext_cap_hdr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_tph_cap_tph_ext_cap_hdr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4602</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_cap_tph_ext_cap_hdr_reg_addr_byte3" type="int">
          <ipxact:name>pf1_tph_cap_tph_ext_cap_hdr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_tph_cap_tph_ext_cap_hdr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4603</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_cap_tph_req_cap_reg_addr_byte0" type="int">
          <ipxact:name>pf1_tph_cap_tph_req_cap_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_tph_cap_tph_req_cap_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4604</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_cap_tph_req_cap_reg_addr_byte1" type="int">
          <ipxact:name>pf1_tph_cap_tph_req_cap_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_tph_cap_tph_req_cap_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4605</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_cap_tph_req_cap_reg_addr_byte2" type="int">
          <ipxact:name>pf1_tph_cap_tph_req_cap_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_tph_cap_tph_req_cap_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4606</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_cap_tph_req_cap_reg_addr_byte3" type="int">
          <ipxact:name>pf1_tph_cap_tph_req_cap_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_tph_cap_tph_req_cap_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4607</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0" type="int">
          <ipxact:name>pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0</ipxact:displayName>
          <ipxact:value>2101756</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1" type="int">
          <ipxact:name>pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1</ipxact:displayName>
          <ipxact:value>2101757</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2" type="int">
          <ipxact:name>pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2</ipxact:displayName>
          <ipxact:value>2101758</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3" type="int">
          <ipxact:name>pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3</ipxact:displayName>
          <ipxact:value>2101759</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_int_vec" type="string">
          <ipxact:name>pf1_tph_req_cap_int_vec</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_int_vec</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_int_vec_vfcomm_cs2" type="string">
          <ipxact:name>pf1_tph_req_cap_int_vec_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_int_vec_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_reg_rsvdp_11" type="int">
          <ipxact:name>pf1_tph_req_cap_reg_rsvdp_11</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_reg_rsvdp_11</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_reg_rsvdp_27" type="int">
          <ipxact:name>pf1_tph_req_cap_reg_rsvdp_27</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_reg_rsvdp_27</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_reg_rsvdp_3" type="int">
          <ipxact:name>pf1_tph_req_cap_reg_rsvdp_3</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_reg_rsvdp_3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2" type="int">
          <ipxact:name>pf1_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2" type="int">
          <ipxact:name>pf1_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2" type="int">
          <ipxact:name>pf1_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_st_table_loc_0" type="string">
          <ipxact:name>pf1_tph_req_cap_st_table_loc_0</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_st_table_loc_0</ipxact:displayName>
          <ipxact:value>pf1_not_in_tph_struct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_st_table_loc_0_vfcomm_cs2" type="string">
          <ipxact:name>pf1_tph_req_cap_st_table_loc_0_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_st_table_loc_0_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>pf1_not_in_tph_struct_vf</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_st_table_loc_1" type="string">
          <ipxact:name>pf1_tph_req_cap_st_table_loc_1</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_st_table_loc_1</ipxact:displayName>
          <ipxact:value>pf1_not_in_msix_table</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_st_table_loc_1_vfcomm_cs2" type="string">
          <ipxact:name>pf1_tph_req_cap_st_table_loc_1_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_st_table_loc_1_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>pf1_not_in_msix_table_vf</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_st_table_size" type="int">
          <ipxact:name>pf1_tph_req_cap_st_table_size</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_st_table_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_st_table_size_vfcomm_cs2" type="int">
          <ipxact:name>pf1_tph_req_cap_st_table_size_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_st_table_size_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_cap_ver" type="int">
          <ipxact:name>pf1_tph_req_cap_ver</ipxact:name>
          <ipxact:displayName>pf1_tph_req_cap_ver</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_device_spec" type="string">
          <ipxact:name>pf1_tph_req_device_spec</ipxact:name>
          <ipxact:displayName>pf1_tph_req_device_spec</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_device_spec_vfcomm_cs2" type="string">
          <ipxact:name>pf1_tph_req_device_spec_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_tph_req_device_spec_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_extended_tph" type="string">
          <ipxact:name>pf1_tph_req_extended_tph</ipxact:name>
          <ipxact:displayName>pf1_tph_req_extended_tph</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_extended_tph_vfcomm_cs2" type="string">
          <ipxact:name>pf1_tph_req_extended_tph_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_tph_req_extended_tph_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_next_ptr" type="int">
          <ipxact:name>pf1_tph_req_next_ptr</ipxact:name>
          <ipxact:displayName>pf1_tph_req_next_ptr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_no_st_mode" type="string">
          <ipxact:name>pf1_tph_req_no_st_mode</ipxact:name>
          <ipxact:displayName>pf1_tph_req_no_st_mode</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_tph_req_no_st_mode_vfcomm_cs2" type="string">
          <ipxact:name>pf1_tph_req_no_st_mode_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf1_tph_req_no_st_mode_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar0_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar0_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar0_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101264</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar0_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_bar0_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar0_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101265</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar0_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_bar0_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar0_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101266</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar0_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf1_type0_hdr_bar0_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar0_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101267</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4112</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar1_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar1_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar1_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101268</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar1_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar1_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar1_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101268</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar1_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_bar1_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar1_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101269</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar1_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_bar1_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar1_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101270</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar1_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf1_type0_hdr_bar1_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar1_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101271</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4116</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar2_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar2_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar2_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101272</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar2_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_bar2_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar2_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101273</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar2_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_bar2_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar2_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101274</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar2_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf1_type0_hdr_bar2_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar2_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101275</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4120</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar3_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar3_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar3_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101276</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar3_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar3_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar3_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101276</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar3_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_bar3_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar3_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101277</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar3_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_bar3_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar3_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101278</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar3_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf1_type0_hdr_bar3_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar3_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101279</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4124</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar4_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar4_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar4_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101280</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar4_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_bar4_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar4_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101281</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar4_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_bar4_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar4_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101282</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar4_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf1_type0_hdr_bar4_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar4_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101283</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4128</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar5_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar5_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar5_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101284</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar5_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar5_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar5_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101284</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar5_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_bar5_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar5_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101285</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar5_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_bar5_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar5_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101286</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar5_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf1_type0_hdr_bar5_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar5_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101287</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4132</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4110</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4136</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4137</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4138</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte3" type="int">
          <ipxact:name>pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_cardbus_cis_ptr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4139</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_class_code_revision_id_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_class_code_revision_id_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_class_code_revision_id_addr_byte0</ipxact:displayName>
          <ipxact:value>4104</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_class_code_revision_id_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_class_code_revision_id_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_class_code_revision_id_addr_byte1</ipxact:displayName>
          <ipxact:value>4105</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_class_code_revision_id_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_class_code_revision_id_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_class_code_revision_id_addr_byte2</ipxact:displayName>
          <ipxact:value>4106</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_class_code_revision_id_addr_byte3" type="int">
          <ipxact:name>pf1_type0_hdr_class_code_revision_id_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_class_code_revision_id_addr_byte3</ipxact:displayName>
          <ipxact:value>4107</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_device_id_vendor_id_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_device_id_vendor_id_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_device_id_vendor_id_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4096</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_device_id_vendor_id_reg_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_device_id_vendor_id_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_device_id_vendor_id_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4097</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_device_id_vendor_id_reg_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_device_id_vendor_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_device_id_vendor_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4098</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_device_id_vendor_id_reg_addr_byte3" type="int">
          <ipxact:name>pf1_type0_hdr_device_id_vendor_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_device_id_vendor_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4099</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2101296</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2101297</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2101298</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_exp_rom_bar_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2101299</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_exp_rom_base_addr_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_exp_rom_base_addr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_exp_rom_base_addr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4144</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4157</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_pci_cap_ptr_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_pci_cap_ptr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_pci_cap_ptr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4148</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0" type="int">
          <ipxact:name>pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4140</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1" type="int">
          <ipxact:name>pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4141</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2" type="int">
          <ipxact:name>pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4142</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3" type="int">
          <ipxact:name>pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4143</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_vf_bar0_reg_rsvdp_0" type="string">
          <ipxact:name>pf1_vf_bar0_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf1_vf_bar0_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_vf_bar1_reg_rsvdp_0" type="string">
          <ipxact:name>pf1_vf_bar1_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf1_vf_bar1_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_vf_bar2_reg_rsvdp_0" type="string">
          <ipxact:name>pf1_vf_bar2_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf1_vf_bar2_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_vf_bar3_reg_rsvdp_0" type="string">
          <ipxact:name>pf1_vf_bar3_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf1_vf_bar3_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_vf_bar4_reg_rsvdp_0" type="string">
          <ipxact:name>pf1_vf_bar4_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf1_vf_bar4_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_vf_bar5_reg_rsvdp_0" type="string">
          <ipxact:name>pf1_vf_bar5_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf1_vf_bar5_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_vf_forward_user_vsec" type="string">
          <ipxact:name>pf1_vf_forward_user_vsec</ipxact:name>
          <ipxact:displayName>pf1_vf_forward_user_vsec</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pipe_ctrl" type="int">
          <ipxact:name>pipe_ctrl</ipxact:name>
          <ipxact:displayName>pipe_ctrl</ipxact:displayName>
          <ipxact:value>16787995</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_aib_loopback_en" type="string">
          <ipxact:name>pld_aib_loopback_en</ipxact:name>
          <ipxact:displayName>pld_aib_loopback_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_aux_gate_en" type="string">
          <ipxact:name>pld_aux_gate_en</ipxact:name>
          <ipxact:displayName>pld_aux_gate_en</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_aux_prog_en" type="string">
          <ipxact:name>pld_aux_prog_en</ipxact:name>
          <ipxact:displayName>pld_aux_prog_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_crs_en" type="string">
          <ipxact:name>pld_crs_en</ipxact:name>
          <ipxact:displayName>pld_crs_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_rx_cpl_bufflimit_bypass" type="string">
          <ipxact:name>pld_rx_cpl_bufflimit_bypass</ipxact:name>
          <ipxact:displayName>pld_rx_cpl_bufflimit_bypass</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_rx_np_bufflimit_bypass" type="string">
          <ipxact:name>pld_rx_np_bufflimit_bypass</ipxact:name>
          <ipxact:displayName>pld_rx_np_bufflimit_bypass</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_rx_parity_ena" type="string">
          <ipxact:name>pld_rx_parity_ena</ipxact:name>
          <ipxact:displayName>pld_rx_parity_ena</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_rx_posted_bufflimit_bypass" type="string">
          <ipxact:name>pld_rx_posted_bufflimit_bypass</ipxact:name>
          <ipxact:displayName>pld_rx_posted_bufflimit_bypass</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_tx_fifo_dyn_empty_dis" type="string">
          <ipxact:name>pld_tx_fifo_dyn_empty_dis</ipxact:name>
          <ipxact:displayName>pld_tx_fifo_dyn_empty_dis</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_tx_fifo_empty_threshold_1" type="int">
          <ipxact:name>pld_tx_fifo_empty_threshold_1</ipxact:name>
          <ipxact:displayName>pld_tx_fifo_empty_threshold_1</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_tx_fifo_empty_threshold_2" type="int">
          <ipxact:name>pld_tx_fifo_empty_threshold_2</ipxact:name>
          <ipxact:displayName>pld_tx_fifo_empty_threshold_2</ipxact:displayName>
          <ipxact:value>12</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_tx_fifo_empty_threshold_3" type="int">
          <ipxact:name>pld_tx_fifo_empty_threshold_3</ipxact:name>
          <ipxact:displayName>pld_tx_fifo_empty_threshold_3</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_tx_fifo_full_threshold" type="int">
          <ipxact:name>pld_tx_fifo_full_threshold</ipxact:name>
          <ipxact:displayName>pld_tx_fifo_full_threshold</ipxact:displayName>
          <ipxact:value>40</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pld_tx_parity_ena" type="string">
          <ipxact:name>pld_tx_parity_ena</ipxact:name>
          <ipxact:displayName>pld_tx_parity_ena</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="powerdown_mode" type="string">
          <ipxact:name>powerdown_mode</ipxact:name>
          <ipxact:displayName>powerdown_mode</ipxact:displayName>
          <ipxact:value>powerup</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_lane_flip_en" type="string">
          <ipxact:name>rx_lane_flip_en</ipxact:name>
          <ipxact:displayName>rx_lane_flip_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="sim_mode" type="string">
          <ipxact:name>sim_mode</ipxact:name>
          <ipxact:displayName>sim_mode</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ssm_aux_prog_en" type="string">
          <ipxact:name>ssm_aux_prog_en</ipxact:name>
          <ipxact:displayName>ssm_aux_prog_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="sup_mode" type="string">
          <ipxact:name>sup_mode</ipxact:name>
          <ipxact:displayName>sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="test_in_override" type="string">
          <ipxact:name>test_in_override</ipxact:name>
          <ipxact:displayName>test_in_override</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_avst_dsk_en" type="string">
          <ipxact:name>tx_avst_dsk_en</ipxact:name>
          <ipxact:displayName>tx_avst_dsk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_lane_flip_en" type="string">
          <ipxact:name>tx_lane_flip_en</ipxact:name>
          <ipxact:displayName>tx_lane_flip_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="user_mode_del_count" type="int">
          <ipxact:name>user_mode_del_count</ipxact:name>
          <ipxact:displayName>user_mode_del_count</ipxact:displayName>
          <ipxact:value>5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="valid_ecc_err_rpt_en" type="string">
          <ipxact:name>valid_ecc_err_rpt_en</ipxact:name>
          <ipxact:displayName>valid_ecc_err_rpt_en</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_ari_cap_version" type="int">
          <ipxact:name>vf1_pf0_ari_cap_version</ipxact:name>
          <ipxact:displayName>vf1_pf0_ari_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_ari_cap_vf_ari_base_addr_byte2" type="int">
          <ipxact:name>vf1_pf0_ari_cap_vf_ari_base_addr_byte2</ipxact:name>
          <ipxact:displayName>vf1_pf0_ari_cap_vf_ari_base_addr_byte2</ipxact:displayName>
          <ipxact:value>1048834</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_ari_cap_vf_ari_base_addr_byte3" type="int">
          <ipxact:name>vf1_pf0_ari_cap_vf_ari_base_addr_byte3</ipxact:name>
          <ipxact:displayName>vf1_pf0_ari_cap_vf_ari_base_addr_byte3</ipxact:displayName>
          <ipxact:value>1048835</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_ari_next_offset" type="int">
          <ipxact:name>vf1_pf0_ari_next_offset</ipxact:name>
          <ipxact:displayName>vf1_pf0_ari_next_offset</ipxact:displayName>
          <ipxact:value>344</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_pcie_cap_vf_shadow_link_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>vf1_pf0_pcie_cap_vf_shadow_link_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>vf1_pf0_pcie_cap_vf_shadow_link_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>1048701</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_shadow_pcie_cap_aspm_opt_compliance" type="string">
          <ipxact:name>vf1_pf0_shadow_pcie_cap_aspm_opt_compliance</ipxact:name>
          <ipxact:displayName>vf1_pf0_shadow_pcie_cap_aspm_opt_compliance</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_shadow_pcie_cap_clock_power_man" type="string">
          <ipxact:name>vf1_pf0_shadow_pcie_cap_clock_power_man</ipxact:name>
          <ipxact:displayName>vf1_pf0_shadow_pcie_cap_clock_power_man</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_shadow_pcie_cap_dll_active_rep_cap" type="string">
          <ipxact:name>vf1_pf0_shadow_pcie_cap_dll_active_rep_cap</ipxact:name>
          <ipxact:displayName>vf1_pf0_shadow_pcie_cap_dll_active_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_shadow_pcie_cap_l1_exit_latency_commclk_ena" type="int">
          <ipxact:name>vf1_pf0_shadow_pcie_cap_l1_exit_latency_commclk_ena</ipxact:name>
          <ipxact:displayName>vf1_pf0_shadow_pcie_cap_l1_exit_latency_commclk_ena</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_shadow_pcie_cap_link_bw_not_cap" type="string">
          <ipxact:name>vf1_pf0_shadow_pcie_cap_link_bw_not_cap</ipxact:name>
          <ipxact:displayName>vf1_pf0_shadow_pcie_cap_link_bw_not_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_shadow_pcie_cap_surprise_down_err_rep_cap" type="string">
          <ipxact:name>vf1_pf0_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:name>
          <ipxact:displayName>vf1_pf0_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte2" type="int">
          <ipxact:name>vf1_pf0_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>vf1_pf0_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>1048850</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte3" type="int">
          <ipxact:name>vf1_pf0_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>vf1_pf0_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>1048851</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_tph_req_cap_ver" type="int">
          <ipxact:name>vf1_pf0_tph_req_cap_ver</ipxact:name>
          <ipxact:displayName>vf1_pf0_tph_req_cap_ver</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_tph_req_next_ptr" type="int">
          <ipxact:name>vf1_pf0_tph_req_next_ptr</ipxact:name>
          <ipxact:displayName>vf1_pf0_tph_req_next_ptr</ipxact:displayName>
          <ipxact:value>552</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf0_vf_shadow_link_capabilities_reg_shadow_rsvdp_23" type="string">
          <ipxact:name>vf1_pf0_vf_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:name>
          <ipxact:displayName>vf1_pf0_vf_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_ari_cap_version" type="int">
          <ipxact:name>vf1_pf1_ari_cap_version</ipxact:name>
          <ipxact:displayName>vf1_pf1_ari_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_ari_cap_vf_ari_base_addr_byte2" type="int">
          <ipxact:name>vf1_pf1_ari_cap_vf_ari_base_addr_byte2</ipxact:name>
          <ipxact:displayName>vf1_pf1_ari_cap_vf_ari_base_addr_byte2</ipxact:displayName>
          <ipxact:value>1052930</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_ari_cap_vf_ari_base_addr_byte3" type="int">
          <ipxact:name>vf1_pf1_ari_cap_vf_ari_base_addr_byte3</ipxact:name>
          <ipxact:displayName>vf1_pf1_ari_cap_vf_ari_base_addr_byte3</ipxact:displayName>
          <ipxact:value>1052931</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_ari_next_offset" type="int">
          <ipxact:name>vf1_pf1_ari_next_offset</ipxact:name>
          <ipxact:displayName>vf1_pf1_ari_next_offset</ipxact:displayName>
          <ipxact:value>344</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_pcie_cap_vf_shadow_link_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>vf1_pf1_pcie_cap_vf_shadow_link_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>vf1_pf1_pcie_cap_vf_shadow_link_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>1052797</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_shadow_pcie_cap_aspm_opt_compliance" type="string">
          <ipxact:name>vf1_pf1_shadow_pcie_cap_aspm_opt_compliance</ipxact:name>
          <ipxact:displayName>vf1_pf1_shadow_pcie_cap_aspm_opt_compliance</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_shadow_pcie_cap_clock_power_man" type="string">
          <ipxact:name>vf1_pf1_shadow_pcie_cap_clock_power_man</ipxact:name>
          <ipxact:displayName>vf1_pf1_shadow_pcie_cap_clock_power_man</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_shadow_pcie_cap_dll_active_rep_cap" type="string">
          <ipxact:name>vf1_pf1_shadow_pcie_cap_dll_active_rep_cap</ipxact:name>
          <ipxact:displayName>vf1_pf1_shadow_pcie_cap_dll_active_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_shadow_pcie_cap_l1_exit_latency_commclk_ena" type="int">
          <ipxact:name>vf1_pf1_shadow_pcie_cap_l1_exit_latency_commclk_ena</ipxact:name>
          <ipxact:displayName>vf1_pf1_shadow_pcie_cap_l1_exit_latency_commclk_ena</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_shadow_pcie_cap_link_bw_not_cap" type="string">
          <ipxact:name>vf1_pf1_shadow_pcie_cap_link_bw_not_cap</ipxact:name>
          <ipxact:displayName>vf1_pf1_shadow_pcie_cap_link_bw_not_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_shadow_pcie_cap_surprise_down_err_rep_cap" type="string">
          <ipxact:name>vf1_pf1_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:name>
          <ipxact:displayName>vf1_pf1_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte2" type="int">
          <ipxact:name>vf1_pf1_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>vf1_pf1_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>1052946</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte3" type="int">
          <ipxact:name>vf1_pf1_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>vf1_pf1_tph_cap_vf_tph_ext_cap_hdr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>1052947</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_tph_req_cap_ver" type="int">
          <ipxact:name>vf1_pf1_tph_req_cap_ver</ipxact:name>
          <ipxact:displayName>vf1_pf1_tph_req_cap_ver</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_tph_req_next_ptr" type="int">
          <ipxact:name>vf1_pf1_tph_req_next_ptr</ipxact:name>
          <ipxact:displayName>vf1_pf1_tph_req_next_ptr</ipxact:displayName>
          <ipxact:value>552</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf1_pf1_vf_shadow_link_capabilities_reg_shadow_rsvdp_23" type="string">
          <ipxact:name>vf1_pf1_vf_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:name>
          <ipxact:displayName>vf1_pf1_vf_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_dbi_reserved_0" type="int">
          <ipxact:name>vf_dbi_reserved_0</ipxact:name>
          <ipxact:displayName>vf_dbi_reserved_0</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_dbi_reserved_1" type="int">
          <ipxact:name>vf_dbi_reserved_1</ipxact:name>
          <ipxact:displayName>vf_dbi_reserved_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_dbi_reserved_2" type="int">
          <ipxact:name>vf_dbi_reserved_2</ipxact:name>
          <ipxact:displayName>vf_dbi_reserved_2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_dbi_reserved_3" type="int">
          <ipxact:name>vf_dbi_reserved_3</ipxact:name>
          <ipxact:displayName>vf_dbi_reserved_3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_dbi_reserved_4" type="int">
          <ipxact:name>vf_dbi_reserved_4</ipxact:name>
          <ipxact:displayName>vf_dbi_reserved_4</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_dbi_reserved_5" type="int">
          <ipxact:name>vf_dbi_reserved_5</ipxact:name>
          <ipxact:displayName>vf_dbi_reserved_5</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_reserved_0_addr" type="int">
          <ipxact:name>vf_reserved_0_addr</ipxact:name>
          <ipxact:displayName>vf_reserved_0_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_reserved_1_addr" type="int">
          <ipxact:name>vf_reserved_1_addr</ipxact:name>
          <ipxact:displayName>vf_reserved_1_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_reserved_2_addr" type="int">
          <ipxact:name>vf_reserved_2_addr</ipxact:name>
          <ipxact:displayName>vf_reserved_2_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_reserved_3_addr" type="int">
          <ipxact:name>vf_reserved_3_addr</ipxact:name>
          <ipxact:displayName>vf_reserved_3_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_reserved_4_addr" type="int">
          <ipxact:name>vf_reserved_4_addr</ipxact:name>
          <ipxact:displayName>vf_reserved_4_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vf_reserved_5_addr" type="int">
          <ipxact:name>vf_reserved_5_addr</ipxact:name>
          <ipxact:displayName>vf_reserved_5_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_drop_vendor0_msg" type="string">
          <ipxact:name>virtual_drop_vendor0_msg</ipxact:name>
          <ipxact:displayName>virtual_drop_vendor0_msg</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_drop_vendor1_msg" type="string">
          <ipxact:name>virtual_drop_vendor1_msg</ipxact:name>
          <ipxact:displayName>virtual_drop_vendor1_msg</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_ep_native" type="string">
          <ipxact:name>virtual_ep_native</ipxact:name>
          <ipxact:displayName>virtual_ep_native</ipxact:displayName>
          <ipxact:value>native</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_gen2_pma_pll_usage" type="string">
          <ipxact:name>virtual_gen2_pma_pll_usage</ipxact:name>
          <ipxact:displayName>virtual_gen2_pma_pll_usage</ipxact:displayName>
          <ipxact:value>not_applicable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_hrdrstctrl_en" type="string">
          <ipxact:name>virtual_hrdrstctrl_en</ipxact:name>
          <ipxact:displayName>virtual_hrdrstctrl_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_link_rate" type="string">
          <ipxact:name>virtual_link_rate</ipxact:name>
          <ipxact:displayName>virtual_link_rate</ipxact:displayName>
          <ipxact:value>gen3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_link_width" type="string">
          <ipxact:name>virtual_link_width</ipxact:name>
          <ipxact:displayName>virtual_link_width</ipxact:displayName>
          <ipxact:value>x1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_maxpayload_size" type="string">
          <ipxact:name>virtual_maxpayload_size</ipxact:name>
          <ipxact:displayName>virtual_maxpayload_size</ipxact:displayName>
          <ipxact:value>max_payload_512</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_ats_cap_enable" type="string">
          <ipxact:name>virtual_pf0_ats_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf0_ats_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_bar1_mask_bit0" type="string">
          <ipxact:name>virtual_pf0_bar1_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf0_bar1_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_bar3_mask_bit0" type="string">
          <ipxact:name>virtual_pf0_bar3_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf0_bar3_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_bar5_mask_bit0" type="string">
          <ipxact:name>virtual_pf0_bar5_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf0_bar5_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_io_decode" type="string">
          <ipxact:name>virtual_pf0_io_decode</ipxact:name>
          <ipxact:displayName>virtual_pf0_io_decode</ipxact:displayName>
          <ipxact:value>io32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_msi_enable" type="string">
          <ipxact:name>virtual_pf0_msi_enable</ipxact:name>
          <ipxact:displayName>virtual_pf0_msi_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_msix_enable" type="string">
          <ipxact:name>virtual_pf0_msix_enable</ipxact:name>
          <ipxact:displayName>virtual_pf0_msix_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_pb_cap_enable" type="string">
          <ipxact:name>virtual_pf0_pb_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf0_pb_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_prefetch_decode" type="string">
          <ipxact:name>virtual_pf0_prefetch_decode</ipxact:name>
          <ipxact:displayName>virtual_pf0_prefetch_decode</ipxact:displayName>
          <ipxact:value>pref64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_sn_cap_enable" type="string">
          <ipxact:name>virtual_pf0_sn_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf0_sn_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_sriov_enable" type="string">
          <ipxact:name>virtual_pf0_sriov_enable</ipxact:name>
          <ipxact:displayName>virtual_pf0_sriov_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_sriov_num_vf_ari" type="int">
          <ipxact:name>virtual_pf0_sriov_num_vf_ari</ipxact:name>
          <ipxact:displayName>virtual_pf0_sriov_num_vf_ari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_sriov_num_vf_non_ari" type="int">
          <ipxact:name>virtual_pf0_sriov_num_vf_non_ari</ipxact:name>
          <ipxact:displayName>virtual_pf0_sriov_num_vf_non_ari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_sriov_vf_bar0_enabled" type="string">
          <ipxact:name>virtual_pf0_sriov_vf_bar0_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf0_sriov_vf_bar0_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_sriov_vf_bar1_enabled" type="string">
          <ipxact:name>virtual_pf0_sriov_vf_bar1_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf0_sriov_vf_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_sriov_vf_bar2_enabled" type="string">
          <ipxact:name>virtual_pf0_sriov_vf_bar2_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf0_sriov_vf_bar2_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_sriov_vf_bar3_enabled" type="string">
          <ipxact:name>virtual_pf0_sriov_vf_bar3_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf0_sriov_vf_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_sriov_vf_bar4_enabled" type="string">
          <ipxact:name>virtual_pf0_sriov_vf_bar4_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf0_sriov_vf_bar4_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_sriov_vf_bar5_enabled" type="string">
          <ipxact:name>virtual_pf0_sriov_vf_bar5_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf0_sriov_vf_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_tph_cap_enable" type="string">
          <ipxact:name>virtual_pf0_tph_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf0_tph_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf0_user_vsec_cap_enable" type="string">
          <ipxact:name>virtual_pf0_user_vsec_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf0_user_vsec_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_ats_cap_enable" type="string">
          <ipxact:name>virtual_pf1_ats_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf1_ats_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_bar1_mask_bit0" type="string">
          <ipxact:name>virtual_pf1_bar1_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf1_bar1_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_bar3_mask_bit0" type="string">
          <ipxact:name>virtual_pf1_bar3_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf1_bar3_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_bar5_mask_bit0" type="string">
          <ipxact:name>virtual_pf1_bar5_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf1_bar5_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_enable" type="string">
          <ipxact:name>virtual_pf1_enable</ipxact:name>
          <ipxact:displayName>virtual_pf1_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_msi_enable" type="string">
          <ipxact:name>virtual_pf1_msi_enable</ipxact:name>
          <ipxact:displayName>virtual_pf1_msi_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_msix_enable" type="string">
          <ipxact:name>virtual_pf1_msix_enable</ipxact:name>
          <ipxact:displayName>virtual_pf1_msix_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_pb_cap_enable" type="string">
          <ipxact:name>virtual_pf1_pb_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf1_pb_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_sn_cap_enable" type="string">
          <ipxact:name>virtual_pf1_sn_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf1_sn_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_sriov_enable" type="string">
          <ipxact:name>virtual_pf1_sriov_enable</ipxact:name>
          <ipxact:displayName>virtual_pf1_sriov_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_sriov_num_vf_ari" type="int">
          <ipxact:name>virtual_pf1_sriov_num_vf_ari</ipxact:name>
          <ipxact:displayName>virtual_pf1_sriov_num_vf_ari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_sriov_num_vf_non_ari" type="int">
          <ipxact:name>virtual_pf1_sriov_num_vf_non_ari</ipxact:name>
          <ipxact:displayName>virtual_pf1_sriov_num_vf_non_ari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_sriov_vf_bar0_enabled" type="string">
          <ipxact:name>virtual_pf1_sriov_vf_bar0_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf1_sriov_vf_bar0_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_sriov_vf_bar1_enabled" type="string">
          <ipxact:name>virtual_pf1_sriov_vf_bar1_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf1_sriov_vf_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_sriov_vf_bar2_enabled" type="string">
          <ipxact:name>virtual_pf1_sriov_vf_bar2_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf1_sriov_vf_bar2_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_sriov_vf_bar3_enabled" type="string">
          <ipxact:name>virtual_pf1_sriov_vf_bar3_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf1_sriov_vf_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_sriov_vf_bar4_enabled" type="string">
          <ipxact:name>virtual_pf1_sriov_vf_bar4_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf1_sriov_vf_bar4_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_sriov_vf_bar5_enabled" type="string">
          <ipxact:name>virtual_pf1_sriov_vf_bar5_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf1_sriov_vf_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_tph_cap_enable" type="string">
          <ipxact:name>virtual_pf1_tph_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf1_tph_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf1_user_vsec_cap_enable" type="string">
          <ipxact:name>virtual_pf1_user_vsec_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf1_user_vsec_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_phase23_txpreset" type="string">
          <ipxact:name>virtual_phase23_txpreset</ipxact:name>
          <ipxact:displayName>virtual_phase23_txpreset</ipxact:displayName>
          <ipxact:value>preset8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_rp_ep_mode" type="string">
          <ipxact:name>virtual_rp_ep_mode</ipxact:name>
          <ipxact:displayName>virtual_rp_ep_mode</ipxact:displayName>
          <ipxact:value>ep</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_txeq_mode" type="string">
          <ipxact:name>virtual_txeq_mode</ipxact:name>
          <ipxact:displayName>virtual_txeq_mode</ipxact:displayName>
          <ipxact:value>eq_pipe_dir_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_uc_calibration_en" type="string">
          <ipxact:name>virtual_uc_calibration_en</ipxact:name>
          <ipxact:displayName>virtual_uc_calibration_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_vf1_pf0_ats_cap_enable" type="string">
          <ipxact:name>virtual_vf1_pf0_ats_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_vf1_pf0_ats_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_vf1_pf0_tph_cap_enable" type="string">
          <ipxact:name>virtual_vf1_pf0_tph_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_vf1_pf0_tph_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_vf1_pf0_user_vsec_cap_enable" type="string">
          <ipxact:name>virtual_vf1_pf0_user_vsec_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_vf1_pf0_user_vsec_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_vf1_pf1_ats_cap_enable" type="string">
          <ipxact:name>virtual_vf1_pf1_ats_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_vf1_pf1_ats_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_vf1_pf1_tph_cap_enable" type="string">
          <ipxact:name>virtual_vf1_pf1_tph_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_vf1_pf1_tph_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_vf1_pf1_user_vsec_cap_enable" type="string">
          <ipxact:name>virtual_vf1_pf1_user_vsec_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_vf1_pf1_user_vsec_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vsec_legacy_interr_mask_en" type="string">
          <ipxact:name>vsec_legacy_interr_mask_en</ipxact:name>
          <ipxact:displayName>vsec_legacy_interr_mask_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="vsec_next_offset" type="int">
          <ipxact:name>vsec_next_offset</ipxact:name>
          <ipxact:displayName>vsec_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="silicon_rev" type="string">
          <ipxact:name>silicon_rev</ipxact:name>
          <ipxact:displayName>silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2ea</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdts_intf_sel" type="string">
          <ipxact:name>cdts_intf_sel</ipxact:name>
          <ipxact:displayName>cdts_intf_sel</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_dbi_pf1_table_size" type="int">
          <ipxact:name>cfg_dbi_pf1_table_size</ipxact:name>
          <ipxact:displayName>cfg_dbi_pf1_table_size</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_dbi_pf2_start_addr" type="int">
          <ipxact:name>cfg_dbi_pf2_start_addr</ipxact:name>
          <ipxact:displayName>cfg_dbi_pf2_start_addr</ipxact:displayName>
          <ipxact:value>512</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_dbi_pf2_table_size" type="int">
          <ipxact:name>cfg_dbi_pf2_table_size</ipxact:name>
          <ipxact:displayName>cfg_dbi_pf2_table_size</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_dbi_pf3_start_addr" type="int">
          <ipxact:name>cfg_dbi_pf3_start_addr</ipxact:name>
          <ipxact:displayName>cfg_dbi_pf3_start_addr</ipxact:displayName>
          <ipxact:value>704</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cfg_dbi_pf3_table_size" type="int">
          <ipxact:name>cfg_dbi_pf3_table_size</ipxact:name>
          <ipxact:displayName>cfg_dbi_pf3_table_size</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_mcgb_rst_mask" type="string">
          <ipxact:name>hrc_mcgb_rst_mask</ipxact:name>
          <ipxact:displayName>hrc_mcgb_rst_mask</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_pwrup_seq_mask" type="string">
          <ipxact:name>hrc_pwrup_seq_mask</ipxact:name>
          <ipxact:displayName>hrc_pwrup_seq_mask</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rst_asrt_seq_en" type="string">
          <ipxact:name>hrc_rst_asrt_seq_en</ipxact:name>
          <ipxact:displayName>hrc_rst_asrt_seq_en</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rx_seq_en" type="string">
          <ipxact:name>hrc_rx_seq_en</ipxact:name>
          <ipxact:displayName>hrc_rx_seq_en</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_rx_seq_sel" type="string">
          <ipxact:name>hrc_rx_seq_sel</ipxact:name>
          <ipxact:displayName>hrc_rx_seq_sel</ipxact:displayName>
          <ipxact:value>ns_320</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_spd_change_value" type="string">
          <ipxact:name>hrc_spd_change_value</ipxact:name>
          <ipxact:displayName>hrc_spd_change_value</ipxact:displayName>
          <ipxact:value>big_delay0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hrc_tx_seq_en" type="string">
          <ipxact:name>hrc_tx_seq_en</ipxact:name>
          <ipxact:displayName>hrc_tx_seq_en</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf0_pcie_cap_device_capabilities_reg_addr_byte3" type="int">
          <ipxact:name>pf0_pcie_cap_device_capabilities_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf0_pcie_cap_device_capabilities_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>119</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf1_pcie_cap_device_capabilities_reg_addr_byte3" type="int">
          <ipxact:name>pf1_pcie_cap_device_capabilities_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf1_pcie_cap_device_capabilities_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>4215</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_aer_cap_aer_ext_cap_hdr_off_addr_byte2" type="int">
          <ipxact:name>pf2_aer_cap_aer_ext_cap_hdr_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_aer_cap_aer_ext_cap_hdr_off_addr_byte2</ipxact:displayName>
          <ipxact:value>8450</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_aer_cap_aer_ext_cap_hdr_off_addr_byte3" type="int">
          <ipxact:name>pf2_aer_cap_aer_ext_cap_hdr_off_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_aer_cap_aer_ext_cap_hdr_off_addr_byte3</ipxact:displayName>
          <ipxact:value>8451</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_aer_cap_version" type="int">
          <ipxact:name>pf2_aer_cap_version</ipxact:name>
          <ipxact:displayName>pf2_aer_cap_version</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_aer_next_offset" type="int">
          <ipxact:name>pf2_aer_next_offset</ipxact:name>
          <ipxact:displayName>pf2_aer_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_ari_cap_ari_base_addr_byte2" type="int">
          <ipxact:name>pf2_ari_cap_ari_base_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_ari_cap_ari_base_addr_byte2</ipxact:displayName>
          <ipxact:value>8570</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_ari_cap_ari_base_addr_byte3" type="int">
          <ipxact:name>pf2_ari_cap_ari_base_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_ari_cap_ari_base_addr_byte3</ipxact:displayName>
          <ipxact:value>8571</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_ari_cap_version" type="int">
          <ipxact:name>pf2_ari_cap_version</ipxact:name>
          <ipxact:displayName>pf2_ari_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_ari_next_offset" type="int">
          <ipxact:name>pf2_ari_next_offset</ipxact:name>
          <ipxact:displayName>pf2_ari_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_ats_cap_ats_cap_hdr_reg_addr_byte2" type="int">
          <ipxact:name>pf2_ats_cap_ats_cap_hdr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_ats_cap_ats_cap_hdr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8838</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_ats_cap_ats_cap_hdr_reg_addr_byte3" type="int">
          <ipxact:name>pf2_ats_cap_ats_cap_hdr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_ats_cap_ats_cap_hdr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8839</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_ats_cap_ats_capabilities_ctrl_reg_addr_byte0" type="int">
          <ipxact:name>pf2_ats_cap_ats_capabilities_ctrl_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_ats_cap_ats_capabilities_ctrl_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8840</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_ats_cap_version" type="int">
          <ipxact:name>pf2_ats_cap_version</ipxact:name>
          <ipxact:displayName>pf2_ats_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_ats_capabilities_ctrl_reg_rsvdp_7" type="string">
          <ipxact:name>pf2_ats_capabilities_ctrl_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf2_ats_capabilities_ctrl_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_ats_next_offset" type="int">
          <ipxact:name>pf2_ats_next_offset</ipxact:name>
          <ipxact:displayName>pf2_ats_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_aux_curr" type="int">
          <ipxact:name>pf2_aux_curr</ipxact:name>
          <ipxact:displayName>pf2_aux_curr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar0_mem_io" type="string">
          <ipxact:name>pf2_bar0_mem_io</ipxact:name>
          <ipxact:displayName>pf2_bar0_mem_io</ipxact:displayName>
          <ipxact:value>pf2_bar0_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar0_prefetch" type="string">
          <ipxact:name>pf2_bar0_prefetch</ipxact:name>
          <ipxact:displayName>pf2_bar0_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar0_start" type="int">
          <ipxact:name>pf2_bar0_start</ipxact:name>
          <ipxact:displayName>pf2_bar0_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar0_type" type="string">
          <ipxact:name>pf2_bar0_type</ipxact:name>
          <ipxact:displayName>pf2_bar0_type</ipxact:displayName>
          <ipxact:value>pf2_bar0_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar1_mem_io" type="string">
          <ipxact:name>pf2_bar1_mem_io</ipxact:name>
          <ipxact:displayName>pf2_bar1_mem_io</ipxact:displayName>
          <ipxact:value>pf2_bar1_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar1_prefetch" type="string">
          <ipxact:name>pf2_bar1_prefetch</ipxact:name>
          <ipxact:displayName>pf2_bar1_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar1_start" type="int">
          <ipxact:name>pf2_bar1_start</ipxact:name>
          <ipxact:displayName>pf2_bar1_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar1_type" type="string">
          <ipxact:name>pf2_bar1_type</ipxact:name>
          <ipxact:displayName>pf2_bar1_type</ipxact:displayName>
          <ipxact:value>pf2_bar1_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar2_mem_io" type="string">
          <ipxact:name>pf2_bar2_mem_io</ipxact:name>
          <ipxact:displayName>pf2_bar2_mem_io</ipxact:displayName>
          <ipxact:value>pf2_bar2_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar2_prefetch" type="string">
          <ipxact:name>pf2_bar2_prefetch</ipxact:name>
          <ipxact:displayName>pf2_bar2_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar2_start" type="int">
          <ipxact:name>pf2_bar2_start</ipxact:name>
          <ipxact:displayName>pf2_bar2_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar2_type" type="string">
          <ipxact:name>pf2_bar2_type</ipxact:name>
          <ipxact:displayName>pf2_bar2_type</ipxact:displayName>
          <ipxact:value>pf2_bar2_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar3_mem_io" type="string">
          <ipxact:name>pf2_bar3_mem_io</ipxact:name>
          <ipxact:displayName>pf2_bar3_mem_io</ipxact:displayName>
          <ipxact:value>pf2_bar3_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar3_prefetch" type="string">
          <ipxact:name>pf2_bar3_prefetch</ipxact:name>
          <ipxact:displayName>pf2_bar3_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar3_start" type="int">
          <ipxact:name>pf2_bar3_start</ipxact:name>
          <ipxact:displayName>pf2_bar3_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar3_type" type="string">
          <ipxact:name>pf2_bar3_type</ipxact:name>
          <ipxact:displayName>pf2_bar3_type</ipxact:displayName>
          <ipxact:value>pf2_bar3_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar4_mem_io" type="string">
          <ipxact:name>pf2_bar4_mem_io</ipxact:name>
          <ipxact:displayName>pf2_bar4_mem_io</ipxact:displayName>
          <ipxact:value>pf2_bar4_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar4_prefetch" type="string">
          <ipxact:name>pf2_bar4_prefetch</ipxact:name>
          <ipxact:displayName>pf2_bar4_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar4_start" type="int">
          <ipxact:name>pf2_bar4_start</ipxact:name>
          <ipxact:displayName>pf2_bar4_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar4_type" type="string">
          <ipxact:name>pf2_bar4_type</ipxact:name>
          <ipxact:displayName>pf2_bar4_type</ipxact:displayName>
          <ipxact:value>pf2_bar4_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar5_mem_io" type="string">
          <ipxact:name>pf2_bar5_mem_io</ipxact:name>
          <ipxact:displayName>pf2_bar5_mem_io</ipxact:displayName>
          <ipxact:value>pf2_bar5_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar5_prefetch" type="string">
          <ipxact:name>pf2_bar5_prefetch</ipxact:name>
          <ipxact:displayName>pf2_bar5_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar5_start" type="int">
          <ipxact:name>pf2_bar5_start</ipxact:name>
          <ipxact:displayName>pf2_bar5_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_bar5_type" type="string">
          <ipxact:name>pf2_bar5_type</ipxact:name>
          <ipxact:displayName>pf2_bar5_type</ipxact:displayName>
          <ipxact:value>pf2_bar5_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_base_class_code" type="int">
          <ipxact:name>pf2_base_class_code</ipxact:name>
          <ipxact:displayName>pf2_base_class_code</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_cap_id_nxt_ptr_reg_rsvdp_20" type="string">
          <ipxact:name>pf2_cap_id_nxt_ptr_reg_rsvdp_20</ipxact:name>
          <ipxact:displayName>pf2_cap_id_nxt_ptr_reg_rsvdp_20</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_cap_pointer" type="int">
          <ipxact:name>pf2_cap_pointer</ipxact:name>
          <ipxact:displayName>pf2_cap_pointer</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_con_status_reg_rsvdp_2" type="string">
          <ipxact:name>pf2_con_status_reg_rsvdp_2</ipxact:name>
          <ipxact:displayName>pf2_con_status_reg_rsvdp_2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_con_status_reg_rsvdp_4" type="int">
          <ipxact:name>pf2_con_status_reg_rsvdp_4</ipxact:name>
          <ipxact:displayName>pf2_con_status_reg_rsvdp_4</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_d1_support" type="string">
          <ipxact:name>pf2_d1_support</ipxact:name>
          <ipxact:displayName>pf2_d1_support</ipxact:displayName>
          <ipxact:value>pf2_d1_not_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_d2_support" type="string">
          <ipxact:name>pf2_d2_support</ipxact:name>
          <ipxact:displayName>pf2_d2_support</ipxact:displayName>
          <ipxact:value>pf2_d2_not_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_0" type="int">
          <ipxact:name>pf2_dbi_reserved_0</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_0</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_1" type="int">
          <ipxact:name>pf2_dbi_reserved_1</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_10" type="int">
          <ipxact:name>pf2_dbi_reserved_10</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_10</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_11" type="int">
          <ipxact:name>pf2_dbi_reserved_11</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_11</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_12" type="int">
          <ipxact:name>pf2_dbi_reserved_12</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_13" type="int">
          <ipxact:name>pf2_dbi_reserved_13</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_13</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_14" type="int">
          <ipxact:name>pf2_dbi_reserved_14</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_14</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_15" type="int">
          <ipxact:name>pf2_dbi_reserved_15</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_15</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_16" type="int">
          <ipxact:name>pf2_dbi_reserved_16</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_16</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_17" type="int">
          <ipxact:name>pf2_dbi_reserved_17</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_17</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_18" type="int">
          <ipxact:name>pf2_dbi_reserved_18</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_18</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_19" type="int">
          <ipxact:name>pf2_dbi_reserved_19</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_19</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_2" type="int">
          <ipxact:name>pf2_dbi_reserved_2</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_3" type="int">
          <ipxact:name>pf2_dbi_reserved_3</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_4" type="int">
          <ipxact:name>pf2_dbi_reserved_4</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_4</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_5" type="int">
          <ipxact:name>pf2_dbi_reserved_5</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_5</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_6" type="int">
          <ipxact:name>pf2_dbi_reserved_6</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_6</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_7" type="int">
          <ipxact:name>pf2_dbi_reserved_7</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_7</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_8" type="int">
          <ipxact:name>pf2_dbi_reserved_8</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_8</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dbi_reserved_9" type="int">
          <ipxact:name>pf2_dbi_reserved_9</ipxact:name>
          <ipxact:displayName>pf2_dbi_reserved_9</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_device_capabilities_reg_rsvdp_12" type="int">
          <ipxact:name>pf2_device_capabilities_reg_rsvdp_12</ipxact:name>
          <ipxact:displayName>pf2_device_capabilities_reg_rsvdp_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_device_capabilities_reg_rsvdp_16" type="int">
          <ipxact:name>pf2_device_capabilities_reg_rsvdp_16</ipxact:name>
          <ipxact:displayName>pf2_device_capabilities_reg_rsvdp_16</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_device_capabilities_reg_rsvdp_29" type="int">
          <ipxact:name>pf2_device_capabilities_reg_rsvdp_29</ipxact:name>
          <ipxact:displayName>pf2_device_capabilities_reg_rsvdp_29</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_dsi" type="string">
          <ipxact:name>pf2_dsi</ipxact:name>
          <ipxact:displayName>pf2_dsi</ipxact:displayName>
          <ipxact:value>pf2_not_required</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_exp_rom_bar_mask_reg_rsvdp_1" type="int">
          <ipxact:name>pf2_exp_rom_bar_mask_reg_rsvdp_1</ipxact:name>
          <ipxact:displayName>pf2_exp_rom_bar_mask_reg_rsvdp_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_exp_rom_base_addr_reg_rsvdp_1" type="int">
          <ipxact:name>pf2_exp_rom_base_addr_reg_rsvdp_1</ipxact:name>
          <ipxact:displayName>pf2_exp_rom_base_addr_reg_rsvdp_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_forward_user_vsec" type="string">
          <ipxact:name>pf2_forward_user_vsec</ipxact:name>
          <ipxact:displayName>pf2_forward_user_vsec</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_global_inval_spprtd" type="string">
          <ipxact:name>pf2_global_inval_spprtd</ipxact:name>
          <ipxact:displayName>pf2_global_inval_spprtd</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_header_type" type="int">
          <ipxact:name>pf2_header_type</ipxact:name>
          <ipxact:displayName>pf2_header_type</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_int_pin" type="string">
          <ipxact:name>pf2_int_pin</ipxact:name>
          <ipxact:displayName>pf2_int_pin</ipxact:displayName>
          <ipxact:value>pf2_no_int</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_invalidate_q_depth" type="int">
          <ipxact:name>pf2_invalidate_q_depth</ipxact:name>
          <ipxact:displayName>pf2_invalidate_q_depth</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_link_capabilities_reg_rsvdp_23" type="string">
          <ipxact:name>pf2_link_capabilities_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf2_link_capabilities_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_link_control_link_status_reg_rsvdp_12" type="int">
          <ipxact:name>pf2_link_control_link_status_reg_rsvdp_12</ipxact:name>
          <ipxact:displayName>pf2_link_control_link_status_reg_rsvdp_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_link_control_link_status_reg_rsvdp_2" type="string">
          <ipxact:name>pf2_link_control_link_status_reg_rsvdp_2</ipxact:name>
          <ipxact:displayName>pf2_link_control_link_status_reg_rsvdp_2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_link_control_link_status_reg_rsvdp_25" type="int">
          <ipxact:name>pf2_link_control_link_status_reg_rsvdp_25</ipxact:name>
          <ipxact:displayName>pf2_link_control_link_status_reg_rsvdp_25</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_link_control_link_status_reg_rsvdp_9" type="string">
          <ipxact:name>pf2_link_control_link_status_reg_rsvdp_9</ipxact:name>
          <ipxact:displayName>pf2_link_control_link_status_reg_rsvdp_9</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1" type="int">
          <ipxact:name>pf2_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8273</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2" type="int">
          <ipxact:name>pf2_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8274</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_msix_pba_offset_reg_addr_byte0" type="int">
          <ipxact:name>pf2_msix_cap_msix_pba_offset_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_msix_pba_offset_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8376</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_msix_pba_offset_reg_addr_byte1" type="int">
          <ipxact:name>pf2_msix_cap_msix_pba_offset_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_msix_pba_offset_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8377</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_msix_pba_offset_reg_addr_byte2" type="int">
          <ipxact:name>pf2_msix_cap_msix_pba_offset_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_msix_pba_offset_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8378</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_msix_pba_offset_reg_addr_byte3" type="int">
          <ipxact:name>pf2_msix_cap_msix_pba_offset_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_msix_pba_offset_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8379</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_msix_table_offset_reg_addr_byte0" type="int">
          <ipxact:name>pf2_msix_cap_msix_table_offset_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_msix_table_offset_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8372</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_msix_table_offset_reg_addr_byte1" type="int">
          <ipxact:name>pf2_msix_cap_msix_table_offset_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_msix_table_offset_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8373</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_msix_table_offset_reg_addr_byte2" type="int">
          <ipxact:name>pf2_msix_cap_msix_table_offset_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_msix_table_offset_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8374</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_msix_table_offset_reg_addr_byte3" type="int">
          <ipxact:name>pf2_msix_cap_msix_table_offset_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_msix_table_offset_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8375</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1" type="int">
          <ipxact:name>pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8369</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2" type="int">
          <ipxact:name>pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8370</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3" type="int">
          <ipxact:name>pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8371</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2" type="int">
          <ipxact:name>pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2</ipxact:displayName>
          <ipxact:value>2105522</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3" type="int">
          <ipxact:name>pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3</ipxact:displayName>
          <ipxact:value>2105523</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_multi_func" type="string">
          <ipxact:name>pf2_multi_func</ipxact:name>
          <ipxact:displayName>pf2_multi_func</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_no_soft_rst" type="string">
          <ipxact:name>pf2_no_soft_rst</ipxact:name>
          <ipxact:displayName>pf2_no_soft_rst</ipxact:displayName>
          <ipxact:value>pf2_internally_reset</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_page_aligned_req" type="string">
          <ipxact:name>pf2_page_aligned_req</ipxact:name>
          <ipxact:displayName>pf2_page_aligned_req</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msi_64_bit_addr_cap" type="string">
          <ipxact:name>pf2_pci_msi_64_bit_addr_cap</ipxact:name>
          <ipxact:displayName>pf2_pci_msi_64_bit_addr_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msi_cap_next_offset" type="int">
          <ipxact:name>pf2_pci_msi_cap_next_offset</ipxact:name>
          <ipxact:displayName>pf2_pci_msi_cap_next_offset</ipxact:displayName>
          <ipxact:value>112</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msi_enable" type="string">
          <ipxact:name>pf2_pci_msi_enable</ipxact:name>
          <ipxact:displayName>pf2_pci_msi_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msi_multiple_msg_cap" type="string">
          <ipxact:name>pf2_pci_msi_multiple_msg_cap</ipxact:name>
          <ipxact:displayName>pf2_pci_msi_multiple_msg_cap</ipxact:displayName>
          <ipxact:value>pf2_msi_vec_1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msi_multiple_msg_en" type="int">
          <ipxact:name>pf2_pci_msi_multiple_msg_en</ipxact:name>
          <ipxact:displayName>pf2_pci_msi_multiple_msg_en</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_bir" type="int">
          <ipxact:name>pf2_pci_msix_bir</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_bir</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_cap_id_next_ctrl_reg_rsvdp_27" type="int">
          <ipxact:name>pf2_pci_msix_cap_id_next_ctrl_reg_rsvdp_27</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_cap_id_next_ctrl_reg_rsvdp_27</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2" type="int">
          <ipxact:name>pf2_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_cap_next_offset" type="int">
          <ipxact:name>pf2_pci_msix_cap_next_offset</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_cap_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_enable" type="string">
          <ipxact:name>pf2_pci_msix_enable</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_enable_vfcomm_cs2" type="string">
          <ipxact:name>pf2_pci_msix_enable_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_enable_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_function_mask" type="string">
          <ipxact:name>pf2_pci_msix_function_mask</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_function_mask</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_function_mask_vfcomm_cs2" type="string">
          <ipxact:name>pf2_pci_msix_function_mask_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_function_mask_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_pba" type="int">
          <ipxact:name>pf2_pci_msix_pba</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_pba</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_pba_offset" type="int">
          <ipxact:name>pf2_pci_msix_pba_offset</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_pba_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_table_offset" type="int">
          <ipxact:name>pf2_pci_msix_table_offset</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_table_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_table_size" type="int">
          <ipxact:name>pf2_pci_msix_table_size</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_table_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_msix_table_size_vfcomm_cs2" type="int">
          <ipxact:name>pf2_pci_msix_table_size_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_pci_msix_table_size_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar0_enabled" type="string">
          <ipxact:name>pf2_pci_type0_bar0_enabled</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar0_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar0_mask_31_1" type="int">
          <ipxact:name>pf2_pci_type0_bar0_mask_31_1</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar0_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar1_dummy_mask_7_1" type="int">
          <ipxact:name>pf2_pci_type0_bar1_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar1_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar1_enabled" type="string">
          <ipxact:name>pf2_pci_type0_bar1_enabled</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar1_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf2_pci_type0_bar1_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar1_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar1_mask_31_1" type="int">
          <ipxact:name>pf2_pci_type0_bar1_mask_31_1</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar1_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar2_enabled" type="string">
          <ipxact:name>pf2_pci_type0_bar2_enabled</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar2_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar2_mask_31_1" type="int">
          <ipxact:name>pf2_pci_type0_bar2_mask_31_1</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar2_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar3_dummy_mask_7_1" type="int">
          <ipxact:name>pf2_pci_type0_bar3_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar3_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar3_enabled" type="string">
          <ipxact:name>pf2_pci_type0_bar3_enabled</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar3_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf2_pci_type0_bar3_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar3_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar3_mask_31_1" type="int">
          <ipxact:name>pf2_pci_type0_bar3_mask_31_1</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar3_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar4_enabled" type="string">
          <ipxact:name>pf2_pci_type0_bar4_enabled</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar4_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar4_mask_31_1" type="int">
          <ipxact:name>pf2_pci_type0_bar4_mask_31_1</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar4_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar5_dummy_mask_7_1" type="int">
          <ipxact:name>pf2_pci_type0_bar5_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar5_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar5_enabled" type="string">
          <ipxact:name>pf2_pci_type0_bar5_enabled</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar5_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf2_pci_type0_bar5_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar5_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_bar5_mask_31_1" type="int">
          <ipxact:name>pf2_pci_type0_bar5_mask_31_1</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_bar5_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_device_id" type="int">
          <ipxact:name>pf2_pci_type0_device_id</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_device_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pci_type0_vendor_id" type="int">
          <ipxact:name>pf2_pci_type0_vendor_id</ipxact:name>
          <ipxact:displayName>pf2_pci_type0_vendor_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_active_state_link_pm_control" type="string">
          <ipxact:name>pf2_pcie_cap_active_state_link_pm_control</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_active_state_link_pm_control</ipxact:displayName>
          <ipxact:value>pf2_aspm_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_active_state_link_pm_support" type="string">
          <ipxact:name>pf2_pcie_cap_active_state_link_pm_support</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_active_state_link_pm_support</ipxact:displayName>
          <ipxact:value>pf2_no_aspm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_aspm_opt_compliance" type="string">
          <ipxact:name>pf2_pcie_cap_aspm_opt_compliance</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_aspm_opt_compliance</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_aux_power_pm_en" type="string">
          <ipxact:name>pf2_pcie_cap_aux_power_pm_en</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_aux_power_pm_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_clock_power_man" type="string">
          <ipxact:name>pf2_pcie_cap_clock_power_man</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_clock_power_man</ipxact:displayName>
          <ipxact:value>pf2_refclk_remove_not_ok</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_common_clk_config" type="string">
          <ipxact:name>pf2_pcie_cap_common_clk_config</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_common_clk_config</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_device_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf2_pcie_cap_device_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_device_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8308</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_device_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf2_pcie_cap_device_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_device_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8309</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_device_capabilities_reg_addr_byte3" type="int">
          <ipxact:name>pf2_pcie_cap_device_capabilities_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_device_capabilities_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8311</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_device_control_device_status_addr_byte1" type="int">
          <ipxact:name>pf2_pcie_cap_device_control_device_status_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_device_control_device_status_addr_byte1</ipxact:displayName>
          <ipxact:value>8313</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_dll_active" type="string">
          <ipxact:name>pf2_pcie_cap_dll_active</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_dll_active</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_dll_active_rep_cap" type="string">
          <ipxact:name>pf2_pcie_cap_dll_active_rep_cap</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_dll_active_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_en_clk_power_man" type="string">
          <ipxact:name>pf2_pcie_cap_en_clk_power_man</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_en_clk_power_man</ipxact:displayName>
          <ipxact:value>pf2_clkreq_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_en_no_snoop" type="string">
          <ipxact:name>pf2_pcie_cap_en_no_snoop</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_en_no_snoop</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_enter_compliance" type="string">
          <ipxact:name>pf2_pcie_cap_enter_compliance</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_enter_compliance</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_ep_l0s_accpt_latency" type="int">
          <ipxact:name>pf2_pcie_cap_ep_l0s_accpt_latency</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_ep_l0s_accpt_latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_ep_l1_accpt_latency" type="int">
          <ipxact:name>pf2_pcie_cap_ep_l1_accpt_latency</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_ep_l1_accpt_latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_ext_tag_en" type="string">
          <ipxact:name>pf2_pcie_cap_ext_tag_en</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_ext_tag_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_ext_tag_supp" type="string">
          <ipxact:name>pf2_pcie_cap_ext_tag_supp</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_ext_tag_supp</ipxact:displayName>
          <ipxact:value>pf2_not_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_extended_synch" type="string">
          <ipxact:name>pf2_pcie_cap_extended_synch</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_extended_synch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_flr_cap" type="string">
          <ipxact:name>pf2_pcie_cap_flr_cap</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_flr_cap</ipxact:displayName>
          <ipxact:value>pf2_not_capable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_hw_auto_speed_disable" type="string">
          <ipxact:name>pf2_pcie_cap_hw_auto_speed_disable</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_hw_auto_speed_disable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd" type="string">
          <ipxact:name>pf2_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31" type="string">
          <ipxact:name>pf2_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_initiate_flr" type="string">
          <ipxact:name>pf2_pcie_cap_initiate_flr</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_initiate_flr</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_l0s_exit_latency_commclk_dis" type="int">
          <ipxact:name>pf2_pcie_cap_l0s_exit_latency_commclk_dis</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_l0s_exit_latency_commclk_dis</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_l0s_exit_latency_commclk_ena_cs2" type="int">
          <ipxact:name>pf2_pcie_cap_l0s_exit_latency_commclk_ena_cs2</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_l0s_exit_latency_commclk_ena_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_l1_exit_latency_commclk_dis" type="int">
          <ipxact:name>pf2_pcie_cap_l1_exit_latency_commclk_dis</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_l1_exit_latency_commclk_dis</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_l1_exit_latency_commclk_ena_cs2" type="int">
          <ipxact:name>pf2_pcie_cap_l1_exit_latency_commclk_ena_cs2</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_l1_exit_latency_commclk_ena_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_auto_bw_int_en" type="string">
          <ipxact:name>pf2_pcie_cap_link_auto_bw_int_en</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_auto_bw_int_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_auto_bw_status" type="string">
          <ipxact:name>pf2_pcie_cap_link_auto_bw_status</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_auto_bw_status</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_bw_man_int_en" type="string">
          <ipxact:name>pf2_pcie_cap_link_bw_man_int_en</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_bw_man_int_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_bw_man_status" type="string">
          <ipxact:name>pf2_pcie_cap_link_bw_man_status</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_bw_man_status</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_bw_not_cap" type="string">
          <ipxact:name>pf2_pcie_cap_link_bw_not_cap</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_bw_not_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf2_pcie_cap_link_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8316</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf2_pcie_cap_link_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8317</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_capabilities_reg_addr_byte2" type="int">
          <ipxact:name>pf2_pcie_cap_link_capabilities_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_capabilities_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8318</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_capabilities_reg_addr_byte3" type="int">
          <ipxact:name>pf2_pcie_cap_link_capabilities_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_capabilities_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8319</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_control2_link_status2_reg_addr_byte0" type="int">
          <ipxact:name>pf2_pcie_cap_link_control2_link_status2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_control2_link_status2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12591264</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_control_link_status_reg_addr_byte0" type="int">
          <ipxact:name>pf2_pcie_cap_link_control_link_status_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_control_link_status_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4202624</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_control_link_status_reg_addr_byte1" type="int">
          <ipxact:name>pf2_pcie_cap_link_control_link_status_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_control_link_status_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4202625</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_control_link_status_reg_addr_byte2" type="int">
          <ipxact:name>pf2_pcie_cap_link_control_link_status_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_control_link_status_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4202626</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_disable" type="string">
          <ipxact:name>pf2_pcie_cap_link_disable</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_disable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_link_training" type="string">
          <ipxact:name>pf2_pcie_cap_link_training</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_link_training</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_max_link_speed" type="string">
          <ipxact:name>pf2_pcie_cap_max_link_speed</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_max_link_speed</ipxact:displayName>
          <ipxact:value>pf2_max_8gts</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_max_link_width" type="string">
          <ipxact:name>pf2_pcie_cap_max_link_width</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_max_link_width</ipxact:displayName>
          <ipxact:value>pf2_x1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_max_payload_size" type="string">
          <ipxact:name>pf2_pcie_cap_max_payload_size</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_max_payload_size</ipxact:displayName>
          <ipxact:value>pf2_payload_512</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_max_read_req_size" type="int">
          <ipxact:name>pf2_pcie_cap_max_read_req_size</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_max_read_req_size</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_nego_link_width" type="string">
          <ipxact:name>pf2_pcie_cap_nego_link_width</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_nego_link_width</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_next_ptr" type="int">
          <ipxact:name>pf2_pcie_cap_next_ptr</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_next_ptr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1" type="int">
          <ipxact:name>pf2_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8305</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3" type="int">
          <ipxact:name>pf2_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8307</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_phantom_func_en" type="string">
          <ipxact:name>pf2_pcie_cap_phantom_func_en</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_phantom_func_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_phantom_func_support" type="int">
          <ipxact:name>pf2_pcie_cap_phantom_func_support</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_phantom_func_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_port_num" type="int">
          <ipxact:name>pf2_pcie_cap_port_num</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_port_num</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_rcb" type="string">
          <ipxact:name>pf2_pcie_cap_rcb</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_rcb</ipxact:displayName>
          <ipxact:value>pf2_rcb_64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_retrain_link" type="string">
          <ipxact:name>pf2_pcie_cap_retrain_link</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_retrain_link</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_role_based_err_report" type="string">
          <ipxact:name>pf2_pcie_cap_role_based_err_report</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_role_based_err_report</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_sel_deemphasis" type="string">
          <ipxact:name>pf2_pcie_cap_sel_deemphasis</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_sel_deemphasis</ipxact:displayName>
          <ipxact:value>pf2_minus_6db</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_shadow_link_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf2_pcie_cap_shadow_link_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_shadow_link_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105468</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_shadow_link_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf2_pcie_cap_shadow_link_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_shadow_link_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105469</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_slot_clk_config" type="string">
          <ipxact:name>pf2_pcie_cap_slot_clk_config</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_slot_clk_config</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_surprise_down_err_rep_cap" type="string">
          <ipxact:name>pf2_pcie_cap_surprise_down_err_rep_cap</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_surprise_down_err_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_target_link_speed" type="string">
          <ipxact:name>pf2_pcie_cap_target_link_speed</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_target_link_speed</ipxact:displayName>
          <ipxact:value>pf2_trgt_gen3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_cap_tx_margin" type="string">
          <ipxact:name>pf2_pcie_cap_tx_margin</ipxact:name>
          <ipxact:displayName>pf2_pcie_cap_tx_margin</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_int_msg_num" type="int">
          <ipxact:name>pf2_pcie_int_msg_num</ipxact:name>
          <ipxact:displayName>pf2_pcie_int_msg_num</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pcie_slot_imp" type="string">
          <ipxact:name>pf2_pcie_slot_imp</ipxact:name>
          <ipxact:displayName>pf2_pcie_slot_imp</ipxact:displayName>
          <ipxact:value>pf2_not_implemented</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pm_cap_cap_id_nxt_ptr_reg_addr_byte1" type="int">
          <ipxact:name>pf2_pm_cap_cap_id_nxt_ptr_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_pm_cap_cap_id_nxt_ptr_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8257</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pm_cap_cap_id_nxt_ptr_reg_addr_byte2" type="int">
          <ipxact:name>pf2_pm_cap_cap_id_nxt_ptr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_pm_cap_cap_id_nxt_ptr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8258</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pm_cap_cap_id_nxt_ptr_reg_addr_byte3" type="int">
          <ipxact:name>pf2_pm_cap_cap_id_nxt_ptr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_pm_cap_cap_id_nxt_ptr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8259</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pm_cap_con_status_reg_addr_byte0" type="int">
          <ipxact:name>pf2_pm_cap_con_status_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_pm_cap_con_status_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8260</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pm_next_pointer" type="int">
          <ipxact:name>pf2_pm_next_pointer</ipxact:name>
          <ipxact:displayName>pf2_pm_next_pointer</ipxact:displayName>
          <ipxact:value>80</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pm_spec_ver" type="int">
          <ipxact:name>pf2_pm_spec_ver</ipxact:name>
          <ipxact:displayName>pf2_pm_spec_ver</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pme_clk" type="string">
          <ipxact:name>pf2_pme_clk</ipxact:name>
          <ipxact:displayName>pf2_pme_clk</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_pme_support" type="int">
          <ipxact:name>pf2_pme_support</ipxact:name>
          <ipxact:displayName>pf2_pme_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_power_state" type="int">
          <ipxact:name>pf2_power_state</ipxact:name>
          <ipxact:displayName>pf2_power_state</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_program_interface" type="int">
          <ipxact:name>pf2_program_interface</ipxact:name>
          <ipxact:displayName>pf2_program_interface</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_0_addr" type="int">
          <ipxact:name>pf2_reserved_0_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_0_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_10_addr" type="int">
          <ipxact:name>pf2_reserved_10_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_10_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_11_addr" type="int">
          <ipxact:name>pf2_reserved_11_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_11_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_12_addr" type="int">
          <ipxact:name>pf2_reserved_12_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_12_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_13_addr" type="int">
          <ipxact:name>pf2_reserved_13_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_13_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_14_addr" type="int">
          <ipxact:name>pf2_reserved_14_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_14_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_15_addr" type="int">
          <ipxact:name>pf2_reserved_15_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_15_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_16_addr" type="int">
          <ipxact:name>pf2_reserved_16_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_16_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_17_addr" type="int">
          <ipxact:name>pf2_reserved_17_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_17_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_18_addr" type="int">
          <ipxact:name>pf2_reserved_18_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_18_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_19_addr" type="int">
          <ipxact:name>pf2_reserved_19_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_19_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_1_addr" type="int">
          <ipxact:name>pf2_reserved_1_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_1_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_2_addr" type="int">
          <ipxact:name>pf2_reserved_2_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_2_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_3_addr" type="int">
          <ipxact:name>pf2_reserved_3_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_3_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_4_addr" type="int">
          <ipxact:name>pf2_reserved_4_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_4_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_5_addr" type="int">
          <ipxact:name>pf2_reserved_5_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_5_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_6_addr" type="int">
          <ipxact:name>pf2_reserved_6_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_6_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_7_addr" type="int">
          <ipxact:name>pf2_reserved_7_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_7_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_8_addr" type="int">
          <ipxact:name>pf2_reserved_8_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_8_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_reserved_9_addr" type="int">
          <ipxact:name>pf2_reserved_9_addr</ipxact:name>
          <ipxact:displayName>pf2_reserved_9_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_revision_id" type="int">
          <ipxact:name>pf2_revision_id</ipxact:name>
          <ipxact:displayName>pf2_revision_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_rom_bar_enable" type="string">
          <ipxact:name>pf2_rom_bar_enable</ipxact:name>
          <ipxact:displayName>pf2_rom_bar_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_rom_bar_enabled" type="string">
          <ipxact:name>pf2_rom_bar_enabled</ipxact:name>
          <ipxact:displayName>pf2_rom_bar_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_rom_mask" type="int">
          <ipxact:name>pf2_rom_mask</ipxact:name>
          <ipxact:displayName>pf2_rom_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_shadow_link_capabilities_reg_shadow_rsvdp_23" type="string">
          <ipxact:name>pf2_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf2_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_shadow_pcie_cap_active_state_link_pm_support" type="int">
          <ipxact:name>pf2_shadow_pcie_cap_active_state_link_pm_support</ipxact:name>
          <ipxact:displayName>pf2_shadow_pcie_cap_active_state_link_pm_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_shadow_pcie_cap_aspm_opt_compliance" type="string">
          <ipxact:name>pf2_shadow_pcie_cap_aspm_opt_compliance</ipxact:name>
          <ipxact:displayName>pf2_shadow_pcie_cap_aspm_opt_compliance</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_shadow_pcie_cap_clock_power_man" type="string">
          <ipxact:name>pf2_shadow_pcie_cap_clock_power_man</ipxact:name>
          <ipxact:displayName>pf2_shadow_pcie_cap_clock_power_man</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_shadow_pcie_cap_dll_active_rep_cap" type="string">
          <ipxact:name>pf2_shadow_pcie_cap_dll_active_rep_cap</ipxact:name>
          <ipxact:displayName>pf2_shadow_pcie_cap_dll_active_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_shadow_pcie_cap_link_bw_not_cap" type="string">
          <ipxact:name>pf2_shadow_pcie_cap_link_bw_not_cap</ipxact:name>
          <ipxact:displayName>pf2_shadow_pcie_cap_link_bw_not_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_shadow_pcie_cap_max_link_width" type="int">
          <ipxact:name>pf2_shadow_pcie_cap_max_link_width</ipxact:name>
          <ipxact:displayName>pf2_shadow_pcie_cap_max_link_width</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_shadow_pcie_cap_surprise_down_err_rep_cap" type="string">
          <ipxact:name>pf2_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:name>
          <ipxact:displayName>pf2_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_shadow_sriov_vf_stride_ari_cs2" type="int">
          <ipxact:name>pf2_shadow_sriov_vf_stride_ari_cs2</ipxact:name>
          <ipxact:displayName>pf2_shadow_sriov_vf_stride_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_cap_ser_num_reg_dw_1_addr_byte0" type="int">
          <ipxact:name>pf2_sn_cap_ser_num_reg_dw_1_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sn_cap_ser_num_reg_dw_1_addr_byte0</ipxact:displayName>
          <ipxact:value>8556</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_cap_ser_num_reg_dw_1_addr_byte1" type="int">
          <ipxact:name>pf2_sn_cap_ser_num_reg_dw_1_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sn_cap_ser_num_reg_dw_1_addr_byte1</ipxact:displayName>
          <ipxact:value>8557</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_cap_ser_num_reg_dw_1_addr_byte2" type="int">
          <ipxact:name>pf2_sn_cap_ser_num_reg_dw_1_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sn_cap_ser_num_reg_dw_1_addr_byte2</ipxact:displayName>
          <ipxact:value>8558</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_cap_ser_num_reg_dw_1_addr_byte3" type="int">
          <ipxact:name>pf2_sn_cap_ser_num_reg_dw_1_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sn_cap_ser_num_reg_dw_1_addr_byte3</ipxact:displayName>
          <ipxact:value>8559</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_cap_ser_num_reg_dw_2_addr_byte0" type="int">
          <ipxact:name>pf2_sn_cap_ser_num_reg_dw_2_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sn_cap_ser_num_reg_dw_2_addr_byte0</ipxact:displayName>
          <ipxact:value>8560</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_cap_ser_num_reg_dw_2_addr_byte1" type="int">
          <ipxact:name>pf2_sn_cap_ser_num_reg_dw_2_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sn_cap_ser_num_reg_dw_2_addr_byte1</ipxact:displayName>
          <ipxact:value>8561</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_cap_ser_num_reg_dw_2_addr_byte2" type="int">
          <ipxact:name>pf2_sn_cap_ser_num_reg_dw_2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sn_cap_ser_num_reg_dw_2_addr_byte2</ipxact:displayName>
          <ipxact:value>8562</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_cap_ser_num_reg_dw_2_addr_byte3" type="int">
          <ipxact:name>pf2_sn_cap_ser_num_reg_dw_2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sn_cap_ser_num_reg_dw_2_addr_byte3</ipxact:displayName>
          <ipxact:value>8563</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_cap_sn_base_addr_byte2" type="int">
          <ipxact:name>pf2_sn_cap_sn_base_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sn_cap_sn_base_addr_byte2</ipxact:displayName>
          <ipxact:value>8554</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_cap_sn_base_addr_byte3" type="int">
          <ipxact:name>pf2_sn_cap_sn_base_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sn_cap_sn_base_addr_byte3</ipxact:displayName>
          <ipxact:value>8555</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_cap_version" type="int">
          <ipxact:name>pf2_sn_cap_version</ipxact:name>
          <ipxact:displayName>pf2_sn_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sn_next_offset" type="int">
          <ipxact:name>pf2_sn_next_offset</ipxact:name>
          <ipxact:displayName>pf2_sn_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_sriov_initial_vfs_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_sriov_initial_vfs_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_sriov_initial_vfs_addr_byte0</ipxact:displayName>
          <ipxact:value>2105796</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_sriov_initial_vfs_addr_byte1" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_sriov_initial_vfs_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_sriov_initial_vfs_addr_byte1</ipxact:displayName>
          <ipxact:value>2105797</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0</ipxact:displayName>
          <ipxact:value>2105804</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1</ipxact:displayName>
          <ipxact:value>2105805</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2</ipxact:displayName>
          <ipxact:value>2105806</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3</ipxact:displayName>
          <ipxact:value>2105807</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105820</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte1" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105821</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte2" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105822</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte3" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar0_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105823</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105824</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte1" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105825</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte2" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105826</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte3" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar1_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105827</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105828</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte1" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105829</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte2" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105830</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte3" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar2_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105831</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105832</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte1" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105833</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte2" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105834</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte3" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar3_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105835</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105836</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte1" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105837</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte2" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105838</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte3" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar4_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105839</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105840</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte1" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105841</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte2" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105842</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte3" type="int">
          <ipxact:name>pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_shadow_vf_bar5_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105843</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sriov_bar1_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_sriov_bar1_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sriov_bar1_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105824</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sriov_bar3_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_sriov_bar3_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sriov_bar3_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105832</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sriov_bar5_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_sriov_bar5_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sriov_bar5_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105840</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sriov_base_reg_addr_byte2" type="int">
          <ipxact:name>pf2_sriov_cap_sriov_base_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sriov_base_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8634</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sriov_base_reg_addr_byte3" type="int">
          <ipxact:name>pf2_sriov_cap_sriov_base_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sriov_base_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8635</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sriov_initial_vfs_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_sriov_initial_vfs_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sriov_initial_vfs_addr_byte0</ipxact:displayName>
          <ipxact:value>8644</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sriov_initial_vfs_addr_byte1" type="int">
          <ipxact:name>pf2_sriov_cap_sriov_initial_vfs_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sriov_initial_vfs_addr_byte1</ipxact:displayName>
          <ipxact:value>8645</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sriov_vf_offset_position_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_sriov_vf_offset_position_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sriov_vf_offset_position_addr_byte0</ipxact:displayName>
          <ipxact:value>8652</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sriov_vf_offset_position_addr_byte1" type="int">
          <ipxact:name>pf2_sriov_cap_sriov_vf_offset_position_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sriov_vf_offset_position_addr_byte1</ipxact:displayName>
          <ipxact:value>8653</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sriov_vf_offset_position_addr_byte2" type="int">
          <ipxact:name>pf2_sriov_cap_sriov_vf_offset_position_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sriov_vf_offset_position_addr_byte2</ipxact:displayName>
          <ipxact:value>8654</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sriov_vf_offset_position_addr_byte3" type="int">
          <ipxact:name>pf2_sriov_cap_sriov_vf_offset_position_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sriov_vf_offset_position_addr_byte3</ipxact:displayName>
          <ipxact:value>8655</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sup_page_sizes_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_sup_page_sizes_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sup_page_sizes_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8660</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sup_page_sizes_reg_addr_byte1" type="int">
          <ipxact:name>pf2_sriov_cap_sup_page_sizes_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sup_page_sizes_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8661</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sup_page_sizes_reg_addr_byte2" type="int">
          <ipxact:name>pf2_sriov_cap_sup_page_sizes_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sup_page_sizes_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8662</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_sup_page_sizes_reg_addr_byte3" type="int">
          <ipxact:name>pf2_sriov_cap_sup_page_sizes_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_sup_page_sizes_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8663</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_version" type="int">
          <ipxact:name>pf2_sriov_cap_version</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_vf_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_vf_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_vf_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8668</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_vf_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_vf_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_vf_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8672</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_vf_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_vf_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_vf_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8676</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_vf_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_vf_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_vf_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8680</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_vf_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_vf_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_vf_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8684</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_vf_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf2_sriov_cap_vf_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_vf_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8688</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_vf_device_id_reg_addr_byte2" type="int">
          <ipxact:name>pf2_sriov_cap_vf_device_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_vf_device_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8658</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_cap_vf_device_id_reg_addr_byte3" type="int">
          <ipxact:name>pf2_sriov_cap_vf_device_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_sriov_cap_vf_device_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8659</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_initial_vfs_ari_cs2" type="int">
          <ipxact:name>pf2_sriov_initial_vfs_ari_cs2</ipxact:name>
          <ipxact:displayName>pf2_sriov_initial_vfs_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_initial_vfs_nonari" type="int">
          <ipxact:name>pf2_sriov_initial_vfs_nonari</ipxact:name>
          <ipxact:displayName>pf2_sriov_initial_vfs_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_next_offset" type="int">
          <ipxact:name>pf2_sriov_next_offset</ipxact:name>
          <ipxact:displayName>pf2_sriov_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar0_mask" type="string">
          <ipxact:name>pf2_sriov_vf_bar0_mask</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar0_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar0_prefetch" type="string">
          <ipxact:name>pf2_sriov_vf_bar0_prefetch</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar0_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar0_start" type="int">
          <ipxact:name>pf2_sriov_vf_bar0_start</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar0_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar0_type" type="string">
          <ipxact:name>pf2_sriov_vf_bar0_type</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar0_type</ipxact:displayName>
          <ipxact:value>pf2_sriov_vf_bar0_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar1_dummy_mask_7_1" type="int">
          <ipxact:name>pf2_sriov_vf_bar1_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar1_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar1_enabled" type="string">
          <ipxact:name>pf2_sriov_vf_bar1_enabled</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar1_mask" type="string">
          <ipxact:name>pf2_sriov_vf_bar1_mask</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar1_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar1_prefetch" type="string">
          <ipxact:name>pf2_sriov_vf_bar1_prefetch</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar1_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar1_start" type="int">
          <ipxact:name>pf2_sriov_vf_bar1_start</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar1_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar1_type" type="string">
          <ipxact:name>pf2_sriov_vf_bar1_type</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar1_type</ipxact:displayName>
          <ipxact:value>pf2_sriov_vf_bar1_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar2_mask" type="string">
          <ipxact:name>pf2_sriov_vf_bar2_mask</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar2_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar2_prefetch" type="string">
          <ipxact:name>pf2_sriov_vf_bar2_prefetch</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar2_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar2_start" type="int">
          <ipxact:name>pf2_sriov_vf_bar2_start</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar2_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar2_type" type="string">
          <ipxact:name>pf2_sriov_vf_bar2_type</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar2_type</ipxact:displayName>
          <ipxact:value>pf2_sriov_vf_bar2_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar3_dummy_mask_7_1" type="int">
          <ipxact:name>pf2_sriov_vf_bar3_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar3_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar3_enabled" type="string">
          <ipxact:name>pf2_sriov_vf_bar3_enabled</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar3_mask" type="string">
          <ipxact:name>pf2_sriov_vf_bar3_mask</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar3_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar3_prefetch" type="string">
          <ipxact:name>pf2_sriov_vf_bar3_prefetch</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar3_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar3_start" type="int">
          <ipxact:name>pf2_sriov_vf_bar3_start</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar3_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar3_type" type="string">
          <ipxact:name>pf2_sriov_vf_bar3_type</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar3_type</ipxact:displayName>
          <ipxact:value>pf2_sriov_vf_bar3_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar4_mask" type="string">
          <ipxact:name>pf2_sriov_vf_bar4_mask</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar4_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar4_prefetch" type="string">
          <ipxact:name>pf2_sriov_vf_bar4_prefetch</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar4_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar4_start" type="int">
          <ipxact:name>pf2_sriov_vf_bar4_start</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar4_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar4_type" type="string">
          <ipxact:name>pf2_sriov_vf_bar4_type</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar4_type</ipxact:displayName>
          <ipxact:value>pf2_sriov_vf_bar4_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar5_dummy_mask_7_1" type="int">
          <ipxact:name>pf2_sriov_vf_bar5_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar5_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar5_enabled" type="string">
          <ipxact:name>pf2_sriov_vf_bar5_enabled</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar5_mask" type="string">
          <ipxact:name>pf2_sriov_vf_bar5_mask</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar5_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar5_prefetch" type="string">
          <ipxact:name>pf2_sriov_vf_bar5_prefetch</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar5_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar5_start" type="int">
          <ipxact:name>pf2_sriov_vf_bar5_start</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar5_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_bar5_type" type="string">
          <ipxact:name>pf2_sriov_vf_bar5_type</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_bar5_type</ipxact:displayName>
          <ipxact:value>pf2_sriov_vf_bar5_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_device_id" type="int">
          <ipxact:name>pf2_sriov_vf_device_id</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_device_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_offset_ari_cs2" type="int">
          <ipxact:name>pf2_sriov_vf_offset_ari_cs2</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_offset_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_offset_position_nonari" type="int">
          <ipxact:name>pf2_sriov_vf_offset_position_nonari</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_offset_position_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_sriov_vf_stride_nonari" type="int">
          <ipxact:name>pf2_sriov_vf_stride_nonari</ipxact:name>
          <ipxact:displayName>pf2_sriov_vf_stride_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_subclass_code" type="int">
          <ipxact:name>pf2_subclass_code</ipxact:name>
          <ipxact:displayName>pf2_subclass_code</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_subsys_dev_id" type="int">
          <ipxact:name>pf2_subsys_dev_id</ipxact:name>
          <ipxact:displayName>pf2_subsys_dev_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_subsys_vendor_id" type="int">
          <ipxact:name>pf2_subsys_vendor_id</ipxact:name>
          <ipxact:displayName>pf2_subsys_vendor_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_cap_tph_ext_cap_hdr_reg_addr_byte2" type="int">
          <ipxact:name>pf2_tph_cap_tph_ext_cap_hdr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_tph_cap_tph_ext_cap_hdr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8698</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_cap_tph_ext_cap_hdr_reg_addr_byte3" type="int">
          <ipxact:name>pf2_tph_cap_tph_ext_cap_hdr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_tph_cap_tph_ext_cap_hdr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8699</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_cap_tph_req_cap_reg_addr_byte0" type="int">
          <ipxact:name>pf2_tph_cap_tph_req_cap_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_tph_cap_tph_req_cap_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8700</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_cap_tph_req_cap_reg_addr_byte1" type="int">
          <ipxact:name>pf2_tph_cap_tph_req_cap_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_tph_cap_tph_req_cap_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8701</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_cap_tph_req_cap_reg_addr_byte2" type="int">
          <ipxact:name>pf2_tph_cap_tph_req_cap_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_tph_cap_tph_req_cap_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8702</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_cap_tph_req_cap_reg_addr_byte3" type="int">
          <ipxact:name>pf2_tph_cap_tph_req_cap_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_tph_cap_tph_req_cap_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8703</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0" type="int">
          <ipxact:name>pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0</ipxact:displayName>
          <ipxact:value>2105852</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1" type="int">
          <ipxact:name>pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1</ipxact:displayName>
          <ipxact:value>2105853</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2" type="int">
          <ipxact:name>pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2</ipxact:displayName>
          <ipxact:value>2105854</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3" type="int">
          <ipxact:name>pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3</ipxact:displayName>
          <ipxact:value>2105855</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_int_vec" type="string">
          <ipxact:name>pf2_tph_req_cap_int_vec</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_int_vec</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_int_vec_vfcomm_cs2" type="string">
          <ipxact:name>pf2_tph_req_cap_int_vec_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_int_vec_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_reg_rsvdp_11" type="int">
          <ipxact:name>pf2_tph_req_cap_reg_rsvdp_11</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_reg_rsvdp_11</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_reg_rsvdp_27" type="int">
          <ipxact:name>pf2_tph_req_cap_reg_rsvdp_27</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_reg_rsvdp_27</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_reg_rsvdp_3" type="int">
          <ipxact:name>pf2_tph_req_cap_reg_rsvdp_3</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_reg_rsvdp_3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2" type="int">
          <ipxact:name>pf2_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2" type="int">
          <ipxact:name>pf2_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2" type="int">
          <ipxact:name>pf2_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_st_table_loc_0" type="string">
          <ipxact:name>pf2_tph_req_cap_st_table_loc_0</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_st_table_loc_0</ipxact:displayName>
          <ipxact:value>pf2_not_in_tph_struct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_st_table_loc_0_vfcomm_cs2" type="string">
          <ipxact:name>pf2_tph_req_cap_st_table_loc_0_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_st_table_loc_0_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>pf2_not_in_tph_struct_vf</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_st_table_loc_1" type="string">
          <ipxact:name>pf2_tph_req_cap_st_table_loc_1</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_st_table_loc_1</ipxact:displayName>
          <ipxact:value>pf2_not_in_msix_table</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_st_table_loc_1_vfcomm_cs2" type="string">
          <ipxact:name>pf2_tph_req_cap_st_table_loc_1_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_st_table_loc_1_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>pf2_not_in_msix_table_vf</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_st_table_size" type="int">
          <ipxact:name>pf2_tph_req_cap_st_table_size</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_st_table_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_st_table_size_vfcomm_cs2" type="int">
          <ipxact:name>pf2_tph_req_cap_st_table_size_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_st_table_size_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_cap_ver" type="int">
          <ipxact:name>pf2_tph_req_cap_ver</ipxact:name>
          <ipxact:displayName>pf2_tph_req_cap_ver</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_device_spec" type="string">
          <ipxact:name>pf2_tph_req_device_spec</ipxact:name>
          <ipxact:displayName>pf2_tph_req_device_spec</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_device_spec_vfcomm_cs2" type="string">
          <ipxact:name>pf2_tph_req_device_spec_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_tph_req_device_spec_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_extended_tph" type="string">
          <ipxact:name>pf2_tph_req_extended_tph</ipxact:name>
          <ipxact:displayName>pf2_tph_req_extended_tph</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_extended_tph_vfcomm_cs2" type="string">
          <ipxact:name>pf2_tph_req_extended_tph_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_tph_req_extended_tph_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_next_ptr" type="int">
          <ipxact:name>pf2_tph_req_next_ptr</ipxact:name>
          <ipxact:displayName>pf2_tph_req_next_ptr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_no_st_mode" type="string">
          <ipxact:name>pf2_tph_req_no_st_mode</ipxact:name>
          <ipxact:displayName>pf2_tph_req_no_st_mode</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_tph_req_no_st_mode_vfcomm_cs2" type="string">
          <ipxact:name>pf2_tph_req_no_st_mode_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf2_tph_req_no_st_mode_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar0_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar0_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar0_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105360</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar0_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_bar0_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar0_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105361</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar0_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_bar0_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar0_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105362</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar0_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf2_type0_hdr_bar0_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar0_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105363</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8208</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar1_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar1_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar1_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105364</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar1_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar1_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar1_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105364</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar1_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_bar1_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar1_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105365</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar1_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_bar1_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar1_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105366</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar1_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf2_type0_hdr_bar1_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar1_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105367</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8212</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar2_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar2_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar2_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105368</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar2_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_bar2_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar2_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105369</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar2_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_bar2_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar2_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105370</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar2_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf2_type0_hdr_bar2_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar2_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105371</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8216</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar3_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar3_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar3_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105372</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar3_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar3_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar3_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105372</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar3_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_bar3_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar3_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105373</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar3_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_bar3_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar3_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105374</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar3_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf2_type0_hdr_bar3_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar3_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105375</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8220</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar4_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar4_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar4_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105376</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar4_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_bar4_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar4_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105377</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar4_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_bar4_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar4_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105378</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar4_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf2_type0_hdr_bar4_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar4_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105379</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8224</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar5_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar5_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar5_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105380</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar5_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar5_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar5_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105380</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar5_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_bar5_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar5_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105381</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar5_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_bar5_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar5_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105382</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar5_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf2_type0_hdr_bar5_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar5_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105383</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8228</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8206</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8232</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8233</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8234</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte3" type="int">
          <ipxact:name>pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_cardbus_cis_ptr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8235</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_class_code_revision_id_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_class_code_revision_id_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_class_code_revision_id_addr_byte0</ipxact:displayName>
          <ipxact:value>8200</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_class_code_revision_id_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_class_code_revision_id_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_class_code_revision_id_addr_byte1</ipxact:displayName>
          <ipxact:value>8201</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_class_code_revision_id_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_class_code_revision_id_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_class_code_revision_id_addr_byte2</ipxact:displayName>
          <ipxact:value>8202</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_class_code_revision_id_addr_byte3" type="int">
          <ipxact:name>pf2_type0_hdr_class_code_revision_id_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_class_code_revision_id_addr_byte3</ipxact:displayName>
          <ipxact:value>8203</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_device_id_vendor_id_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_device_id_vendor_id_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_device_id_vendor_id_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8192</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_device_id_vendor_id_reg_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_device_id_vendor_id_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_device_id_vendor_id_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8193</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_device_id_vendor_id_reg_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_device_id_vendor_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_device_id_vendor_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8194</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_device_id_vendor_id_reg_addr_byte3" type="int">
          <ipxact:name>pf2_type0_hdr_device_id_vendor_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_device_id_vendor_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8195</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2105392</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2105393</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2105394</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_exp_rom_bar_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2105395</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_exp_rom_base_addr_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_exp_rom_base_addr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_exp_rom_base_addr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8240</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8253</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_pci_cap_ptr_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_pci_cap_ptr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_pci_cap_ptr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8244</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0" type="int">
          <ipxact:name>pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>8236</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1" type="int">
          <ipxact:name>pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>8237</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2" type="int">
          <ipxact:name>pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>8238</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3" type="int">
          <ipxact:name>pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf2_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>8239</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_vf_bar0_reg_rsvdp_0" type="string">
          <ipxact:name>pf2_vf_bar0_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf2_vf_bar0_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_vf_bar1_reg_rsvdp_0" type="string">
          <ipxact:name>pf2_vf_bar1_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf2_vf_bar1_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_vf_bar2_reg_rsvdp_0" type="string">
          <ipxact:name>pf2_vf_bar2_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf2_vf_bar2_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_vf_bar3_reg_rsvdp_0" type="string">
          <ipxact:name>pf2_vf_bar3_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf2_vf_bar3_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_vf_bar4_reg_rsvdp_0" type="string">
          <ipxact:name>pf2_vf_bar4_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf2_vf_bar4_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf2_vf_bar5_reg_rsvdp_0" type="string">
          <ipxact:name>pf2_vf_bar5_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf2_vf_bar5_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_aer_cap_aer_ext_cap_hdr_off_addr_byte2" type="int">
          <ipxact:name>pf3_aer_cap_aer_ext_cap_hdr_off_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_aer_cap_aer_ext_cap_hdr_off_addr_byte2</ipxact:displayName>
          <ipxact:value>12546</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_aer_cap_aer_ext_cap_hdr_off_addr_byte3" type="int">
          <ipxact:name>pf3_aer_cap_aer_ext_cap_hdr_off_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_aer_cap_aer_ext_cap_hdr_off_addr_byte3</ipxact:displayName>
          <ipxact:value>12547</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_aer_cap_version" type="int">
          <ipxact:name>pf3_aer_cap_version</ipxact:name>
          <ipxact:displayName>pf3_aer_cap_version</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_aer_next_offset" type="int">
          <ipxact:name>pf3_aer_next_offset</ipxact:name>
          <ipxact:displayName>pf3_aer_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_ari_cap_ari_base_addr_byte2" type="int">
          <ipxact:name>pf3_ari_cap_ari_base_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_ari_cap_ari_base_addr_byte2</ipxact:displayName>
          <ipxact:value>12666</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_ari_cap_ari_base_addr_byte3" type="int">
          <ipxact:name>pf3_ari_cap_ari_base_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_ari_cap_ari_base_addr_byte3</ipxact:displayName>
          <ipxact:value>12667</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_ari_cap_version" type="int">
          <ipxact:name>pf3_ari_cap_version</ipxact:name>
          <ipxact:displayName>pf3_ari_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_ari_next_offset" type="int">
          <ipxact:name>pf3_ari_next_offset</ipxact:name>
          <ipxact:displayName>pf3_ari_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_ats_cap_ats_cap_hdr_reg_addr_byte2" type="int">
          <ipxact:name>pf3_ats_cap_ats_cap_hdr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_ats_cap_ats_cap_hdr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12934</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_ats_cap_ats_cap_hdr_reg_addr_byte3" type="int">
          <ipxact:name>pf3_ats_cap_ats_cap_hdr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_ats_cap_ats_cap_hdr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12935</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_ats_cap_ats_capabilities_ctrl_reg_addr_byte0" type="int">
          <ipxact:name>pf3_ats_cap_ats_capabilities_ctrl_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_ats_cap_ats_capabilities_ctrl_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12936</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_ats_cap_version" type="int">
          <ipxact:name>pf3_ats_cap_version</ipxact:name>
          <ipxact:displayName>pf3_ats_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_ats_capabilities_ctrl_reg_rsvdp_7" type="string">
          <ipxact:name>pf3_ats_capabilities_ctrl_reg_rsvdp_7</ipxact:name>
          <ipxact:displayName>pf3_ats_capabilities_ctrl_reg_rsvdp_7</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_ats_next_offset" type="int">
          <ipxact:name>pf3_ats_next_offset</ipxact:name>
          <ipxact:displayName>pf3_ats_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_aux_curr" type="int">
          <ipxact:name>pf3_aux_curr</ipxact:name>
          <ipxact:displayName>pf3_aux_curr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar0_mem_io" type="string">
          <ipxact:name>pf3_bar0_mem_io</ipxact:name>
          <ipxact:displayName>pf3_bar0_mem_io</ipxact:displayName>
          <ipxact:value>pf3_bar0_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar0_prefetch" type="string">
          <ipxact:name>pf3_bar0_prefetch</ipxact:name>
          <ipxact:displayName>pf3_bar0_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar0_start" type="int">
          <ipxact:name>pf3_bar0_start</ipxact:name>
          <ipxact:displayName>pf3_bar0_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar0_type" type="string">
          <ipxact:name>pf3_bar0_type</ipxact:name>
          <ipxact:displayName>pf3_bar0_type</ipxact:displayName>
          <ipxact:value>pf3_bar0_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar1_mem_io" type="string">
          <ipxact:name>pf3_bar1_mem_io</ipxact:name>
          <ipxact:displayName>pf3_bar1_mem_io</ipxact:displayName>
          <ipxact:value>pf3_bar1_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar1_prefetch" type="string">
          <ipxact:name>pf3_bar1_prefetch</ipxact:name>
          <ipxact:displayName>pf3_bar1_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar1_start" type="int">
          <ipxact:name>pf3_bar1_start</ipxact:name>
          <ipxact:displayName>pf3_bar1_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar1_type" type="string">
          <ipxact:name>pf3_bar1_type</ipxact:name>
          <ipxact:displayName>pf3_bar1_type</ipxact:displayName>
          <ipxact:value>pf3_bar1_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar2_mem_io" type="string">
          <ipxact:name>pf3_bar2_mem_io</ipxact:name>
          <ipxact:displayName>pf3_bar2_mem_io</ipxact:displayName>
          <ipxact:value>pf3_bar2_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar2_prefetch" type="string">
          <ipxact:name>pf3_bar2_prefetch</ipxact:name>
          <ipxact:displayName>pf3_bar2_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar2_start" type="int">
          <ipxact:name>pf3_bar2_start</ipxact:name>
          <ipxact:displayName>pf3_bar2_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar2_type" type="string">
          <ipxact:name>pf3_bar2_type</ipxact:name>
          <ipxact:displayName>pf3_bar2_type</ipxact:displayName>
          <ipxact:value>pf3_bar2_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar3_mem_io" type="string">
          <ipxact:name>pf3_bar3_mem_io</ipxact:name>
          <ipxact:displayName>pf3_bar3_mem_io</ipxact:displayName>
          <ipxact:value>pf3_bar3_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar3_prefetch" type="string">
          <ipxact:name>pf3_bar3_prefetch</ipxact:name>
          <ipxact:displayName>pf3_bar3_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar3_start" type="int">
          <ipxact:name>pf3_bar3_start</ipxact:name>
          <ipxact:displayName>pf3_bar3_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar3_type" type="string">
          <ipxact:name>pf3_bar3_type</ipxact:name>
          <ipxact:displayName>pf3_bar3_type</ipxact:displayName>
          <ipxact:value>pf3_bar3_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar4_mem_io" type="string">
          <ipxact:name>pf3_bar4_mem_io</ipxact:name>
          <ipxact:displayName>pf3_bar4_mem_io</ipxact:displayName>
          <ipxact:value>pf3_bar4_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar4_prefetch" type="string">
          <ipxact:name>pf3_bar4_prefetch</ipxact:name>
          <ipxact:displayName>pf3_bar4_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar4_start" type="int">
          <ipxact:name>pf3_bar4_start</ipxact:name>
          <ipxact:displayName>pf3_bar4_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar4_type" type="string">
          <ipxact:name>pf3_bar4_type</ipxact:name>
          <ipxact:displayName>pf3_bar4_type</ipxact:displayName>
          <ipxact:value>pf3_bar4_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar5_mem_io" type="string">
          <ipxact:name>pf3_bar5_mem_io</ipxact:name>
          <ipxact:displayName>pf3_bar5_mem_io</ipxact:displayName>
          <ipxact:value>pf3_bar5_mem</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar5_prefetch" type="string">
          <ipxact:name>pf3_bar5_prefetch</ipxact:name>
          <ipxact:displayName>pf3_bar5_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar5_start" type="int">
          <ipxact:name>pf3_bar5_start</ipxact:name>
          <ipxact:displayName>pf3_bar5_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_bar5_type" type="string">
          <ipxact:name>pf3_bar5_type</ipxact:name>
          <ipxact:displayName>pf3_bar5_type</ipxact:displayName>
          <ipxact:value>pf3_bar5_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_base_class_code" type="int">
          <ipxact:name>pf3_base_class_code</ipxact:name>
          <ipxact:displayName>pf3_base_class_code</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_cap_id_nxt_ptr_reg_rsvdp_20" type="string">
          <ipxact:name>pf3_cap_id_nxt_ptr_reg_rsvdp_20</ipxact:name>
          <ipxact:displayName>pf3_cap_id_nxt_ptr_reg_rsvdp_20</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_cap_pointer" type="int">
          <ipxact:name>pf3_cap_pointer</ipxact:name>
          <ipxact:displayName>pf3_cap_pointer</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_con_status_reg_rsvdp_2" type="string">
          <ipxact:name>pf3_con_status_reg_rsvdp_2</ipxact:name>
          <ipxact:displayName>pf3_con_status_reg_rsvdp_2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_con_status_reg_rsvdp_4" type="int">
          <ipxact:name>pf3_con_status_reg_rsvdp_4</ipxact:name>
          <ipxact:displayName>pf3_con_status_reg_rsvdp_4</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_d1_support" type="string">
          <ipxact:name>pf3_d1_support</ipxact:name>
          <ipxact:displayName>pf3_d1_support</ipxact:displayName>
          <ipxact:value>pf3_d1_not_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_d2_support" type="string">
          <ipxact:name>pf3_d2_support</ipxact:name>
          <ipxact:displayName>pf3_d2_support</ipxact:displayName>
          <ipxact:value>pf3_d2_not_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_0" type="int">
          <ipxact:name>pf3_dbi_reserved_0</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_0</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_1" type="int">
          <ipxact:name>pf3_dbi_reserved_1</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_10" type="int">
          <ipxact:name>pf3_dbi_reserved_10</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_10</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_11" type="int">
          <ipxact:name>pf3_dbi_reserved_11</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_11</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_12" type="int">
          <ipxact:name>pf3_dbi_reserved_12</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_13" type="int">
          <ipxact:name>pf3_dbi_reserved_13</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_13</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_14" type="int">
          <ipxact:name>pf3_dbi_reserved_14</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_14</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_15" type="int">
          <ipxact:name>pf3_dbi_reserved_15</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_15</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_16" type="int">
          <ipxact:name>pf3_dbi_reserved_16</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_16</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_17" type="int">
          <ipxact:name>pf3_dbi_reserved_17</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_17</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_18" type="int">
          <ipxact:name>pf3_dbi_reserved_18</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_18</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_19" type="int">
          <ipxact:name>pf3_dbi_reserved_19</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_19</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_2" type="int">
          <ipxact:name>pf3_dbi_reserved_2</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_3" type="int">
          <ipxact:name>pf3_dbi_reserved_3</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_4" type="int">
          <ipxact:name>pf3_dbi_reserved_4</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_4</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_5" type="int">
          <ipxact:name>pf3_dbi_reserved_5</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_5</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_6" type="int">
          <ipxact:name>pf3_dbi_reserved_6</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_6</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_7" type="int">
          <ipxact:name>pf3_dbi_reserved_7</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_7</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_8" type="int">
          <ipxact:name>pf3_dbi_reserved_8</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_8</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dbi_reserved_9" type="int">
          <ipxact:name>pf3_dbi_reserved_9</ipxact:name>
          <ipxact:displayName>pf3_dbi_reserved_9</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_device_capabilities_reg_rsvdp_12" type="int">
          <ipxact:name>pf3_device_capabilities_reg_rsvdp_12</ipxact:name>
          <ipxact:displayName>pf3_device_capabilities_reg_rsvdp_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_device_capabilities_reg_rsvdp_16" type="int">
          <ipxact:name>pf3_device_capabilities_reg_rsvdp_16</ipxact:name>
          <ipxact:displayName>pf3_device_capabilities_reg_rsvdp_16</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_device_capabilities_reg_rsvdp_29" type="int">
          <ipxact:name>pf3_device_capabilities_reg_rsvdp_29</ipxact:name>
          <ipxact:displayName>pf3_device_capabilities_reg_rsvdp_29</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_dsi" type="string">
          <ipxact:name>pf3_dsi</ipxact:name>
          <ipxact:displayName>pf3_dsi</ipxact:displayName>
          <ipxact:value>pf3_not_required</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_exp_rom_bar_mask_reg_rsvdp_1" type="int">
          <ipxact:name>pf3_exp_rom_bar_mask_reg_rsvdp_1</ipxact:name>
          <ipxact:displayName>pf3_exp_rom_bar_mask_reg_rsvdp_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_exp_rom_base_addr_reg_rsvdp_1" type="int">
          <ipxact:name>pf3_exp_rom_base_addr_reg_rsvdp_1</ipxact:name>
          <ipxact:displayName>pf3_exp_rom_base_addr_reg_rsvdp_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_forward_user_vsec" type="string">
          <ipxact:name>pf3_forward_user_vsec</ipxact:name>
          <ipxact:displayName>pf3_forward_user_vsec</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_global_inval_spprtd" type="string">
          <ipxact:name>pf3_global_inval_spprtd</ipxact:name>
          <ipxact:displayName>pf3_global_inval_spprtd</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_header_type" type="int">
          <ipxact:name>pf3_header_type</ipxact:name>
          <ipxact:displayName>pf3_header_type</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_int_pin" type="string">
          <ipxact:name>pf3_int_pin</ipxact:name>
          <ipxact:displayName>pf3_int_pin</ipxact:displayName>
          <ipxact:value>pf3_no_int</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_invalidate_q_depth" type="int">
          <ipxact:name>pf3_invalidate_q_depth</ipxact:name>
          <ipxact:displayName>pf3_invalidate_q_depth</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_link_capabilities_reg_rsvdp_23" type="string">
          <ipxact:name>pf3_link_capabilities_reg_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf3_link_capabilities_reg_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_link_control_link_status_reg_rsvdp_12" type="int">
          <ipxact:name>pf3_link_control_link_status_reg_rsvdp_12</ipxact:name>
          <ipxact:displayName>pf3_link_control_link_status_reg_rsvdp_12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_link_control_link_status_reg_rsvdp_2" type="string">
          <ipxact:name>pf3_link_control_link_status_reg_rsvdp_2</ipxact:name>
          <ipxact:displayName>pf3_link_control_link_status_reg_rsvdp_2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_link_control_link_status_reg_rsvdp_25" type="int">
          <ipxact:name>pf3_link_control_link_status_reg_rsvdp_25</ipxact:name>
          <ipxact:displayName>pf3_link_control_link_status_reg_rsvdp_25</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_link_control_link_status_reg_rsvdp_9" type="string">
          <ipxact:name>pf3_link_control_link_status_reg_rsvdp_9</ipxact:name>
          <ipxact:displayName>pf3_link_control_link_status_reg_rsvdp_9</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1" type="int">
          <ipxact:name>pf3_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12369</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2" type="int">
          <ipxact:name>pf3_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_msi_cap_pci_msi_cap_id_next_ctrl_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12370</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_msix_pba_offset_reg_addr_byte0" type="int">
          <ipxact:name>pf3_msix_cap_msix_pba_offset_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_msix_pba_offset_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12472</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_msix_pba_offset_reg_addr_byte1" type="int">
          <ipxact:name>pf3_msix_cap_msix_pba_offset_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_msix_pba_offset_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12473</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_msix_pba_offset_reg_addr_byte2" type="int">
          <ipxact:name>pf3_msix_cap_msix_pba_offset_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_msix_pba_offset_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12474</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_msix_pba_offset_reg_addr_byte3" type="int">
          <ipxact:name>pf3_msix_cap_msix_pba_offset_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_msix_pba_offset_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12475</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_msix_table_offset_reg_addr_byte0" type="int">
          <ipxact:name>pf3_msix_cap_msix_table_offset_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_msix_table_offset_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12468</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_msix_table_offset_reg_addr_byte1" type="int">
          <ipxact:name>pf3_msix_cap_msix_table_offset_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_msix_table_offset_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12469</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_msix_table_offset_reg_addr_byte2" type="int">
          <ipxact:name>pf3_msix_cap_msix_table_offset_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_msix_table_offset_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12470</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_msix_table_offset_reg_addr_byte3" type="int">
          <ipxact:name>pf3_msix_cap_msix_table_offset_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_msix_table_offset_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12471</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1" type="int">
          <ipxact:name>pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12465</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2" type="int">
          <ipxact:name>pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12466</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3" type="int">
          <ipxact:name>pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12467</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2" type="int">
          <ipxact:name>pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte2</ipxact:displayName>
          <ipxact:value>2109618</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3" type="int">
          <ipxact:name>pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_msix_cap_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_addr_byte3</ipxact:displayName>
          <ipxact:value>2109619</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_multi_func" type="string">
          <ipxact:name>pf3_multi_func</ipxact:name>
          <ipxact:displayName>pf3_multi_func</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_no_soft_rst" type="string">
          <ipxact:name>pf3_no_soft_rst</ipxact:name>
          <ipxact:displayName>pf3_no_soft_rst</ipxact:displayName>
          <ipxact:value>pf3_internally_reset</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_page_aligned_req" type="string">
          <ipxact:name>pf3_page_aligned_req</ipxact:name>
          <ipxact:displayName>pf3_page_aligned_req</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msi_64_bit_addr_cap" type="string">
          <ipxact:name>pf3_pci_msi_64_bit_addr_cap</ipxact:name>
          <ipxact:displayName>pf3_pci_msi_64_bit_addr_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msi_cap_next_offset" type="int">
          <ipxact:name>pf3_pci_msi_cap_next_offset</ipxact:name>
          <ipxact:displayName>pf3_pci_msi_cap_next_offset</ipxact:displayName>
          <ipxact:value>112</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msi_enable" type="string">
          <ipxact:name>pf3_pci_msi_enable</ipxact:name>
          <ipxact:displayName>pf3_pci_msi_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msi_multiple_msg_cap" type="string">
          <ipxact:name>pf3_pci_msi_multiple_msg_cap</ipxact:name>
          <ipxact:displayName>pf3_pci_msi_multiple_msg_cap</ipxact:displayName>
          <ipxact:value>pf3_msi_vec_1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msi_multiple_msg_en" type="int">
          <ipxact:name>pf3_pci_msi_multiple_msg_en</ipxact:name>
          <ipxact:displayName>pf3_pci_msi_multiple_msg_en</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_bir" type="int">
          <ipxact:name>pf3_pci_msix_bir</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_bir</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_cap_id_next_ctrl_reg_rsvdp_27" type="int">
          <ipxact:name>pf3_pci_msix_cap_id_next_ctrl_reg_rsvdp_27</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_cap_id_next_ctrl_reg_rsvdp_27</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2" type="int">
          <ipxact:name>pf3_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_cap_id_next_ctrl_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_cap_next_offset" type="int">
          <ipxact:name>pf3_pci_msix_cap_next_offset</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_cap_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_enable" type="string">
          <ipxact:name>pf3_pci_msix_enable</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_enable_vfcomm_cs2" type="string">
          <ipxact:name>pf3_pci_msix_enable_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_enable_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_function_mask" type="string">
          <ipxact:name>pf3_pci_msix_function_mask</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_function_mask</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_function_mask_vfcomm_cs2" type="string">
          <ipxact:name>pf3_pci_msix_function_mask_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_function_mask_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_pba" type="int">
          <ipxact:name>pf3_pci_msix_pba</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_pba</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_pba_offset" type="int">
          <ipxact:name>pf3_pci_msix_pba_offset</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_pba_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_table_offset" type="int">
          <ipxact:name>pf3_pci_msix_table_offset</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_table_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_table_size" type="int">
          <ipxact:name>pf3_pci_msix_table_size</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_table_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_msix_table_size_vfcomm_cs2" type="int">
          <ipxact:name>pf3_pci_msix_table_size_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_pci_msix_table_size_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar0_enabled" type="string">
          <ipxact:name>pf3_pci_type0_bar0_enabled</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar0_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar0_mask_31_1" type="int">
          <ipxact:name>pf3_pci_type0_bar0_mask_31_1</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar0_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar1_dummy_mask_7_1" type="int">
          <ipxact:name>pf3_pci_type0_bar1_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar1_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar1_enabled" type="string">
          <ipxact:name>pf3_pci_type0_bar1_enabled</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar1_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf3_pci_type0_bar1_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar1_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar1_mask_31_1" type="int">
          <ipxact:name>pf3_pci_type0_bar1_mask_31_1</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar1_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar2_enabled" type="string">
          <ipxact:name>pf3_pci_type0_bar2_enabled</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar2_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar2_mask_31_1" type="int">
          <ipxact:name>pf3_pci_type0_bar2_mask_31_1</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar2_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar3_dummy_mask_7_1" type="int">
          <ipxact:name>pf3_pci_type0_bar3_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar3_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar3_enabled" type="string">
          <ipxact:name>pf3_pci_type0_bar3_enabled</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar3_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf3_pci_type0_bar3_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar3_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar3_mask_31_1" type="int">
          <ipxact:name>pf3_pci_type0_bar3_mask_31_1</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar3_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar4_enabled" type="string">
          <ipxact:name>pf3_pci_type0_bar4_enabled</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar4_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar4_mask_31_1" type="int">
          <ipxact:name>pf3_pci_type0_bar4_mask_31_1</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar4_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar5_dummy_mask_7_1" type="int">
          <ipxact:name>pf3_pci_type0_bar5_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar5_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar5_enabled" type="string">
          <ipxact:name>pf3_pci_type0_bar5_enabled</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar5_enabled_or_mask64lsb" type="string">
          <ipxact:name>pf3_pci_type0_bar5_enabled_or_mask64lsb</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar5_enabled_or_mask64lsb</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_bar5_mask_31_1" type="int">
          <ipxact:name>pf3_pci_type0_bar5_mask_31_1</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_bar5_mask_31_1</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_device_id" type="int">
          <ipxact:name>pf3_pci_type0_device_id</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_device_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pci_type0_vendor_id" type="int">
          <ipxact:name>pf3_pci_type0_vendor_id</ipxact:name>
          <ipxact:displayName>pf3_pci_type0_vendor_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_active_state_link_pm_control" type="string">
          <ipxact:name>pf3_pcie_cap_active_state_link_pm_control</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_active_state_link_pm_control</ipxact:displayName>
          <ipxact:value>pf3_aspm_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_active_state_link_pm_support" type="string">
          <ipxact:name>pf3_pcie_cap_active_state_link_pm_support</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_active_state_link_pm_support</ipxact:displayName>
          <ipxact:value>pf3_no_aspm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_aspm_opt_compliance" type="string">
          <ipxact:name>pf3_pcie_cap_aspm_opt_compliance</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_aspm_opt_compliance</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_aux_power_pm_en" type="string">
          <ipxact:name>pf3_pcie_cap_aux_power_pm_en</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_aux_power_pm_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_clock_power_man" type="string">
          <ipxact:name>pf3_pcie_cap_clock_power_man</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_clock_power_man</ipxact:displayName>
          <ipxact:value>pf3_refclk_remove_not_ok</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_common_clk_config" type="string">
          <ipxact:name>pf3_pcie_cap_common_clk_config</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_common_clk_config</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_device_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf3_pcie_cap_device_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_device_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12404</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_device_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf3_pcie_cap_device_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_device_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12405</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_device_capabilities_reg_addr_byte3" type="int">
          <ipxact:name>pf3_pcie_cap_device_capabilities_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_device_capabilities_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12407</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_device_control_device_status_addr_byte1" type="int">
          <ipxact:name>pf3_pcie_cap_device_control_device_status_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_device_control_device_status_addr_byte1</ipxact:displayName>
          <ipxact:value>12409</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_dll_active" type="string">
          <ipxact:name>pf3_pcie_cap_dll_active</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_dll_active</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_dll_active_rep_cap" type="string">
          <ipxact:name>pf3_pcie_cap_dll_active_rep_cap</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_dll_active_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_en_clk_power_man" type="string">
          <ipxact:name>pf3_pcie_cap_en_clk_power_man</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_en_clk_power_man</ipxact:displayName>
          <ipxact:value>pf3_clkreq_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_en_no_snoop" type="string">
          <ipxact:name>pf3_pcie_cap_en_no_snoop</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_en_no_snoop</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_enter_compliance" type="string">
          <ipxact:name>pf3_pcie_cap_enter_compliance</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_enter_compliance</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_ep_l0s_accpt_latency" type="int">
          <ipxact:name>pf3_pcie_cap_ep_l0s_accpt_latency</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_ep_l0s_accpt_latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_ep_l1_accpt_latency" type="int">
          <ipxact:name>pf3_pcie_cap_ep_l1_accpt_latency</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_ep_l1_accpt_latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_ext_tag_en" type="string">
          <ipxact:name>pf3_pcie_cap_ext_tag_en</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_ext_tag_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_ext_tag_supp" type="string">
          <ipxact:name>pf3_pcie_cap_ext_tag_supp</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_ext_tag_supp</ipxact:displayName>
          <ipxact:value>pf3_not_supported</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_extended_synch" type="string">
          <ipxact:name>pf3_pcie_cap_extended_synch</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_extended_synch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_flr_cap" type="string">
          <ipxact:name>pf3_pcie_cap_flr_cap</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_flr_cap</ipxact:displayName>
          <ipxact:value>pf3_not_capable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_hw_auto_speed_disable" type="string">
          <ipxact:name>pf3_pcie_cap_hw_auto_speed_disable</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_hw_auto_speed_disable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd" type="string">
          <ipxact:name>pf3_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvd</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31" type="string">
          <ipxact:name>pf3_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_rsvdp_31</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_initiate_flr" type="string">
          <ipxact:name>pf3_pcie_cap_initiate_flr</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_initiate_flr</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_l0s_exit_latency_commclk_dis" type="int">
          <ipxact:name>pf3_pcie_cap_l0s_exit_latency_commclk_dis</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_l0s_exit_latency_commclk_dis</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_l0s_exit_latency_commclk_ena_cs2" type="int">
          <ipxact:name>pf3_pcie_cap_l0s_exit_latency_commclk_ena_cs2</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_l0s_exit_latency_commclk_ena_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_l1_exit_latency_commclk_dis" type="int">
          <ipxact:name>pf3_pcie_cap_l1_exit_latency_commclk_dis</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_l1_exit_latency_commclk_dis</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_l1_exit_latency_commclk_ena_cs2" type="int">
          <ipxact:name>pf3_pcie_cap_l1_exit_latency_commclk_ena_cs2</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_l1_exit_latency_commclk_ena_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_auto_bw_int_en" type="string">
          <ipxact:name>pf3_pcie_cap_link_auto_bw_int_en</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_auto_bw_int_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_auto_bw_status" type="string">
          <ipxact:name>pf3_pcie_cap_link_auto_bw_status</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_auto_bw_status</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_bw_man_int_en" type="string">
          <ipxact:name>pf3_pcie_cap_link_bw_man_int_en</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_bw_man_int_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_bw_man_status" type="string">
          <ipxact:name>pf3_pcie_cap_link_bw_man_status</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_bw_man_status</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_bw_not_cap" type="string">
          <ipxact:name>pf3_pcie_cap_link_bw_not_cap</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_bw_not_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf3_pcie_cap_link_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12412</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf3_pcie_cap_link_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12413</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_capabilities_reg_addr_byte2" type="int">
          <ipxact:name>pf3_pcie_cap_link_capabilities_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_capabilities_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12414</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_capabilities_reg_addr_byte3" type="int">
          <ipxact:name>pf3_pcie_cap_link_capabilities_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_capabilities_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12415</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_control2_link_status2_reg_addr_byte0" type="int">
          <ipxact:name>pf3_pcie_cap_link_control2_link_status2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_control2_link_status2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12595360</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_control_link_status_reg_addr_byte0" type="int">
          <ipxact:name>pf3_pcie_cap_link_control_link_status_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_control_link_status_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>4206720</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_control_link_status_reg_addr_byte1" type="int">
          <ipxact:name>pf3_pcie_cap_link_control_link_status_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_control_link_status_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>4206721</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_control_link_status_reg_addr_byte2" type="int">
          <ipxact:name>pf3_pcie_cap_link_control_link_status_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_control_link_status_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>4206722</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_disable" type="string">
          <ipxact:name>pf3_pcie_cap_link_disable</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_disable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_link_training" type="string">
          <ipxact:name>pf3_pcie_cap_link_training</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_link_training</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_max_link_speed" type="string">
          <ipxact:name>pf3_pcie_cap_max_link_speed</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_max_link_speed</ipxact:displayName>
          <ipxact:value>pf3_max_8gts</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_max_link_width" type="string">
          <ipxact:name>pf3_pcie_cap_max_link_width</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_max_link_width</ipxact:displayName>
          <ipxact:value>pf3_x1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_max_payload_size" type="string">
          <ipxact:name>pf3_pcie_cap_max_payload_size</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_max_payload_size</ipxact:displayName>
          <ipxact:value>pf3_payload_512</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_max_read_req_size" type="int">
          <ipxact:name>pf3_pcie_cap_max_read_req_size</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_max_read_req_size</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_nego_link_width" type="string">
          <ipxact:name>pf3_pcie_cap_nego_link_width</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_nego_link_width</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_next_ptr" type="int">
          <ipxact:name>pf3_pcie_cap_next_ptr</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_next_ptr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1" type="int">
          <ipxact:name>pf3_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12401</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3" type="int">
          <ipxact:name>pf3_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_pcie_cap_id_pcie_next_cap_ptr_pcie_cap_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12403</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_phantom_func_en" type="string">
          <ipxact:name>pf3_pcie_cap_phantom_func_en</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_phantom_func_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_phantom_func_support" type="int">
          <ipxact:name>pf3_pcie_cap_phantom_func_support</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_phantom_func_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_port_num" type="int">
          <ipxact:name>pf3_pcie_cap_port_num</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_port_num</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_rcb" type="string">
          <ipxact:name>pf3_pcie_cap_rcb</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_rcb</ipxact:displayName>
          <ipxact:value>pf3_rcb_64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_retrain_link" type="string">
          <ipxact:name>pf3_pcie_cap_retrain_link</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_retrain_link</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_role_based_err_report" type="string">
          <ipxact:name>pf3_pcie_cap_role_based_err_report</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_role_based_err_report</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_sel_deemphasis" type="string">
          <ipxact:name>pf3_pcie_cap_sel_deemphasis</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_sel_deemphasis</ipxact:displayName>
          <ipxact:value>pf3_minus_6db</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_shadow_link_capabilities_reg_addr_byte0" type="int">
          <ipxact:name>pf3_pcie_cap_shadow_link_capabilities_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_shadow_link_capabilities_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109564</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_shadow_link_capabilities_reg_addr_byte1" type="int">
          <ipxact:name>pf3_pcie_cap_shadow_link_capabilities_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_shadow_link_capabilities_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109565</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_slot_clk_config" type="string">
          <ipxact:name>pf3_pcie_cap_slot_clk_config</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_slot_clk_config</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_surprise_down_err_rep_cap" type="string">
          <ipxact:name>pf3_pcie_cap_surprise_down_err_rep_cap</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_surprise_down_err_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_target_link_speed" type="string">
          <ipxact:name>pf3_pcie_cap_target_link_speed</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_target_link_speed</ipxact:displayName>
          <ipxact:value>pf3_trgt_gen3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_cap_tx_margin" type="string">
          <ipxact:name>pf3_pcie_cap_tx_margin</ipxact:name>
          <ipxact:displayName>pf3_pcie_cap_tx_margin</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_int_msg_num" type="int">
          <ipxact:name>pf3_pcie_int_msg_num</ipxact:name>
          <ipxact:displayName>pf3_pcie_int_msg_num</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pcie_slot_imp" type="string">
          <ipxact:name>pf3_pcie_slot_imp</ipxact:name>
          <ipxact:displayName>pf3_pcie_slot_imp</ipxact:displayName>
          <ipxact:value>pf3_not_implemented</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pm_cap_cap_id_nxt_ptr_reg_addr_byte1" type="int">
          <ipxact:name>pf3_pm_cap_cap_id_nxt_ptr_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_pm_cap_cap_id_nxt_ptr_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12353</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pm_cap_cap_id_nxt_ptr_reg_addr_byte2" type="int">
          <ipxact:name>pf3_pm_cap_cap_id_nxt_ptr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_pm_cap_cap_id_nxt_ptr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12354</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pm_cap_cap_id_nxt_ptr_reg_addr_byte3" type="int">
          <ipxact:name>pf3_pm_cap_cap_id_nxt_ptr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_pm_cap_cap_id_nxt_ptr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12355</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pm_cap_con_status_reg_addr_byte0" type="int">
          <ipxact:name>pf3_pm_cap_con_status_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_pm_cap_con_status_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12356</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pm_next_pointer" type="int">
          <ipxact:name>pf3_pm_next_pointer</ipxact:name>
          <ipxact:displayName>pf3_pm_next_pointer</ipxact:displayName>
          <ipxact:value>80</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pm_spec_ver" type="int">
          <ipxact:name>pf3_pm_spec_ver</ipxact:name>
          <ipxact:displayName>pf3_pm_spec_ver</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pme_clk" type="string">
          <ipxact:name>pf3_pme_clk</ipxact:name>
          <ipxact:displayName>pf3_pme_clk</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_pme_support" type="int">
          <ipxact:name>pf3_pme_support</ipxact:name>
          <ipxact:displayName>pf3_pme_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_power_state" type="int">
          <ipxact:name>pf3_power_state</ipxact:name>
          <ipxact:displayName>pf3_power_state</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_program_interface" type="int">
          <ipxact:name>pf3_program_interface</ipxact:name>
          <ipxact:displayName>pf3_program_interface</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_0_addr" type="int">
          <ipxact:name>pf3_reserved_0_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_0_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_10_addr" type="int">
          <ipxact:name>pf3_reserved_10_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_10_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_11_addr" type="int">
          <ipxact:name>pf3_reserved_11_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_11_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_12_addr" type="int">
          <ipxact:name>pf3_reserved_12_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_12_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_13_addr" type="int">
          <ipxact:name>pf3_reserved_13_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_13_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_14_addr" type="int">
          <ipxact:name>pf3_reserved_14_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_14_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_15_addr" type="int">
          <ipxact:name>pf3_reserved_15_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_15_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_16_addr" type="int">
          <ipxact:name>pf3_reserved_16_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_16_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_17_addr" type="int">
          <ipxact:name>pf3_reserved_17_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_17_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_18_addr" type="int">
          <ipxact:name>pf3_reserved_18_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_18_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_19_addr" type="int">
          <ipxact:name>pf3_reserved_19_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_19_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_1_addr" type="int">
          <ipxact:name>pf3_reserved_1_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_1_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_2_addr" type="int">
          <ipxact:name>pf3_reserved_2_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_2_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_3_addr" type="int">
          <ipxact:name>pf3_reserved_3_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_3_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_4_addr" type="int">
          <ipxact:name>pf3_reserved_4_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_4_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_5_addr" type="int">
          <ipxact:name>pf3_reserved_5_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_5_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_6_addr" type="int">
          <ipxact:name>pf3_reserved_6_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_6_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_7_addr" type="int">
          <ipxact:name>pf3_reserved_7_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_7_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_8_addr" type="int">
          <ipxact:name>pf3_reserved_8_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_8_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_reserved_9_addr" type="int">
          <ipxact:name>pf3_reserved_9_addr</ipxact:name>
          <ipxact:displayName>pf3_reserved_9_addr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_revision_id" type="int">
          <ipxact:name>pf3_revision_id</ipxact:name>
          <ipxact:displayName>pf3_revision_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_rom_bar_enable" type="string">
          <ipxact:name>pf3_rom_bar_enable</ipxact:name>
          <ipxact:displayName>pf3_rom_bar_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_rom_bar_enabled" type="string">
          <ipxact:name>pf3_rom_bar_enabled</ipxact:name>
          <ipxact:displayName>pf3_rom_bar_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_rom_mask" type="int">
          <ipxact:name>pf3_rom_mask</ipxact:name>
          <ipxact:displayName>pf3_rom_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_shadow_link_capabilities_reg_shadow_rsvdp_23" type="string">
          <ipxact:name>pf3_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:name>
          <ipxact:displayName>pf3_shadow_link_capabilities_reg_shadow_rsvdp_23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_shadow_pcie_cap_active_state_link_pm_support" type="int">
          <ipxact:name>pf3_shadow_pcie_cap_active_state_link_pm_support</ipxact:name>
          <ipxact:displayName>pf3_shadow_pcie_cap_active_state_link_pm_support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_shadow_pcie_cap_aspm_opt_compliance" type="string">
          <ipxact:name>pf3_shadow_pcie_cap_aspm_opt_compliance</ipxact:name>
          <ipxact:displayName>pf3_shadow_pcie_cap_aspm_opt_compliance</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_shadow_pcie_cap_clock_power_man" type="string">
          <ipxact:name>pf3_shadow_pcie_cap_clock_power_man</ipxact:name>
          <ipxact:displayName>pf3_shadow_pcie_cap_clock_power_man</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_shadow_pcie_cap_dll_active_rep_cap" type="string">
          <ipxact:name>pf3_shadow_pcie_cap_dll_active_rep_cap</ipxact:name>
          <ipxact:displayName>pf3_shadow_pcie_cap_dll_active_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_shadow_pcie_cap_link_bw_not_cap" type="string">
          <ipxact:name>pf3_shadow_pcie_cap_link_bw_not_cap</ipxact:name>
          <ipxact:displayName>pf3_shadow_pcie_cap_link_bw_not_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_shadow_pcie_cap_max_link_width" type="int">
          <ipxact:name>pf3_shadow_pcie_cap_max_link_width</ipxact:name>
          <ipxact:displayName>pf3_shadow_pcie_cap_max_link_width</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_shadow_pcie_cap_surprise_down_err_rep_cap" type="string">
          <ipxact:name>pf3_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:name>
          <ipxact:displayName>pf3_shadow_pcie_cap_surprise_down_err_rep_cap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_shadow_sriov_vf_stride_ari_cs2" type="int">
          <ipxact:name>pf3_shadow_sriov_vf_stride_ari_cs2</ipxact:name>
          <ipxact:displayName>pf3_shadow_sriov_vf_stride_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_cap_ser_num_reg_dw_1_addr_byte0" type="int">
          <ipxact:name>pf3_sn_cap_ser_num_reg_dw_1_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sn_cap_ser_num_reg_dw_1_addr_byte0</ipxact:displayName>
          <ipxact:value>12652</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_cap_ser_num_reg_dw_1_addr_byte1" type="int">
          <ipxact:name>pf3_sn_cap_ser_num_reg_dw_1_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sn_cap_ser_num_reg_dw_1_addr_byte1</ipxact:displayName>
          <ipxact:value>12653</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_cap_ser_num_reg_dw_1_addr_byte2" type="int">
          <ipxact:name>pf3_sn_cap_ser_num_reg_dw_1_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sn_cap_ser_num_reg_dw_1_addr_byte2</ipxact:displayName>
          <ipxact:value>12654</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_cap_ser_num_reg_dw_1_addr_byte3" type="int">
          <ipxact:name>pf3_sn_cap_ser_num_reg_dw_1_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sn_cap_ser_num_reg_dw_1_addr_byte3</ipxact:displayName>
          <ipxact:value>12655</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_cap_ser_num_reg_dw_2_addr_byte0" type="int">
          <ipxact:name>pf3_sn_cap_ser_num_reg_dw_2_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sn_cap_ser_num_reg_dw_2_addr_byte0</ipxact:displayName>
          <ipxact:value>12656</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_cap_ser_num_reg_dw_2_addr_byte1" type="int">
          <ipxact:name>pf3_sn_cap_ser_num_reg_dw_2_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sn_cap_ser_num_reg_dw_2_addr_byte1</ipxact:displayName>
          <ipxact:value>12657</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_cap_ser_num_reg_dw_2_addr_byte2" type="int">
          <ipxact:name>pf3_sn_cap_ser_num_reg_dw_2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sn_cap_ser_num_reg_dw_2_addr_byte2</ipxact:displayName>
          <ipxact:value>12658</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_cap_ser_num_reg_dw_2_addr_byte3" type="int">
          <ipxact:name>pf3_sn_cap_ser_num_reg_dw_2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sn_cap_ser_num_reg_dw_2_addr_byte3</ipxact:displayName>
          <ipxact:value>12659</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_cap_sn_base_addr_byte2" type="int">
          <ipxact:name>pf3_sn_cap_sn_base_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sn_cap_sn_base_addr_byte2</ipxact:displayName>
          <ipxact:value>12650</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_cap_sn_base_addr_byte3" type="int">
          <ipxact:name>pf3_sn_cap_sn_base_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sn_cap_sn_base_addr_byte3</ipxact:displayName>
          <ipxact:value>12651</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_cap_version" type="int">
          <ipxact:name>pf3_sn_cap_version</ipxact:name>
          <ipxact:displayName>pf3_sn_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sn_next_offset" type="int">
          <ipxact:name>pf3_sn_next_offset</ipxact:name>
          <ipxact:displayName>pf3_sn_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_sriov_initial_vfs_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_sriov_initial_vfs_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_sriov_initial_vfs_addr_byte0</ipxact:displayName>
          <ipxact:value>2109892</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_sriov_initial_vfs_addr_byte1" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_sriov_initial_vfs_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_sriov_initial_vfs_addr_byte1</ipxact:displayName>
          <ipxact:value>2109893</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte0</ipxact:displayName>
          <ipxact:value>2109900</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte1</ipxact:displayName>
          <ipxact:value>2109901</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte2</ipxact:displayName>
          <ipxact:value>2109902</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_sriov_vf_offset_position_addr_byte3</ipxact:displayName>
          <ipxact:value>2109903</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109916</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte1" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109917</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte2" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109918</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte3" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar0_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109919</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109920</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte1" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109921</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte2" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109922</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte3" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar1_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109923</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109924</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte1" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109925</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte2" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109926</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte3" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar2_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109927</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109928</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte1" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109929</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte2" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109930</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte3" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar3_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109931</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109932</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte1" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109933</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte2" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109934</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte3" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar4_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109935</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109936</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte1" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109937</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte2" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109938</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte3" type="int">
          <ipxact:name>pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_shadow_vf_bar5_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109939</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sriov_bar1_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_sriov_bar1_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sriov_bar1_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109920</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sriov_bar3_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_sriov_bar3_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sriov_bar3_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109928</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sriov_bar5_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_sriov_bar5_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sriov_bar5_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109936</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sriov_base_reg_addr_byte2" type="int">
          <ipxact:name>pf3_sriov_cap_sriov_base_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sriov_base_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12730</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sriov_base_reg_addr_byte3" type="int">
          <ipxact:name>pf3_sriov_cap_sriov_base_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sriov_base_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12731</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sriov_initial_vfs_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_sriov_initial_vfs_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sriov_initial_vfs_addr_byte0</ipxact:displayName>
          <ipxact:value>12740</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sriov_initial_vfs_addr_byte1" type="int">
          <ipxact:name>pf3_sriov_cap_sriov_initial_vfs_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sriov_initial_vfs_addr_byte1</ipxact:displayName>
          <ipxact:value>12741</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sriov_vf_offset_position_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_sriov_vf_offset_position_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sriov_vf_offset_position_addr_byte0</ipxact:displayName>
          <ipxact:value>12748</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sriov_vf_offset_position_addr_byte1" type="int">
          <ipxact:name>pf3_sriov_cap_sriov_vf_offset_position_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sriov_vf_offset_position_addr_byte1</ipxact:displayName>
          <ipxact:value>12749</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sriov_vf_offset_position_addr_byte2" type="int">
          <ipxact:name>pf3_sriov_cap_sriov_vf_offset_position_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sriov_vf_offset_position_addr_byte2</ipxact:displayName>
          <ipxact:value>12750</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sriov_vf_offset_position_addr_byte3" type="int">
          <ipxact:name>pf3_sriov_cap_sriov_vf_offset_position_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sriov_vf_offset_position_addr_byte3</ipxact:displayName>
          <ipxact:value>12751</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sup_page_sizes_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_sup_page_sizes_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sup_page_sizes_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12756</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sup_page_sizes_reg_addr_byte1" type="int">
          <ipxact:name>pf3_sriov_cap_sup_page_sizes_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sup_page_sizes_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12757</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sup_page_sizes_reg_addr_byte2" type="int">
          <ipxact:name>pf3_sriov_cap_sup_page_sizes_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sup_page_sizes_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12758</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_sup_page_sizes_reg_addr_byte3" type="int">
          <ipxact:name>pf3_sriov_cap_sup_page_sizes_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_sup_page_sizes_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12759</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_version" type="int">
          <ipxact:name>pf3_sriov_cap_version</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_version</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_vf_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_vf_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_vf_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12764</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_vf_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_vf_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_vf_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12768</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_vf_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_vf_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_vf_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12772</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_vf_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_vf_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_vf_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12776</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_vf_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_vf_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_vf_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12780</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_vf_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf3_sriov_cap_vf_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_vf_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12784</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_vf_device_id_reg_addr_byte2" type="int">
          <ipxact:name>pf3_sriov_cap_vf_device_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_vf_device_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12754</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_cap_vf_device_id_reg_addr_byte3" type="int">
          <ipxact:name>pf3_sriov_cap_vf_device_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_sriov_cap_vf_device_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12755</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_initial_vfs_ari_cs2" type="int">
          <ipxact:name>pf3_sriov_initial_vfs_ari_cs2</ipxact:name>
          <ipxact:displayName>pf3_sriov_initial_vfs_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_initial_vfs_nonari" type="int">
          <ipxact:name>pf3_sriov_initial_vfs_nonari</ipxact:name>
          <ipxact:displayName>pf3_sriov_initial_vfs_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_next_offset" type="int">
          <ipxact:name>pf3_sriov_next_offset</ipxact:name>
          <ipxact:displayName>pf3_sriov_next_offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar0_mask" type="string">
          <ipxact:name>pf3_sriov_vf_bar0_mask</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar0_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar0_prefetch" type="string">
          <ipxact:name>pf3_sriov_vf_bar0_prefetch</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar0_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar0_start" type="int">
          <ipxact:name>pf3_sriov_vf_bar0_start</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar0_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar0_type" type="string">
          <ipxact:name>pf3_sriov_vf_bar0_type</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar0_type</ipxact:displayName>
          <ipxact:value>pf3_sriov_vf_bar0_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar1_dummy_mask_7_1" type="int">
          <ipxact:name>pf3_sriov_vf_bar1_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar1_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar1_enabled" type="string">
          <ipxact:name>pf3_sriov_vf_bar1_enabled</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar1_mask" type="string">
          <ipxact:name>pf3_sriov_vf_bar1_mask</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar1_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar1_prefetch" type="string">
          <ipxact:name>pf3_sriov_vf_bar1_prefetch</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar1_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar1_start" type="int">
          <ipxact:name>pf3_sriov_vf_bar1_start</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar1_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar1_type" type="string">
          <ipxact:name>pf3_sriov_vf_bar1_type</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar1_type</ipxact:displayName>
          <ipxact:value>pf3_sriov_vf_bar1_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar2_mask" type="string">
          <ipxact:name>pf3_sriov_vf_bar2_mask</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar2_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar2_prefetch" type="string">
          <ipxact:name>pf3_sriov_vf_bar2_prefetch</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar2_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar2_start" type="int">
          <ipxact:name>pf3_sriov_vf_bar2_start</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar2_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar2_type" type="string">
          <ipxact:name>pf3_sriov_vf_bar2_type</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar2_type</ipxact:displayName>
          <ipxact:value>pf3_sriov_vf_bar2_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar3_dummy_mask_7_1" type="int">
          <ipxact:name>pf3_sriov_vf_bar3_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar3_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar3_enabled" type="string">
          <ipxact:name>pf3_sriov_vf_bar3_enabled</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar3_mask" type="string">
          <ipxact:name>pf3_sriov_vf_bar3_mask</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar3_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar3_prefetch" type="string">
          <ipxact:name>pf3_sriov_vf_bar3_prefetch</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar3_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar3_start" type="int">
          <ipxact:name>pf3_sriov_vf_bar3_start</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar3_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar3_type" type="string">
          <ipxact:name>pf3_sriov_vf_bar3_type</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar3_type</ipxact:displayName>
          <ipxact:value>pf3_sriov_vf_bar3_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar4_mask" type="string">
          <ipxact:name>pf3_sriov_vf_bar4_mask</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar4_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar4_prefetch" type="string">
          <ipxact:name>pf3_sriov_vf_bar4_prefetch</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar4_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar4_start" type="int">
          <ipxact:name>pf3_sriov_vf_bar4_start</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar4_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar4_type" type="string">
          <ipxact:name>pf3_sriov_vf_bar4_type</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar4_type</ipxact:displayName>
          <ipxact:value>pf3_sriov_vf_bar4_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar5_dummy_mask_7_1" type="int">
          <ipxact:name>pf3_sriov_vf_bar5_dummy_mask_7_1</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar5_dummy_mask_7_1</ipxact:displayName>
          <ipxact:value>127</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar5_enabled" type="string">
          <ipxact:name>pf3_sriov_vf_bar5_enabled</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar5_mask" type="string">
          <ipxact:name>pf3_sriov_vf_bar5_mask</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar5_mask</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar5_prefetch" type="string">
          <ipxact:name>pf3_sriov_vf_bar5_prefetch</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar5_prefetch</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar5_start" type="int">
          <ipxact:name>pf3_sriov_vf_bar5_start</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar5_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_bar5_type" type="string">
          <ipxact:name>pf3_sriov_vf_bar5_type</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_bar5_type</ipxact:displayName>
          <ipxact:value>pf3_sriov_vf_bar5_mem32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_device_id" type="int">
          <ipxact:name>pf3_sriov_vf_device_id</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_device_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_offset_ari_cs2" type="int">
          <ipxact:name>pf3_sriov_vf_offset_ari_cs2</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_offset_ari_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_offset_position_nonari" type="int">
          <ipxact:name>pf3_sriov_vf_offset_position_nonari</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_offset_position_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_sriov_vf_stride_nonari" type="int">
          <ipxact:name>pf3_sriov_vf_stride_nonari</ipxact:name>
          <ipxact:displayName>pf3_sriov_vf_stride_nonari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_subclass_code" type="int">
          <ipxact:name>pf3_subclass_code</ipxact:name>
          <ipxact:displayName>pf3_subclass_code</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_subsys_dev_id" type="int">
          <ipxact:name>pf3_subsys_dev_id</ipxact:name>
          <ipxact:displayName>pf3_subsys_dev_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_subsys_vendor_id" type="int">
          <ipxact:name>pf3_subsys_vendor_id</ipxact:name>
          <ipxact:displayName>pf3_subsys_vendor_id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_cap_tph_ext_cap_hdr_reg_addr_byte2" type="int">
          <ipxact:name>pf3_tph_cap_tph_ext_cap_hdr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_tph_cap_tph_ext_cap_hdr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12794</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_cap_tph_ext_cap_hdr_reg_addr_byte3" type="int">
          <ipxact:name>pf3_tph_cap_tph_ext_cap_hdr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_tph_cap_tph_ext_cap_hdr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12795</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_cap_tph_req_cap_reg_addr_byte0" type="int">
          <ipxact:name>pf3_tph_cap_tph_req_cap_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_tph_cap_tph_req_cap_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12796</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_cap_tph_req_cap_reg_addr_byte1" type="int">
          <ipxact:name>pf3_tph_cap_tph_req_cap_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_tph_cap_tph_req_cap_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12797</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_cap_tph_req_cap_reg_addr_byte2" type="int">
          <ipxact:name>pf3_tph_cap_tph_req_cap_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_tph_cap_tph_req_cap_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12798</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_cap_tph_req_cap_reg_addr_byte3" type="int">
          <ipxact:name>pf3_tph_cap_tph_req_cap_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_tph_cap_tph_req_cap_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12799</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0" type="int">
          <ipxact:name>pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte0</ipxact:displayName>
          <ipxact:value>2109948</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1" type="int">
          <ipxact:name>pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte1</ipxact:displayName>
          <ipxact:value>2109949</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2" type="int">
          <ipxact:name>pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte2</ipxact:displayName>
          <ipxact:value>2109950</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3" type="int">
          <ipxact:name>pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_tph_cap_tph_req_cap_reg_vfcomm_cs2_addr_byte3</ipxact:displayName>
          <ipxact:value>2109951</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_int_vec" type="string">
          <ipxact:name>pf3_tph_req_cap_int_vec</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_int_vec</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_int_vec_vfcomm_cs2" type="string">
          <ipxact:name>pf3_tph_req_cap_int_vec_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_int_vec_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_reg_rsvdp_11" type="int">
          <ipxact:name>pf3_tph_req_cap_reg_rsvdp_11</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_reg_rsvdp_11</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_reg_rsvdp_27" type="int">
          <ipxact:name>pf3_tph_req_cap_reg_rsvdp_27</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_reg_rsvdp_27</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_reg_rsvdp_3" type="int">
          <ipxact:name>pf3_tph_req_cap_reg_rsvdp_3</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_reg_rsvdp_3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2" type="int">
          <ipxact:name>pf3_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_reg_vfcomm_cs2_rsvdp_11_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2" type="int">
          <ipxact:name>pf3_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_reg_vfcomm_cs2_rsvdp_27_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2" type="int">
          <ipxact:name>pf3_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_reg_vfcomm_cs2_rsvdp_3_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_st_table_loc_0" type="string">
          <ipxact:name>pf3_tph_req_cap_st_table_loc_0</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_st_table_loc_0</ipxact:displayName>
          <ipxact:value>pf3_not_in_tph_struct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_st_table_loc_0_vfcomm_cs2" type="string">
          <ipxact:name>pf3_tph_req_cap_st_table_loc_0_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_st_table_loc_0_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>pf3_not_in_tph_struct_vf</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_st_table_loc_1" type="string">
          <ipxact:name>pf3_tph_req_cap_st_table_loc_1</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_st_table_loc_1</ipxact:displayName>
          <ipxact:value>pf3_not_in_msix_table</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_st_table_loc_1_vfcomm_cs2" type="string">
          <ipxact:name>pf3_tph_req_cap_st_table_loc_1_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_st_table_loc_1_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>pf3_not_in_msix_table_vf</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_st_table_size" type="int">
          <ipxact:name>pf3_tph_req_cap_st_table_size</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_st_table_size</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_st_table_size_vfcomm_cs2" type="int">
          <ipxact:name>pf3_tph_req_cap_st_table_size_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_st_table_size_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_cap_ver" type="int">
          <ipxact:name>pf3_tph_req_cap_ver</ipxact:name>
          <ipxact:displayName>pf3_tph_req_cap_ver</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_device_spec" type="string">
          <ipxact:name>pf3_tph_req_device_spec</ipxact:name>
          <ipxact:displayName>pf3_tph_req_device_spec</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_device_spec_vfcomm_cs2" type="string">
          <ipxact:name>pf3_tph_req_device_spec_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_tph_req_device_spec_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_extended_tph" type="string">
          <ipxact:name>pf3_tph_req_extended_tph</ipxact:name>
          <ipxact:displayName>pf3_tph_req_extended_tph</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_extended_tph_vfcomm_cs2" type="string">
          <ipxact:name>pf3_tph_req_extended_tph_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_tph_req_extended_tph_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_next_ptr" type="int">
          <ipxact:name>pf3_tph_req_next_ptr</ipxact:name>
          <ipxact:displayName>pf3_tph_req_next_ptr</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_no_st_mode" type="string">
          <ipxact:name>pf3_tph_req_no_st_mode</ipxact:name>
          <ipxact:displayName>pf3_tph_req_no_st_mode</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_tph_req_no_st_mode_vfcomm_cs2" type="string">
          <ipxact:name>pf3_tph_req_no_st_mode_vfcomm_cs2</ipxact:name>
          <ipxact:displayName>pf3_tph_req_no_st_mode_vfcomm_cs2</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar0_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar0_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar0_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109456</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar0_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_bar0_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar0_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109457</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar0_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_bar0_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar0_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109458</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar0_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf3_type0_hdr_bar0_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar0_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109459</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar0_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar0_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar0_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12304</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar1_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar1_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar1_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109460</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar1_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar1_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar1_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109460</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar1_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_bar1_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar1_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109461</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar1_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_bar1_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar1_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109462</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar1_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf3_type0_hdr_bar1_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar1_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109463</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar1_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar1_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar1_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12308</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar2_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar2_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar2_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109464</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar2_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_bar2_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar2_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109465</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar2_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_bar2_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar2_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109466</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar2_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf3_type0_hdr_bar2_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar2_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109467</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar2_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar2_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar2_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12312</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar3_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar3_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar3_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109468</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar3_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar3_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar3_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109468</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar3_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_bar3_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar3_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109469</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar3_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_bar3_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar3_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109470</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar3_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf3_type0_hdr_bar3_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar3_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109471</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar3_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar3_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar3_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12316</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar4_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar4_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar4_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109472</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar4_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_bar4_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar4_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109473</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar4_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_bar4_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar4_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109474</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar4_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf3_type0_hdr_bar4_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar4_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109475</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar4_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar4_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar4_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12320</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar5_enable_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar5_enable_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar5_enable_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109476</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar5_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar5_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar5_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109476</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar5_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_bar5_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar5_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109477</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar5_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_bar5_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar5_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109478</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar5_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf3_type0_hdr_bar5_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar5_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109479</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bar5_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_bar5_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bar5_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12324</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_bist_header_type_latency_cache_line_size_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12302</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12328</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12329</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12330</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte3" type="int">
          <ipxact:name>pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_cardbus_cis_ptr_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12331</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_class_code_revision_id_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_class_code_revision_id_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_class_code_revision_id_addr_byte0</ipxact:displayName>
          <ipxact:value>12296</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_class_code_revision_id_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_class_code_revision_id_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_class_code_revision_id_addr_byte1</ipxact:displayName>
          <ipxact:value>12297</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_class_code_revision_id_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_class_code_revision_id_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_class_code_revision_id_addr_byte2</ipxact:displayName>
          <ipxact:value>12298</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_class_code_revision_id_addr_byte3" type="int">
          <ipxact:name>pf3_type0_hdr_class_code_revision_id_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_class_code_revision_id_addr_byte3</ipxact:displayName>
          <ipxact:value>12299</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_device_id_vendor_id_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_device_id_vendor_id_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_device_id_vendor_id_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12288</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_device_id_vendor_id_reg_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_device_id_vendor_id_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_device_id_vendor_id_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12289</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_device_id_vendor_id_reg_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_device_id_vendor_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_device_id_vendor_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12290</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_device_id_vendor_id_reg_addr_byte3" type="int">
          <ipxact:name>pf3_type0_hdr_device_id_vendor_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_device_id_vendor_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12291</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>2109488</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>2109489</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>2109490</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte3" type="int">
          <ipxact:name>pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_exp_rom_bar_mask_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>2109491</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_exp_rom_base_addr_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_exp_rom_base_addr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_exp_rom_base_addr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12336</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_max_latency_min_grant_interrupt_pin_interrupt_line_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12349</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_pci_cap_ptr_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_pci_cap_ptr_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_pci_cap_ptr_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12340</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0" type="int">
          <ipxact:name>pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte0</ipxact:displayName>
          <ipxact:value>12332</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1" type="int">
          <ipxact:name>pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte1</ipxact:displayName>
          <ipxact:value>12333</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2" type="int">
          <ipxact:name>pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte2</ipxact:displayName>
          <ipxact:value>12334</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3" type="int">
          <ipxact:name>pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3</ipxact:name>
          <ipxact:displayName>pf3_type0_hdr_subsystem_id_subsystem_vendor_id_reg_addr_byte3</ipxact:displayName>
          <ipxact:value>12335</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_vf_bar0_reg_rsvdp_0" type="string">
          <ipxact:name>pf3_vf_bar0_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf3_vf_bar0_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_vf_bar1_reg_rsvdp_0" type="string">
          <ipxact:name>pf3_vf_bar1_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf3_vf_bar1_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_vf_bar2_reg_rsvdp_0" type="string">
          <ipxact:name>pf3_vf_bar2_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf3_vf_bar2_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_vf_bar3_reg_rsvdp_0" type="string">
          <ipxact:name>pf3_vf_bar3_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf3_vf_bar3_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_vf_bar4_reg_rsvdp_0" type="string">
          <ipxact:name>pf3_vf_bar4_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf3_vf_bar4_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pf3_vf_bar5_reg_rsvdp_0" type="string">
          <ipxact:name>pf3_vf_bar5_reg_rsvdp_0</ipxact:name>
          <ipxact:displayName>pf3_vf_bar5_reg_rsvdp_0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_ats_cap_enable" type="string">
          <ipxact:name>virtual_pf2_ats_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf2_ats_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_bar1_mask_bit0" type="string">
          <ipxact:name>virtual_pf2_bar1_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf2_bar1_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_bar3_mask_bit0" type="string">
          <ipxact:name>virtual_pf2_bar3_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf2_bar3_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_bar5_mask_bit0" type="string">
          <ipxact:name>virtual_pf2_bar5_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf2_bar5_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_enable" type="string">
          <ipxact:name>virtual_pf2_enable</ipxact:name>
          <ipxact:displayName>virtual_pf2_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_msi_enable" type="string">
          <ipxact:name>virtual_pf2_msi_enable</ipxact:name>
          <ipxact:displayName>virtual_pf2_msi_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_msix_enable" type="string">
          <ipxact:name>virtual_pf2_msix_enable</ipxact:name>
          <ipxact:displayName>virtual_pf2_msix_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_pb_cap_enable" type="string">
          <ipxact:name>virtual_pf2_pb_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf2_pb_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_sn_cap_enable" type="string">
          <ipxact:name>virtual_pf2_sn_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf2_sn_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_sriov_enable" type="string">
          <ipxact:name>virtual_pf2_sriov_enable</ipxact:name>
          <ipxact:displayName>virtual_pf2_sriov_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_sriov_num_vf_ari" type="int">
          <ipxact:name>virtual_pf2_sriov_num_vf_ari</ipxact:name>
          <ipxact:displayName>virtual_pf2_sriov_num_vf_ari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_sriov_num_vf_non_ari" type="int">
          <ipxact:name>virtual_pf2_sriov_num_vf_non_ari</ipxact:name>
          <ipxact:displayName>virtual_pf2_sriov_num_vf_non_ari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_sriov_vf_bar0_enabled" type="string">
          <ipxact:name>virtual_pf2_sriov_vf_bar0_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf2_sriov_vf_bar0_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_sriov_vf_bar1_enabled" type="string">
          <ipxact:name>virtual_pf2_sriov_vf_bar1_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf2_sriov_vf_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_sriov_vf_bar2_enabled" type="string">
          <ipxact:name>virtual_pf2_sriov_vf_bar2_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf2_sriov_vf_bar2_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_sriov_vf_bar3_enabled" type="string">
          <ipxact:name>virtual_pf2_sriov_vf_bar3_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf2_sriov_vf_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_sriov_vf_bar4_enabled" type="string">
          <ipxact:name>virtual_pf2_sriov_vf_bar4_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf2_sriov_vf_bar4_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_sriov_vf_bar5_enabled" type="string">
          <ipxact:name>virtual_pf2_sriov_vf_bar5_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf2_sriov_vf_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_tph_cap_enable" type="string">
          <ipxact:name>virtual_pf2_tph_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf2_tph_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf2_user_vsec_cap_enable" type="string">
          <ipxact:name>virtual_pf2_user_vsec_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf2_user_vsec_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_ats_cap_enable" type="string">
          <ipxact:name>virtual_pf3_ats_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf3_ats_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_bar1_mask_bit0" type="string">
          <ipxact:name>virtual_pf3_bar1_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf3_bar1_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_bar3_mask_bit0" type="string">
          <ipxact:name>virtual_pf3_bar3_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf3_bar3_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_bar5_mask_bit0" type="string">
          <ipxact:name>virtual_pf3_bar5_mask_bit0</ipxact:name>
          <ipxact:displayName>virtual_pf3_bar5_mask_bit0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_enable" type="string">
          <ipxact:name>virtual_pf3_enable</ipxact:name>
          <ipxact:displayName>virtual_pf3_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_msi_enable" type="string">
          <ipxact:name>virtual_pf3_msi_enable</ipxact:name>
          <ipxact:displayName>virtual_pf3_msi_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_msix_enable" type="string">
          <ipxact:name>virtual_pf3_msix_enable</ipxact:name>
          <ipxact:displayName>virtual_pf3_msix_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_pb_cap_enable" type="string">
          <ipxact:name>virtual_pf3_pb_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf3_pb_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_sn_cap_enable" type="string">
          <ipxact:name>virtual_pf3_sn_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf3_sn_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_sriov_enable" type="string">
          <ipxact:name>virtual_pf3_sriov_enable</ipxact:name>
          <ipxact:displayName>virtual_pf3_sriov_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_sriov_num_vf_ari" type="int">
          <ipxact:name>virtual_pf3_sriov_num_vf_ari</ipxact:name>
          <ipxact:displayName>virtual_pf3_sriov_num_vf_ari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_sriov_num_vf_non_ari" type="int">
          <ipxact:name>virtual_pf3_sriov_num_vf_non_ari</ipxact:name>
          <ipxact:displayName>virtual_pf3_sriov_num_vf_non_ari</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_sriov_vf_bar0_enabled" type="string">
          <ipxact:name>virtual_pf3_sriov_vf_bar0_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf3_sriov_vf_bar0_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_sriov_vf_bar1_enabled" type="string">
          <ipxact:name>virtual_pf3_sriov_vf_bar1_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf3_sriov_vf_bar1_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_sriov_vf_bar2_enabled" type="string">
          <ipxact:name>virtual_pf3_sriov_vf_bar2_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf3_sriov_vf_bar2_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_sriov_vf_bar3_enabled" type="string">
          <ipxact:name>virtual_pf3_sriov_vf_bar3_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf3_sriov_vf_bar3_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_sriov_vf_bar4_enabled" type="string">
          <ipxact:name>virtual_pf3_sriov_vf_bar4_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf3_sriov_vf_bar4_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_sriov_vf_bar5_enabled" type="string">
          <ipxact:name>virtual_pf3_sriov_vf_bar5_enabled</ipxact:name>
          <ipxact:displayName>virtual_pf3_sriov_vf_bar5_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_tph_cap_enable" type="string">
          <ipxact:name>virtual_pf3_tph_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf3_tph_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="virtual_pf3_user_vsec_cap_enable" type="string">
          <ipxact:name>virtual_pf3_user_vsec_cap_enable</ipxact:name>
          <ipxact:displayName>virtual_pf3_user_vsec_cap_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="AUTO_RXM_IRQ_INTERRUPTS_USED" type="string">
          <ipxact:name>AUTO_RXM_IRQ_INTERRUPTS_USED</ipxact:name>
          <ipxact:displayName>Auto INTERRUPTS_USED</ipxact:displayName>
          <ipxact:value>-1</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </altera:altera_module_parameters>
    <altera:altera_assignments>
      <ipxact:parameters>
        <ipxact:parameter parameterId="testbench.partner.map.hip_ctrl" type="string">
          <ipxact:name>testbench.partner.map.hip_ctrl</ipxact:name>
          <ipxact:value>pcie_tb.hip_ctrl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.map.hip_pipe" type="string">
          <ipxact:name>testbench.partner.map.hip_pipe</ipxact:name>
          <ipxact:value>pcie_tb.hip_pipe</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.map.hip_serial" type="string">
          <ipxact:name>testbench.partner.map.hip_serial</ipxact:name>
          <ipxact:value>pcie_tb.hip_serial</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.map.npor" type="string">
          <ipxact:name>testbench.partner.map.npor</ipxact:name>
          <ipxact:value>pcie_tb.npor</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.map.refclk" type="string">
          <ipxact:name>testbench.partner.map.refclk</ipxact:name>
          <ipxact:value>pcie_tb.refclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.class" type="string">
          <ipxact:name>testbench.partner.pcie_tb.class</ipxact:name>
          <ipxact:value>altera_pcie_s10_tbed</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.CRETE_TYPE" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.CRETE_TYPE</ipxact:name>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.apps_type_hwtcl" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.apps_type_hwtcl</ipxact:name>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.bfm_drive_interface_clk_hwtcl" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.bfm_drive_interface_clk_hwtcl</ipxact:name>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.bfm_drive_interface_control_hwtcl" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.bfm_drive_interface_control_hwtcl</ipxact:name>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.bfm_drive_interface_npor_hwtcl" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.bfm_drive_interface_npor_hwtcl</ipxact:name>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.bfm_drive_interface_pipe_hwtcl" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.bfm_drive_interface_pipe_hwtcl</ipxact:name>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.gen123_lane_rate_mode_hwtcl" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.gen123_lane_rate_mode_hwtcl</ipxact:name>
          <ipxact:value>Gen3 (8.0 Gbps)</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.lane_mask_hwtcl" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.lane_mask_hwtcl</ipxact:name>
          <ipxact:value>x1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.pll_refclk_freq_hwtcl" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.pll_refclk_freq_hwtcl</ipxact:name>
          <ipxact:value>100 MHz</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.port_type_hwtcl" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.port_type_hwtcl</ipxact:name>
          <ipxact:value>Root Port</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.select_example_design_sim_BFM_hwtcl" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.select_example_design_sim_BFM_hwtcl</ipxact:name>
          <ipxact:value>Intel FPGA BFM</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.parameter.serial_sim_hwtcl" type="string">
          <ipxact:name>testbench.partner.pcie_tb.parameter.serial_sim_hwtcl</ipxact:name>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="testbench.partner.pcie_tb.version" type="string">
          <ipxact:name>testbench.partner.pcie_tb.version</ipxact:name>
          <ipxact:value>20.0.0</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </altera:altera_assignments>
    <altera:altera_system_parameters>
      <ipxact:parameters>
        <ipxact:parameter parameterId="device" type="string">
          <ipxact:name>device</ipxact:name>
          <ipxact:displayName>Device</ipxact:displayName>
          <ipxact:value>1SM16BEU2F55E2VG</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="deviceFamily" type="string">
          <ipxact:name>deviceFamily</ipxact:name>
          <ipxact:displayName>Device family</ipxact:displayName>
          <ipxact:value>Stratix 10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="deviceSpeedGrade" type="string">
          <ipxact:name>deviceSpeedGrade</ipxact:name>
          <ipxact:displayName>Device Speed Grade</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="generationId" type="int">
          <ipxact:name>generationId</ipxact:name>
          <ipxact:displayName>Generation Id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bonusData" type="string">
          <ipxact:name>bonusData</ipxact:name>
          <ipxact:displayName>bonusData</ipxact:displayName>
          <ipxact:value>bonusData 
{
   element pcie_s10_hip_avmm_bridge_0
   {
      datum _sortIndex
      {
         value = "0";
         type = "int";
      }
   }
}
</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hideFromIPCatalog" type="bit">
          <ipxact:name>hideFromIPCatalog</ipxact:name>
          <ipxact:displayName>Hide from IP Catalog</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="lockedInterfaceDefinition" type="string">
          <ipxact:name>lockedInterfaceDefinition</ipxact:name>
          <ipxact:displayName>lockedInterfaceDefinition</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="systemInfos" type="string">
          <ipxact:name>systemInfos</ipxact:name>
          <ipxact:displayName>systemInfos</ipxact:displayName>
          <ipxact:value>&lt;systemInfosDefinition&gt;
    &lt;connPtSystemInfos&gt;
        &lt;entry&gt;
            &lt;key&gt;coreclkout_hip&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;coreclkout_hip&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos/&gt;
                &lt;consumedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;CLOCK_RATE&lt;/key&gt;
                        &lt;value&gt;125000000&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/consumedSystemInfos&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
        &lt;entry&gt;
            &lt;key&gt;cra&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;cra&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos/&gt;
                &lt;consumedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_MAP&lt;/key&gt;
                        &lt;value&gt;&amp;lt;address-map&amp;gt;&amp;lt;slave name='cra' start='0x0' end='0x8000' datawidth='32' /&amp;gt;&amp;lt;/address-map&amp;gt;&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_WIDTH&lt;/key&gt;
                        &lt;value&gt;15&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;MAX_SLAVE_DATA_WIDTH&lt;/key&gt;
                        &lt;value&gt;32&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/consumedSystemInfos&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
        &lt;entry&gt;
            &lt;key&gt;rxm_bar0&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;rxm_bar0&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_WIDTH&lt;/key&gt;
                    &lt;/entry&gt;
                &lt;/suppliedSystemInfos&gt;
                &lt;consumedSystemInfos/&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
        &lt;entry&gt;
            &lt;key&gt;rxm_bar1&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;rxm_bar1&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_WIDTH&lt;/key&gt;
                    &lt;/entry&gt;
                &lt;/suppliedSystemInfos&gt;
                &lt;consumedSystemInfos/&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
        &lt;entry&gt;
            &lt;key&gt;rxm_bar2&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;rxm_bar2&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_WIDTH&lt;/key&gt;
                    &lt;/entry&gt;
                &lt;/suppliedSystemInfos&gt;
                &lt;consumedSystemInfos/&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
        &lt;entry&gt;
            &lt;key&gt;rxm_bar4&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;rxm_bar4&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_WIDTH&lt;/key&gt;
                    &lt;/entry&gt;
                &lt;/suppliedSystemInfos&gt;
                &lt;consumedSystemInfos/&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
        &lt;entry&gt;
            &lt;key&gt;rxm_irq&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;rxm_irq&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;INTERRUPTS_USED&lt;/key&gt;
                    &lt;/entry&gt;
                &lt;/suppliedSystemInfos&gt;
                &lt;consumedSystemInfos/&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
        &lt;entry&gt;
            &lt;key&gt;txs&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;txs&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos/&gt;
                &lt;consumedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_MAP&lt;/key&gt;
                        &lt;value&gt;&amp;lt;address-map&amp;gt;&amp;lt;slave name='txs' start='0x0' end='0x10000000000000000' datawidth='64' /&amp;gt;&amp;lt;/address-map&amp;gt;&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_WIDTH&lt;/key&gt;
                        &lt;value&gt;64&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;MAX_SLAVE_DATA_WIDTH&lt;/key&gt;
                        &lt;value&gt;64&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/consumedSystemInfos&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
    &lt;/connPtSystemInfos&gt;
&lt;/systemInfosDefinition&gt;</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </altera:altera_system_parameters>
    <altera:altera_interface_boundary>
      <altera:interface_mapping altera:name="app_nreset_status" altera:internal="pcie_s10_hip_avmm_bridge_0.app_nreset_status" altera:type="reset" altera:dir="start">
        <altera:port_mapping altera:name="app_nreset_status" altera:internal="app_nreset_status"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="coreclkout_hip" altera:internal="pcie_s10_hip_avmm_bridge_0.coreclkout_hip" altera:type="clock" altera:dir="start">
        <altera:port_mapping altera:name="coreclkout_hip" altera:internal="coreclkout_hip"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="cra" altera:internal="pcie_s10_hip_avmm_bridge_0.cra" altera:type="avalon" altera:dir="end">
        <altera:port_mapping altera:name="cra_address_i" altera:internal="cra_address_i"></altera:port_mapping>
        <altera:port_mapping altera:name="cra_byteenable_i" altera:internal="cra_byteenable_i"></altera:port_mapping>
        <altera:port_mapping altera:name="cra_chipselect_i" altera:internal="cra_chipselect_i"></altera:port_mapping>
        <altera:port_mapping altera:name="cra_read_i" altera:internal="cra_read_i"></altera:port_mapping>
        <altera:port_mapping altera:name="cra_readdata_o" altera:internal="cra_readdata_o"></altera:port_mapping>
        <altera:port_mapping altera:name="cra_readdatavalid_o" altera:internal="cra_readdatavalid_o"></altera:port_mapping>
        <altera:port_mapping altera:name="cra_waitrequest_o" altera:internal="cra_waitrequest_o"></altera:port_mapping>
        <altera:port_mapping altera:name="cra_write_i" altera:internal="cra_write_i"></altera:port_mapping>
        <altera:port_mapping altera:name="cra_writedata_i" altera:internal="cra_writedata_i"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="cra_irq" altera:internal="pcie_s10_hip_avmm_bridge_0.cra_irq" altera:type="interrupt" altera:dir="end">
        <altera:port_mapping altera:name="cra_irq_o" altera:internal="cra_irq_o"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="hip_ctrl" altera:internal="pcie_s10_hip_avmm_bridge_0.hip_ctrl" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="simu_mode_pipe" altera:internal="simu_mode_pipe"></altera:port_mapping>
        <altera:port_mapping altera:name="test_in" altera:internal="test_in"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="hip_pipe" altera:internal="pcie_s10_hip_avmm_bridge_0.hip_pipe" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="currentcoeff0" altera:internal="currentcoeff0"></altera:port_mapping>
        <altera:port_mapping altera:name="currentrxpreset0" altera:internal="currentrxpreset0"></altera:port_mapping>
        <altera:port_mapping altera:name="dirfeedback0" altera:internal="dirfeedback0"></altera:port_mapping>
        <altera:port_mapping altera:name="invalidreq0" altera:internal="invalidreq0"></altera:port_mapping>
        <altera:port_mapping altera:name="phystatus0" altera:internal="phystatus0"></altera:port_mapping>
        <altera:port_mapping altera:name="powerdown0" altera:internal="powerdown0"></altera:port_mapping>
        <altera:port_mapping altera:name="rate0" altera:internal="rate0"></altera:port_mapping>
        <altera:port_mapping altera:name="rxblkst0" altera:internal="rxblkst0"></altera:port_mapping>
        <altera:port_mapping altera:name="rxdata0" altera:internal="rxdata0"></altera:port_mapping>
        <altera:port_mapping altera:name="rxdatak0" altera:internal="rxdatak0"></altera:port_mapping>
        <altera:port_mapping altera:name="rxdataskip0" altera:internal="rxdataskip0"></altera:port_mapping>
        <altera:port_mapping altera:name="rxelecidle0" altera:internal="rxelecidle0"></altera:port_mapping>
        <altera:port_mapping altera:name="rxeqeval0" altera:internal="rxeqeval0"></altera:port_mapping>
        <altera:port_mapping altera:name="rxeqinprogress0" altera:internal="rxeqinprogress0"></altera:port_mapping>
        <altera:port_mapping altera:name="rxpolarity0" altera:internal="rxpolarity0"></altera:port_mapping>
        <altera:port_mapping altera:name="rxstatus0" altera:internal="rxstatus0"></altera:port_mapping>
        <altera:port_mapping altera:name="rxsynchd0" altera:internal="rxsynchd0"></altera:port_mapping>
        <altera:port_mapping altera:name="rxvalid0" altera:internal="rxvalid0"></altera:port_mapping>
        <altera:port_mapping altera:name="sim_ltssmstate" altera:internal="sim_ltssmstate"></altera:port_mapping>
        <altera:port_mapping altera:name="sim_pipe_mask_tx_pll_lock" altera:internal="sim_pipe_mask_tx_pll_lock"></altera:port_mapping>
        <altera:port_mapping altera:name="sim_pipe_pclk_in" altera:internal="sim_pipe_pclk_in"></altera:port_mapping>
        <altera:port_mapping altera:name="sim_pipe_rate" altera:internal="sim_pipe_rate"></altera:port_mapping>
        <altera:port_mapping altera:name="txblkst0" altera:internal="txblkst0"></altera:port_mapping>
        <altera:port_mapping altera:name="txcompl0" altera:internal="txcompl0"></altera:port_mapping>
        <altera:port_mapping altera:name="txdata0" altera:internal="txdata0"></altera:port_mapping>
        <altera:port_mapping altera:name="txdatak0" altera:internal="txdatak0"></altera:port_mapping>
        <altera:port_mapping altera:name="txdataskip0" altera:internal="txdataskip0"></altera:port_mapping>
        <altera:port_mapping altera:name="txdeemph0" altera:internal="txdeemph0"></altera:port_mapping>
        <altera:port_mapping altera:name="txdetectrx0" altera:internal="txdetectrx0"></altera:port_mapping>
        <altera:port_mapping altera:name="txelecidle0" altera:internal="txelecidle0"></altera:port_mapping>
        <altera:port_mapping altera:name="txmargin0" altera:internal="txmargin0"></altera:port_mapping>
        <altera:port_mapping altera:name="txswing0" altera:internal="txswing0"></altera:port_mapping>
        <altera:port_mapping altera:name="txsynchd0" altera:internal="txsynchd0"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="hip_serial" altera:internal="pcie_s10_hip_avmm_bridge_0.hip_serial" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_in0" altera:internal="rx_in0"></altera:port_mapping>
        <altera:port_mapping altera:name="tx_out0" altera:internal="tx_out0"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="ninit_done" altera:internal="pcie_s10_hip_avmm_bridge_0.ninit_done" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="ninit_done" altera:internal="ninit_done"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="npor" altera:internal="pcie_s10_hip_avmm_bridge_0.npor" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="npor" altera:internal="npor"></altera:port_mapping>
        <altera:port_mapping altera:name="pin_perst" altera:internal="pin_perst"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="refclk" altera:internal="pcie_s10_hip_avmm_bridge_0.refclk" altera:type="clock" altera:dir="end">
        <altera:port_mapping altera:name="refclk" altera:internal="refclk"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rxm_bar0" altera:internal="pcie_s10_hip_avmm_bridge_0.rxm_bar0" altera:type="avalon" altera:dir="start">
        <altera:port_mapping altera:name="rxm_bar0_address_o" altera:internal="rxm_bar0_address_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar0_byteenable_o" altera:internal="rxm_bar0_byteenable_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar0_read_o" altera:internal="rxm_bar0_read_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar0_readdata_i" altera:internal="rxm_bar0_readdata_i"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar0_readdatavalid_i" altera:internal="rxm_bar0_readdatavalid_i"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar0_waitrequest_i" altera:internal="rxm_bar0_waitrequest_i"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar0_write_o" altera:internal="rxm_bar0_write_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar0_writedata_o" altera:internal="rxm_bar0_writedata_o"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rxm_bar1" altera:internal="pcie_s10_hip_avmm_bridge_0.rxm_bar1"></altera:interface_mapping>
      <altera:interface_mapping altera:name="rxm_bar2" altera:internal="pcie_s10_hip_avmm_bridge_0.rxm_bar2" altera:type="avalon" altera:dir="start">
        <altera:port_mapping altera:name="rxm_bar2_address_o" altera:internal="rxm_bar2_address_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar2_burstcount_o" altera:internal="rxm_bar2_burstcount_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar2_byteenable_o" altera:internal="rxm_bar2_byteenable_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar2_read_o" altera:internal="rxm_bar2_read_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar2_readdata_i" altera:internal="rxm_bar2_readdata_i"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar2_readdatavalid_i" altera:internal="rxm_bar2_readdatavalid_i"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar2_waitrequest_i" altera:internal="rxm_bar2_waitrequest_i"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar2_write_o" altera:internal="rxm_bar2_write_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar2_writedata_o" altera:internal="rxm_bar2_writedata_o"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rxm_bar4" altera:internal="pcie_s10_hip_avmm_bridge_0.rxm_bar4" altera:type="avalon" altera:dir="start">
        <altera:port_mapping altera:name="rxm_bar4_address_o" altera:internal="rxm_bar4_address_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar4_burstcount_o" altera:internal="rxm_bar4_burstcount_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar4_byteenable_o" altera:internal="rxm_bar4_byteenable_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar4_read_o" altera:internal="rxm_bar4_read_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar4_readdata_i" altera:internal="rxm_bar4_readdata_i"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar4_readdatavalid_i" altera:internal="rxm_bar4_readdatavalid_i"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar4_waitrequest_i" altera:internal="rxm_bar4_waitrequest_i"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar4_write_o" altera:internal="rxm_bar4_write_o"></altera:port_mapping>
        <altera:port_mapping altera:name="rxm_bar4_writedata_o" altera:internal="rxm_bar4_writedata_o"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rxm_irq" altera:internal="pcie_s10_hip_avmm_bridge_0.rxm_irq" altera:type="interrupt" altera:dir="start">
        <altera:port_mapping altera:name="rxm_irq_i" altera:internal="rxm_irq_i"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="txs" altera:internal="pcie_s10_hip_avmm_bridge_0.txs" altera:type="avalon" altera:dir="end">
        <altera:port_mapping altera:name="txs_address_i" altera:internal="txs_address_i"></altera:port_mapping>
        <altera:port_mapping altera:name="txs_burstcount_i" altera:internal="txs_burstcount_i"></altera:port_mapping>
        <altera:port_mapping altera:name="txs_byteenable_i" altera:internal="txs_byteenable_i"></altera:port_mapping>
        <altera:port_mapping altera:name="txs_chipselect_i" altera:internal="txs_chipselect_i"></altera:port_mapping>
        <altera:port_mapping altera:name="txs_read_i" altera:internal="txs_read_i"></altera:port_mapping>
        <altera:port_mapping altera:name="txs_readdata_o" altera:internal="txs_readdata_o"></altera:port_mapping>
        <altera:port_mapping altera:name="txs_readdatavalid_o" altera:internal="txs_readdatavalid_o"></altera:port_mapping>
        <altera:port_mapping altera:name="txs_waitrequest_o" altera:internal="txs_waitrequest_o"></altera:port_mapping>
        <altera:port_mapping altera:name="txs_write_i" altera:internal="txs_write_i"></altera:port_mapping>
        <altera:port_mapping altera:name="txs_writedata_i" altera:internal="txs_writedata_i"></altera:port_mapping>
      </altera:interface_mapping>
    </altera:altera_interface_boundary>
    <altera:altera_has_warnings>false</altera:altera_has_warnings>
    <altera:altera_has_errors>false</altera:altera_has_errors>
  </ipxact:vendorExtensions>
</ipxact:component>