	component nPhyCV is
		port (
			pll_powerdown      : in  std_logic_vector(4 downto 0)   := (others => 'X'); -- pll_powerdown
			tx_analogreset     : in  std_logic_vector(4 downto 0)   := (others => 'X'); -- tx_analogreset
			tx_digitalreset    : in  std_logic_vector(4 downto 0)   := (others => 'X'); -- tx_digitalreset
			tx_pll_refclk      : in  std_logic_vector(0 downto 0)   := (others => 'X'); -- tx_pll_refclk
			tx_serial_data     : out std_logic_vector(4 downto 0);                      -- tx_serial_data
			pll_locked         : out std_logic_vector(4 downto 0);                      -- pll_locked
			rx_analogreset     : in  std_logic_vector(4 downto 0)   := (others => 'X'); -- rx_analogreset
			rx_digitalreset    : in  std_logic_vector(4 downto 0)   := (others => 'X'); -- rx_digitalreset
			rx_cdr_refclk      : in  std_logic_vector(0 downto 0)   := (others => 'X'); -- rx_cdr_refclk
			rx_serial_data     : in  std_logic_vector(4 downto 0)   := (others => 'X'); -- rx_serial_data
			rx_is_lockedtodata : out std_logic_vector(4 downto 0);                      -- rx_is_lockedtodata
			tx_parallel_data   : in  std_logic_vector(219 downto 0) := (others => 'X'); -- tx_parallel_data
			rx_parallel_data   : out std_logic_vector(319 downto 0);                    -- rx_parallel_data
			tx_std_coreclkin   : in  std_logic_vector(4 downto 0)   := (others => 'X'); -- tx_std_coreclkin
			rx_std_coreclkin   : in  std_logic_vector(4 downto 0)   := (others => 'X'); -- rx_std_coreclkin
			tx_std_clkout      : out std_logic_vector(4 downto 0);                      -- tx_std_clkout
			rx_std_clkout      : out std_logic_vector(4 downto 0);                      -- rx_std_clkout
			tx_cal_busy        : out std_logic_vector(4 downto 0);                      -- tx_cal_busy
			rx_cal_busy        : out std_logic_vector(4 downto 0);                      -- rx_cal_busy
			reconfig_to_xcvr   : in  std_logic_vector(699 downto 0) := (others => 'X'); -- reconfig_to_xcvr
			reconfig_from_xcvr : out std_logic_vector(459 downto 0)                     -- reconfig_from_xcvr
		);
	end component nPhyCV;

