<?xml version="1.0" ?>
<ipxact:component xmlns:altera="http://www.altera.com/XMLSchema/IPXact2014/extensions" xmlns:ipxact="http://www.accellera.org/XMLSchema/IPXACT/1685-2014">
  <ipxact:vendor>Intel Corporation</ipxact:vendor>
  <ipxact:library>alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia</ipxact:library>
  <ipxact:name>alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia</ipxact:name>
  <ipxact:version>19.2.1</ipxact:version>
  <ipxact:busInterfaces>
    <ipxact:busInterface>
      <ipxact:name>tx_analogreset</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>tx_analogreset</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_analogreset</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_analogreset</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_analogreset</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_analogreset</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>tx_digitalreset</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>tx_digitalreset</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_digitalreset</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_digitalreset</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_digitalreset</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_digitalreset</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>tx_analogreset_stat</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>tx_analogreset_stat</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_analogreset_stat</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_analogreset_stat</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_analogreset_stat</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_analogreset_stat</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>tx_digitalreset_stat</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>tx_digitalreset_stat</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_digitalreset_stat</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_digitalreset_stat</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_digitalreset_stat</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_digitalreset_stat</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>tx_cal_busy</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>tx_cal_busy</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_cal_busy</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_cal_busy</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_cal_busy</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_cal_busy</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>tx_serial_clk0</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="hssi_serial_clock" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="hssi_serial_clock" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_serial_clk0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_cdr_refclk0</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="clock" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="clock" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_cdr_refclk0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>tx_serial_data</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>tx_serial_data</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_serial_data</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_serial_data</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_serial_data</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_serial_data</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_seriallpbken</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_seriallpbken</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_seriallpbken</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_is_lockedtodata</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_is_lockedtodata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_is_lockedtodata</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>tx_coreclkin</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="clock" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="clock" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_coreclkin</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_coreclkin</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="clock" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="clock" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_coreclkin</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>tx_clkout</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="clock" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="clock" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_clkout</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:master></ipxact:master>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedDirectClock" type="string">
          <ipxact:name>associatedDirectClock</ipxact:name>
          <ipxact:displayName>Associated direct clock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clockRateKnown" type="bit">
          <ipxact:name>clockRateKnown</ipxact:name>
          <ipxact:displayName>Clock rate known</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_clkout</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="clock" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="clock" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_clkout</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:master></ipxact:master>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedDirectClock" type="string">
          <ipxact:name>associatedDirectClock</ipxact:name>
          <ipxact:displayName>Associated direct clock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clockRateKnown" type="bit">
          <ipxact:name>clockRateKnown</ipxact:name>
          <ipxact:displayName>Clock rate known</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_clkout2</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="clock" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="clock" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_clkout2</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:master></ipxact:master>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedDirectClock" type="string">
          <ipxact:name>associatedDirectClock</ipxact:name>
          <ipxact:displayName>Associated direct clock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clockRateKnown" type="bit">
          <ipxact:name>clockRateKnown</ipxact:name>
          <ipxact:displayName>Clock rate known</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>tx_parallel_data</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>tx_parallel_data</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_parallel_data</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_parallel_data</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_parallel_data</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_parallel_data</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>latency_sclk</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="clock" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="clock" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>latency_sclk</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>tx_fifo_latency_pulse</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>tx_fifo_latency_pulse</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_fifo_latency_pulse</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_fifo_latency_pulse</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_fifo_latency_pulse</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_fifo_latency_pulse</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>tx_pcs_fifo_latency_pulse</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>tx_pcs_fifo_latency_pulse</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>tx_pcs_fifo_latency_pulse</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_pcs_fifo_latency_pulse</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_pcs_fifo_latency_pulse</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_pcs_fifo_latency_pulse</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_enh_highber</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_enh_highber</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_enh_highber</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_enh_highber_clr_cnt</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_enh_highber_clr_cnt</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_enh_highber_clr_cnt</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_enh_clr_errblk_count</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_enh_clr_errblk_count</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_enh_clr_errblk_count</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>rx_enh_blk_lock</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="conduit" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rx_enh_blk_lock</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rx_enh_blk_lock</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>reconfig_clk</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="clock" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="clock" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>reconfig_clk</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>reconfig_reset</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="reset" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="reset" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>reset</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>reconfig_reset</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value>reconfig_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="synchronousEdges" type="string">
          <ipxact:name>synchronousEdges</ipxact:name>
          <ipxact:displayName>Synchronous edges</ipxact:displayName>
          <ipxact:value>DEASSERT</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>reconfig_avmm</ipxact:name>
      <ipxact:busType vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="altera" library="altera" name="avalon" version="19.4"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>write</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>reconfig_write</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>read</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>reconfig_read</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>address</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>reconfig_address</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>writedata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>reconfig_writedata</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>readdata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>reconfig_readdata</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>waitrequest</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>reconfig_waitrequest</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="addressAlignment" type="string">
          <ipxact:name>addressAlignment</ipxact:name>
          <ipxact:displayName>Slave addressing</ipxact:displayName>
          <ipxact:value>DYNAMIC</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressGroup" type="int">
          <ipxact:name>addressGroup</ipxact:name>
          <ipxact:displayName>Address group</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressSpan" type="string">
          <ipxact:name>addressSpan</ipxact:name>
          <ipxact:displayName>Address span</ipxact:displayName>
          <ipxact:value>8192</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressUnits" type="string">
          <ipxact:name>addressUnits</ipxact:name>
          <ipxact:displayName>Address units</ipxact:displayName>
          <ipxact:value>WORDS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="alwaysBurstMaxBurst" type="bit">
          <ipxact:name>alwaysBurstMaxBurst</ipxact:name>
          <ipxact:displayName>Always burst maximum burst</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value>reconfig_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>Associated reset</ipxact:displayName>
          <ipxact:value>reconfig_reset</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bitsPerSymbol" type="int">
          <ipxact:name>bitsPerSymbol</ipxact:name>
          <ipxact:displayName>Bits per symbol</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bridgedAddressOffset" type="string">
          <ipxact:name>bridgedAddressOffset</ipxact:name>
          <ipxact:displayName>Bridged Address Offset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bridgesToMaster" type="string">
          <ipxact:name>bridgesToMaster</ipxact:name>
          <ipxact:displayName>Bridges to master</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstOnBurstBoundariesOnly" type="bit">
          <ipxact:name>burstOnBurstBoundariesOnly</ipxact:name>
          <ipxact:displayName>Burst on burst boundaries only</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="burstcountUnits" type="string">
          <ipxact:name>burstcountUnits</ipxact:name>
          <ipxact:displayName>Burstcount units</ipxact:displayName>
          <ipxact:value>WORDS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="constantBurstBehavior" type="bit">
          <ipxact:name>constantBurstBehavior</ipxact:name>
          <ipxact:displayName>Constant burst behavior</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="explicitAddressSpan" type="string">
          <ipxact:name>explicitAddressSpan</ipxact:name>
          <ipxact:displayName>Explicit address span</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="holdTime" type="int">
          <ipxact:name>holdTime</ipxact:name>
          <ipxact:displayName>Hold</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="interleaveBursts" type="bit">
          <ipxact:name>interleaveBursts</ipxact:name>
          <ipxact:displayName>Interleave bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isBigEndian" type="bit">
          <ipxact:name>isBigEndian</ipxact:name>
          <ipxact:displayName>Big endian</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isFlash" type="bit">
          <ipxact:name>isFlash</ipxact:name>
          <ipxact:displayName>Flash memory</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isMemoryDevice" type="bit">
          <ipxact:name>isMemoryDevice</ipxact:name>
          <ipxact:displayName>Memory device</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isNonVolatileStorage" type="bit">
          <ipxact:name>isNonVolatileStorage</ipxact:name>
          <ipxact:displayName>Non-volatile storage</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="linewrapBursts" type="bit">
          <ipxact:name>linewrapBursts</ipxact:name>
          <ipxact:displayName>Linewrap bursts</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingReadTransactions" type="int">
          <ipxact:name>maximumPendingReadTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending read transactions</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumPendingWriteTransactions" type="int">
          <ipxact:name>maximumPendingWriteTransactions</ipxact:name>
          <ipxact:displayName>Maximum pending write transactions</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumReadLatency" type="int">
          <ipxact:name>minimumReadLatency</ipxact:name>
          <ipxact:displayName>minimumReadLatency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumResponseLatency" type="int">
          <ipxact:name>minimumResponseLatency</ipxact:name>
          <ipxact:displayName>Minimum response latency</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="minimumUninterruptedRunLength" type="int">
          <ipxact:name>minimumUninterruptedRunLength</ipxact:name>
          <ipxact:displayName>Minimum uninterrupted run length</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="printableDevice" type="bit">
          <ipxact:name>printableDevice</ipxact:name>
          <ipxact:displayName>Can receive stdout/stderr</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readLatency" type="int">
          <ipxact:name>readLatency</ipxact:name>
          <ipxact:displayName>Read latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readWaitStates" type="int">
          <ipxact:name>readWaitStates</ipxact:name>
          <ipxact:displayName>Read wait states</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readWaitTime" type="int">
          <ipxact:name>readWaitTime</ipxact:name>
          <ipxact:displayName>Read wait</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerIncomingSignals" type="bit">
          <ipxact:name>registerIncomingSignals</ipxact:name>
          <ipxact:displayName>Register incoming signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="registerOutgoingSignals" type="bit">
          <ipxact:name>registerOutgoingSignals</ipxact:name>
          <ipxact:displayName>Register outgoing signals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="setupTime" type="int">
          <ipxact:name>setupTime</ipxact:name>
          <ipxact:displayName>Setup</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="timingUnits" type="string">
          <ipxact:name>timingUnits</ipxact:name>
          <ipxact:displayName>Timing units</ipxact:displayName>
          <ipxact:value>Cycles</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="transparentBridge" type="bit">
          <ipxact:name>transparentBridge</ipxact:name>
          <ipxact:displayName>Transparent bridge</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="waitrequestAllowance" type="int">
          <ipxact:name>waitrequestAllowance</ipxact:name>
          <ipxact:displayName>Waitrequest allowance</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="wellBehavedWaitrequest" type="bit">
          <ipxact:name>wellBehavedWaitrequest</ipxact:name>
          <ipxact:displayName>Well-behaved waitrequest</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeLatency" type="int">
          <ipxact:name>writeLatency</ipxact:name>
          <ipxact:displayName>Write latency</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeWaitStates" type="int">
          <ipxact:name>writeWaitStates</ipxact:name>
          <ipxact:displayName>Write wait states</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeWaitTime" type="int">
          <ipxact:name>writeWaitTime</ipxact:name>
          <ipxact:displayName>Write wait</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="debug.param.device_revision" type="string">
              <ipxact:name>debug.param.device_revision</ipxact:name>
              <ipxact:value>14nm5bcr2eb</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="debug.typeName" type="string">
              <ipxact:name>debug.typeName</ipxact:name>
              <ipxact:value>altera_xcvr_native.slave</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="embeddedsw.configuration.isFlash" type="string">
              <ipxact:name>embeddedsw.configuration.isFlash</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="embeddedsw.configuration.isMemoryDevice" type="string">
              <ipxact:name>embeddedsw.configuration.isMemoryDevice</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="embeddedsw.configuration.isNonVolatileStorage" type="string">
              <ipxact:name>embeddedsw.configuration.isNonVolatileStorage</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="embeddedsw.configuration.isPrintableDevice" type="string">
              <ipxact:name>embeddedsw.configuration.isPrintableDevice</ipxact:name>
              <ipxact:value>0</ipxact:value>
            </ipxact:parameter>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
  </ipxact:busInterfaces>
  <ipxact:model>
    <ipxact:views>
      <ipxact:view>
        <ipxact:name>QUARTUS_SYNTH</ipxact:name>
        <ipxact:envIdentifier>:quartus.altera.com:</ipxact:envIdentifier>
        <ipxact:componentInstantiationRef>QUARTUS_SYNTH</ipxact:componentInstantiationRef>
      </ipxact:view>
    </ipxact:views>
    <ipxact:instantiations>
      <ipxact:componentInstantiation>
        <ipxact:name>QUARTUS_SYNTH</ipxact:name>
        <ipxact:moduleName>altera_xcvr_native_s10_htile</ipxact:moduleName>
        <ipxact:fileSetRef>
          <ipxact:localName>QUARTUS_SYNTH</ipxact:localName>
        </ipxact:fileSetRef>
      </ipxact:componentInstantiation>
    </ipxact:instantiations>
    <ipxact:ports>
      <ipxact:port>
        <ipxact:name>tx_analogreset</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_analogreset</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_digitalreset</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_digitalreset</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_analogreset_stat</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_analogreset_stat</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_digitalreset_stat</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_digitalreset_stat</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_cal_busy</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_cal_busy</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_serial_clk0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_cdr_refclk0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_serial_data</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_serial_data</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_seriallpbken</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_is_lockedtodata</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_coreclkin</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_coreclkin</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_clkout</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_clkout</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_clkout2</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_parallel_data</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>79</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_parallel_data</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>79</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>latency_sclk</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_fifo_latency_pulse</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_fifo_latency_pulse</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>tx_pcs_fifo_latency_pulse</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_pcs_fifo_latency_pulse</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_enh_highber</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_enh_highber_clr_cnt</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_enh_clr_errblk_count</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rx_enh_blk_lock</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>reconfig_clk</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>reconfig_reset</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>reconfig_write</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>reconfig_read</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>reconfig_address</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>10</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>reconfig_writedata</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>31</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>reconfig_readdata</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>31</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>reconfig_waitrequest</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
    </ipxact:ports>
  </ipxact:model>
  <ipxact:vendorExtensions>
    <altera:entity_info>
      <ipxact:vendor>Intel Corporation</ipxact:vendor>
      <ipxact:library>alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia</ipxact:library>
      <ipxact:name>altera_xcvr_native_s10_htile</ipxact:name>
      <ipxact:version>19.2.1</ipxact:version>
    </altera:entity_info>
    <altera:altera_module_parameters>
      <ipxact:parameters>
        <ipxact:parameter parameterId="rcfg_debug" type="int">
          <ipxact:name>rcfg_debug</ipxact:name>
          <ipxact:displayName>rcfg_debug</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_multi_profile" type="int">
          <ipxact:name>enable_multi_profile</ipxact:name>
          <ipxact:displayName>enable_multi_profile</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_enable" type="int">
          <ipxact:name>rcfg_enable</ipxact:name>
          <ipxact:displayName>Enable dynamic reconfiguration</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_advanced_avmm_options" type="int">
          <ipxact:name>enable_advanced_avmm_options</ipxact:name>
          <ipxact:displayName>enable_advanced_avmm_options</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_jtag_enable" type="int">
          <ipxact:name>rcfg_jtag_enable</ipxact:name>
          <ipxact:displayName>Enable Native PHY Debug Master Endpoint</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_separate_avmm_busy" type="int">
          <ipxact:name>rcfg_separate_avmm_busy</ipxact:name>
          <ipxact:displayName>Separate reconfig_waitrequest from the status of AVMM arbitration with PreSICE</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_enable_avmm_busy_port" type="int">
          <ipxact:name>rcfg_enable_avmm_busy_port</ipxact:name>
          <ipxact:displayName>Enable avmm_busy port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_capability_reg_enable" type="int">
          <ipxact:name>set_capability_reg_enable</ipxact:name>
          <ipxact:displayName>Enable capability registers</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_user_identifier" type="int">
          <ipxact:name>set_user_identifier</ipxact:name>
          <ipxact:displayName>Set user-defined IP identifier</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_csr_soft_logic_enable" type="int">
          <ipxact:name>set_csr_soft_logic_enable</ipxact:name>
          <ipxact:displayName>Enable control and status registers</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dbg_embedded_debug_enable" type="int">
          <ipxact:name>dbg_embedded_debug_enable</ipxact:name>
          <ipxact:displayName>dbg_embedded_debug_enable</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dbg_capability_reg_enable" type="int">
          <ipxact:name>dbg_capability_reg_enable</ipxact:name>
          <ipxact:displayName>dbg_capability_reg_enable</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dbg_user_identifier" type="int">
          <ipxact:name>dbg_user_identifier</ipxact:name>
          <ipxact:displayName>dbg_user_identifier</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dbg_stat_soft_logic_enable" type="int">
          <ipxact:name>dbg_stat_soft_logic_enable</ipxact:name>
          <ipxact:displayName>dbg_stat_soft_logic_enable</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dbg_ctrl_soft_logic_enable" type="int">
          <ipxact:name>dbg_ctrl_soft_logic_enable</ipxact:name>
          <ipxact:displayName>dbg_ctrl_soft_logic_enable</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_file_prefix" type="string">
          <ipxact:name>rcfg_file_prefix</ipxact:name>
          <ipxact:displayName>Configuration file prefix</ipxact:displayName>
          <ipxact:value>alt_mge_phy</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_files_as_common_package" type="int">
          <ipxact:name>rcfg_files_as_common_package</ipxact:name>
          <ipxact:displayName>Declare SystemVerilog package file as common package file</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sv_file_enable" type="int">
          <ipxact:name>rcfg_sv_file_enable</ipxact:name>
          <ipxact:displayName>Generate SystemVerilog package file</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_h_file_enable" type="int">
          <ipxact:name>rcfg_h_file_enable</ipxact:name>
          <ipxact:displayName>Generate C header file</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_txt_file_enable" type="int">
          <ipxact:name>rcfg_txt_file_enable</ipxact:name>
          <ipxact:displayName>Generate text file</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_mif_file_enable" type="int">
          <ipxact:name>rcfg_mif_file_enable</ipxact:name>
          <ipxact:displayName>Generate MIF (Memory Initialize File)</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_multi_enable" type="int">
          <ipxact:name>rcfg_multi_enable</ipxact:name>
          <ipxact:displayName>Enable multiple reconfiguration profiles</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_rcfg_emb_strm_enable" type="int">
          <ipxact:name>set_rcfg_emb_strm_enable</ipxact:name>
          <ipxact:displayName>Enable embedded reconfiguration streamer</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_emb_strm_enable" type="int">
          <ipxact:name>rcfg_emb_strm_enable</ipxact:name>
          <ipxact:displayName>rcfg_emb_strm_enable</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_reduced_files_enable" type="int">
          <ipxact:name>rcfg_reduced_files_enable</ipxact:name>
          <ipxact:displayName>Generate reduced reconfiguration files</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_profile_cnt" type="int">
          <ipxact:name>rcfg_profile_cnt</ipxact:name>
          <ipxact:displayName>Number of reconfiguration profiles</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_profile_select" type="int">
          <ipxact:name>rcfg_profile_select</ipxact:name>
          <ipxact:displayName>Store current configuration to profile:</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_profile_data0" type="string">
          <ipxact:name>rcfg_profile_data0</ipxact:name>
          <ipxact:displayName>rcfg_profile_data0</ipxact:displayName>
          <ipxact:value>rcfg_debug 0 rcfg_enable 1 rcfg_jtag_enable 0 rcfg_separate_avmm_busy 0 rcfg_enable_avmm_busy_port 0 set_capability_reg_enable 0 set_user_identifier 0 set_csr_soft_logic_enable 0 support_mode user_mode channel_type GX protocol_mode teng_1588_mode pma_mode basic duplex_mode duplex channels 1 set_data_rate 10312.5 rcfg_iface_enable 0 enable_simple_interface 0 enable_split_interface 0 set_enable_calibration 1 enable_double_rate_transfer 0 enable_direct_reset_control 0 disable_reset_sequencer 0 disable_digital_reset_sequencer 0 enable_ehip 0 avmm_ehip_mode disable_hip adapter_ehip_mode disable_hip bonded_mode not_bonded set_pcs_bonding_master Auto pcs_reset_sequencing_mode not_bonded manual_pcs_bonding_mode individual manual_pcs_bonding_comp_cnt 0 manual_tx_hssi_aib_bonding_mode individual manual_tx_hssi_aib_bonding_comp_cnt 0 manual_tx_core_aib_bonding_mode individual manual_tx_core_aib_bonding_comp_cnt 0 manual_rx_hssi_aib_bonding_mode individual manual_rx_hssi_aib_bonding_comp_cnt 0 manual_rx_core_aib_bonding_mode individual manual_rx_core_aib_bonding_comp_cnt 0 manual_tx_hssi_aib_indv indv_en manual_tx_core_aib_indv indv_en manual_rx_hssi_aib_indv indv_en manual_rx_core_aib_indv indv_en tx_pma_clk_div 1 plls 1 pll_select 0 enable_port_tx_pma_iqtxrx_clkout 0 enable_port_tx_pma_elecidle 0 number_physical_bonding_clocks 1 enable_qpi_mode 0 enable_qpi_async_transfer 1 enable_port_tx_pma_qpipullup 0 enable_port_tx_pma_qpipulldn 0 enable_port_tx_pma_rxfound 0 enable_port_rx_pma_qpipulldn 0 enable_port_tx_pma_txdetectrx 0 cdr_refclk_cnt 1 cdr_refclk_select 0 set_cdr_refclk_freq 644.53125 rx_ppm_detect_threshold 100 enable_port_rx_pma_iqtxrx_clkout 0 enable_port_rx_pma_clkslip 0 enable_port_rx_is_lockedtodata 1 enable_port_rx_is_lockedtoref 0 enable_ports_rx_manual_cdr_mode 0 enable_ports_rx_prbs 0 enable_port_rx_seriallpbken 1 std_pcs_pma_width 10 std_low_latency_bypass_enable 0 enable_hip 0 enable_hard_reset 0 set_hip_cal_en 0 hip_mode disable_hip hip_prot_mode gen1 hip_channels x1 std_tx_byte_ser_mode Disabled std_rx_byte_deser_mode Disabled std_tx_8b10b_enable 1 std_tx_8b10b_disp_ctrl_enable 0 std_rx_8b10b_enable 1 std_rx_rmfifo_mode disabled std_rx_rmfifo_pattern_n 0 std_rx_rmfifo_pattern_p 0 enable_port_rx_std_rmfifo_full 0 enable_port_rx_std_rmfifo_empty 0 pcie_rate_match Bypass std_tx_bitslip_enable 0 enable_port_tx_std_bitslipboundarysel 0 std_rx_word_aligner_mode {synchronous state machine} std_rx_word_aligner_pattern_len 10 std_rx_word_aligner_pattern 0 std_rx_word_aligner_rknumber 3 std_rx_word_aligner_renumber 3 std_rx_word_aligner_rgnumber 3 std_rx_word_aligner_fast_sync_status_enable 0 enable_port_rx_std_wa_patternalign 0 enable_port_rx_std_wa_a1a2size 0 enable_port_rx_std_bitslipboundarysel 1 enable_port_rx_std_bitslip 0 std_tx_bitrev_enable 0 std_tx_byterev_enable 0 std_tx_polinv_enable 0 enable_port_tx_polinv 0 std_rx_bitrev_enable 0 enable_port_rx_std_bitrev_ena 0 std_rx_byterev_enable 0 enable_port_rx_std_byterev_ena 0 std_rx_polinv_enable 0 enable_port_rx_polinv 0 enable_port_rx_std_signaldetect 0 enable_ports_pipe_sw 0 enable_ports_pipe_rx_elecidle 0 enable_ports_pipe_hclk 0 enh_pcs_pma_width 32 enh_pld_pcs_width 66 enh_low_latency_enable 0 enh_advanced_user_mode 0 enh_tx_frmgen_enable 0 enh_tx_frmgen_mfrm_length 2048 enh_tx_frmgen_burst_enable 0 enable_port_tx_enh_frame 0 enable_port_tx_enh_frame_diag_status 0 enable_port_tx_enh_frame_burst_en 0 enh_rx_frmsync_enable 0 enh_rx_frmsync_mfrm_length 2048 enable_port_rx_enh_frame 0 enable_port_rx_enh_frame_lock 0 enable_port_rx_enh_frame_diag_status 0 enh_tx_crcgen_enable 0 enh_tx_crcerr_enable 0 enh_rx_crcchk_enable 0 enable_port_rx_enh_crc32_err 0 enable_port_rx_enh_highber 1 enable_port_rx_enh_highber_clr_cnt 1 enable_port_rx_enh_clr_errblk_count 1 enh_tx_64b66b_enable 1 enh_rx_64b66b_enable 1 enh_tx_sh_err 0 enh_tx_scram_enable 1 enh_tx_scram_seed 288230376151711743 enh_rx_descram_enable 1 enh_tx_dispgen_enable 0 enh_rx_dispchk_enable 0 enh_tx_randomdispbit_enable 0 enh_rx_blksync_enable 1 enable_port_rx_enh_blk_lock 1 enh_tx_bitslip_enable 0 enh_tx_polinv_enable 0 enh_rx_bitslip_enable 0 enh_rx_polinv_enable 0 enable_port_tx_enh_bitslip 0 enable_port_rx_enh_bitslip 0 enh_rx_krfec_err_mark_enable 0 enh_rx_krfec_err_mark_type 10G enh_tx_krfec_burst_err_enable 0 enh_tx_krfec_burst_err_len 1 enable_port_krfec_tx_enh_frame 0 enable_port_krfec_rx_enh_frame 0 enable_port_krfec_rx_enh_frame_diag_status 0 pcs_direct_width 8 enable_tx_fast_pipeln_reg 0 enable_rx_fast_pipeln_reg 0 parallel_loopback_mode disable loopback_tx_clk_sel internal_clk enable_debug_ports 0 tx_fifo_mode {Phase compensation} tx_fifo_pfull 10 tx_fifo_pempty 2 enable_port_tx_fifo_full 0 enable_port_tx_fifo_empty 0 enable_port_tx_fifo_pfull 0 enable_port_tx_fifo_pempty 0 enable_port_tx_pcs_fifo_full 0 enable_port_tx_pcs_fifo_empty 0 enable_port_tx_dll_lock 0 rx_fifo_mode {Phase compensation} rx_fifo_pfull 10 rx_fifo_pempty 2 rx_fifo_align_del 0 rx_fifo_control_del 0 enable_port_rx_data_valid 1 enable_port_rx_fifo_full 0 enable_port_rx_fifo_empty 0 enable_port_rx_fifo_pfull 0 enable_port_rx_fifo_pempty 0 enable_port_rx_fifo_del 0 enable_port_rx_fifo_insert 0 enable_port_rx_fifo_rd_en 0 enable_port_rx_fifo_align_clr 0 enable_port_rx_pcs_fifo_full 0 enable_port_rx_pcs_fifo_empty 0 tx_clkout_sel pcs_clkout enable_port_tx_clkout2 0 tx_clkout2_sel pcs_clkout enable_port_tx_clkout_hioint 0 enable_port_tx_clkout2_hioint 0 tx_pma_div_clkout_divider 33 tx_coreclkin_clock_network dedicated tx_pcs_bonding_clock_network dedicated rx_clkout_sel pcs_clkout enable_port_rx_clkout2 1 rx_clkout2_sel pma_div_clkout enable_port_rx_clkout_hioint 0 enable_port_rx_clkout2_hioint 0 rx_pma_div_clkout_divider 33 rx_coreclkin_clock_network dedicated osc_clk_divider 1 enable_port_tx_fifo_latency_adj_ena 0 enable_port_rx_fifo_latency_adj_ena 0 enable_port_latency_measurement 1 enable_port_clock_delay_measurement 0 delay_measurement_clkout_sel clock_delay_measurement_clkout delay_measurement_clkout2_sel clock_delay_measurement_clkout set_prbs_soft_logic_enable 0 enable_rcfg_tx_digitalreset_release_ctrl 0 anlg_voltage 1_0V anlg_link sr tx_pma_analog_mode user_custom tx_pma_optimal_settings 1 tx_pma_output_swing_ctrl 12 tx_pma_pre_emp_sign_pre_tap_1t negative tx_pma_pre_emp_switching_ctrl_pre_tap_1t 0 tx_pma_pre_emp_sign_1st_post_tap negative tx_pma_pre_emp_switching_ctrl_1st_post_tap 0 tx_pma_slew_rate_ctrl 0 tx_pma_term_sel r_r1 tx_pma_compensation_en enable rx_pma_adapt_mode manual rx_pma_term_sel r_r1 rx_ctle_ac_gain 0 rx_ctle_eq_gain 0 rx_vga_dc_gain 0 enable_ports_adaptation 0 rx_pma_analog_mode user_custom  ovrd_tx_dv_mode 0 ovrd_rx_dv_mode 0 usr_tx_dv_mode enable usr_rx_dv_mode enable enable_background_cal_gui 0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_profile_data1" type="string">
          <ipxact:name>rcfg_profile_data1</ipxact:name>
          <ipxact:displayName>rcfg_profile_data1</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_profile_data2" type="string">
          <ipxact:name>rcfg_profile_data2</ipxact:name>
          <ipxact:displayName>rcfg_profile_data2</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_profile_data3" type="string">
          <ipxact:name>rcfg_profile_data3</ipxact:name>
          <ipxact:displayName>rcfg_profile_data3</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_profile_data4" type="string">
          <ipxact:name>rcfg_profile_data4</ipxact:name>
          <ipxact:displayName>rcfg_profile_data4</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_profile_data5" type="string">
          <ipxact:name>rcfg_profile_data5</ipxact:name>
          <ipxact:displayName>rcfg_profile_data5</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_profile_data6" type="string">
          <ipxact:name>rcfg_profile_data6</ipxact:name>
          <ipxact:displayName>rcfg_profile_data6</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_profile_data7" type="string">
          <ipxact:name>rcfg_profile_data7</ipxact:name>
          <ipxact:displayName>rcfg_profile_data7</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_profile_data0" type="string">
          <ipxact:name>rcfg_sdc_derived_profile_data0</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_profile_data0</ipxact:displayName>
          <ipxact:value>enable_multi_profile 1 disable_digital_reset_sequencer 0 dbg_embedded_debug_enable 0 dbg_capability_reg_enable 0 dbg_user_identifier 0 dbg_stat_soft_logic_enable 0 dbg_ctrl_soft_logic_enable 0 l_tx_transfer_clk_hz 515625000 l_rx_transfer_clk_hz 515625000 enable_background_cal 0 disable_reset_sequencer 0 l_tx_fifo_transfer_mode x2 l_rx_fifo_transfer_mode x2 l_num_tx_digitalreset 1 l_num_rx_digitalreset 1 l_enable_channel_bonding 0 l_enable_pma_bonding 0 l_enable_pcs_bonding 0 l_tx_hssi_aib_indv indv_en l_tx_core_aib_indv indv_en l_rx_hssi_aib_indv indv_en l_rx_core_aib_indv indv_en display_std_tx_pld_adapt_width 8 display_std_rx_pld_adapt_width 8 datapath_select Enhanced</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_profile_data1" type="string">
          <ipxact:name>rcfg_sdc_derived_profile_data1</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_profile_data1</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_profile_data2" type="string">
          <ipxact:name>rcfg_sdc_derived_profile_data2</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_profile_data2</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_profile_data3" type="string">
          <ipxact:name>rcfg_sdc_derived_profile_data3</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_profile_data3</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_profile_data4" type="string">
          <ipxact:name>rcfg_sdc_derived_profile_data4</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_profile_data4</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_profile_data5" type="string">
          <ipxact:name>rcfg_sdc_derived_profile_data5</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_profile_data5</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_profile_data6" type="string">
          <ipxact:name>rcfg_sdc_derived_profile_data6</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_profile_data6</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_profile_data7" type="string">
          <ipxact:name>rcfg_sdc_derived_profile_data7</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_profile_data7</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_params" type="string">
          <ipxact:name>rcfg_params</ipxact:name>
          <ipxact:displayName>rcfg_params</ipxact:displayName>
          <ipxact:value>rcfg_debug,rcfg_enable,rcfg_jtag_enable,rcfg_separate_avmm_busy,rcfg_enable_avmm_busy_port,set_capability_reg_enable,set_user_identifier,set_csr_soft_logic_enable,support_mode,channel_type,protocol_mode,pma_mode,duplex_mode,channels,set_data_rate,rcfg_iface_enable,enable_simple_interface,enable_split_interface,set_enable_calibration,enable_double_rate_transfer,enable_background_cal_gui,enable_direct_reset_control,disable_reset_sequencer,disable_digital_reset_sequencer,bonded_mode,set_pcs_bonding_master,pcs_reset_sequencing_mode,manual_pcs_bonding_mode,manual_pcs_bonding_comp_cnt,manual_tx_hssi_aib_bonding_mode,manual_tx_hssi_aib_bonding_comp_cnt,manual_tx_core_aib_bonding_mode,manual_tx_core_aib_bonding_comp_cnt,manual_rx_hssi_aib_bonding_mode,manual_rx_hssi_aib_bonding_comp_cnt,manual_rx_core_aib_bonding_mode,manual_rx_core_aib_bonding_comp_cnt,manual_tx_hssi_aib_indv,manual_tx_core_aib_indv,manual_rx_hssi_aib_indv,manual_rx_core_aib_indv,tx_pma_clk_div,plls,pll_select,enable_port_tx_pma_iqtxrx_clkout,enable_port_tx_pma_elecidle,number_physical_bonding_clocks,enable_qpi_mode,enable_qpi_async_transfer,enable_port_tx_pma_qpipullup,enable_port_tx_pma_qpipulldn,enable_port_tx_pma_rxfound,enable_port_rx_pma_qpipulldn,enable_port_tx_pma_txdetectrx,cdr_refclk_cnt,cdr_refclk_select,set_cdr_refclk_freq,rx_ppm_detect_threshold,enable_port_rx_pma_iqtxrx_clkout,enable_port_rx_pma_clkslip,enable_port_rx_is_lockedtodata,enable_port_rx_is_lockedtoref,enable_ports_rx_manual_cdr_mode,enable_ports_rx_prbs,enable_port_rx_seriallpbken,std_pcs_pma_width,std_low_latency_bypass_enable,enable_hip,enable_hard_reset,set_hip_cal_en,hip_mode,hip_prot_mode,hip_channels,enable_ehip,avmm_ehip_mode,adapter_ehip_mode,std_tx_byte_ser_mode,std_rx_byte_deser_mode,std_tx_8b10b_enable,std_tx_8b10b_disp_ctrl_enable,std_rx_8b10b_enable,std_rx_rmfifo_mode,std_rx_rmfifo_pattern_n,std_rx_rmfifo_pattern_p,enable_port_rx_std_rmfifo_full,enable_port_rx_std_rmfifo_empty,pcie_rate_match,std_tx_bitslip_enable,enable_port_tx_std_bitslipboundarysel,std_rx_word_aligner_mode,std_rx_word_aligner_pattern_len,std_rx_word_aligner_pattern,std_rx_word_aligner_rknumber,std_rx_word_aligner_renumber,std_rx_word_aligner_rgnumber,std_rx_word_aligner_fast_sync_status_enable,enable_port_rx_std_wa_patternalign,enable_port_rx_std_wa_a1a2size,enable_port_rx_std_bitslipboundarysel,enable_port_rx_std_bitslip,std_tx_bitrev_enable,std_tx_byterev_enable,std_tx_polinv_enable,enable_port_tx_polinv,std_rx_bitrev_enable,enable_port_rx_std_bitrev_ena,std_rx_byterev_enable,enable_port_rx_std_byterev_ena,std_rx_polinv_enable,enable_port_rx_polinv,enable_port_rx_std_signaldetect,enable_ports_pipe_sw,enable_ports_pipe_rx_elecidle,enable_ports_pipe_hclk,enh_pcs_pma_width,enh_pld_pcs_width,enh_low_latency_enable,enh_advanced_user_mode,enh_tx_frmgen_enable,enh_tx_frmgen_mfrm_length,enh_tx_frmgen_burst_enable,enable_port_tx_enh_frame,enable_port_tx_enh_frame_diag_status,enable_port_tx_enh_frame_burst_en,enh_rx_frmsync_enable,enh_rx_frmsync_mfrm_length,enable_port_rx_enh_frame,enable_port_rx_enh_frame_lock,enable_port_rx_enh_frame_diag_status,enh_tx_crcgen_enable,enh_tx_crcerr_enable,enh_rx_crcchk_enable,enable_port_rx_enh_crc32_err,enable_port_rx_enh_highber,enable_port_rx_enh_highber_clr_cnt,enable_port_rx_enh_clr_errblk_count,enh_tx_64b66b_enable,enh_rx_64b66b_enable,enh_tx_sh_err,enh_tx_scram_enable,enh_tx_scram_seed,enh_rx_descram_enable,enh_tx_dispgen_enable,enh_rx_dispchk_enable,enh_tx_randomdispbit_enable,enh_rx_blksync_enable,enable_port_rx_enh_blk_lock,enh_tx_bitslip_enable,enh_tx_polinv_enable,enh_rx_bitslip_enable,enh_rx_polinv_enable,enable_port_tx_enh_bitslip,enable_port_rx_enh_bitslip,enh_rx_krfec_err_mark_enable,enh_rx_krfec_err_mark_type,enh_tx_krfec_burst_err_enable,enh_tx_krfec_burst_err_len,enable_port_krfec_tx_enh_frame,enable_port_krfec_rx_enh_frame,enable_port_krfec_rx_enh_frame_diag_status,pcs_direct_width,enable_tx_fast_pipeln_reg,enable_rx_fast_pipeln_reg,parallel_loopback_mode,loopback_tx_clk_sel,enable_debug_ports,tx_fifo_mode,tx_fifo_pfull,tx_fifo_pempty,enable_port_tx_fifo_full,enable_port_tx_fifo_empty,enable_port_tx_fifo_pfull,enable_port_tx_fifo_pempty,enable_port_tx_pcs_fifo_full,enable_port_tx_pcs_fifo_empty,enable_port_tx_dll_lock,rx_fifo_mode,rx_fifo_pfull,rx_fifo_pempty,rx_fifo_align_del,rx_fifo_control_del,enable_port_rx_data_valid,enable_port_rx_fifo_full,enable_port_rx_fifo_empty,enable_port_rx_fifo_pfull,enable_port_rx_fifo_pempty,enable_port_rx_fifo_del,enable_port_rx_fifo_insert,enable_port_rx_fifo_rd_en,enable_port_rx_fifo_align_clr,enable_port_rx_pcs_fifo_full,enable_port_rx_pcs_fifo_empty,tx_clkout_sel,enable_port_tx_clkout2,tx_clkout2_sel,enable_port_tx_clkout_hioint,enable_port_tx_clkout2_hioint,tx_pma_div_clkout_divider,tx_coreclkin_clock_network,tx_pcs_bonding_clock_network,rx_clkout_sel,enable_port_rx_clkout2,rx_clkout2_sel,enable_port_rx_clkout_hioint,enable_port_rx_clkout2_hioint,rx_pma_div_clkout_divider,rx_coreclkin_clock_network,osc_clk_divider,enable_port_tx_fifo_latency_adj_ena,enable_port_rx_fifo_latency_adj_ena,enable_port_latency_measurement,enable_port_clock_delay_measurement,delay_measurement_clkout_sel,delay_measurement_clkout2_sel,ovrd_tx_dv_mode,usr_tx_dv_mode,ovrd_rx_dv_mode,usr_rx_dv_mode,set_prbs_soft_logic_enable,enable_rcfg_tx_digitalreset_release_ctrl,anlg_voltage,anlg_link,enable_ports_adaptation,tx_pma_analog_mode,rx_pma_analog_mode,tx_pma_optimal_settings,tx_pma_output_swing_ctrl,tx_pma_pre_emp_sign_pre_tap_1t,tx_pma_pre_emp_switching_ctrl_pre_tap_1t,tx_pma_pre_emp_sign_1st_post_tap,tx_pma_pre_emp_switching_ctrl_1st_post_tap,tx_pma_slew_rate_ctrl,tx_pma_term_sel,tx_pma_compensation_en,rx_pma_adapt_mode,rx_pma_term_sel,rx_ctle_ac_gain,rx_ctle_eq_gain,rx_vga_dc_gain</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_param_labels" type="string">
          <ipxact:name>rcfg_param_labels</ipxact:name>
          <ipxact:displayName>IP Parameters</ipxact:displayName>
          <ipxact:value>rcfg_debug,Enable dynamic reconfiguration,Enable Native PHY Debug Master Endpoint,Separate reconfig_waitrequest from the status of AVMM arbitration with PreSICE,Enable avmm_busy port,Enable capability registers,Set user-defined IP identifier,Enable control and status registers,Protocol support mode,Transceiver channel type,Transceiver configuration rules,PMA configuration rules,Transceiver mode,Number of data channels,Data rate,Enable datapath and interface reconfiguration,Enable simplified data interface,Provide separate interface for each channel,Enable calibration,Enable double rate transfer mode,Enable background calibration,Enable direct reset control,Disable reset sequencer,Disable digital reset sequencer,TX channel bonding mode,PCS TX channel bonding master,PCS reset sequence,PCS TX channel bonding mode,PCS TX bonding compensation counter,TX HSSI AIB bonding mode,TX HSSI AIB compensation counter,TX Core AIB bonding mode,TX Core AIB compensation counter,RX HSSI AIB bonding mode,RX HSSI AIB compensation counter,RX Core AIB bonding mode,RX Core AIB compensation counter,TX HSSI AIB sychronous bonding setting,TX Core AIB sychronous bonding setting,RX HSSI AIB sychronous bonding setting,RX Core AIB sychronous bonding setting,TX local clock division factor,Number of TX PLL clock inputs per channel,Initial TX PLL clock input selection,Enable tx_pma_iqtxrx_clkout port,Enable tx_pma_elecidle port,Number of physical bonding clock ports to use.,Enable QPI mode,Use asynchronous QPI signals,Enable tx_pma_qpipullup port,Enable tx_pma_qpipulldn port,Enable tx_pma_rxfound port,Enable rx_pma_qpipulldn port,Enable tx_pma_txdetectrx port,Number of CDR reference clocks,Selected CDR reference clock,Selected CDR reference clock frequency,PPM detector threshold,Enable rx_pma_iqtxrx_clkout port,Enable rx_pma_clkslip port,Enable rx_is_lockedtodata port,Enable rx_is_lockedtoref port,Enable rx_set_locktodata and rx_set_locktoref ports,Enable PRBS verifier control and status ports,Enable rx_seriallpbken port,Standard PCS / PMA interface width,Enable 'Standard PCS' low latency mode,Enable PCIe hard IP support,Enable hard reset controller (HIP),Enable PCIe hard IP calibration,PCIe channel HIP mode,PCIe HIP protocol mode,Number of PCIe HIP channels,Enable Ethernet Hard IP Support,Ethernet channel AVMM HIP mode,Ethernet channel Adapter HIP mode,TX byte serializer mode,RX byte deserializer mode,Enable TX 8B/10B encoder,Enable TX 8B/10B disparity control,Enable RX 8B/10B decoder,RX rate match FIFO mode,RX rate match insert/delete -ve pattern (hex),RX rate match insert/delete +ve pattern (hex),Enable rx_std_rmfifo_full port,Enable rx_std_rmfifo_empty port,PCI Express Gen 3 rate match FIFO mode,Enable TX bitslip,Enable tx_std_bitslipboundarysel port,RX word aligner mode,RX word aligner pattern length,RX word aligner pattern (hex),Number of word alignment patterns to achieve sync,Number of invalid data words to lose sync,Number of valid data words to decrement error count,Enable fast sync status reporting for deterministic latency SM,Enable rx_std_wa_patternalign port,Enable rx_std_wa_a1a2size port,Enable rx_std_bitslipboundarysel port,Enable rx_bitslip port,Enable TX bit reversal,Enable TX byte reversal,Enable TX polarity inversion,Enable tx_polinv port,Enable RX bit reversal,Enable rx_std_bitrev_ena port,Enable RX byte reversal,Enable rx_std_byterev_ena port,Enable RX polarity inversion,Enable rx_polinv port,Enable rx_std_signaldetect port,Enable PCIe dynamic datarate switch ports,Enable PCIe electrical idle control and status ports,Enable PCIe pipe_hclk_in and pipe_hclk_out ports,Enhanced PCS / PMA interface width,FPGA fabric / Enhanced PCS interface width,Enable 'Enhanced PCS' low latency mode,Enable 'Enhanced PCS' advanced user mode,Enable Interlaken frame generator,Frame generator metaframe length,Enable frame generator burst control,Enable tx_enh_frame port,Enable tx_enh_frame_diag_status port,Enable tx_enh_frame_burst_en port,Enable Interlaken frame synchronizer,Frame synchronizer metaframe length,Enable rx_enh_frame port,Enable rx_enh_frame_lock port,Enable rx_enh_frame_diag_status port,Enable Interlaken TX CRC-32 generator,Enable Interlaken TX CRC-32 generator error insertion,Enable Interlaken RX CRC-32 checker,Enable rx_enh_crc32_err port,Enable rx_enh_highber port (10GBASE-R),Enable rx_enh_highber_clr_cnt port (10GBASE-R),Enable rx_enh_clr_errblk_count port (10GBASE-R &amp; FEC),Enable TX 64b/66b encoder,Enable RX 64b/66b decoder,Enable TX sync header error insertion,Enable TX scrambler (10GBASE-R/Interlaken),TX scrambler seed (10GBASE-R/Interlaken),Enable RX descrambler (10GBASE-R/Interlaken),Enable Interlaken TX disparity generator,Enable Interlaken RX disparity checker,Enable Interlaken TX random disparity bit,Enable RX block synchronizer,Enable rx_enh_blk_lock port,Enable TX data bitslip,Enable TX data polarity inversion,Enable RX data bitslip,Enable RX data polarity inversion,Enable tx_enh_bitslip port,Enable rx_bitslip port,Enable RX KR-FEC error marking,Error marking type,Enable KR-FEC TX error insertion,KR-FEC TX error insertion spacing,Enable tx_enh_frame port,Enable rx_enh_frame port,Enable rx_enh_frame_diag_status port,PCS Direct interface width,Enable TX fast pipeline registers,Enable RX fast pipeline registers,Parallel loopback mode,Parallel loopback mode TX clock source selection,Enable PCS reset status ports,TX Core Interface FIFO mode,TX FIFO partially full threshold,TX FIFO partially empty threshold,Enable tx_fifo_full port,Enable tx_fifo_empty port,Enable tx_fifo_pfull port,Enable tx_fifo_pempty port,Enable tx_pcs_fifo_full port,Enable tx_pcs_fifo_empty port,Enable tx_dll_lock port,RX PCS-Core Interface FIFO mode (PCS FIFO-Core FIFO),RX FIFO partially full threshold,RX FIFO partially empty threshold,Enable RX FIFO alignment word deletion (Interlaken),Enable RX FIFO control word deletion (Interlaken),Enable rx_data_valid port,Enable rx_fifo_full port,Enable rx_fifo_empty port,Enable rx_fifo_pfull port,Enable rx_fifo_pempty port,Enable rx_fifo_del port (10GBASE-R),Enable rx_fifo_insert port (10GBASE-R),Enable rx_fifo_rd_en port,Enable rx_fifo_align_clr port (Interlaken),Enable rx_pcs_fifo_full port,Enable rx_pcs_fifo_empty port,Selected tx_clkout clock source,Enable tx_clkout2 port,Selected tx_clkout2 clock source,Enable tx_clkout_hioint port,Enable tx_clkout2_hioint port,TX pma_div_clkout division factor,Selected tx_coreclkin clock network,Selected TX PCS bonding clock network,Selected rx_clkout clock source,Enable rx_clkout2 port,Selected rx_clkout2 clock source,Enable rx_clkout_hioint port,Enable rx_clkout2_hioint port,RX pma_div_clkout division factor,Selected rx_coreclkin clock network,OSC clock division factor,Enable TX FIFO latency adjustment port,Enable RX FIFO latency adjustment port,Enable latency measurement ports,Enable clock delay measurement ports,Selected delay_measurement_clkout clock source,Selected delay_measurement_clkout2 clock source,Enable TX Data Valid Gen manual setting,Generate TX Data Valid by Core AIB FIFO,Enable RX Data Valid Rcv manual setting,Consume RX Data Valid by Core AIB FIFO,Enable prbs soft accumulators,Enable rcfg_tx_digitalreset_release_ctrl port,VCCR_GXB and VCCT_GXB supply voltage for the Transceiver,Tranceiver Link Type,Enable adaptation control ports,TX PMA analog mode rules,RX PMA analog mode rules,Use default TX PMA analog settings,Output Swing Level (VOD),Pre-Emphasis First Pre-Tap Polarity,Pre-Emphasis First Pre-Tap Magnitude,Pre-Emphasis First Post-Tap Polarity,Pre-Emphasis First Post-Tap Magnitude,Slew Rate Control,On-Chip Termination,High Speed Compensation,RX adaptation mode,RX On-chip Termination,CTLE AC Gain,CTLE EQ Gain,VGA DC Gain</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_param_vals0" type="string">
          <ipxact:name>rcfg_param_vals0</ipxact:name>
          <ipxact:displayName>Profile 0</ipxact:displayName>
          <ipxact:value>0,1,0,0,0,0,0,0,user_mode,GX,teng_1588_mode,basic,duplex,1,10312.5,0,0,0,1,0,0,0,0,0,not_bonded,Auto,not_bonded,individual,0,individual,0,individual,0,individual,0,individual,0,indv_en,indv_en,indv_en,indv_en,1,1,0,0,0,1,0,1,0,0,0,0,0,1,0,644.53125,100,0,0,1,0,0,0,1,10,0,0,0,0,disable_hip,gen1,x1,0,disable_hip,disable_hip,Disabled,Disabled,1,0,1,disabled,0,0,0,0,Bypass,0,0,synchronous state machine,10,0,3,3,3,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,32,66,0,0,0,2048,0,0,0,0,0,2048,0,0,0,0,0,0,0,1,1,1,1,1,0,1,288230376151711743,1,0,0,0,1,1,0,0,0,0,0,0,0,10G,0,1,0,0,0,8,0,0,disable,internal_clk,0,Phase compensation,10,2,0,0,0,0,0,0,0,Phase compensation,10,2,0,0,1,0,0,0,0,0,0,0,0,0,0,pcs_clkout,0,pcs_clkout,0,0,33,dedicated,dedicated,pcs_clkout,1,pma_div_clkout,0,0,33,dedicated,1,0,0,1,0,clock_delay_measurement_clkout,clock_delay_measurement_clkout,0,enable,0,enable,0,0,1_0V,sr,0,user_custom,user_custom,1,12,negative,0,negative,0,0,r_r1,enable,manual,r_r1,0,0,0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_param_vals1" type="string">
          <ipxact:name>rcfg_param_vals1</ipxact:name>
          <ipxact:displayName>Profile 1</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_param_vals2" type="string">
          <ipxact:name>rcfg_param_vals2</ipxact:name>
          <ipxact:displayName>Profile 2</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_param_vals3" type="string">
          <ipxact:name>rcfg_param_vals3</ipxact:name>
          <ipxact:displayName>Profile 3</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_param_vals4" type="string">
          <ipxact:name>rcfg_param_vals4</ipxact:name>
          <ipxact:displayName>Profile 4</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_param_vals5" type="string">
          <ipxact:name>rcfg_param_vals5</ipxact:name>
          <ipxact:displayName>Profile 5</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_param_vals6" type="string">
          <ipxact:name>rcfg_param_vals6</ipxact:name>
          <ipxact:displayName>Profile 6</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_param_vals7" type="string">
          <ipxact:name>rcfg_param_vals7</ipxact:name>
          <ipxact:displayName>Profile 7</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_params" type="string">
          <ipxact:name>rcfg_sdc_derived_params</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_params</ipxact:displayName>
          <ipxact:value>enable_multi_profile,dbg_embedded_debug_enable,dbg_capability_reg_enable,dbg_user_identifier,dbg_stat_soft_logic_enable,dbg_ctrl_soft_logic_enable,l_tx_transfer_clk_hz,l_rx_transfer_clk_hz,enable_background_cal,l_tx_fifo_transfer_mode,l_rx_fifo_transfer_mode,l_num_tx_digitalreset,l_num_rx_digitalreset,l_enable_channel_bonding,l_enable_pma_bonding,l_enable_pcs_bonding,l_tx_hssi_aib_indv,l_tx_core_aib_indv,l_rx_hssi_aib_indv,l_rx_core_aib_indv,display_std_tx_pld_adapt_width,display_std_rx_pld_adapt_width,datapath_select</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_param_vals0" type="string">
          <ipxact:name>rcfg_sdc_derived_param_vals0</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_param_vals0</ipxact:displayName>
          <ipxact:value>1,0,0,0,0,0,515625000,515625000,0,x2,x2,1,1,0,0,0,indv_en,indv_en,indv_en,indv_en,8,8,Enhanced</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_param_vals1" type="string">
          <ipxact:name>rcfg_sdc_derived_param_vals1</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_param_vals1</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_param_vals2" type="string">
          <ipxact:name>rcfg_sdc_derived_param_vals2</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_param_vals2</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_param_vals3" type="string">
          <ipxact:name>rcfg_sdc_derived_param_vals3</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_param_vals3</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_param_vals4" type="string">
          <ipxact:name>rcfg_sdc_derived_param_vals4</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_param_vals4</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_param_vals5" type="string">
          <ipxact:name>rcfg_sdc_derived_param_vals5</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_param_vals5</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_param_vals6" type="string">
          <ipxact:name>rcfg_sdc_derived_param_vals6</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_param_vals6</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_sdc_derived_param_vals7" type="string">
          <ipxact:name>rcfg_sdc_derived_param_vals7</ipxact:name>
          <ipxact:displayName>rcfg_sdc_derived_param_vals7</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device_family" type="string">
          <ipxact:name>device_family</ipxact:name>
          <ipxact:displayName>device_family</ipxact:displayName>
          <ipxact:value>Stratix 10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device" type="string">
          <ipxact:name>device</ipxact:name>
          <ipxact:displayName>device</ipxact:displayName>
          <ipxact:value>1SG165HU2F50E2VG</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="base_device" type="string">
          <ipxact:name>base_device</ipxact:name>
          <ipxact:displayName>base_device</ipxact:displayName>
          <ipxact:value>Unknown</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device_die_types" type="string">
          <ipxact:name>device_die_types</ipxact:name>
          <ipxact:displayName>device_die_types</ipxact:displayName>
          <ipxact:value>HSSI_CRETE2E,MAIN_ND5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device_die_revisions" type="string">
          <ipxact:name>device_die_revisions</ipxact:name>
          <ipxact:displayName>device_die_revisions</ipxact:displayName>
          <ipxact:value>HSSI_CRETE2E_REVB,MAIN_ND5_REVC</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="design_environment" type="string">
          <ipxact:name>design_environment</ipxact:name>
          <ipxact:displayName>design_environment</ipxact:displayName>
          <ipxact:value>QSYS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device_revision" type="string">
          <ipxact:name>device_revision</ipxact:name>
          <ipxact:displayName>device_revision</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="silicon_revision" type="string">
          <ipxact:name>silicon_revision</ipxact:name>
          <ipxact:displayName>silicon_revision</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_tile_type" type="string">
          <ipxact:name>l_tile_type</ipxact:name>
          <ipxact:displayName>l_tile_type</ipxact:displayName>
          <ipxact:value>htile</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="message_level" type="string">
          <ipxact:name>message_level</ipxact:name>
          <ipxact:displayName>Message level for rule violations</ipxact:displayName>
          <ipxact:value>error</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="reduced_reset_sim_time" type="int">
          <ipxact:name>reduced_reset_sim_time</ipxact:name>
          <ipxact:displayName>Use fast reset for simulation</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="support_mode" type="string">
          <ipxact:name>support_mode</ipxact:name>
          <ipxact:displayName>Protocol support mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="channel_type" type="string">
          <ipxact:name>channel_type</ipxact:name>
          <ipxact:displayName>Transceiver channel type</ipxact:displayName>
          <ipxact:value>GX</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="protocol_mode" type="string">
          <ipxact:name>protocol_mode</ipxact:name>
          <ipxact:displayName>Transceiver configuration rules</ipxact:displayName>
          <ipxact:value>teng_1588_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_protocol_mode" type="string">
          <ipxact:name>l_protocol_mode</ipxact:name>
          <ipxact:displayName>l_protocol_mode</ipxact:displayName>
          <ipxact:value>teng_1588_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_mode" type="string">
          <ipxact:name>pma_mode</ipxact:name>
          <ipxact:displayName>PMA configuration rules</ipxact:displayName>
          <ipxact:value>basic</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="duplex_mode" type="string">
          <ipxact:name>duplex_mode</ipxact:name>
          <ipxact:displayName>Transceiver mode</ipxact:displayName>
          <ipxact:value>duplex</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="channels" type="int">
          <ipxact:name>channels</ipxact:name>
          <ipxact:displayName>Number of data channels</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_data_rate" type="string">
          <ipxact:name>set_data_rate</ipxact:name>
          <ipxact:displayName>Data rate</ipxact:displayName>
          <ipxact:value>10312.5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="data_rate_bps" type="string">
          <ipxact:name>data_rate_bps</ipxact:name>
          <ipxact:displayName>data_rate_bps</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_tx_transfer_clk_hz" type="int">
          <ipxact:name>l_tx_transfer_clk_hz</ipxact:name>
          <ipxact:displayName>l_tx_transfer_clk_hz</ipxact:displayName>
          <ipxact:value>644531250</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_rx_transfer_clk_hz" type="int">
          <ipxact:name>l_rx_transfer_clk_hz</ipxact:name>
          <ipxact:displayName>l_rx_transfer_clk_hz</ipxact:displayName>
          <ipxact:value>644531250</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="core_speedgrade" type="string">
          <ipxact:name>core_speedgrade</ipxact:name>
          <ipxact:displayName>core_speedgrade</ipxact:displayName>
          <ipxact:value>e2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="xcvr_speedgrade" type="string">
          <ipxact:name>xcvr_speedgrade</ipxact:name>
          <ipxact:displayName>xcvr_speedgrade</ipxact:displayName>
          <ipxact:value>e2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pcs_speedgrade" type="string">
          <ipxact:name>pcs_speedgrade</ipxact:name>
          <ipxact:displayName>pcs_speedgrade</ipxact:displayName>
          <ipxact:value>e2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="core_speedgrade_no_temp" type="string">
          <ipxact:name>core_speedgrade_no_temp</ipxact:name>
          <ipxact:displayName>core_speedgrade_no_temp</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="xcvr_speedgrade_no_temp" type="string">
          <ipxact:name>xcvr_speedgrade_no_temp</ipxact:name>
          <ipxact:displayName>xcvr_speedgrade_no_temp</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_iface_enable" type="int">
          <ipxact:name>rcfg_iface_enable</ipxact:name>
          <ipxact:displayName>Enable datapath and interface reconfiguration</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_simple_interface" type="int">
          <ipxact:name>enable_simple_interface</ipxact:name>
          <ipxact:displayName>Enable simplified data interface</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_split_interface" type="int">
          <ipxact:name>enable_split_interface</ipxact:name>
          <ipxact:displayName>Provide separate interface for each channel</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_enable_calibration" type="int">
          <ipxact:name>set_enable_calibration</ipxact:name>
          <ipxact:displayName>Enable calibration</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_calibration" type="int">
          <ipxact:name>enable_calibration</ipxact:name>
          <ipxact:displayName>enable_calibration</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_channel_powerdown" type="int">
          <ipxact:name>enable_channel_powerdown</ipxact:name>
          <ipxact:displayName>Enable PMA/PCS powerdown support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_transparent_pcs" type="int">
          <ipxact:name>enable_transparent_pcs</ipxact:name>
          <ipxact:displayName>Enable transparent PCS</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_double_rate_transfer" type="int">
          <ipxact:name>enable_double_rate_transfer</ipxact:name>
          <ipxact:displayName>Enable double rate transfer mode</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_background_cal_gui" type="int">
          <ipxact:name>enable_background_cal_gui</ipxact:name>
          <ipxact:displayName>Enable background calibration</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_background_cal" type="int">
          <ipxact:name>enable_background_cal</ipxact:name>
          <ipxact:displayName>Enable background calibration</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_enable_eios_rx_protect" type="int">
          <ipxact:name>set_enable_eios_rx_protect</ipxact:name>
          <ipxact:displayName>Enable PIPE EIOS RX Protection</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_eios_rx_protect" type="int">
          <ipxact:name>enable_eios_rx_protect</ipxact:name>
          <ipxact:displayName>Enable PIPE EIOS RX Protection</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_direct_reset_control" type="int">
          <ipxact:name>enable_direct_reset_control</ipxact:name>
          <ipxact:displayName>Enable direct reset control</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="disable_reset_sequencer" type="int">
          <ipxact:name>disable_reset_sequencer</ipxact:name>
          <ipxact:displayName>Disable reset sequencer</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="disable_digital_reset_sequencer" type="int">
          <ipxact:name>disable_digital_reset_sequencer</ipxact:name>
          <ipxact:displayName>Disable digital reset sequencer</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_pma_channel" type="int">
          <ipxact:name>l_enable_pma_channel</ipxact:name>
          <ipxact:displayName>l_enable_pma_channel</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_pcs_channel" type="int">
          <ipxact:name>l_enable_pcs_channel</ipxact:name>
          <ipxact:displayName>l_enable_pcs_channel</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_frequency_rules" type="int">
          <ipxact:name>l_enable_frequency_rules</ipxact:name>
          <ipxact:displayName>l_enable_frequency_rules</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_tx_fifo_transfer_mode" type="string">
          <ipxact:name>l_tx_fifo_transfer_mode</ipxact:name>
          <ipxact:displayName>TX PCS-Core Interface FIFO transfer mode</ipxact:displayName>
          <ipxact:value>x2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_rx_fifo_transfer_mode" type="string">
          <ipxact:name>l_rx_fifo_transfer_mode</ipxact:name>
          <ipxact:displayName>RX PCS-Core Interface FIFO transfer mode</ipxact:displayName>
          <ipxact:value>x2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_num_tx_digitalreset" type="int">
          <ipxact:name>l_num_tx_digitalreset</ipxact:name>
          <ipxact:displayName>Number of TX digital resets</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_num_rx_digitalreset" type="int">
          <ipxact:name>l_num_rx_digitalreset</ipxact:name>
          <ipxact:displayName>Number of RX digital resets</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_release_aib_reset_first" type="int">
          <ipxact:name>l_release_aib_reset_first</ipxact:name>
          <ipxact:displayName>l_release_aib_reset_first</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bonded_mode" type="string">
          <ipxact:name>bonded_mode</ipxact:name>
          <ipxact:displayName>TX channel bonding mode</ipxact:displayName>
          <ipxact:value>not_bonded</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_channel_bonding" type="int">
          <ipxact:name>l_enable_channel_bonding</ipxact:name>
          <ipxact:displayName>l_enable_channel_bonding</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_pma_bonding" type="int">
          <ipxact:name>l_enable_pma_bonding</ipxact:name>
          <ipxact:displayName>l_enable_pma_bonding</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_pcs_bonding" type="int">
          <ipxact:name>l_enable_pcs_bonding</ipxact:name>
          <ipxact:displayName>l_enable_pcs_bonding</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_pcs_bonding_master" type="string">
          <ipxact:name>set_pcs_bonding_master</ipxact:name>
          <ipxact:displayName>PCS TX channel bonding master</ipxact:displayName>
          <ipxact:value>Auto</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pcs_bonding_master" type="int">
          <ipxact:name>pcs_bonding_master</ipxact:name>
          <ipxact:displayName>Actual PCS TX channel bonding master</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pcs_reset_sequencing_mode" type="string">
          <ipxact:name>pcs_reset_sequencing_mode</ipxact:name>
          <ipxact:displayName>PCS reset sequence</ipxact:displayName>
          <ipxact:value>not_bonded</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_manual_bonding_settings" type="int">
          <ipxact:name>enable_manual_bonding_settings</ipxact:name>
          <ipxact:displayName>Enable manual PCS bonding settings</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_pcs_bonding_mode" type="string">
          <ipxact:name>manual_pcs_bonding_mode</ipxact:name>
          <ipxact:displayName>PCS TX channel bonding mode</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_pcs_bonding_comp_cnt" type="int">
          <ipxact:name>manual_pcs_bonding_comp_cnt</ipxact:name>
          <ipxact:displayName>PCS TX bonding compensation counter</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_tx_hssi_aib_bonding_mode" type="string">
          <ipxact:name>manual_tx_hssi_aib_bonding_mode</ipxact:name>
          <ipxact:displayName>TX HSSI AIB bonding mode</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_tx_hssi_aib_bonding_comp_cnt" type="int">
          <ipxact:name>manual_tx_hssi_aib_bonding_comp_cnt</ipxact:name>
          <ipxact:displayName>TX HSSI AIB compensation counter</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_tx_core_aib_bonding_mode" type="string">
          <ipxact:name>manual_tx_core_aib_bonding_mode</ipxact:name>
          <ipxact:displayName>TX Core AIB bonding mode</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_tx_core_aib_bonding_comp_cnt" type="int">
          <ipxact:name>manual_tx_core_aib_bonding_comp_cnt</ipxact:name>
          <ipxact:displayName>TX Core AIB compensation counter</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_rx_hssi_aib_bonding_mode" type="string">
          <ipxact:name>manual_rx_hssi_aib_bonding_mode</ipxact:name>
          <ipxact:displayName>RX HSSI AIB bonding mode</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_rx_hssi_aib_bonding_comp_cnt" type="int">
          <ipxact:name>manual_rx_hssi_aib_bonding_comp_cnt</ipxact:name>
          <ipxact:displayName>RX HSSI AIB compensation counter</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_rx_core_aib_bonding_mode" type="string">
          <ipxact:name>manual_rx_core_aib_bonding_mode</ipxact:name>
          <ipxact:displayName>RX Core AIB bonding mode</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_rx_core_aib_bonding_comp_cnt" type="int">
          <ipxact:name>manual_rx_core_aib_bonding_comp_cnt</ipxact:name>
          <ipxact:displayName>RX Core AIB compensation counter</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_tx_hssi_aib_indv" type="string">
          <ipxact:name>manual_tx_hssi_aib_indv</ipxact:name>
          <ipxact:displayName>TX HSSI AIB sychronous bonding setting</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_tx_core_aib_indv" type="string">
          <ipxact:name>manual_tx_core_aib_indv</ipxact:name>
          <ipxact:displayName>TX Core AIB sychronous bonding setting</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_rx_hssi_aib_indv" type="string">
          <ipxact:name>manual_rx_hssi_aib_indv</ipxact:name>
          <ipxact:displayName>RX HSSI AIB sychronous bonding setting</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="manual_rx_core_aib_indv" type="string">
          <ipxact:name>manual_rx_core_aib_indv</ipxact:name>
          <ipxact:displayName>RX Core AIB sychronous bonding setting</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_tx_hssi_aib_indv" type="string">
          <ipxact:name>l_tx_hssi_aib_indv</ipxact:name>
          <ipxact:displayName>l_tx_hssi_aib_indv</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_tx_core_aib_indv" type="string">
          <ipxact:name>l_tx_core_aib_indv</ipxact:name>
          <ipxact:displayName>l_tx_core_aib_indv</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_rx_hssi_aib_indv" type="string">
          <ipxact:name>l_rx_hssi_aib_indv</ipxact:name>
          <ipxact:displayName>l_rx_hssi_aib_indv</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_rx_core_aib_indv" type="string">
          <ipxact:name>l_rx_core_aib_indv</ipxact:name>
          <ipxact:displayName>l_rx_core_aib_indv</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_clk_div" type="int">
          <ipxact:name>tx_pma_clk_div</ipxact:name>
          <ipxact:displayName>TX local clock division factor</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="plls" type="int">
          <ipxact:name>plls</ipxact:name>
          <ipxact:displayName>Number of TX PLL clock inputs per channel</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pll_select" type="int">
          <ipxact:name>pll_select</ipxact:name>
          <ipxact:displayName>Initial TX PLL clock input selection</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_pma_iqtxrx_clkout" type="int">
          <ipxact:name>enable_port_tx_pma_iqtxrx_clkout</ipxact:name>
          <ipxact:displayName>Enable tx_pma_iqtxrx_clkout port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_pma_elecidle" type="int">
          <ipxact:name>enable_port_tx_pma_elecidle</ipxact:name>
          <ipxact:displayName>Enable tx_pma_elecidle port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="number_physical_bonding_clocks" type="int">
          <ipxact:name>number_physical_bonding_clocks</ipxact:name>
          <ipxact:displayName>Number of physical bonding clock ports to use.</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_qpi_mode" type="int">
          <ipxact:name>enable_qpi_mode</ipxact:name>
          <ipxact:displayName>Enable QPI mode</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_qpi_async_transfer" type="int">
          <ipxact:name>enable_qpi_async_transfer</ipxact:name>
          <ipxact:displayName>Use asynchronous QPI signals</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_pma_qpipullup" type="int">
          <ipxact:name>enable_port_tx_pma_qpipullup</ipxact:name>
          <ipxact:displayName>Enable tx_pma_qpipullup port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_pma_qpipulldn" type="int">
          <ipxact:name>enable_port_tx_pma_qpipulldn</ipxact:name>
          <ipxact:displayName>Enable tx_pma_qpipulldn port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_pma_rxfound" type="int">
          <ipxact:name>enable_port_tx_pma_rxfound</ipxact:name>
          <ipxact:displayName>Enable tx_pma_rxfound port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_pma_qpipulldn" type="int">
          <ipxact:name>enable_port_rx_pma_qpipulldn</ipxact:name>
          <ipxact:displayName>Enable rx_pma_qpipulldn port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_pma_txdetectrx" type="int">
          <ipxact:name>enable_port_tx_pma_txdetectrx</ipxact:name>
          <ipxact:displayName>Enable tx_pma_txdetectrx port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_refclk_cnt" type="int">
          <ipxact:name>cdr_refclk_cnt</ipxact:name>
          <ipxact:displayName>Number of CDR reference clocks</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_refclk_select" type="int">
          <ipxact:name>cdr_refclk_select</ipxact:name>
          <ipxact:displayName>Selected CDR reference clock</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_cdr_refclk_freq" type="string">
          <ipxact:name>set_cdr_refclk_freq</ipxact:name>
          <ipxact:displayName>Selected CDR reference clock frequency</ipxact:displayName>
          <ipxact:value>644.53125</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_ppm_detect_threshold" type="string">
          <ipxact:name>rx_ppm_detect_threshold</ipxact:name>
          <ipxact:displayName>PPM detector threshold</ipxact:displayName>
          <ipxact:value>100</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_cdr_refclk_receiver_detect_src" type="string">
          <ipxact:name>set_cdr_refclk_receiver_detect_src</ipxact:name>
          <ipxact:displayName>set_cdr_refclk_receiver_detect_src</ipxact:displayName>
          <ipxact:value>iqclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_pma_iqtxrx_clkout" type="int">
          <ipxact:name>enable_port_rx_pma_iqtxrx_clkout</ipxact:name>
          <ipxact:displayName>Enable rx_pma_iqtxrx_clkout port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_pma_clkslip" type="int">
          <ipxact:name>enable_port_rx_pma_clkslip</ipxact:name>
          <ipxact:displayName>Enable rx_pma_clkslip port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_is_lockedtodata" type="int">
          <ipxact:name>enable_port_rx_is_lockedtodata</ipxact:name>
          <ipxact:displayName>Enable rx_is_lockedtodata port</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_is_lockedtoref" type="int">
          <ipxact:name>enable_port_rx_is_lockedtoref</ipxact:name>
          <ipxact:displayName>Enable rx_is_lockedtoref port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_ports_rx_manual_cdr_mode" type="int">
          <ipxact:name>enable_ports_rx_manual_cdr_mode</ipxact:name>
          <ipxact:displayName>Enable rx_set_locktodata and rx_set_locktoref ports</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_ports_rx_prbs" type="int">
          <ipxact:name>enable_ports_rx_prbs</ipxact:name>
          <ipxact:displayName>Enable PRBS verifier control and status ports</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_seriallpbken" type="int">
          <ipxact:name>enable_port_rx_seriallpbken</ipxact:name>
          <ipxact:displayName>Enable rx_seriallpbken port</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_pcs_pma_width" type="int">
          <ipxact:name>std_pcs_pma_width</ipxact:name>
          <ipxact:displayName>Standard PCS / PMA interface width</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="display_std_tx_pld_adapt_width" type="int">
          <ipxact:name>display_std_tx_pld_adapt_width</ipxact:name>
          <ipxact:displayName>FPGA fabric / Standard TX PCS interface width</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="display_std_rx_pld_adapt_width" type="int">
          <ipxact:name>display_std_rx_pld_adapt_width</ipxact:name>
          <ipxact:displayName>FPGA fabric / Standard RX PCS interface width</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_low_latency_bypass_enable" type="int">
          <ipxact:name>std_low_latency_bypass_enable</ipxact:name>
          <ipxact:displayName>Enable 'Standard PCS' low latency mode</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_hip" type="int">
          <ipxact:name>enable_hip</ipxact:name>
          <ipxact:displayName>Enable PCIe hard IP support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_pcs_channel_hip_en" type="int">
          <ipxact:name>l_pcs_channel_hip_en</ipxact:name>
          <ipxact:displayName>l_pcs_channel_hip_en</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_hard_reset" type="int">
          <ipxact:name>enable_hard_reset</ipxact:name>
          <ipxact:displayName>Enable hard reset controller (HIP)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_pcs_channel_enable_hard_reset" type="int">
          <ipxact:name>l_pcs_channel_enable_hard_reset</ipxact:name>
          <ipxact:displayName>l_pcs_channel_enable_hard_reset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_hip_cal_en" type="int">
          <ipxact:name>set_hip_cal_en</ipxact:name>
          <ipxact:displayName>Enable PCIe hard IP calibration</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hip_cal_en" type="string">
          <ipxact:name>hip_cal_en</ipxact:name>
          <ipxact:displayName>hip_cal_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hip_mode" type="string">
          <ipxact:name>hip_mode</ipxact:name>
          <ipxact:displayName>PCIe channel HIP mode</ipxact:displayName>
          <ipxact:value>disable_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hip_prot_mode" type="string">
          <ipxact:name>hip_prot_mode</ipxact:name>
          <ipxact:displayName>PCIe HIP protocol mode</ipxact:displayName>
          <ipxact:value>gen1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hip_channels" type="string">
          <ipxact:name>hip_channels</ipxact:name>
          <ipxact:displayName>Number of PCIe HIP channels</ipxact:displayName>
          <ipxact:value>x1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_ehip" type="int">
          <ipxact:name>enable_ehip</ipxact:name>
          <ipxact:displayName>Enable Ethernet Hard IP Support</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="avmm_ehip_mode" type="string">
          <ipxact:name>avmm_ehip_mode</ipxact:name>
          <ipxact:displayName>Ethernet channel AVMM HIP mode</ipxact:displayName>
          <ipxact:value>disable_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="adapter_ehip_mode" type="string">
          <ipxact:name>adapter_ehip_mode</ipxact:name>
          <ipxact:displayName>Ethernet channel Adapter HIP mode</ipxact:displayName>
          <ipxact:value>disable_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_tx_byte_ser_mode" type="string">
          <ipxact:name>std_tx_byte_ser_mode</ipxact:name>
          <ipxact:displayName>TX byte serializer mode</ipxact:displayName>
          <ipxact:value>Disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_byte_deser_mode" type="string">
          <ipxact:name>std_rx_byte_deser_mode</ipxact:name>
          <ipxact:displayName>RX byte deserializer mode</ipxact:displayName>
          <ipxact:value>Disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_tx_8b10b_enable" type="int">
          <ipxact:name>std_tx_8b10b_enable</ipxact:name>
          <ipxact:displayName>Enable TX 8B/10B encoder</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_tx_8b10b_disp_ctrl_enable" type="int">
          <ipxact:name>std_tx_8b10b_disp_ctrl_enable</ipxact:name>
          <ipxact:displayName>Enable TX 8B/10B disparity control</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_8b10b_enable" type="int">
          <ipxact:name>std_rx_8b10b_enable</ipxact:name>
          <ipxact:displayName>Enable RX 8B/10B decoder</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_rmfifo_mode" type="string">
          <ipxact:name>std_rx_rmfifo_mode</ipxact:name>
          <ipxact:displayName>RX rate match FIFO mode</ipxact:displayName>
          <ipxact:value>disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_rmfifo_pattern_n" type="int">
          <ipxact:name>std_rx_rmfifo_pattern_n</ipxact:name>
          <ipxact:displayName>RX rate match insert/delete -ve pattern (hex)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_rmfifo_pattern_p" type="int">
          <ipxact:name>std_rx_rmfifo_pattern_p</ipxact:name>
          <ipxact:displayName>RX rate match insert/delete +ve pattern (hex)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_std_rmfifo_full" type="int">
          <ipxact:name>enable_port_rx_std_rmfifo_full</ipxact:name>
          <ipxact:displayName>Enable rx_std_rmfifo_full port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_std_rmfifo_empty" type="int">
          <ipxact:name>enable_port_rx_std_rmfifo_empty</ipxact:name>
          <ipxact:displayName>Enable rx_std_rmfifo_empty port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pcie_rate_match" type="string">
          <ipxact:name>pcie_rate_match</ipxact:name>
          <ipxact:displayName>PCI Express Gen 3 rate match FIFO mode</ipxact:displayName>
          <ipxact:value>Bypass</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_tx_bitslip_enable" type="int">
          <ipxact:name>std_tx_bitslip_enable</ipxact:name>
          <ipxact:displayName>Enable TX bitslip</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_std_bitslipboundarysel" type="int">
          <ipxact:name>enable_port_tx_std_bitslipboundarysel</ipxact:name>
          <ipxact:displayName>Enable tx_std_bitslipboundarysel port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_word_aligner_mode" type="string">
          <ipxact:name>std_rx_word_aligner_mode</ipxact:name>
          <ipxact:displayName>RX word aligner mode</ipxact:displayName>
          <ipxact:value>synchronous state machine</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_word_aligner_pattern_len" type="int">
          <ipxact:name>std_rx_word_aligner_pattern_len</ipxact:name>
          <ipxact:displayName>RX word aligner pattern length</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_word_aligner_pattern" type="longint">
          <ipxact:name>std_rx_word_aligner_pattern</ipxact:name>
          <ipxact:displayName>RX word aligner pattern (hex)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_word_aligner_rknumber" type="int">
          <ipxact:name>std_rx_word_aligner_rknumber</ipxact:name>
          <ipxact:displayName>Number of word alignment patterns to achieve sync</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_word_aligner_renumber" type="int">
          <ipxact:name>std_rx_word_aligner_renumber</ipxact:name>
          <ipxact:displayName>Number of invalid data words to lose sync</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_word_aligner_rgnumber" type="int">
          <ipxact:name>std_rx_word_aligner_rgnumber</ipxact:name>
          <ipxact:displayName>Number of valid data words to decrement error count</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_word_aligner_rvnumber" type="int">
          <ipxact:name>std_rx_word_aligner_rvnumber</ipxact:name>
          <ipxact:displayName>Number of valid data patterns required to achieve word alignment</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_word_aligner_fast_sync_status_enable" type="int">
          <ipxact:name>std_rx_word_aligner_fast_sync_status_enable</ipxact:name>
          <ipxact:displayName>Enable fast sync status reporting for deterministic latency SM</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_std_wa_patternalign" type="int">
          <ipxact:name>enable_port_rx_std_wa_patternalign</ipxact:name>
          <ipxact:displayName>Enable rx_std_wa_patternalign port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_std_wa_a1a2size" type="int">
          <ipxact:name>enable_port_rx_std_wa_a1a2size</ipxact:name>
          <ipxact:displayName>Enable rx_std_wa_a1a2size port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_std_bitslipboundarysel" type="int">
          <ipxact:name>enable_port_rx_std_bitslipboundarysel</ipxact:name>
          <ipxact:displayName>Enable rx_std_bitslipboundarysel port</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_std_bitslip" type="int">
          <ipxact:name>enable_port_rx_std_bitslip</ipxact:name>
          <ipxact:displayName>Enable rx_bitslip port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_tx_bitrev_enable" type="int">
          <ipxact:name>std_tx_bitrev_enable</ipxact:name>
          <ipxact:displayName>Enable TX bit reversal</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_tx_byterev_enable" type="int">
          <ipxact:name>std_tx_byterev_enable</ipxact:name>
          <ipxact:displayName>Enable TX byte reversal</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_tx_polinv_enable" type="int">
          <ipxact:name>std_tx_polinv_enable</ipxact:name>
          <ipxact:displayName>Enable TX polarity inversion</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_polinv" type="int">
          <ipxact:name>enable_port_tx_polinv</ipxact:name>
          <ipxact:displayName>Enable tx_polinv port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_bitrev_enable" type="int">
          <ipxact:name>std_rx_bitrev_enable</ipxact:name>
          <ipxact:displayName>Enable RX bit reversal</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_std_bitrev_ena" type="int">
          <ipxact:name>enable_port_rx_std_bitrev_ena</ipxact:name>
          <ipxact:displayName>Enable rx_std_bitrev_ena port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_byterev_enable" type="int">
          <ipxact:name>std_rx_byterev_enable</ipxact:name>
          <ipxact:displayName>Enable RX byte reversal</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_std_byterev_ena" type="int">
          <ipxact:name>enable_port_rx_std_byterev_ena</ipxact:name>
          <ipxact:displayName>Enable rx_std_byterev_ena port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="std_rx_polinv_enable" type="int">
          <ipxact:name>std_rx_polinv_enable</ipxact:name>
          <ipxact:displayName>Enable RX polarity inversion</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_polinv" type="int">
          <ipxact:name>enable_port_rx_polinv</ipxact:name>
          <ipxact:displayName>Enable rx_polinv port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_std_signaldetect" type="int">
          <ipxact:name>enable_port_rx_std_signaldetect</ipxact:name>
          <ipxact:displayName>Enable rx_std_signaldetect port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_ports_pipe_sw" type="int">
          <ipxact:name>enable_ports_pipe_sw</ipxact:name>
          <ipxact:displayName>Enable PCIe dynamic datarate switch ports</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_ports_pipe_rx_elecidle" type="int">
          <ipxact:name>enable_ports_pipe_rx_elecidle</ipxact:name>
          <ipxact:displayName>Enable PCIe electrical idle control and status ports</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_ports_pipe_hclk" type="int">
          <ipxact:name>enable_ports_pipe_hclk</ipxact:name>
          <ipxact:displayName>Enable PCIe pipe_hclk_in and pipe_hclk_out ports</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_pipe_early_spd_chng" type="int">
          <ipxact:name>l_pipe_early_spd_chng</ipxact:name>
          <ipxact:displayName>l_pipe_early_spd_chng</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_early_spd_chng" type="int">
          <ipxact:name>enable_early_spd_chng</ipxact:name>
          <ipxact:displayName>Enable early speed change</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="early_spd_chng_t1" type="int">
          <ipxact:name>early_spd_chng_t1</ipxact:name>
          <ipxact:displayName>Delay T1 for early_spd_chng</ipxact:displayName>
          <ipxact:value>60</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="early_spd_chng_t2" type="int">
          <ipxact:name>early_spd_chng_t2</ipxact:name>
          <ipxact:displayName>Pulse width T2</ipxact:displayName>
          <ipxact:value>150</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="early_spd_chng_t3" type="int">
          <ipxact:name>early_spd_chng_t3</ipxact:name>
          <ipxact:displayName>Delay T3 for pipe_sw</ipxact:displayName>
          <ipxact:value>1000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_pcs_pma_width" type="int">
          <ipxact:name>enh_pcs_pma_width</ipxact:name>
          <ipxact:displayName>Enhanced PCS / PMA interface width</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_pld_pcs_width" type="int">
          <ipxact:name>enh_pld_pcs_width</ipxact:name>
          <ipxact:displayName>FPGA fabric / Enhanced PCS interface width</ipxact:displayName>
          <ipxact:value>66</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_low_latency_enable" type="int">
          <ipxact:name>enh_low_latency_enable</ipxact:name>
          <ipxact:displayName>Enable 'Enhanced PCS' low latency mode</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_advanced_user_mode" type="int">
          <ipxact:name>enh_advanced_user_mode</ipxact:name>
          <ipxact:displayName>Enable 'Enhanced PCS' advanced user mode</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_frmgen_enable" type="int">
          <ipxact:name>enh_tx_frmgen_enable</ipxact:name>
          <ipxact:displayName>Enable Interlaken frame generator</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_frmgen_mfrm_length" type="int">
          <ipxact:name>enh_tx_frmgen_mfrm_length</ipxact:name>
          <ipxact:displayName>Frame generator metaframe length</ipxact:displayName>
          <ipxact:value>2048</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_frmgen_burst_enable" type="int">
          <ipxact:name>enh_tx_frmgen_burst_enable</ipxact:name>
          <ipxact:displayName>Enable frame generator burst control</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_enh_frame" type="int">
          <ipxact:name>enable_port_tx_enh_frame</ipxact:name>
          <ipxact:displayName>Enable tx_enh_frame port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_enh_frame_diag_status" type="int">
          <ipxact:name>enable_port_tx_enh_frame_diag_status</ipxact:name>
          <ipxact:displayName>Enable tx_enh_frame_diag_status port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_enh_frame_burst_en" type="int">
          <ipxact:name>enable_port_tx_enh_frame_burst_en</ipxact:name>
          <ipxact:displayName>Enable tx_enh_frame_burst_en port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_rx_frmsync_enable" type="int">
          <ipxact:name>enh_rx_frmsync_enable</ipxact:name>
          <ipxact:displayName>Enable Interlaken frame synchronizer</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_rx_frmsync_mfrm_length" type="int">
          <ipxact:name>enh_rx_frmsync_mfrm_length</ipxact:name>
          <ipxact:displayName>Frame synchronizer metaframe length</ipxact:displayName>
          <ipxact:value>2048</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_enh_frame" type="int">
          <ipxact:name>enable_port_rx_enh_frame</ipxact:name>
          <ipxact:displayName>Enable rx_enh_frame port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_enh_frame_lock" type="int">
          <ipxact:name>enable_port_rx_enh_frame_lock</ipxact:name>
          <ipxact:displayName>Enable rx_enh_frame_lock port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_enh_frame_diag_status" type="int">
          <ipxact:name>enable_port_rx_enh_frame_diag_status</ipxact:name>
          <ipxact:displayName>Enable rx_enh_frame_diag_status port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_crcgen_enable" type="int">
          <ipxact:name>enh_tx_crcgen_enable</ipxact:name>
          <ipxact:displayName>Enable Interlaken TX CRC-32 generator</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_crcerr_enable" type="int">
          <ipxact:name>enh_tx_crcerr_enable</ipxact:name>
          <ipxact:displayName>Enable Interlaken TX CRC-32 generator error insertion</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_rx_crcchk_enable" type="int">
          <ipxact:name>enh_rx_crcchk_enable</ipxact:name>
          <ipxact:displayName>Enable Interlaken RX CRC-32 checker</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_enh_crc32_err" type="int">
          <ipxact:name>enable_port_rx_enh_crc32_err</ipxact:name>
          <ipxact:displayName>Enable rx_enh_crc32_err port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_enh_highber" type="int">
          <ipxact:name>enable_port_rx_enh_highber</ipxact:name>
          <ipxact:displayName>Enable rx_enh_highber port (10GBASE-R)</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_enh_highber_clr_cnt" type="int">
          <ipxact:name>enable_port_rx_enh_highber_clr_cnt</ipxact:name>
          <ipxact:displayName>Enable rx_enh_highber_clr_cnt port (10GBASE-R)</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_enh_clr_errblk_count" type="int">
          <ipxact:name>enable_port_rx_enh_clr_errblk_count</ipxact:name>
          <ipxact:displayName>Enable rx_enh_clr_errblk_count port (10GBASE-R &amp; FEC)</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_64b66b_enable" type="int">
          <ipxact:name>enh_tx_64b66b_enable</ipxact:name>
          <ipxact:displayName>Enable TX 64b/66b encoder</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_rx_64b66b_enable" type="int">
          <ipxact:name>enh_rx_64b66b_enable</ipxact:name>
          <ipxact:displayName>Enable RX 64b/66b decoder</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_sh_err" type="int">
          <ipxact:name>enh_tx_sh_err</ipxact:name>
          <ipxact:displayName>Enable TX sync header error insertion</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_scram_enable" type="int">
          <ipxact:name>enh_tx_scram_enable</ipxact:name>
          <ipxact:displayName>Enable TX scrambler (10GBASE-R/Interlaken)</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_scram_seed" type="longint">
          <ipxact:name>enh_tx_scram_seed</ipxact:name>
          <ipxact:displayName>TX scrambler seed (10GBASE-R/Interlaken)</ipxact:displayName>
          <ipxact:value>288230376151711743</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_rx_descram_enable" type="int">
          <ipxact:name>enh_rx_descram_enable</ipxact:name>
          <ipxact:displayName>Enable RX descrambler (10GBASE-R/Interlaken)</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_dispgen_enable" type="int">
          <ipxact:name>enh_tx_dispgen_enable</ipxact:name>
          <ipxact:displayName>Enable Interlaken TX disparity generator</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_rx_dispchk_enable" type="int">
          <ipxact:name>enh_rx_dispchk_enable</ipxact:name>
          <ipxact:displayName>Enable Interlaken RX disparity checker</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_randomdispbit_enable" type="int">
          <ipxact:name>enh_tx_randomdispbit_enable</ipxact:name>
          <ipxact:displayName>Enable Interlaken TX random disparity bit</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_rx_blksync_enable" type="int">
          <ipxact:name>enh_rx_blksync_enable</ipxact:name>
          <ipxact:displayName>Enable RX block synchronizer</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_enh_blk_lock" type="int">
          <ipxact:name>enable_port_rx_enh_blk_lock</ipxact:name>
          <ipxact:displayName>Enable rx_enh_blk_lock port</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_bitslip_enable" type="int">
          <ipxact:name>enh_tx_bitslip_enable</ipxact:name>
          <ipxact:displayName>Enable TX data bitslip</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_polinv_enable" type="int">
          <ipxact:name>enh_tx_polinv_enable</ipxact:name>
          <ipxact:displayName>Enable TX data polarity inversion</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_rx_bitslip_enable" type="int">
          <ipxact:name>enh_rx_bitslip_enable</ipxact:name>
          <ipxact:displayName>Enable RX data bitslip</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_rx_polinv_enable" type="int">
          <ipxact:name>enh_rx_polinv_enable</ipxact:name>
          <ipxact:displayName>Enable RX data polarity inversion</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_enh_bitslip" type="int">
          <ipxact:name>enable_port_tx_enh_bitslip</ipxact:name>
          <ipxact:displayName>Enable tx_enh_bitslip port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_enh_bitslip" type="int">
          <ipxact:name>enable_port_rx_enh_bitslip</ipxact:name>
          <ipxact:displayName>Enable rx_bitslip port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_rx_krfec_err_mark_enable" type="int">
          <ipxact:name>enh_rx_krfec_err_mark_enable</ipxact:name>
          <ipxact:displayName>Enable RX KR-FEC error marking</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_rx_krfec_err_mark_type" type="string">
          <ipxact:name>enh_rx_krfec_err_mark_type</ipxact:name>
          <ipxact:displayName>Error marking type</ipxact:displayName>
          <ipxact:value>10G</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_krfec_burst_err_enable" type="int">
          <ipxact:name>enh_tx_krfec_burst_err_enable</ipxact:name>
          <ipxact:displayName>Enable KR-FEC TX error insertion</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enh_tx_krfec_burst_err_len" type="int">
          <ipxact:name>enh_tx_krfec_burst_err_len</ipxact:name>
          <ipxact:displayName>KR-FEC TX error insertion spacing</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_krfec_tx_enh_frame" type="int">
          <ipxact:name>enable_port_krfec_tx_enh_frame</ipxact:name>
          <ipxact:displayName>Enable tx_enh_frame port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_krfec_rx_enh_frame" type="int">
          <ipxact:name>enable_port_krfec_rx_enh_frame</ipxact:name>
          <ipxact:displayName>Enable rx_enh_frame port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_krfec_rx_enh_frame_diag_status" type="int">
          <ipxact:name>enable_port_krfec_rx_enh_frame_diag_status</ipxact:name>
          <ipxact:displayName>Enable rx_enh_frame_diag_status port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pcs_direct_width" type="int">
          <ipxact:name>pcs_direct_width</ipxact:name>
          <ipxact:displayName>PCS Direct interface width</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_tx_fast_pipeln_reg" type="int">
          <ipxact:name>enable_tx_fast_pipeln_reg</ipxact:name>
          <ipxact:displayName>Enable TX fast pipeline registers</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_rx_fast_pipeln_reg" type="int">
          <ipxact:name>enable_rx_fast_pipeln_reg</ipxact:name>
          <ipxact:displayName>Enable RX fast pipeline registers</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="parallel_loopback_mode" type="string">
          <ipxact:name>parallel_loopback_mode</ipxact:name>
          <ipxact:displayName>Parallel loopback mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="loopback_tx_clk_sel" type="string">
          <ipxact:name>loopback_tx_clk_sel</ipxact:name>
          <ipxact:displayName>Parallel loopback mode TX clock source selection</ipxact:displayName>
          <ipxact:value>internal_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_debug_ports" type="int">
          <ipxact:name>enable_debug_ports</ipxact:name>
          <ipxact:displayName>Enable PCS reset status ports</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_advanced_user_mode" type="int">
          <ipxact:name>enable_advanced_user_mode</ipxact:name>
          <ipxact:displayName>Enable advanced user mode</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_loopback_mode" type="int">
          <ipxact:name>l_enable_loopback_mode</ipxact:name>
          <ipxact:displayName>l_enable_loopback_mode</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_fifo_mode" type="string">
          <ipxact:name>tx_fifo_mode</ipxact:name>
          <ipxact:displayName>TX Core Interface FIFO mode</ipxact:displayName>
          <ipxact:value>Phase compensation</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_fifo_pfull" type="int">
          <ipxact:name>tx_fifo_pfull</ipxact:name>
          <ipxact:displayName>TX FIFO partially full threshold</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_fifo_pempty" type="int">
          <ipxact:name>tx_fifo_pempty</ipxact:name>
          <ipxact:displayName>TX FIFO partially empty threshold</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_fifo_full" type="int">
          <ipxact:name>enable_port_tx_fifo_full</ipxact:name>
          <ipxact:displayName>Enable tx_fifo_full port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_fifo_empty" type="int">
          <ipxact:name>enable_port_tx_fifo_empty</ipxact:name>
          <ipxact:displayName>Enable tx_fifo_empty port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_fifo_pfull" type="int">
          <ipxact:name>enable_port_tx_fifo_pfull</ipxact:name>
          <ipxact:displayName>Enable tx_fifo_pfull port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_fifo_pempty" type="int">
          <ipxact:name>enable_port_tx_fifo_pempty</ipxact:name>
          <ipxact:displayName>Enable tx_fifo_pempty port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_pcs_fifo_full" type="int">
          <ipxact:name>enable_port_tx_pcs_fifo_full</ipxact:name>
          <ipxact:displayName>Enable tx_pcs_fifo_full port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_pcs_fifo_empty" type="int">
          <ipxact:name>enable_port_tx_pcs_fifo_empty</ipxact:name>
          <ipxact:displayName>Enable tx_pcs_fifo_empty port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_dll_lock" type="int">
          <ipxact:name>enable_port_tx_dll_lock</ipxact:name>
          <ipxact:displayName>Enable tx_dll_lock port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_fifo_mode" type="string">
          <ipxact:name>rx_fifo_mode</ipxact:name>
          <ipxact:displayName>RX PCS-Core Interface FIFO mode (PCS FIFO-Core FIFO)</ipxact:displayName>
          <ipxact:value>Phase compensation</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_fifo_pfull" type="int">
          <ipxact:name>rx_fifo_pfull</ipxact:name>
          <ipxact:displayName>RX FIFO partially full threshold</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_fifo_pempty" type="int">
          <ipxact:name>rx_fifo_pempty</ipxact:name>
          <ipxact:displayName>RX FIFO partially empty threshold</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_fifo_align_del" type="int">
          <ipxact:name>rx_fifo_align_del</ipxact:name>
          <ipxact:displayName>Enable RX FIFO alignment word deletion (Interlaken)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_fifo_control_del" type="int">
          <ipxact:name>rx_fifo_control_del</ipxact:name>
          <ipxact:displayName>Enable RX FIFO control word deletion (Interlaken)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_data_valid" type="int">
          <ipxact:name>enable_port_rx_data_valid</ipxact:name>
          <ipxact:displayName>Enable rx_data_valid port</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_fifo_full" type="int">
          <ipxact:name>enable_port_rx_fifo_full</ipxact:name>
          <ipxact:displayName>Enable rx_fifo_full port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_fifo_empty" type="int">
          <ipxact:name>enable_port_rx_fifo_empty</ipxact:name>
          <ipxact:displayName>Enable rx_fifo_empty port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_fifo_pfull" type="int">
          <ipxact:name>enable_port_rx_fifo_pfull</ipxact:name>
          <ipxact:displayName>Enable rx_fifo_pfull port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_fifo_pempty" type="int">
          <ipxact:name>enable_port_rx_fifo_pempty</ipxact:name>
          <ipxact:displayName>Enable rx_fifo_pempty port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_fifo_del" type="int">
          <ipxact:name>enable_port_rx_fifo_del</ipxact:name>
          <ipxact:displayName>Enable rx_fifo_del port (10GBASE-R)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_fifo_insert" type="int">
          <ipxact:name>enable_port_rx_fifo_insert</ipxact:name>
          <ipxact:displayName>Enable rx_fifo_insert port (10GBASE-R)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_fifo_rd_en" type="int">
          <ipxact:name>enable_port_rx_fifo_rd_en</ipxact:name>
          <ipxact:displayName>Enable rx_fifo_rd_en port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_fifo_align_clr" type="int">
          <ipxact:name>enable_port_rx_fifo_align_clr</ipxact:name>
          <ipxact:displayName>Enable rx_fifo_align_clr port (Interlaken)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_pcs_fifo_full" type="int">
          <ipxact:name>enable_port_rx_pcs_fifo_full</ipxact:name>
          <ipxact:displayName>Enable rx_pcs_fifo_full port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_pcs_fifo_empty" type="int">
          <ipxact:name>enable_port_rx_pcs_fifo_empty</ipxact:name>
          <ipxact:displayName>Enable rx_pcs_fifo_empty port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="fifo_depth_message" type="string">
          <ipxact:name>fifo_depth_message</ipxact:name>
          <ipxact:displayName>fifo_depth_message</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_clkout_sel" type="string">
          <ipxact:name>tx_clkout_sel</ipxact:name>
          <ipxact:displayName>Selected tx_clkout clock source</ipxact:displayName>
          <ipxact:value>pcs_clkout</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_clkout2" type="int">
          <ipxact:name>enable_port_tx_clkout2</ipxact:name>
          <ipxact:displayName>Enable tx_clkout2 port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_clkout2_sel" type="string">
          <ipxact:name>tx_clkout2_sel</ipxact:name>
          <ipxact:displayName>Selected tx_clkout2 clock source</ipxact:displayName>
          <ipxact:value>pcs_clkout</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_clkout_hioint" type="int">
          <ipxact:name>enable_port_tx_clkout_hioint</ipxact:name>
          <ipxact:displayName>Enable tx_clkout_hioint port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_clkout2_hioint" type="int">
          <ipxact:name>enable_port_tx_clkout2_hioint</ipxact:name>
          <ipxact:displayName>Enable tx_clkout2_hioint port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_div_clkout_divider" type="string">
          <ipxact:name>tx_pma_div_clkout_divider</ipxact:name>
          <ipxact:displayName>TX pma_div_clkout division factor</ipxact:displayName>
          <ipxact:value>33</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_coreclkin_clock_network" type="string">
          <ipxact:name>tx_coreclkin_clock_network</ipxact:name>
          <ipxact:displayName>Selected tx_coreclkin clock network</ipxact:displayName>
          <ipxact:value>dedicated</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pcs_bonding_clock_network" type="string">
          <ipxact:name>tx_pcs_bonding_clock_network</ipxact:name>
          <ipxact:displayName>Selected TX PCS bonding clock network</ipxact:displayName>
          <ipxact:value>dedicated</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_clkout_sel" type="string">
          <ipxact:name>rx_clkout_sel</ipxact:name>
          <ipxact:displayName>Selected rx_clkout clock source</ipxact:displayName>
          <ipxact:value>pcs_clkout</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_clkout2" type="int">
          <ipxact:name>enable_port_rx_clkout2</ipxact:name>
          <ipxact:displayName>Enable rx_clkout2 port</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_clkout2_sel" type="string">
          <ipxact:name>rx_clkout2_sel</ipxact:name>
          <ipxact:displayName>Selected rx_clkout2 clock source</ipxact:displayName>
          <ipxact:value>pma_div_clkout</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_clkout_hioint" type="int">
          <ipxact:name>enable_port_rx_clkout_hioint</ipxact:name>
          <ipxact:displayName>Enable rx_clkout_hioint port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_clkout2_hioint" type="int">
          <ipxact:name>enable_port_rx_clkout2_hioint</ipxact:name>
          <ipxact:displayName>Enable rx_clkout2_hioint port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_pma_div_clkout_divider" type="string">
          <ipxact:name>rx_pma_div_clkout_divider</ipxact:name>
          <ipxact:displayName>RX pma_div_clkout division factor</ipxact:displayName>
          <ipxact:value>33</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_coreclkin_clock_network" type="string">
          <ipxact:name>rx_coreclkin_clock_network</ipxact:name>
          <ipxact:displayName>Selected rx_coreclkin clock network</ipxact:displayName>
          <ipxact:value>dedicated</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="osc_clk_divider" type="int">
          <ipxact:name>osc_clk_divider</ipxact:name>
          <ipxact:displayName>OSC clock division factor</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_tx_pma_div_clkout" type="int">
          <ipxact:name>l_enable_tx_pma_div_clkout</ipxact:name>
          <ipxact:displayName>l_enable_tx_pma_div_clkout</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_rx_pma_div_clkout" type="int">
          <ipxact:name>l_enable_rx_pma_div_clkout</ipxact:name>
          <ipxact:displayName>l_enable_rx_pma_div_clkout</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_tx_fifo_latency_adj_ena" type="int">
          <ipxact:name>enable_port_tx_fifo_latency_adj_ena</ipxact:name>
          <ipxact:displayName>Enable TX FIFO latency adjustment port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_rx_fifo_latency_adj_ena" type="int">
          <ipxact:name>enable_port_rx_fifo_latency_adj_ena</ipxact:name>
          <ipxact:displayName>Enable RX FIFO latency adjustment port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_latency_measurement" type="int">
          <ipxact:name>enable_port_latency_measurement</ipxact:name>
          <ipxact:displayName>Enable latency measurement ports</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_port_clock_delay_measurement" type="int">
          <ipxact:name>enable_port_clock_delay_measurement</ipxact:name>
          <ipxact:displayName>Enable clock delay measurement ports</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="delay_measurement_clkout_sel" type="string">
          <ipxact:name>delay_measurement_clkout_sel</ipxact:name>
          <ipxact:displayName>Selected delay_measurement_clkout clock source</ipxact:displayName>
          <ipxact:value>clock_delay_measurement_clkout</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="delay_measurement_clkout2_sel" type="string">
          <ipxact:name>delay_measurement_clkout2_sel</ipxact:name>
          <ipxact:displayName>Selected delay_measurement_clkout2 clock source</ipxact:displayName>
          <ipxact:value>clock_delay_measurement_clkout</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="generate_docs" type="int">
          <ipxact:name>generate_docs</ipxact:name>
          <ipxact:displayName>Generate parameter documentation file</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="generate_add_hdl_instance_example" type="int">
          <ipxact:name>generate_add_hdl_instance_example</ipxact:name>
          <ipxact:displayName>Generate '_hw.tcl' 'add_hdl_instance' example file</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="validation_rule_select" type="string">
          <ipxact:name>validation_rule_select</ipxact:name>
          <ipxact:displayName>View validation rule for parameter</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_advanced_options" type="int">
          <ipxact:name>enable_advanced_options</ipxact:name>
          <ipxact:displayName>enable_advanced_options</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_bg_cal_debug" type="int">
          <ipxact:name>enable_bg_cal_debug</ipxact:name>
          <ipxact:displayName>enable_bg_cal_debug</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="disable_bg_cal" type="int">
          <ipxact:name>disable_bg_cal</ipxact:name>
          <ipxact:displayName>disable_bg_cal</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_internal_options" type="int">
          <ipxact:name>enable_internal_options</ipxact:name>
          <ipxact:displayName>enable_internal_options</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_debug_options" type="int">
          <ipxact:name>enable_debug_options</ipxact:name>
          <ipxact:displayName>enable_debug_options</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_physical_bonding_clocks" type="int">
          <ipxact:name>enable_physical_bonding_clocks</ipxact:name>
          <ipxact:displayName>enable_physical_bonding_clocks</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_tx_coreclkin2" type="int">
          <ipxact:name>enable_tx_coreclkin2</ipxact:name>
          <ipxact:displayName>Enable tx_coreclkin2 port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_tx_x2_coreclkin_port" type="int">
          <ipxact:name>enable_tx_x2_coreclkin_port</ipxact:name>
          <ipxact:displayName>enable_tx_x2_coreclkin_port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_enable" type="int">
          <ipxact:name>tx_enable</ipxact:name>
          <ipxact:displayName>tx_enable</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="datapath_select" type="string">
          <ipxact:name>datapath_select</ipxact:name>
          <ipxact:displayName>datapath_select</ipxact:displayName>
          <ipxact:value>Enhanced</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_enable" type="int">
          <ipxact:name>rx_enable</ipxact:name>
          <ipxact:displayName>rx_enable</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_crete_nf" type="int">
          <ipxact:name>l_crete_nf</ipxact:name>
          <ipxact:displayName>l_crete_nf</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_channels" type="int">
          <ipxact:name>l_channels</ipxact:name>
          <ipxact:displayName>l_channels</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_split_iface" type="int">
          <ipxact:name>l_split_iface</ipxact:name>
          <ipxact:displayName>l_split_iface</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_pcs_pma_width" type="int">
          <ipxact:name>l_pcs_pma_width</ipxact:name>
          <ipxact:displayName>l_pcs_pma_width</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_tx_adapt_pcs_width" type="int">
          <ipxact:name>l_tx_adapt_pcs_width</ipxact:name>
          <ipxact:displayName>l_tx_adapt_pcs_width</ipxact:displayName>
          <ipxact:value>66</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_rx_adapt_pcs_width" type="int">
          <ipxact:name>l_rx_adapt_pcs_width</ipxact:name>
          <ipxact:displayName>l_rx_adapt_pcs_width</ipxact:displayName>
          <ipxact:value>66</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_pll_settings" type="string">
          <ipxact:name>l_pll_settings</ipxact:name>
          <ipxact:displayName>l_pll_settings</ipxact:displayName>
          <ipxact:value>343.750000 {refclk 343.750000 m 15 n 1 lpfd 2 lpd 2 fvco 10312.5} 687.500000 {refclk 687.500000 m 15 n 2 lpfd 2 lpd 2 fvco 10312.5} 322.265625 {refclk 322.265625 m 16 n 1 lpfd 2 lpd 2 fvco 10312.5} 644.531250 {refclk 644.531250 m 16 n 2 lpfd 2 lpd 2 fvco 10312.5} 303.308824 {refclk 303.308824 m 17 n 1 lpfd 2 lpd 2 fvco 10312.5} 606.617647 {refclk 606.617647 m 17 n 2 lpfd 2 lpd 2 fvco 10312.5} 286.458333 {refclk 286.458333 m 18 n 1 lpfd 2 lpd 2 fvco 10312.5} 572.916667 {refclk 572.916667 m 18 n 2 lpfd 2 lpd 2 fvco 10312.5} 271.381579 {refclk 271.381579 m 19 n 1 lpfd 2 lpd 2 fvco 10312.5} 542.763158 {refclk 542.763158 m 19 n 2 lpfd 2 lpd 2 fvco 10312.5} 257.812500 {refclk 257.812500 m 20 n 1 lpfd 2 lpd 2 fvco 10312.5} 515.625000 {refclk 515.625000 m 20 n 2 lpfd 2 lpd 2 fvco 10312.5} 245.535714 {refclk 245.535714 m 21 n 1 lpfd 2 lpd 2 fvco 10312.5} 491.071429 {refclk 491.071429 m 21 n 2 lpfd 2 lpd 2 fvco 10312.5} 234.375000 {refclk 234.375000 m 22 n 1 lpfd 2 lpd 2 fvco 10312.5} 468.750000 {refclk 468.750000 m 22 n 2 lpfd 2 lpd 2 fvco 10312.5} 224.184783 {refclk 224.184783 m 23 n 1 lpfd 2 lpd 2 fvco 10312.5} 448.369565 {refclk 448.369565 m 23 n 2 lpfd 2 lpd 2 fvco 10312.5} 214.843750 {refclk 214.843750 m 24 n 1 lpfd 2 lpd 2 fvco 10312.5} 429.687500 {refclk 429.687500 m 24 n 2 lpfd 2 lpd 2 fvco 10312.5} 206.250000 {refclk 206.250000 m 25 n 1 lpfd 2 lpd 2 fvco 10312.5} 412.500000 {refclk 412.500000 m 25 n 2 lpfd 2 lpd 2 fvco 10312.5} 198.317308 {refclk 198.317308 m 26 n 1 lpfd 2 lpd 2 fvco 10312.5} 396.634615 {refclk 396.634615 m 26 n 2 lpfd 2 lpd 2 fvco 10312.5} 793.269231 {refclk 793.269231 m 26 n 4 lpfd 2 lpd 2 fvco 10312.5} 190.972222 {refclk 190.972222 m 27 n 1 lpfd 2 lpd 2 fvco 10312.5} 381.944444 {refclk 381.944444 m 27 n 2 lpfd 2 lpd 2 fvco 10312.5} 763.888889 {refclk 763.888889 m 27 n 4 lpfd 2 lpd 2 fvco 10312.5} 184.151786 {refclk 184.151786 m 28 n 1 lpfd 2 lpd 2 fvco 10312.5} 368.303571 {refclk 368.303571 m 28 n 2 lpfd 2 lpd 2 fvco 10312.5} 736.607143 {refclk 736.607143 m 28 n 4 lpfd 2 lpd 2 fvco 10312.5} 177.801724 {refclk 177.801724 m 29 n 1 lpfd 2 lpd 2 fvco 10312.5} 355.603448 {refclk 355.603448 m 29 n 2 lpfd 2 lpd 2 fvco 10312.5} 711.206897 {refclk 711.206897 m 29 n 4 lpfd 2 lpd 2 fvco 10312.5} 171.875000 {refclk 171.875000 m 30 n 1 lpfd 2 lpd 2 fvco 10312.5} 166.330645 {refclk 166.330645 m 31 n 1 lpfd 2 lpd 2 fvco 10312.5} 332.661290 {refclk 332.661290 m 31 n 2 lpfd 2 lpd 2 fvco 10312.5} 665.322581 {refclk 665.322581 m 31 n 4 lpfd 2 lpd 2 fvco 10312.5} 161.132813 {refclk 161.132813 m 32 n 1 lpfd 2 lpd 2 fvco 10312.5} 156.250000 {refclk 156.250000 m 33 n 1 lpfd 2 lpd 2 fvco 10312.5} 312.500000 {refclk 312.500000 m 33 n 2 lpfd 2 lpd 2 fvco 10312.5} 625.000000 {refclk 625.000000 m 33 n 4 lpfd 2 lpd 2 fvco 10312.5} 151.654412 {refclk 151.654412 m 34 n 1 lpfd 2 lpd 2 fvco 10312.5} 147.321429 {refclk 147.321429 m 35 n 1 lpfd 2 lpd 2 fvco 10312.5} 294.642857 {refclk 294.642857 m 35 n 2 lpfd 2 lpd 2 fvco 10312.5} 589.285714 {refclk 589.285714 m 35 n 4 lpfd 2 lpd 2 fvco 10312.5} 143.229167 {refclk 143.229167 m 36 n 1 lpfd 2 lpd 2 fvco 10312.5} 139.358108 {refclk 139.358108 m 37 n 1 lpfd 2 lpd 2 fvco 10312.5} 278.716216 {refclk 278.716216 m 37 n 2 lpfd 2 lpd 2 fvco 10312.5} 557.432432 {refclk 557.432432 m 37 n 4 lpfd 2 lpd 2 fvco 10312.5} 135.690789 {refclk 135.690789 m 38 n 1 lpfd 2 lpd 2 fvco 10312.5} 132.211538 {refclk 132.211538 m 39 n 1 lpfd 2 lpd 2 fvco 10312.5} 264.423077 {refclk 264.423077 m 39 n 2 lpfd 2 lpd 2 fvco 10312.5} 528.846154 {refclk 528.846154 m 39 n 4 lpfd 2 lpd 2 fvco 10312.5} 128.906250 {refclk 128.906250 m 40 n 1 lpfd 2 lpd 2 fvco 10312.5} 125.762195 {refclk 125.762195 m 41 n 1 lpfd 2 lpd 2 fvco 10312.5} 251.524390 {refclk 251.524390 m 41 n 2 lpfd 2 lpd 2 fvco 10312.5} 503.048780 {refclk 503.048780 m 41 n 4 lpfd 2 lpd 2 fvco 10312.5} 122.767857 {refclk 122.767857 m 42 n 1 lpfd 2 lpd 2 fvco 10312.5} 119.912791 {refclk 119.912791 m 43 n 1 lpfd 2 lpd 2 fvco 10312.5} 239.825581 {refclk 239.825581 m 43 n 2 lpfd 2 lpd 2 fvco 10312.5} 479.651163 {refclk 479.651163 m 43 n 4 lpfd 2 lpd 2 fvco 10312.5} 117.187500 {refclk 117.187500 m 44 n 1 lpfd 2 lpd 2 fvco 10312.5} 114.583333 {refclk 114.583333 m 45 n 1 lpfd 2 lpd 2 fvco 10312.5} 229.166667 {refclk 229.166667 m 45 n 2 lpfd 2 lpd 2 fvco 10312.5} 458.333333 {refclk 458.333333 m 45 n 4 lpfd 2 lpd 2 fvco 10312.5} 112.092391 {refclk 112.092391 m 46 n 1 lpfd 2 lpd 2 fvco 10312.5} 109.707447 {refclk 109.707447 m 47 n 1 lpfd 2 lpd 2 fvco 10312.5} 219.414894 {refclk 219.414894 m 47 n 2 lpfd 2 lpd 2 fvco 10312.5} 438.829787 {refclk 438.829787 m 47 n 4 lpfd 2 lpd 2 fvco 10312.5} 107.421875 {refclk 107.421875 m 48 n 1 lpfd 2 lpd 2 fvco 10312.5} 105.229592 {refclk 105.229592 m 49 n 1 lpfd 2 lpd 2 fvco 10312.5} 210.459184 {refclk 210.459184 m 49 n 2 lpfd 2 lpd 2 fvco 10312.5} 420.918367 {refclk 420.918367 m 49 n 4 lpfd 2 lpd 2 fvco 10312.5} 103.125000 {refclk 103.125000 m 50 n 1 lpfd 2 lpd 2 fvco 10312.5} 101.102941 {refclk 101.102941 m 51 n 1 lpfd 2 lpd 2 fvco 10312.5} 202.205882 {refclk 202.205882 m 51 n 2 lpfd 2 lpd 2 fvco 10312.5} 404.411765 {refclk 404.411765 m 51 n 4 lpfd 2 lpd 2 fvco 10312.5} 99.158654 {refclk 99.158654 m 52 n 1 lpfd 2 lpd 2 fvco 10312.5} 97.287736 {refclk 97.287736 m 53 n 1 lpfd 2 lpd 2 fvco 10312.5} 194.575472 {refclk 194.575472 m 53 n 2 lpfd 2 lpd 2 fvco 10312.5} 389.150943 {refclk 389.150943 m 53 n 4 lpfd 2 lpd 2 fvco 10312.5} 778.301887 {refclk 778.301887 m 53 n 8 lpfd 2 lpd 2 fvco 10312.5} 95.486111 {refclk 95.486111 m 54 n 1 lpfd 2 lpd 2 fvco 10312.5} 93.750000 {refclk 93.750000 m 55 n 1 lpfd 2 lpd 2 fvco 10312.5} 187.500000 {refclk 187.500000 m 55 n 2 lpfd 2 lpd 2 fvco 10312.5} 375.000000 {refclk 375.000000 m 55 n 4 lpfd 2 lpd 2 fvco 10312.5} 750.000000 {refclk 750.000000 m 55 n 8 lpfd 2 lpd 2 fvco 10312.5} 92.075893 {refclk 92.075893 m 56 n 1 lpfd 2 lpd 2 fvco 10312.5} 90.460526 {refclk 90.460526 m 57 n 1 lpfd 2 lpd 2 fvco 10312.5} 180.921053 {refclk 180.921053 m 57 n 2 lpfd 2 lpd 2 fvco 10312.5} 361.842105 {refclk 361.842105 m 57 n 4 lpfd 2 lpd 2 fvco 10312.5} 723.684211 {refclk 723.684211 m 57 n 8 lpfd 2 lpd 2 fvco 10312.5} 88.900862 {refclk 88.900862 m 58 n 1 lpfd 2 lpd 2 fvco 10312.5} 87.394068 {refclk 87.394068 m 59 n 1 lpfd 2 lpd 2 fvco 10312.5} 174.788136 {refclk 174.788136 m 59 n 2 lpfd 2 lpd 2 fvco 10312.5} 349.576271 {refclk 349.576271 m 59 n 4 lpfd 2 lpd 2 fvco 10312.5} 699.152542 {refclk 699.152542 m 59 n 8 lpfd 2 lpd 2 fvco 10312.5} 85.937500 {refclk 85.937500 m 60 n 1 lpfd 2 lpd 2 fvco 10312.5} 84.528689 {refclk 84.528689 m 61 n 1 lpfd 2 lpd 2 fvco 10312.5} 169.057377 {refclk 169.057377 m 61 n 2 lpfd 2 lpd 2 fvco 10312.5} 338.114754 {refclk 338.114754 m 61 n 4 lpfd 2 lpd 2 fvco 10312.5} 676.229508 {refclk 676.229508 m 61 n 8 lpfd 2 lpd 2 fvco 10312.5} 83.165323 {refclk 83.165323 m 62 n 1 lpfd 2 lpd 2 fvco 10312.5} 81.845238 {refclk 81.845238 m 63 n 1 lpfd 2 lpd 2 fvco 10312.5} 163.690476 {refclk 163.690476 m 63 n 2 lpfd 2 lpd 2 fvco 10312.5} 327.380952 {refclk 327.380952 m 63 n 4 lpfd 2 lpd 2 fvco 10312.5} 654.761905 {refclk 654.761905 m 63 n 8 lpfd 2 lpd 2 fvco 10312.5} 80.566406 {refclk 80.566406 m 64 n 1 lpfd 2 lpd 2 fvco 10312.5} 79.326923 {refclk 79.326923 m 65 n 1 lpfd 2 lpd 2 fvco 10312.5} 158.653846 {refclk 158.653846 m 65 n 2 lpfd 2 lpd 2 fvco 10312.5} 317.307692 {refclk 317.307692 m 65 n 4 lpfd 2 lpd 2 fvco 10312.5} 634.615385 {refclk 634.615385 m 65 n 8 lpfd 2 lpd 2 fvco 10312.5} 78.125000 {refclk 78.125000 m 66 n 1 lpfd 2 lpd 2 fvco 10312.5} 76.958955 {refclk 76.958955 m 67 n 1 lpfd 2 lpd 2 fvco 10312.5} 153.917910 {refclk 153.917910 m 67 n 2 lpfd 2 lpd 2 fvco 10312.5} 307.835821 {refclk 307.835821 m 67 n 4 lpfd 2 lpd 2 fvco 10312.5} 615.671642 {refclk 615.671642 m 67 n 8 lpfd 2 lpd 2 fvco 10312.5} 75.827206 {refclk 75.827206 m 68 n 1 lpfd 2 lpd 2 fvco 10312.5} 74.728261 {refclk 74.728261 m 69 n 1 lpfd 2 lpd 2 fvco 10312.5} 149.456522 {refclk 149.456522 m 69 n 2 lpfd 2 lpd 2 fvco 10312.5} 298.913043 {refclk 298.913043 m 69 n 4 lpfd 2 lpd 2 fvco 10312.5} 597.826087 {refclk 597.826087 m 69 n 8 lpfd 2 lpd 2 fvco 10312.5} 73.660714 {refclk 73.660714 m 70 n 1 lpfd 2 lpd 2 fvco 10312.5} 72.623239 {refclk 72.623239 m 71 n 1 lpfd 2 lpd 2 fvco 10312.5} 145.246479 {refclk 145.246479 m 71 n 2 lpfd 2 lpd 2 fvco 10312.5} 290.492958 {refclk 290.492958 m 71 n 4 lpfd 2 lpd 2 fvco 10312.5} 580.985915 {refclk 580.985915 m 71 n 8 lpfd 2 lpd 2 fvco 10312.5} 71.614583 {refclk 71.614583 m 72 n 1 lpfd 2 lpd 2 fvco 10312.5} 70.633562 {refclk 70.633562 m 73 n 1 lpfd 2 lpd 2 fvco 10312.5} 141.267123 {refclk 141.267123 m 73 n 2 lpfd 2 lpd 2 fvco 10312.5} 282.534247 {refclk 282.534247 m 73 n 4 lpfd 2 lpd 2 fvco 10312.5} 565.068493 {refclk 565.068493 m 73 n 8 lpfd 2 lpd 2 fvco 10312.5} 69.679054 {refclk 69.679054 m 74 n 1 lpfd 2 lpd 2 fvco 10312.5} 68.750000 {refclk 68.750000 m 75 n 1 lpfd 2 lpd 2 fvco 10312.5} 137.500000 {refclk 137.500000 m 75 n 2 lpfd 2 lpd 2 fvco 10312.5} 275.000000 {refclk 275.000000 m 75 n 4 lpfd 2 lpd 2 fvco 10312.5} 550.000000 {refclk 550.000000 m 75 n 8 lpfd 2 lpd 2 fvco 10312.5} 67.845395 {refclk 67.845395 m 76 n 1 lpfd 2 lpd 2 fvco 10312.5} 66.964286 {refclk 66.964286 m 77 n 1 lpfd 2 lpd 2 fvco 10312.5} 133.928571 {refclk 133.928571 m 77 n 2 lpfd 2 lpd 2 fvco 10312.5} 267.857143 {refclk 267.857143 m 77 n 4 lpfd 2 lpd 2 fvco 10312.5} 535.714286 {refclk 535.714286 m 77 n 8 lpfd 2 lpd 2 fvco 10312.5} 66.105769 {refclk 66.105769 m 78 n 1 lpfd 2 lpd 2 fvco 10312.5} 65.268987 {refclk 65.268987 m 79 n 1 lpfd 2 lpd 2 fvco 10312.5} 130.537975 {refclk 130.537975 m 79 n 2 lpfd 2 lpd 2 fvco 10312.5} 261.075949 {refclk 261.075949 m 79 n 4 lpfd 2 lpd 2 fvco 10312.5} 522.151899 {refclk 522.151899 m 79 n 8 lpfd 2 lpd 2 fvco 10312.5} 64.453125 {refclk 64.453125 m 80 n 1 lpfd 2 lpd 2 fvco 10312.5} 63.657407 {refclk 63.657407 m 81 n 1 lpfd 2 lpd 2 fvco 10312.5} 127.314815 {refclk 127.314815 m 81 n 2 lpfd 2 lpd 2 fvco 10312.5} 254.629630 {refclk 254.629630 m 81 n 4 lpfd 2 lpd 2 fvco 10312.5} 509.259259 {refclk 509.259259 m 81 n 8 lpfd 2 lpd 2 fvco 10312.5} 62.881098 {refclk 62.881098 m 82 n 1 lpfd 2 lpd 2 fvco 10312.5} 62.123494 {refclk 62.123494 m 83 n 1 lpfd 2 lpd 2 fvco 10312.5} 124.246988 {refclk 124.246988 m 83 n 2 lpfd 2 lpd 2 fvco 10312.5} 248.493976 {refclk 248.493976 m 83 n 4 lpfd 2 lpd 2 fvco 10312.5} 496.987952 {refclk 496.987952 m 83 n 8 lpfd 2 lpd 2 fvco 10312.5} 61.383929 {refclk 61.383929 m 84 n 1 lpfd 2 lpd 2 fvco 10312.5} 60.661765 {refclk 60.661765 m 85 n 1 lpfd 2 lpd 2 fvco 10312.5} 121.323529 {refclk 121.323529 m 85 n 2 lpfd 2 lpd 2 fvco 10312.5} 242.647059 {refclk 242.647059 m 85 n 4 lpfd 2 lpd 2 fvco 10312.5} 485.294118 {refclk 485.294118 m 85 n 8 lpfd 2 lpd 2 fvco 10312.5} 59.956395 {refclk 59.956395 m 86 n 1 lpfd 2 lpd 2 fvco 10312.5} 59.267241 {refclk 59.267241 m 87 n 1 lpfd 2 lpd 2 fvco 10312.5} 118.534483 {refclk 118.534483 m 87 n 2 lpfd 2 lpd 2 fvco 10312.5} 237.068966 {refclk 237.068966 m 87 n 4 lpfd 2 lpd 2 fvco 10312.5} 474.137931 {refclk 474.137931 m 87 n 8 lpfd 2 lpd 2 fvco 10312.5} 58.593750 {refclk 58.593750 m 88 n 1 lpfd 2 lpd 2 fvco 10312.5} 57.935393 {refclk 57.935393 m 89 n 1 lpfd 2 lpd 2 fvco 10312.5} 115.870787 {refclk 115.870787 m 89 n 2 lpfd 2 lpd 2 fvco 10312.5} 231.741573 {refclk 231.741573 m 89 n 4 lpfd 2 lpd 2 fvco 10312.5} 463.483146 {refclk 463.483146 m 89 n 8 lpfd 2 lpd 2 fvco 10312.5} 57.291667 {refclk 57.291667 m 90 n 1 lpfd 2 lpd 2 fvco 10312.5} 56.662088 {refclk 56.662088 m 91 n 1 lpfd 2 lpd 2 fvco 10312.5} 113.324176 {refclk 113.324176 m 91 n 2 lpfd 2 lpd 2 fvco 10312.5} 226.648352 {refclk 226.648352 m 91 n 4 lpfd 2 lpd 2 fvco 10312.5} 453.296703 {refclk 453.296703 m 91 n 8 lpfd 2 lpd 2 fvco 10312.5} 56.046196 {refclk 56.046196 m 92 n 1 lpfd 2 lpd 2 fvco 10312.5} 55.443548 {refclk 55.443548 m 93 n 1 lpfd 2 lpd 2 fvco 10312.5} 110.887097 {refclk 110.887097 m 93 n 2 lpfd 2 lpd 2 fvco 10312.5} 221.774194 {refclk 221.774194 m 93 n 4 lpfd 2 lpd 2 fvco 10312.5} 443.548387 {refclk 443.548387 m 93 n 8 lpfd 2 lpd 2 fvco 10312.5} 54.853723 {refclk 54.853723 m 94 n 1 lpfd 2 lpd 2 fvco 10312.5} 54.276316 {refclk 54.276316 m 95 n 1 lpfd 2 lpd 2 fvco 10312.5} 108.552632 {refclk 108.552632 m 95 n 2 lpfd 2 lpd 2 fvco 10312.5} 217.105263 {refclk 217.105263 m 95 n 4 lpfd 2 lpd 2 fvco 10312.5} 434.210526 {refclk 434.210526 m 95 n 8 lpfd 2 lpd 2 fvco 10312.5} 53.710938 {refclk 53.710938 m 96 n 1 lpfd 2 lpd 2 fvco 10312.5} 53.157216 {refclk 53.157216 m 97 n 1 lpfd 2 lpd 2 fvco 10312.5} 106.314433 {refclk 106.314433 m 97 n 2 lpfd 2 lpd 2 fvco 10312.5} 212.628866 {refclk 212.628866 m 97 n 4 lpfd 2 lpd 2 fvco 10312.5} 425.257732 {refclk 425.257732 m 97 n 8 lpfd 2 lpd 2 fvco 10312.5} 52.614796 {refclk 52.614796 m 98 n 1 lpfd 2 lpd 2 fvco 10312.5} 52.083333 {refclk 52.083333 m 99 n 1 lpfd 2 lpd 2 fvco 10312.5} 104.166667 {refclk 104.166667 m 99 n 2 lpfd 2 lpd 2 fvco 10312.5} 208.333333 {refclk 208.333333 m 99 n 4 lpfd 2 lpd 2 fvco 10312.5} 416.666667 {refclk 416.666667 m 99 n 8 lpfd 2 lpd 2 fvco 10312.5} 51.562500 {refclk 51.562500 m 100 n 1 lpfd 2 lpd 2 fvco 10312.5} 51.051980 {refclk 51.051980 m 101 n 1 lpfd 2 lpd 2 fvco 10312.5} 102.103960 {refclk 102.103960 m 101 n 2 lpfd 2 lpd 2 fvco 10312.5} 204.207921 {refclk 204.207921 m 101 n 4 lpfd 2 lpd 2 fvco 10312.5} 408.415842 {refclk 408.415842 m 101 n 8 lpfd 2 lpd 2 fvco 10312.5} 50.551471 {refclk 50.551471 m 102 n 1 lpfd 2 lpd 2 fvco 10312.5} 50.060680 {refclk 50.060680 m 103 n 1 lpfd 2 lpd 2 fvco 10312.5} 100.121359 {refclk 100.121359 m 103 n 2 lpfd 2 lpd 2 fvco 10312.5} 200.242718 {refclk 200.242718 m 103 n 4 lpfd 2 lpd 2 fvco 10312.5} 400.485437 {refclk 400.485437 m 103 n 8 lpfd 2 lpd 2 fvco 10312.5} 49.579327 {refclk 49.579327 m 104 n 1 lpfd 2 lpd 2 fvco 10312.5} 49.107143 {refclk 49.107143 m 105 n 1 lpfd 2 lpd 2 fvco 10312.5} 98.214286 {refclk 98.214286 m 105 n 2 lpfd 2 lpd 2 fvco 10312.5} 196.428571 {refclk 196.428571 m 105 n 4 lpfd 2 lpd 2 fvco 10312.5} 392.857143 {refclk 392.857143 m 105 n 8 lpfd 2 lpd 2 fvco 10312.5} 48.643868 {refclk 48.643868 m 106 n 1 lpfd 2 lpd 2 fvco 10312.5} 48.189252 {refclk 48.189252 m 107 n 1 lpfd 2 lpd 2 fvco 10312.5} 96.378505 {refclk 96.378505 m 107 n 2 lpfd 2 lpd 2 fvco 10312.5} 192.757009 {refclk 192.757009 m 107 n 4 lpfd 2 lpd 2 fvco 10312.5} 385.514019 {refclk 385.514019 m 107 n 8 lpfd 2 lpd 2 fvco 10312.5} 47.743056 {refclk 47.743056 m 108 n 1 lpfd 2 lpd 2 fvco 10312.5} 47.305046 {refclk 47.305046 m 109 n 1 lpfd 2 lpd 2 fvco 10312.5} 94.610092 {refclk 94.610092 m 109 n 2 lpfd 2 lpd 2 fvco 10312.5} 189.220183 {refclk 189.220183 m 109 n 4 lpfd 2 lpd 2 fvco 10312.5} 378.440367 {refclk 378.440367 m 109 n 8 lpfd 2 lpd 2 fvco 10312.5} 46.875000 {refclk 46.875000 m 110 n 1 lpfd 2 lpd 2 fvco 10312.5} 46.452703 {refclk 46.452703 m 111 n 1 lpfd 2 lpd 2 fvco 10312.5} 92.905405 {refclk 92.905405 m 111 n 2 lpfd 2 lpd 2 fvco 10312.5} 185.810811 {refclk 185.810811 m 111 n 4 lpfd 2 lpd 2 fvco 10312.5} 371.621622 {refclk 371.621622 m 111 n 8 lpfd 2 lpd 2 fvco 10312.5} 46.037946 {refclk 46.037946 m 112 n 1 lpfd 2 lpd 2 fvco 10312.5} 45.630531 {refclk 45.630531 m 113 n 1 lpfd 2 lpd 2 fvco 10312.5} 91.261062 {refclk 91.261062 m 113 n 2 lpfd 2 lpd 2 fvco 10312.5} 182.522124 {refclk 182.522124 m 113 n 4 lpfd 2 lpd 2 fvco 10312.5} 365.044248 {refclk 365.044248 m 113 n 8 lpfd 2 lpd 2 fvco 10312.5} 45.230263 {refclk 45.230263 m 114 n 1 lpfd 2 lpd 2 fvco 10312.5} 44.836957 {refclk 44.836957 m 115 n 1 lpfd 2 lpd 2 fvco 10312.5} 89.673913 {refclk 89.673913 m 115 n 2 lpfd 2 lpd 2 fvco 10312.5} 179.347826 {refclk 179.347826 m 115 n 4 lpfd 2 lpd 2 fvco 10312.5} 358.695652 {refclk 358.695652 m 115 n 8 lpfd 2 lpd 2 fvco 10312.5} 44.450431 {refclk 44.450431 m 116 n 1 lpfd 2 lpd 2 fvco 10312.5} 44.070513 {refclk 44.070513 m 117 n 1 lpfd 2 lpd 2 fvco 10312.5} 88.141026 {refclk 88.141026 m 117 n 2 lpfd 2 lpd 2 fvco 10312.5} 176.282051 {refclk 176.282051 m 117 n 4 lpfd 2 lpd 2 fvco 10312.5} 352.564103 {refclk 352.564103 m 117 n 8 lpfd 2 lpd 2 fvco 10312.5} 43.697034 {refclk 43.697034 m 118 n 1 lpfd 2 lpd 2 fvco 10312.5} 43.329832 {refclk 43.329832 m 119 n 1 lpfd 2 lpd 2 fvco 10312.5} 86.659664 {refclk 86.659664 m 119 n 2 lpfd 2 lpd 2 fvco 10312.5} 173.319328 {refclk 173.319328 m 119 n 4 lpfd 2 lpd 2 fvco 10312.5} 346.638655 {refclk 346.638655 m 119 n 8 lpfd 2 lpd 2 fvco 10312.5} 42.968750 {refclk 42.968750 m 120 n 1 lpfd 2 lpd 2 fvco 10312.5} 42.613636 {refclk 42.613636 m 121 n 1 lpfd 2 lpd 2 fvco 10312.5} 85.227273 {refclk 85.227273 m 121 n 2 lpfd 2 lpd 2 fvco 10312.5} 170.454545 {refclk 170.454545 m 121 n 4 lpfd 2 lpd 2 fvco 10312.5} 340.909091 {refclk 340.909091 m 121 n 8 lpfd 2 lpd 2 fvco 10312.5} 42.264344 {refclk 42.264344 m 122 n 1 lpfd 2 lpd 2 fvco 10312.5} 41.920732 {refclk 41.920732 m 123 n 1 lpfd 2 lpd 2 fvco 10312.5} 83.841463 {refclk 83.841463 m 123 n 2 lpfd 2 lpd 2 fvco 10312.5} 167.682927 {refclk 167.682927 m 123 n 4 lpfd 2 lpd 2 fvco 10312.5} 335.365854 {refclk 335.365854 m 123 n 8 lpfd 2 lpd 2 fvco 10312.5} 41.582661 {refclk 41.582661 m 124 n 1 lpfd 2 lpd 2 fvco 10312.5} 41.250000 {refclk 41.250000 m 125 n 1 lpfd 2 lpd 2 fvco 10312.5} 82.500000 {refclk 82.500000 m 125 n 2 lpfd 2 lpd 2 fvco 10312.5} 165.000000 {refclk 165.000000 m 125 n 4 lpfd 2 lpd 2 fvco 10312.5} 330.000000 {refclk 330.000000 m 125 n 8 lpfd 2 lpd 2 fvco 10312.5} 40.922619 {refclk 40.922619 m 126 n 1 lpfd 2 lpd 2 fvco 10312.5} 40.600394 {refclk 40.600394 m 127 n 1 lpfd 2 lpd 2 fvco 10312.5} 81.200787 {refclk 81.200787 m 127 n 2 lpfd 2 lpd 2 fvco 10312.5} 162.401575 {refclk 162.401575 m 127 n 4 lpfd 2 lpd 2 fvco 10312.5} 324.803150 {refclk 324.803150 m 127 n 8 lpfd 2 lpd 2 fvco 10312.5} allowed_ranges {40.600394 40.922619 41.250000 41.582661 41.920732 42.264344 42.613636 42.968750 43.329832 43.697034 44.070513 44.450431 44.836957 45.230263 45.630531 46.037946 46.452703 46.875000 47.305046 47.743056 48.189252 48.643868 49.107143 49.579327 50.060680 50.551471 51.051980 51.562500 52.083333 52.614796 53.157216 53.710938 54.276316 54.853723 55.443548 56.046196 56.662088 57.291667 57.935393 58.593750 59.267241 59.956395 60.661765 61.383929 62.123494 62.881098 63.657407 64.453125 65.268987 66.105769 66.964286 67.845395 68.750000 69.679054 70.633562 71.614583 72.623239 73.660714 74.728261 75.827206 76.958955 78.125000 79.326923 80.566406 81.200787 81.845238 82.500000 83.165323 83.841463 84.528689 85.227273 85.937500 86.659664 87.394068 88.141026 88.900862 89.673913 90.460526 91.261062 92.075893 92.905405 93.750000 94.610092 95.486111 96.378505 97.287736 98.214286 99.158654 100.121359 101.102941 102.103960 103.125000 104.166667 105.229592 106.314433 107.421875 108.552632 109.707447 110.887097 112.092391 113.324176 114.583333 115.870787 117.187500 118.534483 119.912791 121.323529 122.767857 124.246988 125.762195 127.314815 128.906250 130.537975 132.211538 133.928571 135.690789 137.500000 139.358108 141.267123 143.229167 145.246479 147.321429 149.456522 151.654412 153.917910 156.250000 158.653846 161.132813 162.401575 163.690476 165.000000 166.330645 167.682927 169.057377 170.454545 171.875000 173.319328 174.788136 176.282051 177.801724 179.347826 180.921053 182.522124 184.151786 185.810811 187.500000 189.220183 190.972222 192.757009 194.575472 196.428571 198.317308 200.242718 202.205882 204.207921 206.250000 208.333333 210.459184 212.628866 214.843750 217.105263 219.414894 221.774194 224.184783 226.648352 229.166667 231.741573 234.375000 237.068966 239.825581 242.647059 245.535714 248.493976 251.524390 254.629630 257.812500 261.075949 264.423077 267.857143 271.381579 275.000000 278.716216 282.534247 286.458333 290.492958 294.642857 298.913043 303.308824 307.835821 312.500000 317.307692 322.265625 324.803150 327.380952 330.000000 332.661290 335.365854 338.114754 340.909091 343.750000 346.638655 349.576271 352.564103 355.603448 358.695652 361.842105 365.044248 368.303571 371.621622 375.000000 378.440367 381.944444 385.514019 389.150943 392.857143 396.634615 400.485437 404.411765 408.415842 412.500000 416.666667 420.918367 425.257732 429.687500 434.210526 438.829787 443.548387 448.369565 453.296703 458.333333 463.483146 468.750000 474.137931 479.651163 485.294118 491.071429 496.987952 503.048780 509.259259 515.625000 522.151899 528.846154 535.714286 542.763158 550.000000 557.432432 565.068493 572.916667 580.985915 589.285714 597.826087 606.617647 615.671642 625.000000 634.615385 644.531250 654.761905 665.322581 676.229508 687.500000 699.152542 711.206897 723.684211 736.607143 750.000000 763.888889 778.301887 793.269231}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_pll_settings_key" type="string">
          <ipxact:name>l_pll_settings_key</ipxact:name>
          <ipxact:displayName>l_pll_settings_key</ipxact:displayName>
          <ipxact:value>644.531250</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_std" type="int">
          <ipxact:name>enable_std</ipxact:name>
          <ipxact:displayName>enable_std</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_std_pipe" type="int">
          <ipxact:name>l_enable_std_pipe</ipxact:name>
          <ipxact:displayName>l_enable_std_pipe</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_tx_std" type="int">
          <ipxact:name>l_enable_tx_std</ipxact:name>
          <ipxact:displayName>l_enable_tx_std</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_rx_std" type="int">
          <ipxact:name>l_enable_rx_std</ipxact:name>
          <ipxact:displayName>l_enable_rx_std</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_std_tx_word_count" type="int">
          <ipxact:name>l_std_tx_word_count</ipxact:name>
          <ipxact:displayName>l_std_tx_word_count</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_std_tx_word_width" type="int">
          <ipxact:name>l_std_tx_word_width</ipxact:name>
          <ipxact:displayName>l_std_tx_word_width</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_std_tx_field_width" type="int">
          <ipxact:name>l_std_tx_field_width</ipxact:name>
          <ipxact:displayName>l_std_tx_field_width</ipxact:displayName>
          <ipxact:value>11</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_std_rx_word_count" type="int">
          <ipxact:name>l_std_rx_word_count</ipxact:name>
          <ipxact:displayName>l_std_rx_word_count</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_std_rx_word_width" type="int">
          <ipxact:name>l_std_rx_word_width</ipxact:name>
          <ipxact:displayName>l_std_rx_word_width</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_std_rx_field_width" type="int">
          <ipxact:name>l_std_rx_field_width</ipxact:name>
          <ipxact:displayName>l_std_rx_field_width</ipxact:displayName>
          <ipxact:value>16</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_std_tx_pld_pcs_width" type="int">
          <ipxact:name>l_std_tx_pld_pcs_width</ipxact:name>
          <ipxact:displayName>l_std_tx_pld_pcs_width</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_std_rx_pld_pcs_width" type="int">
          <ipxact:name>l_std_rx_pld_pcs_width</ipxact:name>
          <ipxact:displayName>l_std_rx_pld_pcs_width</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_enh" type="int">
          <ipxact:name>enable_enh</ipxact:name>
          <ipxact:displayName>enable_enh</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_tx_enh" type="int">
          <ipxact:name>l_enable_tx_enh</ipxact:name>
          <ipxact:displayName>l_enable_tx_enh</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_rx_enh" type="int">
          <ipxact:name>l_enable_rx_enh</ipxact:name>
          <ipxact:displayName>l_enable_rx_enh</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_pcs_dir" type="int">
          <ipxact:name>enable_pcs_dir</ipxact:name>
          <ipxact:displayName>enable_pcs_dir</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_tx_pcs_dir" type="int">
          <ipxact:name>l_enable_tx_pcs_dir</ipxact:name>
          <ipxact:displayName>l_enable_tx_pcs_dir</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_enable_rx_pcs_dir" type="int">
          <ipxact:name>l_enable_rx_pcs_dir</ipxact:name>
          <ipxact:displayName>l_enable_rx_pcs_dir</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_rcfg_ifaces" type="int">
          <ipxact:name>l_rcfg_ifaces</ipxact:name>
          <ipxact:displayName>l_rcfg_ifaces</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_rcfg_addr_bits" type="int">
          <ipxact:name>l_rcfg_addr_bits</ipxact:name>
          <ipxact:displayName>l_rcfg_addr_bits</ipxact:displayName>
          <ipxact:value>11</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ovrd_tx_dv_mode" type="int">
          <ipxact:name>ovrd_tx_dv_mode</ipxact:name>
          <ipxact:displayName>Enable TX Data Valid Gen manual setting</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="usr_tx_dv_mode" type="string">
          <ipxact:name>usr_tx_dv_mode</ipxact:name>
          <ipxact:displayName>Generate TX Data Valid by Core AIB FIFO</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ovrd_rx_dv_mode" type="int">
          <ipxact:name>ovrd_rx_dv_mode</ipxact:name>
          <ipxact:displayName>Enable RX Data Valid Rcv manual setting</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="usr_rx_dv_mode" type="string">
          <ipxact:name>usr_rx_dv_mode</ipxact:name>
          <ipxact:displayName>Consume RX Data Valid by Core AIB FIFO</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_shared" type="int">
          <ipxact:name>rcfg_shared</ipxact:name>
          <ipxact:displayName>Share reconfiguration interface</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rcfg_use_clk_reset_only" type="int">
          <ipxact:name>rcfg_use_clk_reset_only</ipxact:name>
          <ipxact:displayName>Use AVMM clock and reset ports only</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="adme_prot_mode" type="string">
          <ipxact:name>adme_prot_mode</ipxact:name>
          <ipxact:displayName>adme_prot_mode</ipxact:displayName>
          <ipxact:value>teng_1588_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="adme_pma_mode" type="string">
          <ipxact:name>adme_pma_mode</ipxact:name>
          <ipxact:displayName>adme_pma_mode</ipxact:displayName>
          <ipxact:value>basic</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="adme_tx_power_mode" type="string">
          <ipxact:name>adme_tx_power_mode</ipxact:name>
          <ipxact:displayName>adme_tx_power_mode</ipxact:displayName>
          <ipxact:value>mid_power</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="adme_data_rate" type="string">
          <ipxact:name>adme_data_rate</ipxact:name>
          <ipxact:displayName>adme_data_rate</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="adme_enable_bg_cal" type="string">
          <ipxact:name>adme_enable_bg_cal</ipxact:name>
          <ipxact:displayName>adme_enable_bg_cal</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_embedded_debug_enable" type="int">
          <ipxact:name>set_embedded_debug_enable</ipxact:name>
          <ipxact:displayName>Enable embedded debug</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_prbs_soft_logic_enable" type="int">
          <ipxact:name>set_prbs_soft_logic_enable</ipxact:name>
          <ipxact:displayName>Enable prbs soft accumulators</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="set_odi_soft_logic_enable" type="int">
          <ipxact:name>set_odi_soft_logic_enable</ipxact:name>
          <ipxact:displayName>Enable odi acceleration logic</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dbg_prbs_soft_logic_enable" type="int">
          <ipxact:name>dbg_prbs_soft_logic_enable</ipxact:name>
          <ipxact:displayName>dbg_prbs_soft_logic_enable</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dbg_odi_soft_logic_enable" type="int">
          <ipxact:name>dbg_odi_soft_logic_enable</ipxact:name>
          <ipxact:displayName>dbg_odi_soft_logic_enable</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_rcfg_datapath_message" type="int">
          <ipxact:name>l_rcfg_datapath_message</ipxact:name>
          <ipxact:displayName>l_rcfg_datapath_message</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_rcfg_tx_digitalreset_release_ctrl" type="int">
          <ipxact:name>enable_rcfg_tx_digitalreset_release_ctrl</ipxact:name>
          <ipxact:displayName>Enable rcfg_tx_digitalreset_release_ctrl port</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cannot_gen_exdesign_msg" type="string">
          <ipxact:name>cannot_gen_exdesign_msg</ipxact:name>
          <ipxact:displayName>cannot_gen_exdesign_msg</ipxact:displayName>
          <ipxact:value>Design example cannot be generated for the current configuration. Please check under Design Example tab and system message below for more detailed information.</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cannot_gen_exdesign_gen_msg" type="string">
          <ipxact:name>cannot_gen_exdesign_gen_msg</ipxact:name>
          <ipxact:displayName>cannot_gen_exdesign_gen_msg</ipxact:displayName>
          <ipxact:value>A design example is not available for current transceiver configuration rule. (Transceiver configuration rules:"&lt;b&gt;"10GBASE-R 1588"&lt;/b&gt; (teng_1588_mode)")</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cannot_gen_exdesign_prot_msg" type="string">
          <ipxact:name>cannot_gen_exdesign_prot_msg</ipxact:name>
          <ipxact:displayName>cannot_gen_exdesign_prot_msg</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="can_gen_exdesign_basic_std" type="int">
          <ipxact:name>can_gen_exdesign_basic_std</ipxact:name>
          <ipxact:displayName>can_gen_exdesign_basic_std</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="can_gen_exdesign_basic_enh" type="int">
          <ipxact:name>can_gen_exdesign_basic_enh</ipxact:name>
          <ipxact:displayName>can_gen_exdesign_basic_enh</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="can_gen_exdesign_pcs_direct" type="int">
          <ipxact:name>can_gen_exdesign_pcs_direct</ipxact:name>
          <ipxact:displayName>can_gen_exdesign_pcs_direct</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="can_gen_exdesign_pcie_pipe" type="int">
          <ipxact:name>can_gen_exdesign_pcie_pipe</ipxact:name>
          <ipxact:displayName>can_gen_exdesign_pcie_pipe</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="can_gen_exdesign_cpri_auto" type="int">
          <ipxact:name>can_gen_exdesign_cpri_auto</ipxact:name>
          <ipxact:displayName>can_gen_exdesign_cpri_auto</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="suppress_design_example_messages" type="int">
          <ipxact:name>suppress_design_example_messages</ipxact:name>
          <ipxact:displayName>suppress_design_example_messages</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_workaround_rules" type="int">
          <ipxact:name>enable_workaround_rules</ipxact:name>
          <ipxact:displayName>Enable workaround rules</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pll_type" type="string">
          <ipxact:name>tx_pll_type</ipxact:name>
          <ipxact:displayName>Tx PLL type</ipxact:displayName>
          <ipxact:value>ATX</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="design_example_tx_pll_kind" type="string">
          <ipxact:name>design_example_tx_pll_kind</ipxact:name>
          <ipxact:displayName>Tx PLL kind</ipxact:displayName>
          <ipxact:value>altera_xcvr_atx_pll_s10_htile</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pll_refclk" type="real">
          <ipxact:name>tx_pll_refclk</ipxact:name>
          <ipxact:displayName>Tx PLL reference clock frequency</ipxact:displayName>
          <ipxact:value>644.53125</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="use_tx_clkout2" type="int">
          <ipxact:name>use_tx_clkout2</ipxact:name>
          <ipxact:displayName>Use tx_clkout2 as source for tx_coreclkin</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="use_rx_clkout2" type="int">
          <ipxact:name>use_rx_clkout2</ipxact:name>
          <ipxact:displayName>Use rx_clkout2 as source for rx_coreclkin</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_de_hardware_debug" type="int">
          <ipxact:name>enable_de_hardware_debug</ipxact:name>
          <ipxact:displayName>Enable soft register map for System Console</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="lcl_enable_fast_sim_option" type="int">
          <ipxact:name>lcl_enable_fast_sim_option</ipxact:name>
          <ipxact:displayName>lcl_enable_fast_sim_option</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_fast_sim" type="int">
          <ipxact:name>enable_fast_sim</ipxact:name>
          <ipxact:displayName>Enable fast simulations</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_mac_total_control" type="int">
          <ipxact:name>enable_mac_total_control</ipxact:name>
          <ipxact:displayName>Enable MAC total control of PHY settings</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_insert_eios_err" type="int">
          <ipxact:name>enable_insert_eios_err</ipxact:name>
          <ipxact:displayName>Enable PCIe EIOS error insertion</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tile_type_suffix" type="string">
          <ipxact:name>tile_type_suffix</ipxact:name>
          <ipxact:displayName>Xcvr Tile Type Suffix</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="design_example_filename" type="string">
          <ipxact:name>design_example_filename</ipxact:name>
          <ipxact:displayName>Design example filename</ipxact:displayName>
          <ipxact:value>top</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="anlg_voltage" type="string">
          <ipxact:name>anlg_voltage</ipxact:name>
          <ipxact:displayName>VCCR_GXB and VCCT_GXB supply voltage for the Transceiver</ipxact:displayName>
          <ipxact:value>1_0V</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="anlg_link" type="string">
          <ipxact:name>anlg_link</ipxact:name>
          <ipxact:displayName>Tranceiver Link Type</ipxact:displayName>
          <ipxact:value>sr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_ports_adaptation" type="int">
          <ipxact:name>enable_ports_adaptation</ipxact:name>
          <ipxact:displayName>Enable adaptation control ports</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="qsf_assignments_enable" type="int">
          <ipxact:name>qsf_assignments_enable</ipxact:name>
          <ipxact:displayName>Provide sample QSF assignments</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="qsf_assignments_list" type="string">
          <ipxact:name>qsf_assignments_list</ipxact:name>
          <ipxact:displayName>Sample QSF Assignments</ipxact:displayName>
          <ipxact:value># These QSF assignments are provided for your reference.,# Normally you do not need these assignments. The IP will,# make these settings for you. Refer to the user guide for,# scenarios where you might want to override default IP settings.,# Replace your pin names in the pin lists below.,set tx_pin_list { &lt;tx_pin_0&gt; &lt;tx_pin_1&gt; },set rx_pin_list { &lt;rx_pin_0&gt; &lt;rx_pin_1&gt; },# TX pin assignments,foreach tx_pin $tx_pin_list {,set_instance_assignment -name HSSI_PARAMETER "cdr_pll_power_mode=mid_power" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_pm_cr2_rx_path_pma_rx_divclk_hz=322265625" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_power_mode=mid_power" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_pm_cr2_rx_path_power_mode=mid_power" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_pm_cr2_rx_path_power_rail_er=1030" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_sel_vcm_ctle=vocm_eq_gndref" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_vcm_sel=vcm_l1" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_vcm_sel_vccref=5" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_power_mode=mid_power" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_odi_power_mode=mid_power" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_sd_power_mode=mid_power" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pm_cr2_tx_path_pma_tx_divclk_hz=322265625" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pm_cr2_tx_path_power_mode=mid_power" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pm_cr2_tx_path_power_rail_et=1030" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_uc_vcc_setting=vcc_setting1" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_power_rail_er=1030" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_powermode_ac_cgb=cgb_ac_off" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_powermode_dc_cgb=powerdown_cgb" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_uc_vcc_setting=vcc_setting1" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_ser_power_rail_er=1030" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_ser_powermode_ac_ser=ac_clk_divtx_user_0_jitcomp1p0" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_ser_powermode_dc_ser=dc_clk_divtx_user_0_jitcomp1p0" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_ser_uc_vcc_setting=vcc_setting1" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pm_cr2_tx_path_analog_mode=user_custom" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_compensation_en=enable" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_compensation_posttap_en=disable" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_cpen_ctrl=cp_l1" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pm_cr2_tx_path_datarate_bps=10312500000" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pm_cr2_tx_path_gt_enabled=disable" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_link=link_off" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pm_cr2_tx_path_link=sr" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_optimal=true" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pm_cr2_tx_path_optimal=true" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_powermode_ac_post_tap=tx_post_tap_ac_off" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_powermode_ac_pre_tap=tx_pre_tap_ac_off" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_powermode_ac_tx_vod_no_jitcomp=tx_vod_no_jitcomp_ac_l0" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_powermode_ac_tx_vod_w_jitcomp=tx_vod_w_jitcomp_ac_l31" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_powermode_dc_post_tap=powerdown_tx_post_tap" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_powermode_dc_pre_tap=powerdown_tx_pre_tap" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_powermode_dc_tx_vod_no_jitcomp=powerdown_tx_vod_no_jitcomp" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_powermode_dc_tx_vod_w_jitcomp=tx_vod_w_jitcomp_dc_l31" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pre_emp_sign_1st_post_tap=fir_post_1t_neg" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pre_emp_sign_pre_tap_1t=fir_pre_1t_neg" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pre_emp_switching_ctrl_1st_post_tap=0" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pre_emp_switching_ctrl_pre_tap_1t=0" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_slew_rate_ctrl=slew_r5" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_term_sel=r_r1" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_vod_output_swing_ctrl=31" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_vreg_output=vccdreg_nominal" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_bitslip_enable=disable_bitslip" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_datarate_bps=10312500000" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_uc_cgb_vreg_boost=no_voltage_boost" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_x1_clock_source_sel=lcpll_top" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_x1_div_m_sel=divbypass" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_ser_ser_clk_divtx_user_sel=divtx_user_off" -to ${tx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_sequencer_tx_path_rstn_overrideb=use_sequencer" -to ${tx_pin},},# RX pin assignments,foreach rx_pin $rx_pin_list {,set_instance_assignment -name HSSI_PARAMETER "cdr_pll_power_mode=mid_power" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_pm_cr2_rx_path_pma_rx_divclk_hz=322265625" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_power_mode=mid_power" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_pm_cr2_rx_path_power_mode=mid_power" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_pm_cr2_rx_path_power_rail_er=1030" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_sel_vcm_ctle=vocm_eq_gndref" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_vcm_sel=vcm_l1" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_vcm_sel_vccref=5" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_power_mode=mid_power" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_odi_power_mode=mid_power" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_sd_power_mode=mid_power" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pm_cr2_tx_path_pma_tx_divclk_hz=322265625" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pm_cr2_tx_path_power_mode=mid_power" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_pm_cr2_tx_path_power_rail_et=1030" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_buf_uc_vcc_setting=vcc_setting1" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_power_rail_er=1030" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_powermode_ac_cgb=cgb_ac_off" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_powermode_dc_cgb=powerdown_cgb" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_cgb_uc_vcc_setting=vcc_setting1" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_ser_power_rail_er=1030" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_ser_powermode_ac_ser=ac_clk_divtx_user_0_jitcomp1p0" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_ser_powermode_dc_ser=dc_clk_divtx_user_0_jitcomp1p0" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_tx_ser_uc_vcc_setting=vcc_setting1" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adapt_mode=manual" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_ac_ctle_en=radp_ac_ctle_en_disable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_ac_ctle_hold_en=radp_ac_ctle_hold_en_not_hold" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_ac_ctle_initial_value=radp_ac_ctle_initial_value_8" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_ac_ctle_mode_sel=radp_ac_ctle_mode_sel_concurrent" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_ctle_bypass_ac=radp_ctle_bypass_ac_bypass" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_ctle_bypass_dc=radp_ctle_bypass_dc_bypass" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dc_ctle_en=radp_dc_ctle_en_disable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dc_ctle_mode0_win_size=radp_dc_ctle_mode0_win_size_4_taps" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dc_ctle_mode0_win_start=0" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dc_ctle_mode2_h2_limit=7" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dc_ctle_mode_sel=radp_dc_ctle_mode_sel_mode_2" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dc_ctle_onetime=radp_dc_ctle_onetime_disable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dfe_en=radp_dfe_en_disable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dfe_fxtap_bypass=radp_dfe_fxtap_bypass_bypass" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dfe_hold_sel=radp_dfe_hold_sel_no" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dfe_tap1_initial_value=radp_dfe_tap1_initial_value_0" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dfe_tap_sel_en=radp_dfe_tap_sel_en_no" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dlev_bypass=radp_dlev_bypass_bypass" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_dlev_en=radp_dlev_en_disable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_vga_bypass=radp_vga_bypass_bypass" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_vga_ctle_low_limit=radp_vga_ctle_low_limit_0" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_vga_dlev_target=15" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_adp_vga_en=radp_vga_en_disable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_optimal=true" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_powermode_ac_adaptation=adapt_ac_off" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_powermode_ac_deser_adapt=adapt_deser_ac_off" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_powermode_ac_dfe_adapt=adapt_dfe_ac_off" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_powermode_dc_adaptation=powerdown_adapt" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_powermode_dc_deser_adapt=powerdown_adapt_deser" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_adapt_powermode_dc_dfe_adapt=powerdown_adapt_dfe" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "cdr_pll_analog_mode=user_custom" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "cdr_pll_bypass_a_edge=bypass_a_edge_off" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "cdr_pll_optimal=true" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_pm_cr2_rx_path_analog_mode=user_custom" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_ctle_ac_gain=0" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_ctle_eq_gain=0" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_ctle_rf_cal=3" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_pm_cr2_rx_path_datarate_bps=10312500000" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_pm_cr2_rx_path_gt_enabled=disable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_link=link_off" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_pm_cr2_rx_path_link=sr" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_optimal=true" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_pm_cr2_rx_path_optimal=true" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_rx_ltr_load_init=rx_load_original" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_term_sel=r_r4" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_vga_dc_gain=0" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_buf_vga_ib_max_en=vga_ib_max_disable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_deser_datarate_bps=10312500000" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_deser_optimal=true" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_datarate_bps=10312500000" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_dfe_mode=cdr_mode" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_latch_xcouple_disable=latch_xcouple_enable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_optimal=true" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_pdb_edge_pre_h1=cdr_pre_h1_enable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_pdb_edge_pst_h1=cdr_pst_h1_disable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_pdb_tap_10t15=tap10t15_dfe_powerdown" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_pdb_tap_4t9=tap4t9_dfe_powerdown" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_pdb_tapsum=tapsum_disable" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_powermode_ac_dfe=ac_cdr_mode" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_powermode_dc_dfe=powerdown_dfe" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_dfe_tapsum_bw_sel=tapsum_medbw" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_odi_datarate_bps=10312500000" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_odi_monitor_bw_sel=bw_4" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_odi_optimal=true" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_odi_xrx_path_x119_rx_path_rstn_overrideb=use_sequencer" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_odi_vreg_voltage_sel=vreg0" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_sd_link=sr" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_sd_optimal=true" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_rx_sd_sd_threshold=sdlv_3" -to ${rx_pin},set_instance_assignment -name HSSI_PARAMETER "pma_reset_sequencer_rx_path_rstn_overrideb=use_sequencer" -to ${rx_pin},}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="enable_backup_pma_adapt_modes" type="int">
          <ipxact:name>enable_backup_pma_adapt_modes</ipxact:name>
          <ipxact:displayName>enable_backup_pma_adapt_modes</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_analog_mode" type="string">
          <ipxact:name>tx_pma_analog_mode</ipxact:name>
          <ipxact:displayName>TX PMA analog mode rules</ipxact:displayName>
          <ipxact:value>user_custom</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_pma_analog_mode" type="string">
          <ipxact:name>rx_pma_analog_mode</ipxact:name>
          <ipxact:displayName>RX PMA analog mode rules</ipxact:displayName>
          <ipxact:value>user_custom</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_optimal_settings" type="int">
          <ipxact:name>tx_pma_optimal_settings</ipxact:name>
          <ipxact:displayName>Use default TX PMA analog settings</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_tx_pma_optimal_settings" type="string">
          <ipxact:name>l_tx_pma_optimal_settings</ipxact:name>
          <ipxact:displayName>l_tx_pma_optimal_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_tx_pma_optimal_atom_settings" type="string">
          <ipxact:name>l_tx_pma_optimal_atom_settings</ipxact:name>
          <ipxact:displayName>l_tx_pma_optimal_atom_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_output_swing_ctrl" type="int">
          <ipxact:name>tx_pma_output_swing_ctrl</ipxact:name>
          <ipxact:displayName>Output Swing Level (VOD)</ipxact:displayName>
          <ipxact:value>12</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_pre_emp_sign_pre_tap_1t" type="string">
          <ipxact:name>tx_pma_pre_emp_sign_pre_tap_1t</ipxact:name>
          <ipxact:displayName>Pre-Emphasis First Pre-Tap Polarity</ipxact:displayName>
          <ipxact:value>negative</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_pre_emp_switching_ctrl_pre_tap_1t" type="int">
          <ipxact:name>tx_pma_pre_emp_switching_ctrl_pre_tap_1t</ipxact:name>
          <ipxact:displayName>Pre-Emphasis First Pre-Tap Magnitude</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_pre_emp_sign_1st_post_tap" type="string">
          <ipxact:name>tx_pma_pre_emp_sign_1st_post_tap</ipxact:name>
          <ipxact:displayName>Pre-Emphasis First Post-Tap Polarity</ipxact:displayName>
          <ipxact:value>negative</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_pre_emp_switching_ctrl_1st_post_tap" type="int">
          <ipxact:name>tx_pma_pre_emp_switching_ctrl_1st_post_tap</ipxact:name>
          <ipxact:displayName>Pre-Emphasis First Post-Tap Magnitude</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_output_swing_message" type="string">
          <ipxact:name>tx_output_swing_message</ipxact:name>
          <ipxact:displayName>tx_output_swing_message</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_slew_rate_ctrl" type="int">
          <ipxact:name>tx_pma_slew_rate_ctrl</ipxact:name>
          <ipxact:displayName>Slew Rate Control</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_term_sel" type="string">
          <ipxact:name>tx_pma_term_sel</ipxact:name>
          <ipxact:displayName>On-Chip Termination</ipxact:displayName>
          <ipxact:value>r_r1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="tx_pma_compensation_en" type="string">
          <ipxact:name>tx_pma_compensation_en</ipxact:name>
          <ipxact:displayName>High Speed Compensation</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_pma_optimal_settings" type="int">
          <ipxact:name>rx_pma_optimal_settings</ipxact:name>
          <ipxact:displayName>Use default RX PMA analog settings</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_rx_pma_optimal_settings" type="string">
          <ipxact:name>l_rx_pma_optimal_settings</ipxact:name>
          <ipxact:displayName>l_rx_pma_optimal_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_adapt_mode_manual" type="int">
          <ipxact:name>l_adapt_mode_manual</ipxact:name>
          <ipxact:displayName>l_adapt_mode_manual</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="l_adapt_mode_dfe" type="int">
          <ipxact:name>l_adapt_mode_dfe</ipxact:name>
          <ipxact:displayName>l_adapt_mode_dfe</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_pma_adapt_mode" type="string">
          <ipxact:name>rx_pma_adapt_mode</ipxact:name>
          <ipxact:displayName>RX adaptation mode</ipxact:displayName>
          <ipxact:value>manual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_pma_term_sel" type="string">
          <ipxact:name>rx_pma_term_sel</ipxact:name>
          <ipxact:displayName>RX On-chip Termination</ipxact:displayName>
          <ipxact:value>r_r2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_ctle_ac_gain" type="int">
          <ipxact:name>rx_ctle_ac_gain</ipxact:name>
          <ipxact:displayName>CTLE AC Gain</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_ctle_eq_gain" type="int">
          <ipxact:name>rx_ctle_eq_gain</ipxact:name>
          <ipxact:displayName>CTLE EQ Gain</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="rx_vga_dc_gain" type="int">
          <ipxact:name>rx_vga_dc_gain</ipxact:name>
          <ipxact:displayName>VGA DC Gain</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_advanced_user_mode" type="string">
          <ipxact:name>hssi_10g_rx_pcs_advanced_user_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_advanced_user_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_align_del" type="string">
          <ipxact:name>hssi_10g_rx_pcs_align_del</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_align_del</ipxact:displayName>
          <ipxact:value>align_del_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_ber_bit_err_total_cnt" type="string">
          <ipxact:name>hssi_10g_rx_pcs_ber_bit_err_total_cnt</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_ber_bit_err_total_cnt</ipxact:displayName>
          <ipxact:value>bit_err_total_cnt_10g</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_ber_clken" type="string">
          <ipxact:name>hssi_10g_rx_pcs_ber_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_ber_clken</ipxact:displayName>
          <ipxact:value>ber_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_ber_xus_timer_window" type="int">
          <ipxact:name>hssi_10g_rx_pcs_ber_xus_timer_window</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_ber_xus_timer_window</ipxact:displayName>
          <ipxact:value>19530</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_bitslip_mode" type="string">
          <ipxact:name>hssi_10g_rx_pcs_bitslip_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_bitslip_mode</ipxact:displayName>
          <ipxact:value>bitslip_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_blksync_bitslip_type" type="string">
          <ipxact:name>hssi_10g_rx_pcs_blksync_bitslip_type</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_blksync_bitslip_type</ipxact:displayName>
          <ipxact:value>bitslip_comb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_blksync_bitslip_wait_cnt" type="int">
          <ipxact:name>hssi_10g_rx_pcs_blksync_bitslip_wait_cnt</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_blksync_bitslip_wait_cnt</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_blksync_bitslip_wait_type" type="string">
          <ipxact:name>hssi_10g_rx_pcs_blksync_bitslip_wait_type</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_blksync_bitslip_wait_type</ipxact:displayName>
          <ipxact:value>bitslip_cnt</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_blksync_bypass" type="string">
          <ipxact:name>hssi_10g_rx_pcs_blksync_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_blksync_bypass</ipxact:displayName>
          <ipxact:value>blksync_bypass_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_blksync_clken" type="string">
          <ipxact:name>hssi_10g_rx_pcs_blksync_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_blksync_clken</ipxact:displayName>
          <ipxact:value>blksync_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_blksync_enum_invalid_sh_cnt" type="string">
          <ipxact:name>hssi_10g_rx_pcs_blksync_enum_invalid_sh_cnt</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_blksync_enum_invalid_sh_cnt</ipxact:displayName>
          <ipxact:value>enum_invalid_sh_cnt_10g</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_blksync_knum_sh_cnt_postlock" type="string">
          <ipxact:name>hssi_10g_rx_pcs_blksync_knum_sh_cnt_postlock</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_blksync_knum_sh_cnt_postlock</ipxact:displayName>
          <ipxact:value>knum_sh_cnt_postlock_10g</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_blksync_knum_sh_cnt_prelock" type="string">
          <ipxact:name>hssi_10g_rx_pcs_blksync_knum_sh_cnt_prelock</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_blksync_knum_sh_cnt_prelock</ipxact:displayName>
          <ipxact:value>knum_sh_cnt_prelock_10g</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_blksync_pipeln" type="string">
          <ipxact:name>hssi_10g_rx_pcs_blksync_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_blksync_pipeln</ipxact:displayName>
          <ipxact:value>blksync_pipeln_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_clr_errblk_cnt_en" type="string">
          <ipxact:name>hssi_10g_rx_pcs_clr_errblk_cnt_en</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_clr_errblk_cnt_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_control_del" type="string">
          <ipxact:name>hssi_10g_rx_pcs_control_del</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_control_del</ipxact:displayName>
          <ipxact:value>control_del_none</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_crcchk_bypass" type="string">
          <ipxact:name>hssi_10g_rx_pcs_crcchk_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_crcchk_bypass</ipxact:displayName>
          <ipxact:value>crcchk_bypass_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_crcchk_clken" type="string">
          <ipxact:name>hssi_10g_rx_pcs_crcchk_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_crcchk_clken</ipxact:displayName>
          <ipxact:value>crcchk_clk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_crcchk_inv" type="string">
          <ipxact:name>hssi_10g_rx_pcs_crcchk_inv</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_crcchk_inv</ipxact:displayName>
          <ipxact:value>crcchk_inv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_crcchk_pipeln" type="string">
          <ipxact:name>hssi_10g_rx_pcs_crcchk_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_crcchk_pipeln</ipxact:displayName>
          <ipxact:value>crcchk_pipeln_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_crcflag_pipeln" type="string">
          <ipxact:name>hssi_10g_rx_pcs_crcflag_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_crcflag_pipeln</ipxact:displayName>
          <ipxact:value>crcflag_pipeln_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_ctrl_bit_reverse" type="string">
          <ipxact:name>hssi_10g_rx_pcs_ctrl_bit_reverse</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_ctrl_bit_reverse</ipxact:displayName>
          <ipxact:value>ctrl_bit_reverse_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_data_bit_reverse" type="string">
          <ipxact:name>hssi_10g_rx_pcs_data_bit_reverse</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_data_bit_reverse</ipxact:displayName>
          <ipxact:value>data_bit_reverse_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_dec64b66b_clken" type="string">
          <ipxact:name>hssi_10g_rx_pcs_dec64b66b_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_dec64b66b_clken</ipxact:displayName>
          <ipxact:value>dec64b66b_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_dec_64b66b_rxsm_bypass" type="string">
          <ipxact:name>hssi_10g_rx_pcs_dec_64b66b_rxsm_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_dec_64b66b_rxsm_bypass</ipxact:displayName>
          <ipxact:value>dec_64b66b_rxsm_bypass_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_descrm_bypass" type="string">
          <ipxact:name>hssi_10g_rx_pcs_descrm_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_descrm_bypass</ipxact:displayName>
          <ipxact:value>descrm_bypass_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_descrm_clken" type="string">
          <ipxact:name>hssi_10g_rx_pcs_descrm_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_descrm_clken</ipxact:displayName>
          <ipxact:value>descrm_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_descrm_mode" type="string">
          <ipxact:name>hssi_10g_rx_pcs_descrm_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_descrm_mode</ipxact:displayName>
          <ipxact:value>async</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_descrm_pipeln" type="string">
          <ipxact:name>hssi_10g_rx_pcs_descrm_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_descrm_pipeln</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_dft_clk_out_sel" type="string">
          <ipxact:name>hssi_10g_rx_pcs_dft_clk_out_sel</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_dft_clk_out_sel</ipxact:displayName>
          <ipxact:value>rx_master_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_dis_signal_ok" type="string">
          <ipxact:name>hssi_10g_rx_pcs_dis_signal_ok</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_dis_signal_ok</ipxact:displayName>
          <ipxact:value>dis_signal_ok_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_dispchk_bypass" type="string">
          <ipxact:name>hssi_10g_rx_pcs_dispchk_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_dispchk_bypass</ipxact:displayName>
          <ipxact:value>dispchk_bypass_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_empty_flag_type" type="string">
          <ipxact:name>hssi_10g_rx_pcs_empty_flag_type</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_empty_flag_type</ipxact:displayName>
          <ipxact:value>empty_rd_side</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_fast_path" type="string">
          <ipxact:name>hssi_10g_rx_pcs_fast_path</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_fast_path</ipxact:displayName>
          <ipxact:value>fast_path_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_fec_clken" type="string">
          <ipxact:name>hssi_10g_rx_pcs_fec_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_fec_clken</ipxact:displayName>
          <ipxact:value>fec_clk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_fec_enable" type="string">
          <ipxact:name>hssi_10g_rx_pcs_fec_enable</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_fec_enable</ipxact:displayName>
          <ipxact:value>fec_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_fifo_double_read" type="string">
          <ipxact:name>hssi_10g_rx_pcs_fifo_double_read</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_fifo_double_read</ipxact:displayName>
          <ipxact:value>fifo_double_read_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_fifo_stop_rd" type="string">
          <ipxact:name>hssi_10g_rx_pcs_fifo_stop_rd</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_fifo_stop_rd</ipxact:displayName>
          <ipxact:value>n_rd_empty</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_fifo_stop_wr" type="string">
          <ipxact:name>hssi_10g_rx_pcs_fifo_stop_wr</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_fifo_stop_wr</ipxact:displayName>
          <ipxact:value>n_wr_full</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_force_align" type="string">
          <ipxact:name>hssi_10g_rx_pcs_force_align</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_force_align</ipxact:displayName>
          <ipxact:value>force_align_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_frmsync_bypass" type="string">
          <ipxact:name>hssi_10g_rx_pcs_frmsync_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_frmsync_bypass</ipxact:displayName>
          <ipxact:value>frmsync_bypass_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_frmsync_clken" type="string">
          <ipxact:name>hssi_10g_rx_pcs_frmsync_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_frmsync_clken</ipxact:displayName>
          <ipxact:value>frmsync_clk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_frmsync_enum_scrm" type="string">
          <ipxact:name>hssi_10g_rx_pcs_frmsync_enum_scrm</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_frmsync_enum_scrm</ipxact:displayName>
          <ipxact:value>enum_scrm_default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_frmsync_enum_sync" type="string">
          <ipxact:name>hssi_10g_rx_pcs_frmsync_enum_sync</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_frmsync_enum_sync</ipxact:displayName>
          <ipxact:value>enum_sync_default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_frmsync_flag_type" type="string">
          <ipxact:name>hssi_10g_rx_pcs_frmsync_flag_type</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_frmsync_flag_type</ipxact:displayName>
          <ipxact:value>location_only</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_frmsync_knum_sync" type="string">
          <ipxact:name>hssi_10g_rx_pcs_frmsync_knum_sync</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_frmsync_knum_sync</ipxact:displayName>
          <ipxact:value>knum_sync_default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_frmsync_mfrm_length" type="int">
          <ipxact:name>hssi_10g_rx_pcs_frmsync_mfrm_length</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_frmsync_mfrm_length</ipxact:displayName>
          <ipxact:value>2048</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_frmsync_pipeln" type="string">
          <ipxact:name>hssi_10g_rx_pcs_frmsync_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_frmsync_pipeln</ipxact:displayName>
          <ipxact:value>frmsync_pipeln_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_full_flag_type" type="string">
          <ipxact:name>hssi_10g_rx_pcs_full_flag_type</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_full_flag_type</ipxact:displayName>
          <ipxact:value>full_wr_side</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_gb_rx_idwidth" type="string">
          <ipxact:name>hssi_10g_rx_pcs_gb_rx_idwidth</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_gb_rx_idwidth</ipxact:displayName>
          <ipxact:value>idwidth_32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_gb_rx_odwidth" type="string">
          <ipxact:name>hssi_10g_rx_pcs_gb_rx_odwidth</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_gb_rx_odwidth</ipxact:displayName>
          <ipxact:value>odwidth_66</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_gbexp_clken" type="string">
          <ipxact:name>hssi_10g_rx_pcs_gbexp_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_gbexp_clken</ipxact:displayName>
          <ipxact:value>gbexp_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_low_latency_en" type="string">
          <ipxact:name>hssi_10g_rx_pcs_low_latency_en</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_low_latency_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_lpbk_mode" type="string">
          <ipxact:name>hssi_10g_rx_pcs_lpbk_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_lpbk_mode</ipxact:displayName>
          <ipxact:value>lpbk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_master_clk_sel" type="string">
          <ipxact:name>hssi_10g_rx_pcs_master_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_master_clk_sel</ipxact:displayName>
          <ipxact:value>master_rx_pma_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_pempty_flag_type" type="string">
          <ipxact:name>hssi_10g_rx_pcs_pempty_flag_type</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_pempty_flag_type</ipxact:displayName>
          <ipxact:value>pempty_rd_side</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_pfull_flag_type" type="string">
          <ipxact:name>hssi_10g_rx_pcs_pfull_flag_type</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_pfull_flag_type</ipxact:displayName>
          <ipxact:value>pfull_wr_side</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_phcomp_rd_del" type="string">
          <ipxact:name>hssi_10g_rx_pcs_phcomp_rd_del</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_phcomp_rd_del</ipxact:displayName>
          <ipxact:value>phcomp_rd_del2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_pld_if_type" type="string">
          <ipxact:name>hssi_10g_rx_pcs_pld_if_type</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_pld_if_type</ipxact:displayName>
          <ipxact:value>reg</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_prot_mode" type="string">
          <ipxact:name>hssi_10g_rx_pcs_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_prot_mode</ipxact:displayName>
          <ipxact:value>teng_1588_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rand_clken" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rand_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rand_clken</ipxact:displayName>
          <ipxact:value>rand_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rd_clk_sel" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rd_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rd_clk_sel</ipxact:displayName>
          <ipxact:value>rd_rx_pma_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rdfifo_clken" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rdfifo_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rdfifo_clken</ipxact:displayName>
          <ipxact:value>rdfifo_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rx_fifo_write_ctrl" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rx_fifo_write_ctrl</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rx_fifo_write_ctrl</ipxact:displayName>
          <ipxact:value>blklock_stops</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rx_scrm_width" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rx_scrm_width</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rx_scrm_width</ipxact:displayName>
          <ipxact:value>bit64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rx_sh_location" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rx_sh_location</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rx_sh_location</ipxact:displayName>
          <ipxact:value>lsb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rx_signal_ok_sel" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rx_signal_ok_sel</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rx_signal_ok_sel</ipxact:displayName>
          <ipxact:value>synchronized_ver</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rx_sm_bypass" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rx_sm_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rx_sm_bypass</ipxact:displayName>
          <ipxact:value>rx_sm_bypass_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rx_sm_hiber" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rx_sm_hiber</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rx_sm_hiber</ipxact:displayName>
          <ipxact:value>rx_sm_hiber_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rx_sm_pipeln" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rx_sm_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rx_sm_pipeln</ipxact:displayName>
          <ipxact:value>rx_sm_pipeln_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rx_testbus_sel" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rx_testbus_sel</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rx_testbus_sel</ipxact:displayName>
          <ipxact:value>rx_fifo_testbus1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rx_true_b2b" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rx_true_b2b</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rx_true_b2b</ipxact:displayName>
          <ipxact:value>b2b</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rxfifo_empty" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rxfifo_empty</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rxfifo_empty</ipxact:displayName>
          <ipxact:value>empty_default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rxfifo_full" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rxfifo_full</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rxfifo_full</ipxact:displayName>
          <ipxact:value>full_default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rxfifo_mode" type="string">
          <ipxact:name>hssi_10g_rx_pcs_rxfifo_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rxfifo_mode</ipxact:displayName>
          <ipxact:value>register_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rxfifo_pempty" type="int">
          <ipxact:name>hssi_10g_rx_pcs_rxfifo_pempty</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rxfifo_pempty</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_rxfifo_pfull" type="int">
          <ipxact:name>hssi_10g_rx_pcs_rxfifo_pfull</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_rxfifo_pfull</ipxact:displayName>
          <ipxact:value>23</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_stretch_num_stages" type="string">
          <ipxact:name>hssi_10g_rx_pcs_stretch_num_stages</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_stretch_num_stages</ipxact:displayName>
          <ipxact:value>one_stage</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_sup_mode" type="string">
          <ipxact:name>hssi_10g_rx_pcs_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_test_mode" type="string">
          <ipxact:name>hssi_10g_rx_pcs_test_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_test_mode</ipxact:displayName>
          <ipxact:value>test_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_wrfifo_clken" type="string">
          <ipxact:name>hssi_10g_rx_pcs_wrfifo_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_wrfifo_clken</ipxact:displayName>
          <ipxact:value>wrfifo_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_silicon_rev" type="string">
          <ipxact:name>hssi_10g_rx_pcs_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_rx_pcs_reconfig_settings" type="string">
          <ipxact:name>hssi_10g_rx_pcs_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_10g_rx_pcs_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_advanced_user_mode" type="string">
          <ipxact:name>hssi_10g_tx_pcs_advanced_user_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_advanced_user_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_bitslip_en" type="string">
          <ipxact:name>hssi_10g_tx_pcs_bitslip_en</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_bitslip_en</ipxact:displayName>
          <ipxact:value>bitslip_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_bonding_dft_en" type="string">
          <ipxact:name>hssi_10g_tx_pcs_bonding_dft_en</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_bonding_dft_en</ipxact:displayName>
          <ipxact:value>dft_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_bonding_dft_val" type="string">
          <ipxact:name>hssi_10g_tx_pcs_bonding_dft_val</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_bonding_dft_val</ipxact:displayName>
          <ipxact:value>dft_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_comp_cnt" type="int">
          <ipxact:name>hssi_10g_tx_pcs_comp_cnt</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_comp_cnt</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_compin_sel" type="string">
          <ipxact:name>hssi_10g_tx_pcs_compin_sel</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_compin_sel</ipxact:displayName>
          <ipxact:value>compin_master</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_crcgen_bypass" type="string">
          <ipxact:name>hssi_10g_tx_pcs_crcgen_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_crcgen_bypass</ipxact:displayName>
          <ipxact:value>crcgen_bypass_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_crcgen_clken" type="string">
          <ipxact:name>hssi_10g_tx_pcs_crcgen_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_crcgen_clken</ipxact:displayName>
          <ipxact:value>crcgen_clk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_crcgen_err" type="string">
          <ipxact:name>hssi_10g_tx_pcs_crcgen_err</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_crcgen_err</ipxact:displayName>
          <ipxact:value>crcgen_err_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_crcgen_inv" type="string">
          <ipxact:name>hssi_10g_tx_pcs_crcgen_inv</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_crcgen_inv</ipxact:displayName>
          <ipxact:value>crcgen_inv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_ctrl_bit_reverse" type="string">
          <ipxact:name>hssi_10g_tx_pcs_ctrl_bit_reverse</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_ctrl_bit_reverse</ipxact:displayName>
          <ipxact:value>ctrl_bit_reverse_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_ctrl_plane_bonding" type="string">
          <ipxact:name>hssi_10g_tx_pcs_ctrl_plane_bonding</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_ctrl_plane_bonding</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_data_bit_reverse" type="string">
          <ipxact:name>hssi_10g_tx_pcs_data_bit_reverse</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_data_bit_reverse</ipxact:displayName>
          <ipxact:value>data_bit_reverse_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_dft_clk_out_sel" type="string">
          <ipxact:name>hssi_10g_tx_pcs_dft_clk_out_sel</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_dft_clk_out_sel</ipxact:displayName>
          <ipxact:value>tx_master_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_dispgen_bypass" type="string">
          <ipxact:name>hssi_10g_tx_pcs_dispgen_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_dispgen_bypass</ipxact:displayName>
          <ipxact:value>dispgen_bypass_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_dispgen_clken" type="string">
          <ipxact:name>hssi_10g_tx_pcs_dispgen_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_dispgen_clken</ipxact:displayName>
          <ipxact:value>dispgen_clk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_dispgen_err" type="string">
          <ipxact:name>hssi_10g_tx_pcs_dispgen_err</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_dispgen_err</ipxact:displayName>
          <ipxact:value>dispgen_err_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_dispgen_pipeln" type="string">
          <ipxact:name>hssi_10g_tx_pcs_dispgen_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_dispgen_pipeln</ipxact:displayName>
          <ipxact:value>dispgen_pipeln_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_distdwn_bypass_pipeln" type="string">
          <ipxact:name>hssi_10g_tx_pcs_distdwn_bypass_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_distdwn_bypass_pipeln</ipxact:displayName>
          <ipxact:value>distdwn_bypass_pipeln_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_distdwn_master" type="string">
          <ipxact:name>hssi_10g_tx_pcs_distdwn_master</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_distdwn_master</ipxact:displayName>
          <ipxact:value>distdwn_master_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_distup_bypass_pipeln" type="string">
          <ipxact:name>hssi_10g_tx_pcs_distup_bypass_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_distup_bypass_pipeln</ipxact:displayName>
          <ipxact:value>distup_bypass_pipeln_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_distup_master" type="string">
          <ipxact:name>hssi_10g_tx_pcs_distup_master</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_distup_master</ipxact:displayName>
          <ipxact:value>distup_master_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_dv_bond" type="string">
          <ipxact:name>hssi_10g_tx_pcs_dv_bond</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_dv_bond</ipxact:displayName>
          <ipxact:value>dv_bond_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_empty_flag_type" type="string">
          <ipxact:name>hssi_10g_tx_pcs_empty_flag_type</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_empty_flag_type</ipxact:displayName>
          <ipxact:value>empty_rd_side</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_enc64b66b_txsm_clken" type="string">
          <ipxact:name>hssi_10g_tx_pcs_enc64b66b_txsm_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_enc64b66b_txsm_clken</ipxact:displayName>
          <ipxact:value>enc64b66b_txsm_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_enc_64b66b_txsm_bypass" type="string">
          <ipxact:name>hssi_10g_tx_pcs_enc_64b66b_txsm_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_enc_64b66b_txsm_bypass</ipxact:displayName>
          <ipxact:value>enc_64b66b_txsm_bypass_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_fastpath" type="string">
          <ipxact:name>hssi_10g_tx_pcs_fastpath</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_fastpath</ipxact:displayName>
          <ipxact:value>fastpath_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_fec_clken" type="string">
          <ipxact:name>hssi_10g_tx_pcs_fec_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_fec_clken</ipxact:displayName>
          <ipxact:value>fec_clk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_fec_enable" type="string">
          <ipxact:name>hssi_10g_tx_pcs_fec_enable</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_fec_enable</ipxact:displayName>
          <ipxact:value>fec_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_fifo_double_write" type="string">
          <ipxact:name>hssi_10g_tx_pcs_fifo_double_write</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_fifo_double_write</ipxact:displayName>
          <ipxact:value>fifo_double_write_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_fifo_reg_fast" type="string">
          <ipxact:name>hssi_10g_tx_pcs_fifo_reg_fast</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_fifo_reg_fast</ipxact:displayName>
          <ipxact:value>fifo_reg_fast_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_fifo_stop_rd" type="string">
          <ipxact:name>hssi_10g_tx_pcs_fifo_stop_rd</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_fifo_stop_rd</ipxact:displayName>
          <ipxact:value>n_rd_empty</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_fifo_stop_wr" type="string">
          <ipxact:name>hssi_10g_tx_pcs_fifo_stop_wr</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_fifo_stop_wr</ipxact:displayName>
          <ipxact:value>n_wr_full</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_frmgen_burst" type="string">
          <ipxact:name>hssi_10g_tx_pcs_frmgen_burst</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_frmgen_burst</ipxact:displayName>
          <ipxact:value>frmgen_burst_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_frmgen_bypass" type="string">
          <ipxact:name>hssi_10g_tx_pcs_frmgen_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_frmgen_bypass</ipxact:displayName>
          <ipxact:value>frmgen_bypass_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_frmgen_clken" type="string">
          <ipxact:name>hssi_10g_tx_pcs_frmgen_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_frmgen_clken</ipxact:displayName>
          <ipxact:value>frmgen_clk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_frmgen_mfrm_length" type="int">
          <ipxact:name>hssi_10g_tx_pcs_frmgen_mfrm_length</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_frmgen_mfrm_length</ipxact:displayName>
          <ipxact:value>2048</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_frmgen_pipeln" type="string">
          <ipxact:name>hssi_10g_tx_pcs_frmgen_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_frmgen_pipeln</ipxact:displayName>
          <ipxact:value>frmgen_pipeln_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_frmgen_pyld_ins" type="string">
          <ipxact:name>hssi_10g_tx_pcs_frmgen_pyld_ins</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_frmgen_pyld_ins</ipxact:displayName>
          <ipxact:value>frmgen_pyld_ins_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_frmgen_wordslip" type="string">
          <ipxact:name>hssi_10g_tx_pcs_frmgen_wordslip</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_frmgen_wordslip</ipxact:displayName>
          <ipxact:value>frmgen_wordslip_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_full_flag_type" type="string">
          <ipxact:name>hssi_10g_tx_pcs_full_flag_type</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_full_flag_type</ipxact:displayName>
          <ipxact:value>full_wr_side</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_gb_pipeln_bypass" type="string">
          <ipxact:name>hssi_10g_tx_pcs_gb_pipeln_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_gb_pipeln_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_gb_tx_idwidth" type="string">
          <ipxact:name>hssi_10g_tx_pcs_gb_tx_idwidth</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_gb_tx_idwidth</ipxact:displayName>
          <ipxact:value>idwidth_66</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_gb_tx_odwidth" type="string">
          <ipxact:name>hssi_10g_tx_pcs_gb_tx_odwidth</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_gb_tx_odwidth</ipxact:displayName>
          <ipxact:value>odwidth_32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_gbred_clken" type="string">
          <ipxact:name>hssi_10g_tx_pcs_gbred_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_gbred_clken</ipxact:displayName>
          <ipxact:value>gbred_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_indv" type="string">
          <ipxact:name>hssi_10g_tx_pcs_indv</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_indv</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_low_latency_en" type="string">
          <ipxact:name>hssi_10g_tx_pcs_low_latency_en</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_low_latency_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_master_clk_sel" type="string">
          <ipxact:name>hssi_10g_tx_pcs_master_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_master_clk_sel</ipxact:displayName>
          <ipxact:value>master_tx_pma_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_pempty_flag_type" type="string">
          <ipxact:name>hssi_10g_tx_pcs_pempty_flag_type</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_pempty_flag_type</ipxact:displayName>
          <ipxact:value>pempty_rd_side</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_pfull_flag_type" type="string">
          <ipxact:name>hssi_10g_tx_pcs_pfull_flag_type</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_pfull_flag_type</ipxact:displayName>
          <ipxact:value>pfull_wr_side</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_phcomp_rd_del" type="string">
          <ipxact:name>hssi_10g_tx_pcs_phcomp_rd_del</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_phcomp_rd_del</ipxact:displayName>
          <ipxact:value>phcomp_rd_del2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_pld_if_type" type="string">
          <ipxact:name>hssi_10g_tx_pcs_pld_if_type</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_pld_if_type</ipxact:displayName>
          <ipxact:value>reg</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_prot_mode" type="string">
          <ipxact:name>hssi_10g_tx_pcs_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_prot_mode</ipxact:displayName>
          <ipxact:value>teng_1588_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_pseudo_random" type="string">
          <ipxact:name>hssi_10g_tx_pcs_pseudo_random</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_pseudo_random</ipxact:displayName>
          <ipxact:value>all_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_pseudo_seed_a" type="string">
          <ipxact:name>hssi_10g_tx_pcs_pseudo_seed_a</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_pseudo_seed_a</ipxact:displayName>
          <ipxact:value>288230376151711743</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_pseudo_seed_b" type="string">
          <ipxact:name>hssi_10g_tx_pcs_pseudo_seed_b</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_pseudo_seed_b</ipxact:displayName>
          <ipxact:value>288230376151711743</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_random_disp" type="string">
          <ipxact:name>hssi_10g_tx_pcs_random_disp</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_random_disp</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_rdfifo_clken" type="string">
          <ipxact:name>hssi_10g_tx_pcs_rdfifo_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_rdfifo_clken</ipxact:displayName>
          <ipxact:value>rdfifo_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_scrm_bypass" type="string">
          <ipxact:name>hssi_10g_tx_pcs_scrm_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_scrm_bypass</ipxact:displayName>
          <ipxact:value>scrm_bypass_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_scrm_clken" type="string">
          <ipxact:name>hssi_10g_tx_pcs_scrm_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_scrm_clken</ipxact:displayName>
          <ipxact:value>scrm_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_scrm_mode" type="string">
          <ipxact:name>hssi_10g_tx_pcs_scrm_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_scrm_mode</ipxact:displayName>
          <ipxact:value>async</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_scrm_pipeln" type="string">
          <ipxact:name>hssi_10g_tx_pcs_scrm_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_scrm_pipeln</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_sh_err" type="string">
          <ipxact:name>hssi_10g_tx_pcs_sh_err</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_sh_err</ipxact:displayName>
          <ipxact:value>sh_err_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_sop_mark" type="string">
          <ipxact:name>hssi_10g_tx_pcs_sop_mark</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_sop_mark</ipxact:displayName>
          <ipxact:value>sop_mark_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_stretch_num_stages" type="string">
          <ipxact:name>hssi_10g_tx_pcs_stretch_num_stages</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_stretch_num_stages</ipxact:displayName>
          <ipxact:value>one_stage</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_sup_mode" type="string">
          <ipxact:name>hssi_10g_tx_pcs_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_test_mode" type="string">
          <ipxact:name>hssi_10g_tx_pcs_test_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_test_mode</ipxact:displayName>
          <ipxact:value>test_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_tx_scrm_err" type="string">
          <ipxact:name>hssi_10g_tx_pcs_tx_scrm_err</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_tx_scrm_err</ipxact:displayName>
          <ipxact:value>scrm_err_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_tx_scrm_width" type="string">
          <ipxact:name>hssi_10g_tx_pcs_tx_scrm_width</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_tx_scrm_width</ipxact:displayName>
          <ipxact:value>bit64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_tx_sh_location" type="string">
          <ipxact:name>hssi_10g_tx_pcs_tx_sh_location</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_tx_sh_location</ipxact:displayName>
          <ipxact:value>lsb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_tx_sm_bypass" type="string">
          <ipxact:name>hssi_10g_tx_pcs_tx_sm_bypass</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_tx_sm_bypass</ipxact:displayName>
          <ipxact:value>tx_sm_bypass_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_tx_sm_pipeln" type="string">
          <ipxact:name>hssi_10g_tx_pcs_tx_sm_pipeln</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_tx_sm_pipeln</ipxact:displayName>
          <ipxact:value>tx_sm_pipeln_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_tx_testbus_sel" type="string">
          <ipxact:name>hssi_10g_tx_pcs_tx_testbus_sel</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_tx_testbus_sel</ipxact:displayName>
          <ipxact:value>tx_fifo_testbus1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_txfifo_empty" type="string">
          <ipxact:name>hssi_10g_tx_pcs_txfifo_empty</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_txfifo_empty</ipxact:displayName>
          <ipxact:value>empty_default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_txfifo_full" type="string">
          <ipxact:name>hssi_10g_tx_pcs_txfifo_full</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_txfifo_full</ipxact:displayName>
          <ipxact:value>full_default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_txfifo_mode" type="string">
          <ipxact:name>hssi_10g_tx_pcs_txfifo_mode</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_txfifo_mode</ipxact:displayName>
          <ipxact:value>register_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_txfifo_pempty" type="int">
          <ipxact:name>hssi_10g_tx_pcs_txfifo_pempty</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_txfifo_pempty</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_txfifo_pfull" type="int">
          <ipxact:name>hssi_10g_tx_pcs_txfifo_pfull</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_txfifo_pfull</ipxact:displayName>
          <ipxact:value>11</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_wr_clk_sel" type="string">
          <ipxact:name>hssi_10g_tx_pcs_wr_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_wr_clk_sel</ipxact:displayName>
          <ipxact:value>wr_tx_pma_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_wrfifo_clken" type="string">
          <ipxact:name>hssi_10g_tx_pcs_wrfifo_clken</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_wrfifo_clken</ipxact:displayName>
          <ipxact:value>wrfifo_clk_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_silicon_rev" type="string">
          <ipxact:name>hssi_10g_tx_pcs_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_10g_tx_pcs_reconfig_settings" type="string">
          <ipxact:name>hssi_10g_tx_pcs_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_10g_tx_pcs_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_auto_error_replacement" type="string">
          <ipxact:name>hssi_8g_rx_pcs_auto_error_replacement</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_auto_error_replacement</ipxact:displayName>
          <ipxact:value>dis_err_replace</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_auto_speed_nego" type="string">
          <ipxact:name>hssi_8g_rx_pcs_auto_speed_nego</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_auto_speed_nego</ipxact:displayName>
          <ipxact:value>dis_asn</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_bit_reversal" type="string">
          <ipxact:name>hssi_8g_rx_pcs_bit_reversal</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_bit_reversal</ipxact:displayName>
          <ipxact:value>dis_bit_reversal</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_bonding_dft_en" type="string">
          <ipxact:name>hssi_8g_rx_pcs_bonding_dft_en</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_bonding_dft_en</ipxact:displayName>
          <ipxact:value>dft_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_bonding_dft_val" type="string">
          <ipxact:name>hssi_8g_rx_pcs_bonding_dft_val</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_bonding_dft_val</ipxact:displayName>
          <ipxact:value>dft_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_bypass_pipeline_reg" type="string">
          <ipxact:name>hssi_8g_rx_pcs_bypass_pipeline_reg</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_bypass_pipeline_reg</ipxact:displayName>
          <ipxact:value>dis_bypass_pipeline</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_byte_deserializer" type="string">
          <ipxact:name>hssi_8g_rx_pcs_byte_deserializer</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_byte_deserializer</ipxact:displayName>
          <ipxact:value>dis_bds</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_cdr_ctrl_rxvalid_mask" type="string">
          <ipxact:name>hssi_8g_rx_pcs_cdr_ctrl_rxvalid_mask</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_cdr_ctrl_rxvalid_mask</ipxact:displayName>
          <ipxact:value>dis_rxvalid_mask</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clkcmp_pattern_n" type="int">
          <ipxact:name>hssi_8g_rx_pcs_clkcmp_pattern_n</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clkcmp_pattern_n</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clkcmp_pattern_p" type="int">
          <ipxact:name>hssi_8g_rx_pcs_clkcmp_pattern_p</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clkcmp_pattern_p</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_gate_bds_dec_asn" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_gate_bds_dec_asn</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_gate_bds_dec_asn</ipxact:displayName>
          <ipxact:value>en_bds_dec_asn_clk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_gate_cdr_eidle" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_gate_cdr_eidle</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_gate_cdr_eidle</ipxact:displayName>
          <ipxact:value>en_cdr_eidle_clk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_gate_dw_pc_wrclk" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_gate_dw_pc_wrclk</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_gate_dw_pc_wrclk</ipxact:displayName>
          <ipxact:value>en_dw_pc_wrclk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_gate_dw_rm_rd" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_gate_dw_rm_rd</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_gate_dw_rm_rd</ipxact:displayName>
          <ipxact:value>en_dw_rm_rdclk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_gate_dw_rm_wr" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_gate_dw_rm_wr</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_gate_dw_rm_wr</ipxact:displayName>
          <ipxact:value>en_dw_rm_wrclk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_gate_dw_wa" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_gate_dw_wa</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_gate_dw_wa</ipxact:displayName>
          <ipxact:value>en_dw_wa_clk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_gate_pc_rdclk" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_gate_pc_rdclk</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_gate_pc_rdclk</ipxact:displayName>
          <ipxact:value>en_pc_rdclk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_gate_sw_pc_wrclk" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_gate_sw_pc_wrclk</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_gate_sw_pc_wrclk</ipxact:displayName>
          <ipxact:value>en_sw_pc_wrclk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_gate_sw_rm_rd" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_gate_sw_rm_rd</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_gate_sw_rm_rd</ipxact:displayName>
          <ipxact:value>en_sw_rm_rdclk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_gate_sw_rm_wr" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_gate_sw_rm_wr</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_gate_sw_rm_wr</ipxact:displayName>
          <ipxact:value>en_sw_rm_wrclk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_gate_sw_wa" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_gate_sw_wa</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_gate_sw_wa</ipxact:displayName>
          <ipxact:value>en_sw_wa_clk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_clock_observation_in_pld_core" type="string">
          <ipxact:name>hssi_8g_rx_pcs_clock_observation_in_pld_core</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_clock_observation_in_pld_core</ipxact:displayName>
          <ipxact:value>internal_sw_wa_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_ctrl_plane_bonding_compensation" type="string">
          <ipxact:name>hssi_8g_rx_pcs_ctrl_plane_bonding_compensation</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_ctrl_plane_bonding_compensation</ipxact:displayName>
          <ipxact:value>dis_compensation</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_ctrl_plane_bonding_consumption" type="string">
          <ipxact:name>hssi_8g_rx_pcs_ctrl_plane_bonding_consumption</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_ctrl_plane_bonding_consumption</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_ctrl_plane_bonding_distribution" type="string">
          <ipxact:name>hssi_8g_rx_pcs_ctrl_plane_bonding_distribution</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_ctrl_plane_bonding_distribution</ipxact:displayName>
          <ipxact:value>not_master_chnl_distr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_eidle_entry_eios" type="string">
          <ipxact:name>hssi_8g_rx_pcs_eidle_entry_eios</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_eidle_entry_eios</ipxact:displayName>
          <ipxact:value>dis_eidle_eios</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_eidle_entry_iei" type="string">
          <ipxact:name>hssi_8g_rx_pcs_eidle_entry_iei</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_eidle_entry_iei</ipxact:displayName>
          <ipxact:value>dis_eidle_iei</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_eidle_entry_sd" type="string">
          <ipxact:name>hssi_8g_rx_pcs_eidle_entry_sd</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_eidle_entry_sd</ipxact:displayName>
          <ipxact:value>dis_eidle_sd</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_eightb_tenb_decoder" type="string">
          <ipxact:name>hssi_8g_rx_pcs_eightb_tenb_decoder</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_eightb_tenb_decoder</ipxact:displayName>
          <ipxact:value>en_8b10b_ibm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_err_flags_sel" type="string">
          <ipxact:name>hssi_8g_rx_pcs_err_flags_sel</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_err_flags_sel</ipxact:displayName>
          <ipxact:value>err_flags_wa</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_fixed_pat_det" type="string">
          <ipxact:name>hssi_8g_rx_pcs_fixed_pat_det</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_fixed_pat_det</ipxact:displayName>
          <ipxact:value>dis_fixed_patdet</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_fixed_pat_num" type="int">
          <ipxact:name>hssi_8g_rx_pcs_fixed_pat_num</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_fixed_pat_num</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_force_signal_detect" type="string">
          <ipxact:name>hssi_8g_rx_pcs_force_signal_detect</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_force_signal_detect</ipxact:displayName>
          <ipxact:value>en_force_signal_detect</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_gen3_clk_en" type="string">
          <ipxact:name>hssi_8g_rx_pcs_gen3_clk_en</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_gen3_clk_en</ipxact:displayName>
          <ipxact:value>disable_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_gen3_rx_clk_sel" type="string">
          <ipxact:name>hssi_8g_rx_pcs_gen3_rx_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_gen3_rx_clk_sel</ipxact:displayName>
          <ipxact:value>rcvd_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_gen3_tx_clk_sel" type="string">
          <ipxact:name>hssi_8g_rx_pcs_gen3_tx_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_gen3_tx_clk_sel</ipxact:displayName>
          <ipxact:value>tx_pma_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_hip_mode" type="string">
          <ipxact:name>hssi_8g_rx_pcs_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_hip_mode</ipxact:displayName>
          <ipxact:value>dis_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_ibm_invalid_code" type="string">
          <ipxact:name>hssi_8g_rx_pcs_ibm_invalid_code</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_ibm_invalid_code</ipxact:displayName>
          <ipxact:value>dis_ibm_invalid_code</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_invalid_code_flag_only" type="string">
          <ipxact:name>hssi_8g_rx_pcs_invalid_code_flag_only</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_invalid_code_flag_only</ipxact:displayName>
          <ipxact:value>dis_invalid_code_only</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_pad_or_edb_error_replace" type="string">
          <ipxact:name>hssi_8g_rx_pcs_pad_or_edb_error_replace</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_pad_or_edb_error_replace</ipxact:displayName>
          <ipxact:value>replace_edb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_pcs_bypass" type="string">
          <ipxact:name>hssi_8g_rx_pcs_pcs_bypass</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_pcs_bypass</ipxact:displayName>
          <ipxact:value>dis_pcs_bypass</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_phase_comp_rdptr" type="string">
          <ipxact:name>hssi_8g_rx_pcs_phase_comp_rdptr</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_phase_comp_rdptr</ipxact:displayName>
          <ipxact:value>disable_rdptr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_phase_compensation_fifo" type="string">
          <ipxact:name>hssi_8g_rx_pcs_phase_compensation_fifo</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_phase_compensation_fifo</ipxact:displayName>
          <ipxact:value>register_fifo</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_pipe_if_enable" type="string">
          <ipxact:name>hssi_8g_rx_pcs_pipe_if_enable</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_pipe_if_enable</ipxact:displayName>
          <ipxact:value>dis_pipe_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_pma_dw" type="string">
          <ipxact:name>hssi_8g_rx_pcs_pma_dw</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_pma_dw</ipxact:displayName>
          <ipxact:value>ten_bit</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_polinv_8b10b_dec" type="string">
          <ipxact:name>hssi_8g_rx_pcs_polinv_8b10b_dec</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_polinv_8b10b_dec</ipxact:displayName>
          <ipxact:value>dis_polinv_8b10b_dec</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_prot_mode" type="string">
          <ipxact:name>hssi_8g_rx_pcs_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_prot_mode</ipxact:displayName>
          <ipxact:value>disabled_prot_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rate_match" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rate_match</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rate_match</ipxact:displayName>
          <ipxact:value>dis_rm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rate_match_del_thres" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rate_match_del_thres</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rate_match_del_thres</ipxact:displayName>
          <ipxact:value>dis_rm_del_thres</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rate_match_empty_thres" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rate_match_empty_thres</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rate_match_empty_thres</ipxact:displayName>
          <ipxact:value>dis_rm_empty_thres</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rate_match_full_thres" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rate_match_full_thres</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rate_match_full_thres</ipxact:displayName>
          <ipxact:value>dis_rm_full_thres</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rate_match_ins_thres" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rate_match_ins_thres</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rate_match_ins_thres</ipxact:displayName>
          <ipxact:value>dis_rm_ins_thres</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rate_match_start_thres" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rate_match_start_thres</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rate_match_start_thres</ipxact:displayName>
          <ipxact:value>dis_rm_start_thres</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rx_clk2" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rx_clk2</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rx_clk2</ipxact:displayName>
          <ipxact:value>rcvd_clk_clk2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rx_clk_free_running" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rx_clk_free_running</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rx_clk_free_running</ipxact:displayName>
          <ipxact:value>en_rx_clk_free_run</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rx_pcs_urst" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rx_pcs_urst</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rx_pcs_urst</ipxact:displayName>
          <ipxact:value>en_rx_pcs_urst</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rx_rcvd_clk" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rx_rcvd_clk</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rx_rcvd_clk</ipxact:displayName>
          <ipxact:value>rcvd_clk_rcvd_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rx_rd_clk" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rx_rd_clk</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rx_rd_clk</ipxact:displayName>
          <ipxact:value>rx_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rx_refclk" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rx_refclk</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rx_refclk</ipxact:displayName>
          <ipxact:value>dis_refclk_sel</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_rx_wr_clk" type="string">
          <ipxact:name>hssi_8g_rx_pcs_rx_wr_clk</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_rx_wr_clk</ipxact:displayName>
          <ipxact:value>rx_clk2_div_1_2_4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_sup_mode" type="string">
          <ipxact:name>hssi_8g_rx_pcs_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_symbol_swap" type="string">
          <ipxact:name>hssi_8g_rx_pcs_symbol_swap</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_symbol_swap</ipxact:displayName>
          <ipxact:value>dis_symbol_swap</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_sync_sm_idle_eios" type="string">
          <ipxact:name>hssi_8g_rx_pcs_sync_sm_idle_eios</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_sync_sm_idle_eios</ipxact:displayName>
          <ipxact:value>dis_syncsm_idle</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_test_bus_sel" type="string">
          <ipxact:name>hssi_8g_rx_pcs_test_bus_sel</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_test_bus_sel</ipxact:displayName>
          <ipxact:value>tx_testbus</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_tx_rx_parallel_loopback" type="string">
          <ipxact:name>hssi_8g_rx_pcs_tx_rx_parallel_loopback</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_tx_rx_parallel_loopback</ipxact:displayName>
          <ipxact:value>dis_plpbk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_boundary_lock_ctrl" type="string">
          <ipxact:name>hssi_8g_rx_pcs_wa_boundary_lock_ctrl</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_boundary_lock_ctrl</ipxact:displayName>
          <ipxact:value>sync_sm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_clk_slip_spacing" type="int">
          <ipxact:name>hssi_8g_rx_pcs_wa_clk_slip_spacing</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_clk_slip_spacing</ipxact:displayName>
          <ipxact:value>16</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_det_latency_sync_status_beh" type="string">
          <ipxact:name>hssi_8g_rx_pcs_wa_det_latency_sync_status_beh</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_det_latency_sync_status_beh</ipxact:displayName>
          <ipxact:value>dont_care_assert_sync</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_disp_err_flag" type="string">
          <ipxact:name>hssi_8g_rx_pcs_wa_disp_err_flag</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_disp_err_flag</ipxact:displayName>
          <ipxact:value>en_disp_err_flag</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_kchar" type="string">
          <ipxact:name>hssi_8g_rx_pcs_wa_kchar</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_kchar</ipxact:displayName>
          <ipxact:value>dis_kchar</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_pd" type="string">
          <ipxact:name>hssi_8g_rx_pcs_wa_pd</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_pd</ipxact:displayName>
          <ipxact:value>wa_pd_10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_pd_data" type="string">
          <ipxact:name>hssi_8g_rx_pcs_wa_pd_data</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_pd_data</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_pd_polarity" type="string">
          <ipxact:name>hssi_8g_rx_pcs_wa_pd_polarity</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_pd_polarity</ipxact:displayName>
          <ipxact:value>dont_care_both_pol</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_pld_controlled" type="string">
          <ipxact:name>hssi_8g_rx_pcs_wa_pld_controlled</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_pld_controlled</ipxact:displayName>
          <ipxact:value>dis_pld_ctrl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_renumber_data" type="int">
          <ipxact:name>hssi_8g_rx_pcs_wa_renumber_data</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_renumber_data</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_rgnumber_data" type="int">
          <ipxact:name>hssi_8g_rx_pcs_wa_rgnumber_data</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_rgnumber_data</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_rknumber_data" type="int">
          <ipxact:name>hssi_8g_rx_pcs_wa_rknumber_data</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_rknumber_data</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_rosnumber_data" type="int">
          <ipxact:name>hssi_8g_rx_pcs_wa_rosnumber_data</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_rosnumber_data</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_rvnumber_data" type="int">
          <ipxact:name>hssi_8g_rx_pcs_wa_rvnumber_data</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_rvnumber_data</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wa_sync_sm_ctrl" type="string">
          <ipxact:name>hssi_8g_rx_pcs_wa_sync_sm_ctrl</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wa_sync_sm_ctrl</ipxact:displayName>
          <ipxact:value>gige_sync_sm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_wait_cnt" type="int">
          <ipxact:name>hssi_8g_rx_pcs_wait_cnt</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_wait_cnt</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_silicon_rev" type="string">
          <ipxact:name>hssi_8g_rx_pcs_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_rx_pcs_reconfig_settings" type="string">
          <ipxact:name>hssi_8g_rx_pcs_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_8g_rx_pcs_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_auto_speed_nego_gen2" type="string">
          <ipxact:name>hssi_8g_tx_pcs_auto_speed_nego_gen2</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_auto_speed_nego_gen2</ipxact:displayName>
          <ipxact:value>dis_asn_g2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_bit_reversal" type="string">
          <ipxact:name>hssi_8g_tx_pcs_bit_reversal</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_bit_reversal</ipxact:displayName>
          <ipxact:value>dis_bit_reversal</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_bonding_dft_en" type="string">
          <ipxact:name>hssi_8g_tx_pcs_bonding_dft_en</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_bonding_dft_en</ipxact:displayName>
          <ipxact:value>dft_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_bonding_dft_val" type="string">
          <ipxact:name>hssi_8g_tx_pcs_bonding_dft_val</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_bonding_dft_val</ipxact:displayName>
          <ipxact:value>dft_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_bypass_pipeline_reg" type="string">
          <ipxact:name>hssi_8g_tx_pcs_bypass_pipeline_reg</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_bypass_pipeline_reg</ipxact:displayName>
          <ipxact:value>dis_bypass_pipeline</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_byte_serializer" type="string">
          <ipxact:name>hssi_8g_tx_pcs_byte_serializer</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_byte_serializer</ipxact:displayName>
          <ipxact:value>dis_bs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_clock_gate_bs_enc" type="string">
          <ipxact:name>hssi_8g_tx_pcs_clock_gate_bs_enc</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_clock_gate_bs_enc</ipxact:displayName>
          <ipxact:value>en_bs_enc_clk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_clock_gate_dw_fifowr" type="string">
          <ipxact:name>hssi_8g_tx_pcs_clock_gate_dw_fifowr</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_clock_gate_dw_fifowr</ipxact:displayName>
          <ipxact:value>en_dw_fifowr_clk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_clock_gate_fiford" type="string">
          <ipxact:name>hssi_8g_tx_pcs_clock_gate_fiford</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_clock_gate_fiford</ipxact:displayName>
          <ipxact:value>en_fiford_clk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_clock_gate_sw_fifowr" type="string">
          <ipxact:name>hssi_8g_tx_pcs_clock_gate_sw_fifowr</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_clock_gate_sw_fifowr</ipxact:displayName>
          <ipxact:value>en_sw_fifowr_clk_gating</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_clock_observation_in_pld_core" type="string">
          <ipxact:name>hssi_8g_tx_pcs_clock_observation_in_pld_core</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_clock_observation_in_pld_core</ipxact:displayName>
          <ipxact:value>internal_refclk_b</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_ctrl_plane_bonding_compensation" type="string">
          <ipxact:name>hssi_8g_tx_pcs_ctrl_plane_bonding_compensation</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_ctrl_plane_bonding_compensation</ipxact:displayName>
          <ipxact:value>dis_compensation</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_ctrl_plane_bonding_consumption" type="string">
          <ipxact:name>hssi_8g_tx_pcs_ctrl_plane_bonding_consumption</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_ctrl_plane_bonding_consumption</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_ctrl_plane_bonding_distribution" type="string">
          <ipxact:name>hssi_8g_tx_pcs_ctrl_plane_bonding_distribution</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_ctrl_plane_bonding_distribution</ipxact:displayName>
          <ipxact:value>not_master_chnl_distr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_data_selection_8b10b_encoder_input" type="string">
          <ipxact:name>hssi_8g_tx_pcs_data_selection_8b10b_encoder_input</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_data_selection_8b10b_encoder_input</ipxact:displayName>
          <ipxact:value>normal_data_path</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_dynamic_clk_switch" type="string">
          <ipxact:name>hssi_8g_tx_pcs_dynamic_clk_switch</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_dynamic_clk_switch</ipxact:displayName>
          <ipxact:value>dis_dyn_clk_switch</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_eightb_tenb_disp_ctrl" type="string">
          <ipxact:name>hssi_8g_tx_pcs_eightb_tenb_disp_ctrl</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_eightb_tenb_disp_ctrl</ipxact:displayName>
          <ipxact:value>dis_disp_ctrl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_eightb_tenb_encoder" type="string">
          <ipxact:name>hssi_8g_tx_pcs_eightb_tenb_encoder</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_eightb_tenb_encoder</ipxact:displayName>
          <ipxact:value>en_8b10b_ibm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_force_echar" type="string">
          <ipxact:name>hssi_8g_tx_pcs_force_echar</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_force_echar</ipxact:displayName>
          <ipxact:value>dis_force_echar</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_force_kchar" type="string">
          <ipxact:name>hssi_8g_tx_pcs_force_kchar</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_force_kchar</ipxact:displayName>
          <ipxact:value>dis_force_kchar</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_gen3_tx_clk_sel" type="string">
          <ipxact:name>hssi_8g_tx_pcs_gen3_tx_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_gen3_tx_clk_sel</ipxact:displayName>
          <ipxact:value>dis_tx_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_gen3_tx_pipe_clk_sel" type="string">
          <ipxact:name>hssi_8g_tx_pcs_gen3_tx_pipe_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_gen3_tx_pipe_clk_sel</ipxact:displayName>
          <ipxact:value>dis_tx_pipe_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_hip_mode" type="string">
          <ipxact:name>hssi_8g_tx_pcs_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_hip_mode</ipxact:displayName>
          <ipxact:value>dis_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_pcs_bypass" type="string">
          <ipxact:name>hssi_8g_tx_pcs_pcs_bypass</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_pcs_bypass</ipxact:displayName>
          <ipxact:value>dis_pcs_bypass</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_phase_comp_rdptr" type="string">
          <ipxact:name>hssi_8g_tx_pcs_phase_comp_rdptr</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_phase_comp_rdptr</ipxact:displayName>
          <ipxact:value>disable_rdptr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_phase_compensation_fifo" type="string">
          <ipxact:name>hssi_8g_tx_pcs_phase_compensation_fifo</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_phase_compensation_fifo</ipxact:displayName>
          <ipxact:value>register_fifo</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_phfifo_write_clk_sel" type="string">
          <ipxact:name>hssi_8g_tx_pcs_phfifo_write_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_phfifo_write_clk_sel</ipxact:displayName>
          <ipxact:value>tx_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_pma_dw" type="string">
          <ipxact:name>hssi_8g_tx_pcs_pma_dw</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_pma_dw</ipxact:displayName>
          <ipxact:value>ten_bit</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_prot_mode" type="string">
          <ipxact:name>hssi_8g_tx_pcs_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_prot_mode</ipxact:displayName>
          <ipxact:value>disabled_prot_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_refclk_b_clk_sel" type="string">
          <ipxact:name>hssi_8g_tx_pcs_refclk_b_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_refclk_b_clk_sel</ipxact:displayName>
          <ipxact:value>tx_pma_clock</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_revloop_back_rm" type="string">
          <ipxact:name>hssi_8g_tx_pcs_revloop_back_rm</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_revloop_back_rm</ipxact:displayName>
          <ipxact:value>dis_rev_loopback_rx_rm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_sup_mode" type="string">
          <ipxact:name>hssi_8g_tx_pcs_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_symbol_swap" type="string">
          <ipxact:name>hssi_8g_tx_pcs_symbol_swap</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_symbol_swap</ipxact:displayName>
          <ipxact:value>dis_symbol_swap</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_tx_bitslip" type="string">
          <ipxact:name>hssi_8g_tx_pcs_tx_bitslip</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_tx_bitslip</ipxact:displayName>
          <ipxact:value>dis_tx_bitslip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_tx_compliance_controlled_disparity" type="string">
          <ipxact:name>hssi_8g_tx_pcs_tx_compliance_controlled_disparity</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_tx_compliance_controlled_disparity</ipxact:displayName>
          <ipxact:value>dis_txcompliance</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_tx_fast_pld_reg" type="string">
          <ipxact:name>hssi_8g_tx_pcs_tx_fast_pld_reg</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_tx_fast_pld_reg</ipxact:displayName>
          <ipxact:value>dis_tx_fast_pld_reg</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_txclk_freerun" type="string">
          <ipxact:name>hssi_8g_tx_pcs_txclk_freerun</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_txclk_freerun</ipxact:displayName>
          <ipxact:value>en_freerun_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_txpcs_urst" type="string">
          <ipxact:name>hssi_8g_tx_pcs_txpcs_urst</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_txpcs_urst</ipxact:displayName>
          <ipxact:value>en_txpcs_urst</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_silicon_rev" type="string">
          <ipxact:name>hssi_8g_tx_pcs_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_8g_tx_pcs_reconfig_settings" type="string">
          <ipxact:name>hssi_8g_tx_pcs_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_8g_tx_pcs_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_adapter_lpbk_mode" type="string">
          <ipxact:name>hssi_adapt_rx_adapter_lpbk_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_adapter_lpbk_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hd_hssiadapt_aib_hssi_pld_sclk_hz" type="int">
          <ipxact:name>hssi_adapt_rx_hd_hssiadapt_aib_hssi_pld_sclk_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hd_hssiadapt_aib_hssi_pld_sclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hd_hssiadapt_aib_hssi_rx_sr_clk_in_hz" type="int">
          <ipxact:name>hssi_adapt_rx_hd_hssiadapt_aib_hssi_rx_sr_clk_in_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hd_hssiadapt_aib_hssi_rx_sr_clk_in_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_aib_lpbk_mode" type="string">
          <ipxact:name>hssi_adapt_rx_aib_lpbk_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_aib_lpbk_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_align_del" type="string">
          <ipxact:name>hssi_adapt_rx_align_del</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_align_del</ipxact:displayName>
          <ipxact:value>align_del_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_asn_bypass_clock_gate" type="string">
          <ipxact:name>hssi_adapt_rx_asn_bypass_clock_gate</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_asn_bypass_clock_gate</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_asn_bypass_pma_pcie_sw_done" type="string">
          <ipxact:name>hssi_adapt_rx_asn_bypass_pma_pcie_sw_done</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_asn_bypass_pma_pcie_sw_done</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_asn_en" type="string">
          <ipxact:name>hssi_adapt_rx_asn_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_asn_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_asn_wait_for_clock_gate_cnt" type="int">
          <ipxact:name>hssi_adapt_rx_asn_wait_for_clock_gate_cnt</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_asn_wait_for_clock_gate_cnt</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_asn_wait_for_dll_reset_cnt" type="int">
          <ipxact:name>hssi_adapt_rx_asn_wait_for_dll_reset_cnt</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_asn_wait_for_dll_reset_cnt</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_asn_wait_for_fifo_flush_cnt" type="int">
          <ipxact:name>hssi_adapt_rx_asn_wait_for_fifo_flush_cnt</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_asn_wait_for_fifo_flush_cnt</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_asn_wait_for_pma_pcie_sw_done_cnt" type="int">
          <ipxact:name>hssi_adapt_rx_asn_wait_for_pma_pcie_sw_done_cnt</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_asn_wait_for_pma_pcie_sw_done_cnt</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_async_direct_hip_en" type="string">
          <ipxact:name>hssi_adapt_rx_async_direct_hip_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_async_direct_hip_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_bonding_dft_en" type="string">
          <ipxact:name>hssi_adapt_rx_bonding_dft_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_bonding_dft_en</ipxact:displayName>
          <ipxact:value>dft_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_bonding_dft_val" type="string">
          <ipxact:name>hssi_adapt_rx_bonding_dft_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_bonding_dft_val</ipxact:displayName>
          <ipxact:value>dft_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_chnl_bonding" type="string">
          <ipxact:name>hssi_adapt_rx_chnl_bonding</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_chnl_bonding</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_clock_del_measure_enable" type="string">
          <ipxact:name>hssi_adapt_rx_clock_del_measure_enable</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_clock_del_measure_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_comp_cnt" type="int">
          <ipxact:name>hssi_adapt_rx_comp_cnt</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_comp_cnt</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_compin_sel" type="string">
          <ipxact:name>hssi_adapt_rx_compin_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_compin_sel</ipxact:displayName>
          <ipxact:value>compin_master</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_control_del" type="string">
          <ipxact:name>hssi_adapt_rx_control_del</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_control_del</ipxact:displayName>
          <ipxact:value>control_del_none</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hd_hssiadapt_csr_clk_hz" type="int">
          <ipxact:name>hssi_adapt_rx_hd_hssiadapt_csr_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hd_hssiadapt_csr_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_ctrl_plane_bonding" type="string">
          <ipxact:name>hssi_adapt_rx_ctrl_plane_bonding</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_ctrl_plane_bonding</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_datapath_mapping_mode" type="string">
          <ipxact:name>hssi_adapt_rx_datapath_mapping_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_datapath_mapping_mode</ipxact:displayName>
          <ipxact:value>map_10g_2x2x_2x1x_fifo</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_ds_bypass_pipeln" type="string">
          <ipxact:name>hssi_adapt_rx_ds_bypass_pipeln</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_ds_bypass_pipeln</ipxact:displayName>
          <ipxact:value>ds_bypass_pipeln_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_ds_last_chnl" type="string">
          <ipxact:name>hssi_adapt_rx_ds_last_chnl</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_ds_last_chnl</ipxact:displayName>
          <ipxact:value>ds_last_chnl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_ds_master" type="string">
          <ipxact:name>hssi_adapt_rx_ds_master</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_ds_master</ipxact:displayName>
          <ipxact:value>ds_master_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_duplex_mode" type="string">
          <ipxact:name>hssi_adapt_rx_duplex_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_duplex_mode</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_dyn_clk_sw_en" type="string">
          <ipxact:name>hssi_adapt_rx_dyn_clk_sw_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_dyn_clk_sw_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fifo_double_write" type="string">
          <ipxact:name>hssi_adapt_rx_fifo_double_write</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fifo_double_write</ipxact:displayName>
          <ipxact:value>fifo_double_write_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fifo_mode" type="string">
          <ipxact:name>hssi_adapt_rx_fifo_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fifo_mode</ipxact:displayName>
          <ipxact:value>phase_comp</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fifo_rd_clk_scg_en" type="string">
          <ipxact:name>hssi_adapt_rx_fifo_rd_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fifo_rd_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fifo_rd_clk_sel" type="string">
          <ipxact:name>hssi_adapt_rx_fifo_rd_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fifo_rd_clk_sel</ipxact:displayName>
          <ipxact:value>fifo_rd_pma_aib_rx_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fifo_stop_rd" type="string">
          <ipxact:name>hssi_adapt_rx_fifo_stop_rd</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fifo_stop_rd</ipxact:displayName>
          <ipxact:value>rd_empty</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fifo_stop_wr" type="string">
          <ipxact:name>hssi_adapt_rx_fifo_stop_wr</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fifo_stop_wr</ipxact:displayName>
          <ipxact:value>n_wr_full</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fifo_width" type="string">
          <ipxact:name>hssi_adapt_rx_fifo_width</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fifo_width</ipxact:displayName>
          <ipxact:value>fifo_double_width</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fifo_wr_clk_scg_en" type="string">
          <ipxact:name>hssi_adapt_rx_fifo_wr_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fifo_wr_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fifo_wr_clk_sel" type="string">
          <ipxact:name>hssi_adapt_rx_fifo_wr_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fifo_wr_clk_sel</ipxact:displayName>
          <ipxact:value>fifo_wr_pld_pcs_rx_clk_out</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_force_align" type="string">
          <ipxact:name>hssi_adapt_rx_force_align</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_force_align</ipxact:displayName>
          <ipxact:value>force_align_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_free_run_div_clk" type="string">
          <ipxact:name>hssi_adapt_rx_free_run_div_clk</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_free_run_div_clk</ipxact:displayName>
          <ipxact:value>out_of_reset_sync</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fsr_pld_10g_rx_crc32_err_rst_val" type="string">
          <ipxact:name>hssi_adapt_rx_fsr_pld_10g_rx_crc32_err_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fsr_pld_10g_rx_crc32_err_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_crc32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fsr_pld_8g_sigdet_out_rst_val" type="string">
          <ipxact:name>hssi_adapt_rx_fsr_pld_8g_sigdet_out_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fsr_pld_8g_sigdet_out_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_sigdet</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fsr_pld_ltd_b_rst_val" type="string">
          <ipxact:name>hssi_adapt_rx_fsr_pld_ltd_b_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fsr_pld_ltd_b_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_ltdb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fsr_pld_ltr_rst_val" type="string">
          <ipxact:name>hssi_adapt_rx_fsr_pld_ltr_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fsr_pld_ltr_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_ltr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_fsr_pld_rx_fifo_align_clr_rst_val" type="string">
          <ipxact:name>hssi_adapt_rx_fsr_pld_rx_fifo_align_clr_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_fsr_pld_rx_fifo_align_clr_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_alignclr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hd_hssiadapt_hip_aib_clk_2x_hz" type="int">
          <ipxact:name>hssi_adapt_rx_hd_hssiadapt_hip_aib_clk_2x_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hd_hssiadapt_hip_aib_clk_2x_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hd_hssiadapt_hip_aib_clk_hz" type="int">
          <ipxact:name>hssi_adapt_rx_hd_hssiadapt_hip_aib_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hd_hssiadapt_hip_aib_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hip_mode" type="string">
          <ipxact:name>hssi_adapt_rx_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hip_mode</ipxact:displayName>
          <ipxact:value>disable_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hrdrst_dcd_cal_done_bypass" type="string">
          <ipxact:name>hssi_adapt_rx_hrdrst_dcd_cal_done_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hrdrst_dcd_cal_done_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hrdrst_rst_sm_dis" type="string">
          <ipxact:name>hssi_adapt_rx_hrdrst_rst_sm_dis</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hrdrst_rst_sm_dis</ipxact:displayName>
          <ipxact:value>enable_rx_rst_sm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hrdrst_rx_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_adapt_rx_hrdrst_rx_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hrdrst_rx_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hrdrst_user_ctl_en" type="string">
          <ipxact:name>hssi_adapt_rx_hrdrst_user_ctl_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hrdrst_user_ctl_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_indv" type="string">
          <ipxact:name>hssi_adapt_rx_indv</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_indv</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_internal_clk1_sel" type="string">
          <ipxact:name>hssi_adapt_rx_internal_clk1_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_internal_clk1_sel</ipxact:displayName>
          <ipxact:value>pld_pma_tx_clk_out_clk1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_internal_clk1_sel0" type="string">
          <ipxact:name>hssi_adapt_rx_internal_clk1_sel0</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_internal_clk1_sel0</ipxact:displayName>
          <ipxact:value>pma_clks_or_txfifowr_post_ct_or_txfiford_pre_or_post_ct_mux_clk1_mux0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_internal_clk1_sel1" type="string">
          <ipxact:name>hssi_adapt_rx_internal_clk1_sel1</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_internal_clk1_sel1</ipxact:displayName>
          <ipxact:value>pma_clks_or_txfiford_pre_or_post_ct_mux_clk1_mux1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_internal_clk1_sel2" type="string">
          <ipxact:name>hssi_adapt_rx_internal_clk1_sel2</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_internal_clk1_sel2</ipxact:displayName>
          <ipxact:value>pma_clks_or_txfiford_pre_ct_mux_clk1_mux2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_internal_clk1_sel3" type="string">
          <ipxact:name>hssi_adapt_rx_internal_clk1_sel3</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_internal_clk1_sel3</ipxact:displayName>
          <ipxact:value>pma_clks_clk1_mux3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_internal_clk2_sel" type="string">
          <ipxact:name>hssi_adapt_rx_internal_clk2_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_internal_clk2_sel</ipxact:displayName>
          <ipxact:value>pld_pma_tx_clk_out_clk2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_internal_clk2_sel0" type="string">
          <ipxact:name>hssi_adapt_rx_internal_clk2_sel0</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_internal_clk2_sel0</ipxact:displayName>
          <ipxact:value>pma_clks_or_rxfiford_post_ct_or_rxfifowr_pre_or_post_ct_mux_clk2_mux0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_internal_clk2_sel1" type="string">
          <ipxact:name>hssi_adapt_rx_internal_clk2_sel1</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_internal_clk2_sel1</ipxact:displayName>
          <ipxact:value>pma_clks_or_rxfifowr_pre_or_post_ct_mux_clk2_mux1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_internal_clk2_sel2" type="string">
          <ipxact:name>hssi_adapt_rx_internal_clk2_sel2</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_internal_clk2_sel2</ipxact:displayName>
          <ipxact:value>pma_clks_or_rxfifowr_pre_ct_mux_clk2_mux2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_internal_clk2_sel3" type="string">
          <ipxact:name>hssi_adapt_rx_internal_clk2_sel3</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_internal_clk2_sel3</ipxact:displayName>
          <ipxact:value>pma_clks_clk2_mux3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_loopback_mode" type="string">
          <ipxact:name>hssi_adapt_rx_loopback_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_loopback_mode</ipxact:displayName>
          <ipxact:value>loopback_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_adapt_rx_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_phcomp_rd_del" type="string">
          <ipxact:name>hssi_adapt_rx_phcomp_rd_del</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_phcomp_rd_del</ipxact:displayName>
          <ipxact:value>phcomp_rd_del3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_pipe_mode" type="string">
          <ipxact:name>hssi_adapt_rx_pipe_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_pipe_mode</ipxact:displayName>
          <ipxact:value>disable_pipe</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hd_hssiadapt_pld_pcs_rx_clk_out_hz" type="int">
          <ipxact:name>hssi_adapt_rx_hd_hssiadapt_pld_pcs_rx_clk_out_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hd_hssiadapt_pld_pcs_rx_clk_out_hz</ipxact:displayName>
          <ipxact:value>322265625</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hd_hssiadapt_pld_pma_hclk_hz" type="int">
          <ipxact:name>hssi_adapt_rx_hd_hssiadapt_pld_pma_hclk_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hd_hssiadapt_pld_pma_hclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_pma_aib_rx_clk_expected_setting" type="string">
          <ipxact:name>hssi_adapt_rx_pma_aib_rx_clk_expected_setting</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_pma_aib_rx_clk_expected_setting</ipxact:displayName>
          <ipxact:value>x2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hd_hssiadapt_pma_aib_rx_clk_hz" type="int">
          <ipxact:name>hssi_adapt_rx_hd_hssiadapt_pma_aib_rx_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hd_hssiadapt_pma_aib_rx_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_pma_coreclkin_sel" type="string">
          <ipxact:name>hssi_adapt_rx_pma_coreclkin_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_pma_coreclkin_sel</ipxact:displayName>
          <ipxact:value>pma_coreclkin_pld_sel</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_pma_hclk_scg_en" type="string">
          <ipxact:name>hssi_adapt_rx_pma_hclk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_pma_hclk_scg_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_powerdown_mode" type="string">
          <ipxact:name>hssi_adapt_rx_powerdown_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_powerdown_mode</ipxact:displayName>
          <ipxact:value>powerup</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_10g_krfec_rx_diag_data_status_polling_bypass" type="string">
          <ipxact:name>hssi_adapt_rx_rx_10g_krfec_rx_diag_data_status_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_10g_krfec_rx_diag_data_status_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_adp_go_b4txeq_en" type="string">
          <ipxact:name>hssi_adapt_rx_rx_adp_go_b4txeq_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_adp_go_b4txeq_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_datapath_tb_sel" type="string">
          <ipxact:name>hssi_adapt_rx_rx_datapath_tb_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_datapath_tb_sel</ipxact:displayName>
          <ipxact:value>cp_bond</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_eq_iteration" type="string">
          <ipxact:name>hssi_adapt_rx_rx_eq_iteration</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_eq_iteration</ipxact:displayName>
          <ipxact:value>cycles_32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_fifo_power_mode" type="string">
          <ipxact:name>hssi_adapt_rx_rx_fifo_power_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_fifo_power_mode</ipxact:displayName>
          <ipxact:value>full_width_full_depth</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_fifo_read_latency_adjust" type="string">
          <ipxact:name>hssi_adapt_rx_rx_fifo_read_latency_adjust</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_fifo_read_latency_adjust</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_fifo_write_latency_adjust" type="string">
          <ipxact:name>hssi_adapt_rx_rx_fifo_write_latency_adjust</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_fifo_write_latency_adjust</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_invalid_no_change" type="string">
          <ipxact:name>hssi_adapt_rx_rx_invalid_no_change</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_invalid_no_change</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_osc_clock_setting" type="string">
          <ipxact:name>hssi_adapt_rx_rx_osc_clock_setting</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_osc_clock_setting</ipxact:displayName>
          <ipxact:value>osc_clk_div_by1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_parity_sel" type="string">
          <ipxact:name>hssi_adapt_rx_rx_parity_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_parity_sel</ipxact:displayName>
          <ipxact:value>func_sel</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_pcs_testbus_sel" type="string">
          <ipxact:name>hssi_adapt_rx_rx_pcs_testbus_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_pcs_testbus_sel</ipxact:displayName>
          <ipxact:value>direct_tr_tb_bit0_sel</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_pcspma_testbus_sel" type="string">
          <ipxact:name>hssi_adapt_rx_rx_pcspma_testbus_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_pcspma_testbus_sel</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_pld_8g_a1a2_k1k2_flag_polling_bypass" type="string">
          <ipxact:name>hssi_adapt_rx_rx_pld_8g_a1a2_k1k2_flag_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_pld_8g_a1a2_k1k2_flag_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_pld_8g_wa_boundary_polling_bypass" type="string">
          <ipxact:name>hssi_adapt_rx_rx_pld_8g_wa_boundary_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_pld_8g_wa_boundary_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_pld_pma_pcie_sw_done_polling_bypass" type="string">
          <ipxact:name>hssi_adapt_rx_rx_pld_pma_pcie_sw_done_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_pld_pma_pcie_sw_done_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_pld_pma_reser_in_polling_bypass" type="string">
          <ipxact:name>hssi_adapt_rx_rx_pld_pma_reser_in_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_pld_pma_reser_in_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_pld_pma_testbus_polling_bypass" type="string">
          <ipxact:name>hssi_adapt_rx_rx_pld_pma_testbus_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_pld_pma_testbus_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_pld_test_data_polling_bypass" type="string">
          <ipxact:name>hssi_adapt_rx_rx_pld_test_data_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_pld_test_data_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_pma_rstn_cycles" type="string">
          <ipxact:name>hssi_adapt_rx_rx_pma_rstn_cycles</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_pma_rstn_cycles</ipxact:displayName>
          <ipxact:value>four_cycles</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_pma_rstn_en" type="string">
          <ipxact:name>hssi_adapt_rx_rx_pma_rstn_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_pma_rstn_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_post_cursor_en" type="string">
          <ipxact:name>hssi_adapt_rx_rx_post_cursor_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_post_cursor_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_pre_cursor_en" type="string">
          <ipxact:name>hssi_adapt_rx_rx_pre_cursor_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_pre_cursor_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_rmfflag_stretch_enable" type="string">
          <ipxact:name>hssi_adapt_rx_rx_rmfflag_stretch_enable</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_rmfflag_stretch_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_rmfflag_stretch_num_stages" type="string">
          <ipxact:name>hssi_adapt_rx_rx_rmfflag_stretch_num_stages</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_rmfflag_stretch_num_stages</ipxact:displayName>
          <ipxact:value>rmfflag_two_stage</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_rxeq_en" type="string">
          <ipxact:name>hssi_adapt_rx_rx_rxeq_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_rxeq_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_txeq_en" type="string">
          <ipxact:name>hssi_adapt_rx_rx_txeq_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_txeq_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_txeq_time" type="int">
          <ipxact:name>hssi_adapt_rx_rx_txeq_time</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_txeq_time</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_use_rxvalid_for_rxeq" type="string">
          <ipxact:name>hssi_adapt_rx_rx_use_rxvalid_for_rxeq</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_use_rxvalid_for_rxeq</ipxact:displayName>
          <ipxact:value>rxvalid</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rx_usertest_sel" type="string">
          <ipxact:name>hssi_adapt_rx_rx_usertest_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rx_usertest_sel</ipxact:displayName>
          <ipxact:value>direct_tr_usertest3_sel</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rxfifo_empty" type="string">
          <ipxact:name>hssi_adapt_rx_rxfifo_empty</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rxfifo_empty</ipxact:displayName>
          <ipxact:value>empty_default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rxfifo_full" type="string">
          <ipxact:name>hssi_adapt_rx_rxfifo_full</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rxfifo_full</ipxact:displayName>
          <ipxact:value>full_dw</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rxfifo_mode" type="string">
          <ipxact:name>hssi_adapt_rx_rxfifo_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rxfifo_mode</ipxact:displayName>
          <ipxact:value>rxphase_comp</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rxfifo_pempty" type="int">
          <ipxact:name>hssi_adapt_rx_rxfifo_pempty</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rxfifo_pempty</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rxfifo_pfull" type="int">
          <ipxact:name>hssi_adapt_rx_rxfifo_pfull</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rxfifo_pfull</ipxact:displayName>
          <ipxact:value>5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rxfiford_post_ct_sel" type="string">
          <ipxact:name>hssi_adapt_rx_rxfiford_post_ct_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rxfiford_post_ct_sel</ipxact:displayName>
          <ipxact:value>rxfiford_sclk_post_ct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rxfiford_to_aib_sel" type="string">
          <ipxact:name>hssi_adapt_rx_rxfiford_to_aib_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rxfiford_to_aib_sel</ipxact:displayName>
          <ipxact:value>rxfiford_sclk_to_aib</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rxfifowr_post_ct_sel" type="string">
          <ipxact:name>hssi_adapt_rx_rxfifowr_post_ct_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rxfifowr_post_ct_sel</ipxact:displayName>
          <ipxact:value>rxfifowr_sclk_post_ct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_rxfifowr_pre_ct_sel" type="string">
          <ipxact:name>hssi_adapt_rx_rxfifowr_pre_ct_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_rxfifowr_pre_ct_sel</ipxact:displayName>
          <ipxact:value>rxfifowr_sclk_pre_ct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_slv_asn_en" type="string">
          <ipxact:name>hssi_adapt_rx_slv_asn_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_slv_asn_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_hd_hssiadapt_speed_grade" type="string">
          <ipxact:name>hssi_adapt_rx_hd_hssiadapt_speed_grade</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_hd_hssiadapt_speed_grade</ipxact:displayName>
          <ipxact:value>dash_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_stretch_num_stages" type="string">
          <ipxact:name>hssi_adapt_rx_stretch_num_stages</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_stretch_num_stages</ipxact:displayName>
          <ipxact:value>seven_stage</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_sup_mode" type="string">
          <ipxact:name>hssi_adapt_rx_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_txeq_clk_scg_en" type="string">
          <ipxact:name>hssi_adapt_rx_txeq_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_txeq_clk_scg_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_txeq_clk_sel" type="string">
          <ipxact:name>hssi_adapt_rx_txeq_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_txeq_clk_sel</ipxact:displayName>
          <ipxact:value>txeq_pld_pcs_rx_clk_out</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_txeq_mode" type="string">
          <ipxact:name>hssi_adapt_rx_txeq_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_txeq_mode</ipxact:displayName>
          <ipxact:value>eq_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_txeq_rst_sel" type="string">
          <ipxact:name>hssi_adapt_rx_txeq_rst_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_txeq_rst_sel</ipxact:displayName>
          <ipxact:value>txeq_pcs_rx_pld_rst_n</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_txfiford_post_ct_sel" type="string">
          <ipxact:name>hssi_adapt_rx_txfiford_post_ct_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_txfiford_post_ct_sel</ipxact:displayName>
          <ipxact:value>txfiford_sclk_post_ct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_txfiford_pre_ct_sel" type="string">
          <ipxact:name>hssi_adapt_rx_txfiford_pre_ct_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_txfiford_pre_ct_sel</ipxact:displayName>
          <ipxact:value>txfiford_sclk_pre_ct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_txfifowr_from_aib_sel" type="string">
          <ipxact:name>hssi_adapt_rx_txfifowr_from_aib_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_txfifowr_from_aib_sel</ipxact:displayName>
          <ipxact:value>txfifowr_sclk_from_aib</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_txfifowr_post_ct_sel" type="string">
          <ipxact:name>hssi_adapt_rx_txfifowr_post_ct_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_txfifowr_post_ct_sel</ipxact:displayName>
          <ipxact:value>txfifowr_sclk_post_ct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_us_bypass_pipeln" type="string">
          <ipxact:name>hssi_adapt_rx_us_bypass_pipeln</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_us_bypass_pipeln</ipxact:displayName>
          <ipxact:value>us_bypass_pipeln_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_us_last_chnl" type="string">
          <ipxact:name>hssi_adapt_rx_us_last_chnl</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_us_last_chnl</ipxact:displayName>
          <ipxact:value>us_last_chnl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_us_master" type="string">
          <ipxact:name>hssi_adapt_rx_us_master</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_us_master</ipxact:displayName>
          <ipxact:value>us_master_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_word_align_enable" type="string">
          <ipxact:name>hssi_adapt_rx_word_align_enable</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_word_align_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_word_mark" type="string">
          <ipxact:name>hssi_adapt_rx_word_mark</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_word_mark</ipxact:displayName>
          <ipxact:value>wm_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_rx_silicon_rev" type="string">
          <ipxact:name>hssi_adapt_rx_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_adapt_rx_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_aib_clk_sel" type="string">
          <ipxact:name>hssi_adapt_tx_aib_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_aib_clk_sel</ipxact:displayName>
          <ipxact:value>aib_clk_pma_aib_tx_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hd_hssiadapt_aib_hssi_pld_sclk_hz" type="int">
          <ipxact:name>hssi_adapt_tx_hd_hssiadapt_aib_hssi_pld_sclk_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hd_hssiadapt_aib_hssi_pld_sclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hd_hssiadapt_aib_hssi_tx_sr_clk_in_hz" type="int">
          <ipxact:name>hssi_adapt_tx_hd_hssiadapt_aib_hssi_tx_sr_clk_in_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hd_hssiadapt_aib_hssi_tx_sr_clk_in_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hd_hssiadapt_aib_hssi_tx_transfer_clk_hz" type="int">
          <ipxact:name>hssi_adapt_tx_hd_hssiadapt_aib_hssi_tx_transfer_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hd_hssiadapt_aib_hssi_tx_transfer_clk_hz</ipxact:displayName>
          <ipxact:value>644531250</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_bonding_dft_en" type="string">
          <ipxact:name>hssi_adapt_tx_bonding_dft_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_bonding_dft_en</ipxact:displayName>
          <ipxact:value>dft_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_bonding_dft_val" type="string">
          <ipxact:name>hssi_adapt_tx_bonding_dft_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_bonding_dft_val</ipxact:displayName>
          <ipxact:value>dft_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_chnl_bonding" type="string">
          <ipxact:name>hssi_adapt_tx_chnl_bonding</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_chnl_bonding</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_comp_cnt" type="int">
          <ipxact:name>hssi_adapt_tx_comp_cnt</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_comp_cnt</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_compin_sel" type="string">
          <ipxact:name>hssi_adapt_tx_compin_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_compin_sel</ipxact:displayName>
          <ipxact:value>compin_master</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hd_hssiadapt_csr_clk_hz" type="int">
          <ipxact:name>hssi_adapt_tx_hd_hssiadapt_csr_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hd_hssiadapt_csr_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_ctrl_plane_bonding" type="string">
          <ipxact:name>hssi_adapt_tx_ctrl_plane_bonding</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_ctrl_plane_bonding</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_datapath_mapping_mode" type="string">
          <ipxact:name>hssi_adapt_tx_datapath_mapping_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_datapath_mapping_mode</ipxact:displayName>
          <ipxact:value>map_10g_2x2x_2x1x_fifo</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_ds_bypass_pipeln" type="string">
          <ipxact:name>hssi_adapt_tx_ds_bypass_pipeln</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_ds_bypass_pipeln</ipxact:displayName>
          <ipxact:value>ds_bypass_pipeln_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_ds_last_chnl" type="string">
          <ipxact:name>hssi_adapt_tx_ds_last_chnl</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_ds_last_chnl</ipxact:displayName>
          <ipxact:value>ds_last_chnl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_ds_master" type="string">
          <ipxact:name>hssi_adapt_tx_ds_master</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_ds_master</ipxact:displayName>
          <ipxact:value>ds_master_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_duplex_mode" type="string">
          <ipxact:name>hssi_adapt_tx_duplex_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_duplex_mode</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_dv_gating" type="string">
          <ipxact:name>hssi_adapt_tx_dv_gating</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_dv_gating</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_dyn_clk_sw_en" type="string">
          <ipxact:name>hssi_adapt_tx_dyn_clk_sw_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_dyn_clk_sw_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fifo_double_read" type="string">
          <ipxact:name>hssi_adapt_tx_fifo_double_read</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fifo_double_read</ipxact:displayName>
          <ipxact:value>fifo_double_read_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fifo_mode" type="string">
          <ipxact:name>hssi_adapt_tx_fifo_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fifo_mode</ipxact:displayName>
          <ipxact:value>phase_comp</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fifo_rd_clk_scg_en" type="string">
          <ipxact:name>hssi_adapt_tx_fifo_rd_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fifo_rd_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fifo_rd_clk_sel" type="string">
          <ipxact:name>hssi_adapt_tx_fifo_rd_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fifo_rd_clk_sel</ipxact:displayName>
          <ipxact:value>fifo_rd_pld_pcs_tx_clk_out</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fifo_ready_bypass" type="string">
          <ipxact:name>hssi_adapt_tx_fifo_ready_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fifo_ready_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fifo_stop_rd" type="string">
          <ipxact:name>hssi_adapt_tx_fifo_stop_rd</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fifo_stop_rd</ipxact:displayName>
          <ipxact:value>rd_empty</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fifo_stop_wr" type="string">
          <ipxact:name>hssi_adapt_tx_fifo_stop_wr</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fifo_stop_wr</ipxact:displayName>
          <ipxact:value>wr_full</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fifo_width" type="string">
          <ipxact:name>hssi_adapt_tx_fifo_width</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fifo_width</ipxact:displayName>
          <ipxact:value>fifo_double_width</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fifo_wr_clk_scg_en" type="string">
          <ipxact:name>hssi_adapt_tx_fifo_wr_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fifo_wr_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_free_run_div_clk" type="string">
          <ipxact:name>hssi_adapt_tx_free_run_div_clk</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_free_run_div_clk</ipxact:displayName>
          <ipxact:value>out_of_reset_sync</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fsr_hip_fsr_in_bit0_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_fsr_hip_fsr_in_bit0_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fsr_hip_fsr_in_bit0_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_hfsrin0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fsr_hip_fsr_in_bit1_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_fsr_hip_fsr_in_bit1_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fsr_hip_fsr_in_bit1_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_hfsrin1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fsr_hip_fsr_in_bit2_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_fsr_hip_fsr_in_bit2_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fsr_hip_fsr_in_bit2_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_hfsrin2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fsr_hip_fsr_in_bit3_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_fsr_hip_fsr_in_bit3_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fsr_hip_fsr_in_bit3_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_hfsrin3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fsr_hip_fsr_out_bit0_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_fsr_hip_fsr_out_bit0_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fsr_hip_fsr_out_bit0_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_hfsrout0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fsr_hip_fsr_out_bit1_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_fsr_hip_fsr_out_bit1_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fsr_hip_fsr_out_bit1_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_hfsrout1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fsr_hip_fsr_out_bit2_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_fsr_hip_fsr_out_bit2_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fsr_hip_fsr_out_bit2_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_hfsrout2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fsr_hip_fsr_out_bit3_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_fsr_hip_fsr_out_bit3_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fsr_hip_fsr_out_bit3_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_hfsrout3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fsr_mask_tx_pll_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_fsr_mask_tx_pll_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fsr_mask_tx_pll_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_maskpll</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_fsr_pld_txelecidle_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_fsr_pld_txelecidle_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_fsr_pld_txelecidle_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_txelec</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hd_hssiadapt_hip_aib_clk_2x_hz" type="int">
          <ipxact:name>hssi_adapt_tx_hd_hssiadapt_hip_aib_clk_2x_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hd_hssiadapt_hip_aib_clk_2x_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hd_hssiadapt_hip_aib_clk_hz" type="int">
          <ipxact:name>hssi_adapt_tx_hd_hssiadapt_hip_aib_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hd_hssiadapt_hip_aib_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hd_hssiadapt_hip_aib_txeq_clk_out_hz" type="int">
          <ipxact:name>hssi_adapt_tx_hd_hssiadapt_hip_aib_txeq_clk_out_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hd_hssiadapt_hip_aib_txeq_clk_out_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hip_mode" type="string">
          <ipxact:name>hssi_adapt_tx_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hip_mode</ipxact:displayName>
          <ipxact:value>disable_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hip_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_adapt_tx_hip_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hip_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hrdrst_align_bypass" type="string">
          <ipxact:name>hssi_adapt_tx_hrdrst_align_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hrdrst_align_bypass</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hrdrst_dcd_cal_done_bypass" type="string">
          <ipxact:name>hssi_adapt_tx_hrdrst_dcd_cal_done_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hrdrst_dcd_cal_done_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hrdrst_dll_lock_bypass" type="string">
          <ipxact:name>hssi_adapt_tx_hrdrst_dll_lock_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hrdrst_dll_lock_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hrdrst_rst_sm_dis" type="string">
          <ipxact:name>hssi_adapt_tx_hrdrst_rst_sm_dis</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hrdrst_rst_sm_dis</ipxact:displayName>
          <ipxact:value>enable_tx_rst_sm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hrdrst_rx_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_adapt_tx_hrdrst_rx_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hrdrst_rx_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hrdrst_user_ctl_en" type="string">
          <ipxact:name>hssi_adapt_tx_hrdrst_user_ctl_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hrdrst_user_ctl_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_indv" type="string">
          <ipxact:name>hssi_adapt_tx_indv</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_indv</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_loopback_mode" type="string">
          <ipxact:name>hssi_adapt_tx_loopback_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_loopback_mode</ipxact:displayName>
          <ipxact:value>loopback_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_adapt_tx_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_phcomp_rd_del" type="string">
          <ipxact:name>hssi_adapt_tx_phcomp_rd_del</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_phcomp_rd_del</ipxact:displayName>
          <ipxact:value>phcomp_rd_del2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_pipe_mode" type="string">
          <ipxact:name>hssi_adapt_tx_pipe_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_pipe_mode</ipxact:displayName>
          <ipxact:value>disable_pipe</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hd_hssiadapt_pld_pcs_tx_clk_out_hz" type="int">
          <ipxact:name>hssi_adapt_tx_hd_hssiadapt_pld_pcs_tx_clk_out_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hd_hssiadapt_pld_pcs_tx_clk_out_hz</ipxact:displayName>
          <ipxact:value>322265625</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hd_hssiadapt_pld_pma_hclk_hz" type="int">
          <ipxact:name>hssi_adapt_tx_hd_hssiadapt_pld_pma_hclk_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hd_hssiadapt_pld_pma_hclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_pma_aib_tx_clk_expected_setting" type="string">
          <ipxact:name>hssi_adapt_tx_pma_aib_tx_clk_expected_setting</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_pma_aib_tx_clk_expected_setting</ipxact:displayName>
          <ipxact:value>x2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hd_hssiadapt_pma_aib_tx_clk_hz" type="int">
          <ipxact:name>hssi_adapt_tx_hd_hssiadapt_pma_aib_tx_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hd_hssiadapt_pma_aib_tx_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_powerdown_mode" type="string">
          <ipxact:name>hssi_adapt_tx_powerdown_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_powerdown_mode</ipxact:displayName>
          <ipxact:value>powerup</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_presethint_bypass" type="string">
          <ipxact:name>hssi_adapt_tx_presethint_bypass</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_presethint_bypass</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_qpi_sr_enable" type="string">
          <ipxact:name>hssi_adapt_tx_qpi_sr_enable</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_qpi_sr_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_rxqpi_pullup_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_rxqpi_pullup_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_rxqpi_pullup_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_rxqpi</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_hd_hssiadapt_speed_grade" type="string">
          <ipxact:name>hssi_adapt_tx_hd_hssiadapt_speed_grade</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_hd_hssiadapt_speed_grade</ipxact:displayName>
          <ipxact:value>dash_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_stretch_num_stages" type="string">
          <ipxact:name>hssi_adapt_tx_stretch_num_stages</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_stretch_num_stages</ipxact:displayName>
          <ipxact:value>seven_stage</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_sup_mode" type="string">
          <ipxact:name>hssi_adapt_tx_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_tx_datapath_tb_sel" type="string">
          <ipxact:name>hssi_adapt_tx_tx_datapath_tb_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_tx_datapath_tb_sel</ipxact:displayName>
          <ipxact:value>cp_bond</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_tx_fastbond_wren" type="string">
          <ipxact:name>hssi_adapt_tx_tx_fastbond_wren</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_tx_fastbond_wren</ipxact:displayName>
          <ipxact:value>wren_ds_del2_us_del2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_tx_fifo_power_mode" type="string">
          <ipxact:name>hssi_adapt_tx_tx_fifo_power_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_tx_fifo_power_mode</ipxact:displayName>
          <ipxact:value>full_width_full_depth</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_tx_fifo_read_latency_adjust" type="string">
          <ipxact:name>hssi_adapt_tx_tx_fifo_read_latency_adjust</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_tx_fifo_read_latency_adjust</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_tx_fifo_write_latency_adjust" type="string">
          <ipxact:name>hssi_adapt_tx_tx_fifo_write_latency_adjust</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_tx_fifo_write_latency_adjust</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_tx_osc_clock_setting" type="string">
          <ipxact:name>hssi_adapt_tx_tx_osc_clock_setting</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_tx_osc_clock_setting</ipxact:displayName>
          <ipxact:value>osc_clk_div_by1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_tx_qpi_mode_en" type="string">
          <ipxact:name>hssi_adapt_tx_tx_qpi_mode_en</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_tx_qpi_mode_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_tx_rev_lpbk" type="string">
          <ipxact:name>hssi_adapt_tx_tx_rev_lpbk</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_tx_rev_lpbk</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_tx_usertest_sel" type="string">
          <ipxact:name>hssi_adapt_tx_tx_usertest_sel</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_tx_usertest_sel</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_txfifo_empty" type="string">
          <ipxact:name>hssi_adapt_tx_txfifo_empty</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_txfifo_empty</ipxact:displayName>
          <ipxact:value>empty_default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_txfifo_full" type="string">
          <ipxact:name>hssi_adapt_tx_txfifo_full</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_txfifo_full</ipxact:displayName>
          <ipxact:value>full_dw</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_txfifo_mode" type="string">
          <ipxact:name>hssi_adapt_tx_txfifo_mode</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_txfifo_mode</ipxact:displayName>
          <ipxact:value>txphase_comp</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_txfifo_pempty" type="int">
          <ipxact:name>hssi_adapt_tx_txfifo_pempty</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_txfifo_pempty</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_txfifo_pfull" type="int">
          <ipxact:name>hssi_adapt_tx_txfifo_pfull</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_txfifo_pfull</ipxact:displayName>
          <ipxact:value>5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_txqpi_pulldn_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_txqpi_pulldn_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_txqpi_pulldn_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_txqpid</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_txqpi_pullup_rst_val" type="string">
          <ipxact:name>hssi_adapt_tx_txqpi_pullup_rst_val</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_txqpi_pullup_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_txqpiu</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_us_last_chnl" type="string">
          <ipxact:name>hssi_adapt_tx_us_last_chnl</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_us_last_chnl</ipxact:displayName>
          <ipxact:value>us_last_chnl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_us_master" type="string">
          <ipxact:name>hssi_adapt_tx_us_master</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_us_master</ipxact:displayName>
          <ipxact:value>us_master_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_word_align" type="string">
          <ipxact:name>hssi_adapt_tx_word_align</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_word_align</ipxact:displayName>
          <ipxact:value>wa_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_word_align_enable" type="string">
          <ipxact:name>hssi_adapt_tx_word_align_enable</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_word_align_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_adapt_tx_silicon_rev" type="string">
          <ipxact:name>hssi_adapt_tx_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_adapt_tx_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_datasel_gr0" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_datasel_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_datasel_gr0</ipxact:displayName>
          <ipxact:value>aib_datasel0_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_datasel_gr1" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_datasel_gr1</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_datasel_gr1</ipxact:displayName>
          <ipxact:value>aib_datasel1_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_datasel_gr2" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_datasel_gr2</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_datasel_gr2</ipxact:displayName>
          <ipxact:value>aib_datasel2_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_ddrctrl_gr0" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_ddrctrl_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_ddrctrl_gr0</ipxact:displayName>
          <ipxact:value>aib_ddr0_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_ddrctrl_gr1" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_ddrctrl_gr1</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_ddrctrl_gr1</ipxact:displayName>
          <ipxact:value>aib_ddr1_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_iinasyncen" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_iinasyncen</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_iinasyncen</ipxact:displayName>
          <ipxact:value>aib_inasyncen_setting2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_iinclken" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_iinclken</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_iinclken</ipxact:displayName>
          <ipxact:value>aib_inclken_setting3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_outctrl_gr0" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_outctrl_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_outctrl_gr0</ipxact:displayName>
          <ipxact:value>aib_outen0_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_outctrl_gr1" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_outctrl_gr1</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_outctrl_gr1</ipxact:displayName>
          <ipxact:value>aib_outen1_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_outctrl_gr2" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_outctrl_gr2</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_outctrl_gr2</ipxact:displayName>
          <ipxact:value>aib_outen2_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_outctrl_gr3" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_outctrl_gr3</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_outctrl_gr3</ipxact:displayName>
          <ipxact:value>aib_outen3_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_outndrv_r12" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_outndrv_r12</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_outndrv_r12</ipxact:displayName>
          <ipxact:value>aib_ndrv12_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_outndrv_r56" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_outndrv_r56</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_outndrv_r56</ipxact:displayName>
          <ipxact:value>aib_ndrv56_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_outndrv_r78" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_outndrv_r78</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_outndrv_r78</ipxact:displayName>
          <ipxact:value>aib_ndrv78_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_outpdrv_r12" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_outpdrv_r12</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_outpdrv_r12</ipxact:displayName>
          <ipxact:value>aib_pdrv12_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_outpdrv_r56" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_outpdrv_r56</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_outpdrv_r56</ipxact:displayName>
          <ipxact:value>aib_pdrv56_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_outpdrv_r78" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_outpdrv_r78</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_outpdrv_r78</ipxact:displayName>
          <ipxact:value>aib_pdrv78_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_red_rx_shiften" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_red_rx_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_red_rx_shiften</ipxact:displayName>
          <ipxact:value>aib_red_rx_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_clkdiv" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_clkdiv</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_clkdiv</ipxact:displayName>
          <ipxact:value>aib_rx_clkdiv_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_byp" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_byp</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_byp</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_byp_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_byp_iocsr_unused" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_byp_iocsr_unused</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_byp_iocsr_unused</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_byp_disable_iocsr_unused</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_cont_cal" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_cont_cal</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_cont_cal</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_cal_cont</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_cont_cal_iocsr_unused" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_cont_cal_iocsr_unused</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_cont_cal_iocsr_unused</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_cal_single_iocsr_unused</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_dft" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_dft</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_dft</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_dft_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_dft_sel" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_dft_sel</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_dft_sel</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_dft_mode0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_dll_entest" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_dll_entest</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_dll_entest</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_dll_test_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_dy_ctl_static" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_dy_ctl_static</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_dy_ctl_static</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_dy_ctl_static_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_dy_ctlsel" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_dy_ctlsel</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_dy_ctlsel</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_dy_ctlsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_en" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_en</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_en</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_en_iocsr_unused" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_en_iocsr_unused</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_en_iocsr_unused</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_disable_iocsr_unused</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_manual_dn" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_manual_dn</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_manual_dn</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_manual_dn0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_manual_up" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_manual_up</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_manual_up</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_manual_up0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_rst_prgmnvrt" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_rst_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_rst_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_st_rst_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_st_core_dn_prgmnvrt" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_st_core_dn_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_st_core_dn_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_st_core_dn_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_st_core_up_prgmnvrt" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_st_core_up_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_st_core_up_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_st_core_up_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_st_core_updnen" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_st_core_updnen</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_st_core_updnen</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_st_core_updnen_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_st_dftmuxsel" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_st_dftmuxsel</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_st_dftmuxsel</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_st_dftmuxsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_st_dly_pst" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_st_dly_pst</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_st_dly_pst</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_st_dly_pst_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_st_en" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_st_en</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_st_en</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_st_en_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_st_lockreq_muxsel" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_st_lockreq_muxsel</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_st_lockreq_muxsel</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_st_lockreq_muxsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_st_new_dll" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_st_new_dll</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_st_new_dll</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_new_dll_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_st_new_dll2" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_st_new_dll2</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_st_new_dll2</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_new_dll2_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_st_rst" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_st_rst</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_st_rst</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_st_rst_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_dcc_test_clk_pll_en_n" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_dcc_test_clk_pll_en_n</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_dcc_test_clk_pll_en_n</ipxact:displayName>
          <ipxact:value>aib_rx_dcc_test_clk_pll_en_n_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_halfcode" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_halfcode</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_halfcode</ipxact:displayName>
          <ipxact:value>aib_rx_halfcode_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_aib_rx_selflock" type="string">
          <ipxact:name>hssi_aibcr_rx_aib_rx_selflock</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_aib_rx_selflock</ipxact:displayName>
          <ipxact:value>aib_rx_selflock_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_dft_hssitestip_dll_dcc_en" type="string">
          <ipxact:name>hssi_aibcr_rx_dft_hssitestip_dll_dcc_en</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_dft_hssitestip_dll_dcc_en</ipxact:displayName>
          <ipxact:value>disable_dft</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_op_mode" type="string">
          <ipxact:name>hssi_aibcr_rx_op_mode</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_op_mode</ipxact:displayName>
          <ipxact:value>rx_dcc_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_powermode_ac" type="string">
          <ipxact:name>hssi_aibcr_rx_powermode_ac</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_powermode_ac</ipxact:displayName>
          <ipxact:value>rxdatapath_high_speed_pwr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_powermode_dc" type="string">
          <ipxact:name>hssi_aibcr_rx_powermode_dc</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_powermode_dc</ipxact:displayName>
          <ipxact:value>powerup</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_redundancy_en" type="string">
          <ipxact:name>hssi_aibcr_rx_redundancy_en</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_redundancy_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_sup_mode" type="string">
          <ipxact:name>hssi_aibcr_rx_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_rx_silicon_rev" type="string">
          <ipxact:name>hssi_aibcr_rx_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_aibcr_rx_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_datasel_gr0" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_datasel_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_datasel_gr0</ipxact:displayName>
          <ipxact:value>aib_datasel0_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_datasel_gr1" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_datasel_gr1</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_datasel_gr1</ipxact:displayName>
          <ipxact:value>aib_datasel1_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_datasel_gr2" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_datasel_gr2</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_datasel_gr2</ipxact:displayName>
          <ipxact:value>aib_datasel2_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_clkdiv" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_clkdiv</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_clkdiv</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_clkdiv_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_dcc_dll_dft_sel" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_dcc_dll_dft_sel</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_dcc_dll_dft_sel</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_dcc_dll_dft_sel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_dft_ch_muxsel" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_dft_ch_muxsel</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_dft_ch_muxsel</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_dft_ch_muxsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_dly_pst" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_dly_pst</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_dly_pst</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_dly_pst_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_dy_ctl_static" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_dy_ctl_static</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_dy_ctl_static</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_dy_ctl_static_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_dy_ctlsel" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_dy_ctlsel</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_dy_ctlsel</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_dy_ctlsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_entest" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_entest</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_entest</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_test_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_halfcode" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_halfcode</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_halfcode</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_halfcode_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_selflock" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_selflock</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_selflock</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_selflock_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_st_core_dn_prgmnvrt" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_st_core_dn_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_st_core_dn_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_core_dn_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_st_core_up_prgmnvrt" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_st_core_up_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_st_core_up_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_core_up_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_st_core_updnen" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_st_core_updnen</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_st_core_updnen</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_core_updnen_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_st_dftmuxsel" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_st_dftmuxsel</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_st_dftmuxsel</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_dftmuxsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_st_en" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_st_en</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_st_en</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_en_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_st_lockreq_muxsel" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_st_lockreq_muxsel</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_st_lockreq_muxsel</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_lockreq_muxsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_st_new_dll" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_st_new_dll</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_st_new_dll</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_new_dll_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_st_new_dll2" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_st_new_dll2</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_st_new_dll2</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_new_dll2_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_st_rst" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_st_rst</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_st_rst</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_rst_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_st_rst_prgmnvrt" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_st_rst_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_st_rst_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_rst_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_dllstr_align_test_clk_pll_en_n" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_dllstr_align_test_clk_pll_en_n</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_dllstr_align_test_clk_pll_en_n</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_test_clk_pll_en_n_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_inctrl_gr0" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_inctrl_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_inctrl_gr0</ipxact:displayName>
          <ipxact:value>aib_inctrl0_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_inctrl_gr1" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_inctrl_gr1</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_inctrl_gr1</ipxact:displayName>
          <ipxact:value>aib_inctrl1_setting3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_inctrl_gr2" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_inctrl_gr2</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_inctrl_gr2</ipxact:displayName>
          <ipxact:value>aib_inctrl2_setting2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_inctrl_gr3" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_inctrl_gr3</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_inctrl_gr3</ipxact:displayName>
          <ipxact:value>aib_inctrl3_setting2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_outctrl_gr0" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_outctrl_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_outctrl_gr0</ipxact:displayName>
          <ipxact:value>aib_outen0_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_outctrl_gr1" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_outctrl_gr1</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_outctrl_gr1</ipxact:displayName>
          <ipxact:value>aib_outen1_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_outctrl_gr2" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_outctrl_gr2</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_outctrl_gr2</ipxact:displayName>
          <ipxact:value>aib_outen2_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_outndrv_r12" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_outndrv_r12</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_outndrv_r12</ipxact:displayName>
          <ipxact:value>aib_ndrv12_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_outndrv_r34" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_outndrv_r34</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_outndrv_r34</ipxact:displayName>
          <ipxact:value>aib_ndrv34_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_outndrv_r56" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_outndrv_r56</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_outndrv_r56</ipxact:displayName>
          <ipxact:value>aib_ndrv56_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_outndrv_r78" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_outndrv_r78</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_outndrv_r78</ipxact:displayName>
          <ipxact:value>aib_ndrv78_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_outpdrv_r12" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_outpdrv_r12</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_outpdrv_r12</ipxact:displayName>
          <ipxact:value>aib_pdrv12_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_outpdrv_r34" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_outpdrv_r34</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_outpdrv_r34</ipxact:displayName>
          <ipxact:value>aib_pdrv34_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_outpdrv_r56" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_outpdrv_r56</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_outpdrv_r56</ipxact:displayName>
          <ipxact:value>aib_pdrv56_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_outpdrv_r78" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_outpdrv_r78</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_outpdrv_r78</ipxact:displayName>
          <ipxact:value>aib_pdrv78_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_red_dirclkn_shiften" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_red_dirclkn_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_red_dirclkn_shiften</ipxact:displayName>
          <ipxact:value>aib_red_dirclkn_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_red_dirclkp_shiften" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_red_dirclkp_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_red_dirclkp_shiften</ipxact:displayName>
          <ipxact:value>aib_red_dirclkp_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_red_drx_shiften" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_red_drx_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_red_drx_shiften</ipxact:displayName>
          <ipxact:value>aib_red_drx_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_red_dtx_shiften" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_red_dtx_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_red_dtx_shiften</ipxact:displayName>
          <ipxact:value>aib_red_dtx_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_red_pinp_shiften" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_red_pinp_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_red_pinp_shiften</ipxact:displayName>
          <ipxact:value>aib_red_pinp_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_red_rx_shiften" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_red_rx_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_red_rx_shiften</ipxact:displayName>
          <ipxact:value>aib_red_rx_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_red_tx_shiften" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_red_tx_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_red_tx_shiften</ipxact:displayName>
          <ipxact:value>aib_red_tx_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_red_txferclkout_shiften" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_red_txferclkout_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_red_txferclkout_shiften</ipxact:displayName>
          <ipxact:value>aib_red_txferclkout_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_aib_red_txferclkoutn_shiften" type="string">
          <ipxact:name>hssi_aibcr_tx_aib_red_txferclkoutn_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_aib_red_txferclkoutn_shiften</ipxact:displayName>
          <ipxact:value>aib_red_txferclkoutn_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_dfd_dll_dcc_en" type="string">
          <ipxact:name>hssi_aibcr_tx_dfd_dll_dcc_en</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_dfd_dll_dcc_en</ipxact:displayName>
          <ipxact:value>disable_dfd</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_dft_hssitestip_dll_dcc_en" type="string">
          <ipxact:name>hssi_aibcr_tx_dft_hssitestip_dll_dcc_en</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_dft_hssitestip_dll_dcc_en</ipxact:displayName>
          <ipxact:value>disable_dft</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_op_mode" type="string">
          <ipxact:name>hssi_aibcr_tx_op_mode</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_op_mode</ipxact:displayName>
          <ipxact:value>tx_dll_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_powermode_ac" type="string">
          <ipxact:name>hssi_aibcr_tx_powermode_ac</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_powermode_ac</ipxact:displayName>
          <ipxact:value>txdatapath_high_speed_pwr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_powermode_dc" type="string">
          <ipxact:name>hssi_aibcr_tx_powermode_dc</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_powermode_dc</ipxact:displayName>
          <ipxact:value>powerup</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_redundancy_en" type="string">
          <ipxact:name>hssi_aibcr_tx_redundancy_en</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_redundancy_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_sup_mode" type="string">
          <ipxact:name>hssi_aibcr_tx_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibcr_tx_silicon_rev" type="string">
          <ipxact:name>hssi_aibcr_tx_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_aibcr_tx_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_ber_margining_ctrl" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_ber_margining_ctrl</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_ber_margining_ctrl</ipxact:displayName>
          <ipxact:value>aib_ber_margining_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_datasel_gr0" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_datasel_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_datasel_gr0</ipxact:displayName>
          <ipxact:value>aib_datasel0_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_datasel_gr1" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_datasel_gr1</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_datasel_gr1</ipxact:displayName>
          <ipxact:value>aib_datasel1_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_datasel_gr2" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_datasel_gr2</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_datasel_gr2</ipxact:displayName>
          <ipxact:value>aib_datasel2_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_clkdiv" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_clkdiv</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_clkdiv</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_clkdiv_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_dly_pst" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_dly_pst</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_dly_pst</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_dly_pst_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_dy_ctl_static" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_dy_ctl_static</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_dy_ctl_static</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_dy_ctl_static_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_dy_ctlsel" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_dy_ctlsel</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_dy_ctlsel</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_dy_ctlsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_entest" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_entest</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_entest</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_test_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_halfcode" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_halfcode</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_halfcode</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_halfcode_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_selflock" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_selflock</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_selflock</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_selflock_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_st_core_dn_prgmnvrt" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_st_core_dn_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_st_core_dn_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_core_dn_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_st_core_up_prgmnvrt" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_st_core_up_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_st_core_up_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_core_up_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_st_core_updnen" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_st_core_updnen</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_st_core_updnen</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_core_updnen_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_st_dftmuxsel" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_st_dftmuxsel</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_st_dftmuxsel</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_dftmuxsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_st_en" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_st_en</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_st_en</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_en_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_st_hps_ctrl_en" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_st_hps_ctrl_en</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_st_hps_ctrl_en</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_hps_ctrl_en_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_st_lockreq_muxsel" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_st_lockreq_muxsel</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_st_lockreq_muxsel</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_lockreq_muxsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_st_new_dll" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_st_new_dll</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_st_new_dll</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_new_dll_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_st_rst" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_st_rst</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_st_rst</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_rst_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_st_rst_prgmnvrt" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_st_rst_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_st_rst_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_st_rst_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_dllstr_align_test_clk_pll_en_n" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_dllstr_align_test_clk_pll_en_n</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_dllstr_align_test_clk_pll_en_n</ipxact:displayName>
          <ipxact:value>aib_dllstr_align_test_clk_pll_en_n_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_inctrl_gr0" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_inctrl_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_inctrl_gr0</ipxact:displayName>
          <ipxact:value>aib_inctrl0_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_inctrl_gr1" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_inctrl_gr1</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_inctrl_gr1</ipxact:displayName>
          <ipxact:value>aib_inctrl1_setting3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_inctrl_gr2" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_inctrl_gr2</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_inctrl_gr2</ipxact:displayName>
          <ipxact:value>aib_inctrl2_setting2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_inctrl_gr3" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_inctrl_gr3</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_inctrl_gr3</ipxact:displayName>
          <ipxact:value>aib_inctrl3_setting3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_outctrl_gr0" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_outctrl_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_outctrl_gr0</ipxact:displayName>
          <ipxact:value>aib_outen0_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_outctrl_gr1" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_outctrl_gr1</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_outctrl_gr1</ipxact:displayName>
          <ipxact:value>aib_outen1_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_outctrl_gr2" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_outctrl_gr2</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_outctrl_gr2</ipxact:displayName>
          <ipxact:value>aib_outen2_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_outndrv_r12" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_outndrv_r12</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_outndrv_r12</ipxact:displayName>
          <ipxact:value>aib_ndrv12_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_outndrv_r34" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_outndrv_r34</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_outndrv_r34</ipxact:displayName>
          <ipxact:value>aib_ndrv34_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_outndrv_r56" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_outndrv_r56</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_outndrv_r56</ipxact:displayName>
          <ipxact:value>aib_ndrv56_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_outndrv_r78" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_outndrv_r78</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_outndrv_r78</ipxact:displayName>
          <ipxact:value>aib_ndrv78_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_outpdrv_r12" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_outpdrv_r12</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_outpdrv_r12</ipxact:displayName>
          <ipxact:value>aib_pdrv12_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_outpdrv_r34" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_outpdrv_r34</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_outpdrv_r34</ipxact:displayName>
          <ipxact:value>aib_pdrv34_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_outpdrv_r56" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_outpdrv_r56</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_outpdrv_r56</ipxact:displayName>
          <ipxact:value>aib_pdrv56_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_outpdrv_r78" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_outpdrv_r78</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_outpdrv_r78</ipxact:displayName>
          <ipxact:value>aib_pdrv78_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_aib_red_shift_en" type="string">
          <ipxact:name>hssi_aibnd_rx_aib_red_shift_en</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_aib_red_shift_en</ipxact:displayName>
          <ipxact:value>aib_red_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_dft_hssitestip_dll_dcc_en" type="string">
          <ipxact:name>hssi_aibnd_rx_dft_hssitestip_dll_dcc_en</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_dft_hssitestip_dll_dcc_en</ipxact:displayName>
          <ipxact:value>disable_dft</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_op_mode" type="string">
          <ipxact:name>hssi_aibnd_rx_op_mode</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_op_mode</ipxact:displayName>
          <ipxact:value>rx_dll_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_powerdown_mode" type="string">
          <ipxact:name>hssi_aibnd_rx_powerdown_mode</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_powerdown_mode</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_powermode_ac" type="string">
          <ipxact:name>hssi_aibnd_rx_powermode_ac</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_powermode_ac</ipxact:displayName>
          <ipxact:value>rxdatapath_high_speed_pwr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_powermode_dc" type="string">
          <ipxact:name>hssi_aibnd_rx_powermode_dc</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_powermode_dc</ipxact:displayName>
          <ipxact:value>powerup</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_redundancy_en" type="string">
          <ipxact:name>hssi_aibnd_rx_redundancy_en</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_redundancy_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_sup_mode" type="string">
          <ipxact:name>hssi_aibnd_rx_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_rx_silicon_rev" type="string">
          <ipxact:name>hssi_aibnd_rx_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_aibnd_rx_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_datasel_gr0" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_datasel_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_datasel_gr0</ipxact:displayName>
          <ipxact:value>aib_datasel0_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_datasel_gr1" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_datasel_gr1</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_datasel_gr1</ipxact:displayName>
          <ipxact:value>aib_datasel1_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_datasel_gr2" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_datasel_gr2</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_datasel_gr2</ipxact:displayName>
          <ipxact:value>aib_datasel2_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_datasel_gr3" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_datasel_gr3</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_datasel_gr3</ipxact:displayName>
          <ipxact:value>aib_datasel3_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_ddrctrl_gr0" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_ddrctrl_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_ddrctrl_gr0</ipxact:displayName>
          <ipxact:value>aib_ddr0_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_iinasyncen" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_iinasyncen</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_iinasyncen</ipxact:displayName>
          <ipxact:value>aib_inasyncen_setting2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_iinclken" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_iinclken</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_iinclken</ipxact:displayName>
          <ipxact:value>aib_inclken_setting3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_outctrl_gr0" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_outctrl_gr0</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_outctrl_gr0</ipxact:displayName>
          <ipxact:value>aib_outen0_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_outctrl_gr1" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_outctrl_gr1</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_outctrl_gr1</ipxact:displayName>
          <ipxact:value>aib_outen1_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_outctrl_gr2" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_outctrl_gr2</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_outctrl_gr2</ipxact:displayName>
          <ipxact:value>aib_outen2_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_outctrl_gr3" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_outctrl_gr3</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_outctrl_gr3</ipxact:displayName>
          <ipxact:value>aib_outen3_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_outndrv_r34" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_outndrv_r34</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_outndrv_r34</ipxact:displayName>
          <ipxact:value>aib_ndrv34_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_outndrv_r56" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_outndrv_r56</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_outndrv_r56</ipxact:displayName>
          <ipxact:value>aib_ndrv56_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_outpdrv_r34" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_outpdrv_r34</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_outpdrv_r34</ipxact:displayName>
          <ipxact:value>aib_pdrv34_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_outpdrv_r56" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_outpdrv_r56</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_outpdrv_r56</ipxact:displayName>
          <ipxact:value>aib_pdrv56_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_red_dirclkn_shiften" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_red_dirclkn_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_red_dirclkn_shiften</ipxact:displayName>
          <ipxact:value>aib_red_dirclkn_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_red_dirclkp_shiften" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_red_dirclkp_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_red_dirclkp_shiften</ipxact:displayName>
          <ipxact:value>aib_red_dirclkp_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_red_drx_shiften" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_red_drx_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_red_drx_shiften</ipxact:displayName>
          <ipxact:value>aib_red_drx_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_red_dtx_shiften" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_red_dtx_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_red_dtx_shiften</ipxact:displayName>
          <ipxact:value>aib_red_dtx_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_red_pout_shiften" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_red_pout_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_red_pout_shiften</ipxact:displayName>
          <ipxact:value>aib_red_pout_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_red_rx_shiften" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_red_rx_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_red_rx_shiften</ipxact:displayName>
          <ipxact:value>aib_red_rx_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_red_tx_shiften" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_red_tx_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_red_tx_shiften</ipxact:displayName>
          <ipxact:value>aib_red_tx_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_red_txferclkout_shiften" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_red_txferclkout_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_red_txferclkout_shiften</ipxact:displayName>
          <ipxact:value>aib_red_txferclkout_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_red_txferclkoutn_shiften" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_red_txferclkoutn_shiften</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_red_txferclkoutn_shiften</ipxact:displayName>
          <ipxact:value>aib_red_txferclkoutn_shift_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_clkdiv" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_clkdiv</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_clkdiv</ipxact:displayName>
          <ipxact:value>aib_tx_clkdiv_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_byp" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_byp</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_byp</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_byp_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_byp_iocsr_unused" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_byp_iocsr_unused</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_byp_iocsr_unused</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_byp_disable_iocsr_unused</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_cont_cal" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_cont_cal</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_cont_cal</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_cal_cont</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_cont_cal_iocsr_unused" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_cont_cal_iocsr_unused</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_cont_cal_iocsr_unused</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_cal_single_iocsr_unused</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_dft" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_dft</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_dft</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_dft_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_dft_sel" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_dft_sel</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_dft_sel</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_dft_mode0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_dll_dft_sel" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_dll_dft_sel</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_dll_dft_sel</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_dll_dft_sel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_dll_entest" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_dll_entest</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_dll_entest</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_dll_test_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_dy_ctl_static" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_dy_ctl_static</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_dy_ctl_static</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_dy_ctl_static_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_dy_ctlsel" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_dy_ctlsel</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_dy_ctlsel</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_dy_ctlsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_en" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_en</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_en</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_en_iocsr_unused" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_en_iocsr_unused</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_en_iocsr_unused</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_disable_iocsr_unused</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_manual_dn" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_manual_dn</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_manual_dn</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_manual_dn0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_manual_up" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_manual_up</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_manual_up</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_manual_up0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_rst_prgmnvrt" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_rst_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_rst_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_st_rst_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_st_core_dn_prgmnvrt" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_st_core_dn_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_st_core_dn_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_st_core_dn_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_st_core_up_prgmnvrt" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_st_core_up_prgmnvrt</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_st_core_up_prgmnvrt</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_st_core_up_prgmnvrt_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_st_core_updnen" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_st_core_updnen</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_st_core_updnen</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_st_core_updnen_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_st_dftmuxsel" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_st_dftmuxsel</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_st_dftmuxsel</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_st_dftmuxsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_st_dly_pst" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_st_dly_pst</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_st_dly_pst</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_st_dly_pst_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_st_en" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_st_en</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_st_en</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_st_en_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_st_hps_ctrl_en" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_st_hps_ctrl_en</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_st_hps_ctrl_en</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_hps_ctrl_en_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_st_lockreq_muxsel" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_st_lockreq_muxsel</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_st_lockreq_muxsel</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_st_lockreq_muxsel_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_st_new_dll" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_st_new_dll</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_st_new_dll</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_new_dll_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_st_rst" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_st_rst</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_st_rst</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_st_rst_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_dcc_test_clk_pll_en_n" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_dcc_test_clk_pll_en_n</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_dcc_test_clk_pll_en_n</ipxact:displayName>
          <ipxact:value>aib_tx_dcc_test_clk_pll_en_n_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_halfcode" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_halfcode</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_halfcode</ipxact:displayName>
          <ipxact:value>aib_tx_halfcode_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_aib_tx_selflock" type="string">
          <ipxact:name>hssi_aibnd_tx_aib_tx_selflock</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_aib_tx_selflock</ipxact:displayName>
          <ipxact:value>aib_tx_selflock_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_dfd_dll_dcc_en" type="string">
          <ipxact:name>hssi_aibnd_tx_dfd_dll_dcc_en</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_dfd_dll_dcc_en</ipxact:displayName>
          <ipxact:value>disable_dfd</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_dft_hssitestip_dll_dcc_en" type="string">
          <ipxact:name>hssi_aibnd_tx_dft_hssitestip_dll_dcc_en</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_dft_hssitestip_dll_dcc_en</ipxact:displayName>
          <ipxact:value>disable_dft</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_op_mode" type="string">
          <ipxact:name>hssi_aibnd_tx_op_mode</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_op_mode</ipxact:displayName>
          <ipxact:value>tx_dcc_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_powerdown_mode" type="string">
          <ipxact:name>hssi_aibnd_tx_powerdown_mode</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_powerdown_mode</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_powermode_ac" type="string">
          <ipxact:name>hssi_aibnd_tx_powermode_ac</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_powermode_ac</ipxact:displayName>
          <ipxact:value>txdatapath_high_speed_pwr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_powermode_dc" type="string">
          <ipxact:name>hssi_aibnd_tx_powermode_dc</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_powermode_dc</ipxact:displayName>
          <ipxact:value>powerup</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_redundancy_en" type="string">
          <ipxact:name>hssi_aibnd_tx_redundancy_en</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_redundancy_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_sup_mode" type="string">
          <ipxact:name>hssi_aibnd_tx_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_aibnd_tx_silicon_rev" type="string">
          <ipxact:name>hssi_aibnd_tx_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_aibnd_tx_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pcs_arbiter_ctrl" type="string">
          <ipxact:name>hssi_avmm1_if_pcs_arbiter_ctrl</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pcs_arbiter_ctrl</ipxact:displayName>
          <ipxact:value>avmm1_arbiter_uc_sel</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_avmm_clk_dcg_en" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_avmm_clk_dcg_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_avmm_clk_dcg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_avmm_clk_scg_en" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_avmm_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_avmm_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pldadapt_avmm_clk_scg_en" type="string">
          <ipxact:name>hssi_avmm1_if_pldadapt_avmm_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pldadapt_avmm_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pcs_cal_done" type="string">
          <ipxact:name>hssi_avmm1_if_pcs_cal_done</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pcs_cal_done</ipxact:displayName>
          <ipxact:value>avmm1_cal_done_deassert</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pcs_cal_reserved" type="int">
          <ipxact:name>hssi_avmm1_if_pcs_cal_reserved</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pcs_cal_reserved</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pcs_calibration_feature_en" type="string">
          <ipxact:name>hssi_avmm1_if_pcs_calibration_feature_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pcs_calibration_feature_en</ipxact:displayName>
          <ipxact:value>avmm1_pcs_calibration_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pldadapt_gate_dis" type="string">
          <ipxact:name>hssi_avmm1_if_pldadapt_gate_dis</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pldadapt_gate_dis</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pcs_hip_cal_en" type="string">
          <ipxact:name>hssi_avmm1_if_pcs_hip_cal_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pcs_hip_cal_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_nfhssi_calibratio_feature_en" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_nfhssi_calibratio_feature_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_nfhssi_calibratio_feature_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pldadapt_nfhssi_calibratio_feature_en" type="string">
          <ipxact:name>hssi_avmm1_if_pldadapt_nfhssi_calibratio_feature_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pldadapt_nfhssi_calibratio_feature_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pldadapt_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_avmm1_if_pldadapt_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pldadapt_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_read_blocking_enable" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_read_blocking_enable</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_read_blocking_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pldadapt_read_blocking_enable" type="string">
          <ipxact:name>hssi_avmm1_if_pldadapt_read_blocking_enable</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pldadapt_read_blocking_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_uc_blocking_enable" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_uc_blocking_enable</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_uc_blocking_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pldadapt_uc_blocking_enable" type="string">
          <ipxact:name>hssi_avmm1_if_pldadapt_uc_blocking_enable</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pldadapt_uc_blocking_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_write_resp_en" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_write_resp_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_write_resp_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_avmm_osc_clock_setting" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_avmm_osc_clock_setting</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_avmm_osc_clock_setting</ipxact:displayName>
          <ipxact:value>osc_clk_div_by1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pldadapt_avmm_osc_clock_setting" type="string">
          <ipxact:name>hssi_avmm1_if_pldadapt_avmm_osc_clock_setting</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pldadapt_avmm_osc_clock_setting</ipxact:displayName>
          <ipxact:value>osc_clk_div_by1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_avmm_testbus_sel" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_avmm_testbus_sel</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_avmm_testbus_sel</ipxact:displayName>
          <ipxact:value>avmm1_transfer_testbus</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pldadapt_avmm_testbus_sel" type="string">
          <ipxact:name>hssi_avmm1_if_pldadapt_avmm_testbus_sel</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pldadapt_avmm_testbus_sel</ipxact:displayName>
          <ipxact:value>avmm1_transfer_testbus</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_func_mode" type="string">
          <ipxact:name>hssi_avmm1_if_func_mode</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_func_mode</ipxact:displayName>
          <ipxact:value>c3adpt_pmadir</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_sr_hip_mode" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_sr_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_sr_hip_mode</ipxact:displayName>
          <ipxact:value>disable_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_hip_mode" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_hip_mode</ipxact:displayName>
          <ipxact:value>disable_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_pldadapt_hip_mode" type="string">
          <ipxact:name>hssi_avmm1_if_pldadapt_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_pldadapt_hip_mode</ipxact:displayName>
          <ipxact:value>disable_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_sr_powerdown_mode" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_sr_powerdown_mode</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_sr_powerdown_mode</ipxact:displayName>
          <ipxact:value>powerup</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_sr_sr_free_run_div_clk" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_sr_sr_free_run_div_clk</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_sr_sr_free_run_div_clk</ipxact:displayName>
          <ipxact:value>out_of_reset_sync</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_sr_sr_hip_en" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_sr_sr_hip_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_sr_sr_hip_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_sr_sr_osc_clk_div_sel" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_sr_sr_osc_clk_div_sel</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_sr_sr_osc_clk_div_sel</ipxact:displayName>
          <ipxact:value>non_div</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_sr_sr_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_sr_sr_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_sr_sr_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_sr_sr_parity_en" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_sr_sr_parity_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_sr_sr_parity_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_sr_sr_reserved_in_en" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_sr_sr_reserved_in_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_sr_sr_reserved_in_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_sr_sr_reserved_out_en" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_sr_sr_reserved_out_en</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_sr_sr_reserved_out_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_hssiadapt_sr_sup_mode" type="string">
          <ipxact:name>hssi_avmm1_if_hssiadapt_sr_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_hssiadapt_sr_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_topology" type="string">
          <ipxact:name>hssi_avmm1_if_topology</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_topology</ipxact:displayName>
          <ipxact:value>disabled_block</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_silicon_rev" type="string">
          <ipxact:name>hssi_avmm1_if_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_avmm1_if_calibration_type" type="string">
          <ipxact:name>hssi_avmm1_if_calibration_type</ipxact:name>
          <ipxact:displayName>hssi_avmm1_if_calibration_type</ipxact:displayName>
          <ipxact:value>one_time</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_asn_clk_enable" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_asn_clk_enable</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_asn_clk_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_asn_enable" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_asn_enable</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_asn_enable</ipxact:displayName>
          <ipxact:value>dis_asn</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_block_sel" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_block_sel</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_block_sel</ipxact:displayName>
          <ipxact:value>eight_g_pcs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_bypass_early_eios" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_bypass_early_eios</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_bypass_early_eios</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_bypass_pcie_switch" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_bypass_pcie_switch</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_bypass_pcie_switch</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_bypass_pma_ltr" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_bypass_pma_ltr</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_bypass_pma_ltr</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_bypass_pma_sw_done" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_bypass_pma_sw_done</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_bypass_pma_sw_done</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_bypass_ppm_lock" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_bypass_ppm_lock</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_bypass_ppm_lock</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_bypass_send_syncp_fbkp" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_bypass_send_syncp_fbkp</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_bypass_send_syncp_fbkp</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_bypass_txdetectrx" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_bypass_txdetectrx</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_bypass_txdetectrx</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_cdr_control" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_cdr_control</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_cdr_control</ipxact:displayName>
          <ipxact:value>dis_cdr_ctrl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_cid_enable" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_cid_enable</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_cid_enable</ipxact:displayName>
          <ipxact:value>dis_cid_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_cp_cons_sel" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_cp_cons_sel</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_cp_cons_sel</ipxact:displayName>
          <ipxact:value>cp_cons_master</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_cp_dwn_mstr" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_cp_dwn_mstr</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_cp_dwn_mstr</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_cp_up_mstr" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_cp_up_mstr</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_cp_up_mstr</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_ctrl_plane_bonding" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_ctrl_plane_bonding</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_ctrl_plane_bonding</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_data_mask_count" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_data_mask_count</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_data_mask_count</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_data_mask_count_multi" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_data_mask_count_multi</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_data_mask_count_multi</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_dft_observation_clock_selection" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_dft_observation_clock_selection</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_dft_observation_clock_selection</ipxact:displayName>
          <ipxact:value>dft_clk_obsrv_tx0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_early_eios_counter" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_early_eios_counter</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_early_eios_counter</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_force_freqdet" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_force_freqdet</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_force_freqdet</ipxact:displayName>
          <ipxact:value>force_freqdet_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_free_run_clk_enable" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_free_run_clk_enable</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_free_run_clk_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_ignore_sigdet_g23" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_ignore_sigdet_g23</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_ignore_sigdet_g23</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_pc_en_counter" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_pc_en_counter</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_pc_en_counter</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_pc_rst_counter" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_pc_rst_counter</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_pc_rst_counter</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_pcie_hip_mode" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_pcie_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_pcie_hip_mode</ipxact:displayName>
          <ipxact:value>hip_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_ph_fifo_reg_mode" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_ph_fifo_reg_mode</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_ph_fifo_reg_mode</ipxact:displayName>
          <ipxact:value>phfifo_reg_mode_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_phfifo_flush_wait" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_phfifo_flush_wait</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_phfifo_flush_wait</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_pipe_if_g3pcs" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_pipe_if_g3pcs</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_pipe_if_g3pcs</ipxact:displayName>
          <ipxact:value>pipe_if_8gpcs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_pma_done_counter" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_pma_done_counter</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_pma_done_counter</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_pma_if_dft_en" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_pma_if_dft_en</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_pma_if_dft_en</ipxact:displayName>
          <ipxact:value>dft_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_pma_if_dft_val" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_pma_if_dft_val</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_pma_if_dft_val</ipxact:displayName>
          <ipxact:value>dft_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_ppm_cnt_rst" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_ppm_cnt_rst</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_ppm_cnt_rst</ipxact:displayName>
          <ipxact:value>ppm_cnt_rst_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_ppm_deassert_early" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_ppm_deassert_early</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_ppm_deassert_early</ipxact:displayName>
          <ipxact:value>deassert_early_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_ppm_det_buckets" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_ppm_det_buckets</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_ppm_det_buckets</ipxact:displayName>
          <ipxact:value>ppm_100_bucket</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_ppm_gen1_2_cnt" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_ppm_gen1_2_cnt</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_ppm_gen1_2_cnt</ipxact:displayName>
          <ipxact:value>cnt_32k</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_ppm_post_eidle_delay" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_ppm_post_eidle_delay</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_ppm_post_eidle_delay</ipxact:displayName>
          <ipxact:value>cnt_200_cycles</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_ppmsel" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_ppmsel</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_ppmsel</ipxact:displayName>
          <ipxact:value>ppmsel_100</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_prot_mode" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_prot_mode</ipxact:displayName>
          <ipxact:value>other_protocols</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_rxvalid_mask" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_rxvalid_mask</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_rxvalid_mask</ipxact:displayName>
          <ipxact:value>rxvalid_mask_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_sigdet_wait_counter" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_sigdet_wait_counter</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_sigdet_wait_counter</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_sigdet_wait_counter_multi" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_sigdet_wait_counter_multi</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_sigdet_wait_counter_multi</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_sim_mode" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_sim_mode</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_sim_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_spd_chg_rst_wait_cnt_en" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_spd_chg_rst_wait_cnt_en</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_spd_chg_rst_wait_cnt_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_sup_mode" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_testout_sel" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_testout_sel</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_testout_sel</ipxact:displayName>
          <ipxact:value>ppm_det_test</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_wait_clk_on_off_timer" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_wait_clk_on_off_timer</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_wait_clk_on_off_timer</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_wait_pipe_synchronizing" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_wait_pipe_synchronizing</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_wait_pipe_synchronizing</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_wait_send_syncp_fbkp" type="int">
          <ipxact:name>hssi_common_pcs_pma_interface_wait_send_syncp_fbkp</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_wait_send_syncp_fbkp</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_silicon_rev" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pcs_pma_interface_reconfig_settings" type="string">
          <ipxact:name>hssi_common_pcs_pma_interface_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_common_pcs_pma_interface_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pld_pcs_interface_dft_clk_out_en" type="string">
          <ipxact:name>hssi_common_pld_pcs_interface_dft_clk_out_en</ipxact:name>
          <ipxact:displayName>hssi_common_pld_pcs_interface_dft_clk_out_en</ipxact:displayName>
          <ipxact:value>dft_clk_out_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pld_pcs_interface_dft_clk_out_sel" type="string">
          <ipxact:name>hssi_common_pld_pcs_interface_dft_clk_out_sel</ipxact:name>
          <ipxact:displayName>hssi_common_pld_pcs_interface_dft_clk_out_sel</ipxact:displayName>
          <ipxact:value>teng_rx_dft_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pld_pcs_interface_hrdrstctrl_en" type="string">
          <ipxact:name>hssi_common_pld_pcs_interface_hrdrstctrl_en</ipxact:name>
          <ipxact:displayName>hssi_common_pld_pcs_interface_hrdrstctrl_en</ipxact:displayName>
          <ipxact:value>hrst_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pld_pcs_interface_pcs_testbus_block_sel" type="string">
          <ipxact:name>hssi_common_pld_pcs_interface_pcs_testbus_block_sel</ipxact:name>
          <ipxact:displayName>hssi_common_pld_pcs_interface_pcs_testbus_block_sel</ipxact:displayName>
          <ipxact:value>pma_if</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pld_pcs_interface_silicon_rev" type="string">
          <ipxact:name>hssi_common_pld_pcs_interface_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_common_pld_pcs_interface_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_common_pld_pcs_interface_reconfig_settings" type="string">
          <ipxact:name>hssi_common_pld_pcs_interface_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_common_pld_pcs_interface_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_sequencer_rx_path_rstn_overrideb" type="string">
          <ipxact:name>pma_adapt_sequencer_rx_path_rstn_overrideb</ipxact:name>
          <ipxact:displayName>pma_adapt_sequencer_rx_path_rstn_overrideb</ipxact:displayName>
          <ipxact:value>use_sequencer</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_sequencer_silicon_rev" type="string">
          <ipxact:name>pma_adapt_sequencer_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_adapt_sequencer_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_pcie_gen_switch_rx_path_pcie_gen_switch_en" type="string">
          <ipxact:name>pma_pcie_gen_switch_rx_path_pcie_gen_switch_en</ipxact:name>
          <ipxact:displayName>pma_pcie_gen_switch_rx_path_pcie_gen_switch_en</ipxact:displayName>
          <ipxact:value>bypass_pcie_switch</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_pcie_gen_switch_rx_pci_switch_dly" type="int">
          <ipxact:name>pma_pcie_gen_switch_rx_pci_switch_dly</ipxact:name>
          <ipxact:displayName>pma_pcie_gen_switch_rx_pci_switch_dly</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_pcie_gen_switch_silicon_rev" type="string">
          <ipxact:name>pma_pcie_gen_switch_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_pcie_gen_switch_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adapt_mode" type="string">
          <ipxact:name>pma_adapt_adapt_mode</ipxact:name>
          <ipxact:displayName>pma_adapt_adapt_mode</ipxact:displayName>
          <ipxact:value>manual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_ac_ctle_cal_win" type="string">
          <ipxact:name>pma_adapt_adp_ac_ctle_cal_win</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_ac_ctle_cal_win</ipxact:displayName>
          <ipxact:value>radp_ac_ctle_cal_win_4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_ac_ctle_cocurrent_mode_sel" type="string">
          <ipxact:name>pma_adapt_adp_ac_ctle_cocurrent_mode_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_ac_ctle_cocurrent_mode_sel</ipxact:displayName>
          <ipxact:value>radp_ac_ctle_cocurrent_mode_sel_mode_1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_ac_ctle_en" type="string">
          <ipxact:name>pma_adapt_adp_ac_ctle_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_ac_ctle_en</ipxact:displayName>
          <ipxact:value>radp_ac_ctle_en_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_ac_ctle_hold_en" type="string">
          <ipxact:name>pma_adapt_adp_ac_ctle_hold_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_ac_ctle_hold_en</ipxact:displayName>
          <ipxact:value>radp_ac_ctle_hold_en_not_hold</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_ac_ctle_initial_load" type="string">
          <ipxact:name>pma_adapt_adp_ac_ctle_initial_load</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_ac_ctle_initial_load</ipxact:displayName>
          <ipxact:value>radp_ac_ctle_initial_load_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_ac_ctle_initial_value" type="string">
          <ipxact:name>pma_adapt_adp_ac_ctle_initial_value</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_ac_ctle_initial_value</ipxact:displayName>
          <ipxact:value>radp_ac_ctle_initial_value_8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_ac_ctle_mode_sel" type="string">
          <ipxact:name>pma_adapt_adp_ac_ctle_mode_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_ac_ctle_mode_sel</ipxact:displayName>
          <ipxact:value>radp_ac_ctle_mode_sel_concurrent</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_ac_ctle_ph1_win" type="string">
          <ipxact:name>pma_adapt_adp_ac_ctle_ph1_win</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_ac_ctle_ph1_win</ipxact:displayName>
          <ipxact:value>radp_ac_ctle_ph1_win_2p19</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_adapt_control_sel" type="string">
          <ipxact:name>pma_adapt_adp_adapt_control_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_adapt_control_sel</ipxact:displayName>
          <ipxact:value>radp_adapt_control_sel_from_cram</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_adapt_start" type="string">
          <ipxact:name>pma_adapt_adp_adapt_start</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_adapt_start</ipxact:displayName>
          <ipxact:value>radp_adapt_start_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_bist_datapath_en" type="string">
          <ipxact:name>pma_adapt_adp_bist_datapath_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_bist_datapath_en</ipxact:displayName>
          <ipxact:value>radp_bist_datapath_en_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_bist_errcount_rstn" type="string">
          <ipxact:name>pma_adapt_adp_bist_errcount_rstn</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_bist_errcount_rstn</ipxact:displayName>
          <ipxact:value>radp_bist_errcount_rstn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_bist_mode_sel" type="string">
          <ipxact:name>pma_adapt_adp_bist_mode_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_bist_mode_sel</ipxact:displayName>
          <ipxact:value>radp_bist_mode_sel_prbs31</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_clkgate_enb" type="string">
          <ipxact:name>pma_adapt_adp_clkgate_enb</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_clkgate_enb</ipxact:displayName>
          <ipxact:value>radp_clkgate_enb_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_clkout_div_sel" type="string">
          <ipxact:name>pma_adapt_adp_clkout_div_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_clkout_div_sel</ipxact:displayName>
          <ipxact:value>radp_clkout_div_sel_div2_4cycle</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_ctle_bypass_ac" type="string">
          <ipxact:name>pma_adapt_adp_ctle_bypass_ac</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_ctle_bypass_ac</ipxact:displayName>
          <ipxact:value>radp_ctle_bypass_ac_bypass</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_ctle_bypass_dc" type="string">
          <ipxact:name>pma_adapt_adp_ctle_bypass_dc</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_ctle_bypass_dc</ipxact:displayName>
          <ipxact:value>radp_ctle_bypass_dc_bypass</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_accum_depth" type="int">
          <ipxact:name>pma_adapt_adp_dc_ctle_accum_depth</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_accum_depth</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_en" type="string">
          <ipxact:name>pma_adapt_adp_dc_ctle_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_en</ipxact:displayName>
          <ipxact:value>radp_dc_ctle_en_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_hold_en" type="string">
          <ipxact:name>pma_adapt_adp_dc_ctle_hold_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_hold_en</ipxact:displayName>
          <ipxact:value>radp_dc_ctle_hold_en_not_hold</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_initial_load" type="string">
          <ipxact:name>pma_adapt_adp_dc_ctle_initial_load</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_initial_load</ipxact:displayName>
          <ipxact:value>radp_dc_ctle_initial_load_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_initial_value" type="string">
          <ipxact:name>pma_adapt_adp_dc_ctle_initial_value</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_initial_value</ipxact:displayName>
          <ipxact:value>radp_dc_ctle_initial_value_16</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_mode0_win_size" type="string">
          <ipxact:name>pma_adapt_adp_dc_ctle_mode0_win_size</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_mode0_win_size</ipxact:displayName>
          <ipxact:value>radp_dc_ctle_mode0_win_size_4_taps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_mode0_win_start" type="int">
          <ipxact:name>pma_adapt_adp_dc_ctle_mode0_win_start</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_mode0_win_start</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_mode1_h1_ratio" type="int">
          <ipxact:name>pma_adapt_adp_dc_ctle_mode1_h1_ratio</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_mode1_h1_ratio</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_mode2_h2_limit" type="int">
          <ipxact:name>pma_adapt_adp_dc_ctle_mode2_h2_limit</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_mode2_h2_limit</ipxact:displayName>
          <ipxact:value>7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_mode_sel" type="string">
          <ipxact:name>pma_adapt_adp_dc_ctle_mode_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_mode_sel</ipxact:displayName>
          <ipxact:value>radp_dc_ctle_mode_sel_mode_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_onetime" type="string">
          <ipxact:name>pma_adapt_adp_dc_ctle_onetime</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_onetime</ipxact:displayName>
          <ipxact:value>radp_dc_ctle_onetime_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dc_ctle_onetime_threshold" type="string">
          <ipxact:name>pma_adapt_adp_dc_ctle_onetime_threshold</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dc_ctle_onetime_threshold</ipxact:displayName>
          <ipxact:value>radp_dc_ctle_onetime_threshold_256</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dfe_accum_depth" type="int">
          <ipxact:name>pma_adapt_adp_dfe_accum_depth</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dfe_accum_depth</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dfe_en" type="string">
          <ipxact:name>pma_adapt_adp_dfe_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dfe_en</ipxact:displayName>
          <ipxact:value>radp_dfe_en_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dfe_fxtap_bypass" type="string">
          <ipxact:name>pma_adapt_adp_dfe_fxtap_bypass</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dfe_fxtap_bypass</ipxact:displayName>
          <ipxact:value>radp_dfe_fxtap_bypass_bypass</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dfe_hold_en" type="string">
          <ipxact:name>pma_adapt_adp_dfe_hold_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dfe_hold_en</ipxact:displayName>
          <ipxact:value>radp_dfe_hold_en_not_hold</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dfe_hold_sel" type="string">
          <ipxact:name>pma_adapt_adp_dfe_hold_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dfe_hold_sel</ipxact:displayName>
          <ipxact:value>radp_dfe_hold_sel_no</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dfe_onetime" type="string">
          <ipxact:name>pma_adapt_adp_dfe_onetime</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dfe_onetime</ipxact:displayName>
          <ipxact:value>radp_dfe_onetime_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dfe_onetime_threshold" type="string">
          <ipxact:name>pma_adapt_adp_dfe_onetime_threshold</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dfe_onetime_threshold</ipxact:displayName>
          <ipxact:value>radp_dfe_onetime_threshold_2048</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dfe_tap1_initial_load" type="string">
          <ipxact:name>pma_adapt_adp_dfe_tap1_initial_load</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dfe_tap1_initial_load</ipxact:displayName>
          <ipxact:value>radp_dfe_tap1_initial_load_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dfe_tap1_initial_value" type="string">
          <ipxact:name>pma_adapt_adp_dfe_tap1_initial_value</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dfe_tap1_initial_value</ipxact:displayName>
          <ipxact:value>radp_dfe_tap1_initial_value_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dfe_tap_sel_en" type="string">
          <ipxact:name>pma_adapt_adp_dfe_tap_sel_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dfe_tap_sel_en</ipxact:displayName>
          <ipxact:value>radp_dfe_tap_sel_en_no</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dlev_accum_depth" type="int">
          <ipxact:name>pma_adapt_adp_dlev_accum_depth</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dlev_accum_depth</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dlev_bypass" type="string">
          <ipxact:name>pma_adapt_adp_dlev_bypass</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dlev_bypass</ipxact:displayName>
          <ipxact:value>radp_dlev_bypass_bypass</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dlev_en" type="string">
          <ipxact:name>pma_adapt_adp_dlev_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dlev_en</ipxact:displayName>
          <ipxact:value>radp_dlev_en_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dlev_hold_en" type="string">
          <ipxact:name>pma_adapt_adp_dlev_hold_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dlev_hold_en</ipxact:displayName>
          <ipxact:value>radp_dlev_hold_en_not_hold</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dlev_initial_load" type="string">
          <ipxact:name>pma_adapt_adp_dlev_initial_load</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dlev_initial_load</ipxact:displayName>
          <ipxact:value>radp_dlev_initial_load_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dlev_initial_value" type="string">
          <ipxact:name>pma_adapt_adp_dlev_initial_value</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dlev_initial_value</ipxact:displayName>
          <ipxact:value>radp_dlev_initial_value_38</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dlev_onetime" type="string">
          <ipxact:name>pma_adapt_adp_dlev_onetime</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dlev_onetime</ipxact:displayName>
          <ipxact:value>radp_dlev_onetime_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dlev_onetime_threshold" type="string">
          <ipxact:name>pma_adapt_adp_dlev_onetime_threshold</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dlev_onetime_threshold</ipxact:displayName>
          <ipxact:value>radp_dlev_onetime_threshold_4096</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_dlev_sel" type="string">
          <ipxact:name>pma_adapt_adp_dlev_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_dlev_sel</ipxact:displayName>
          <ipxact:value>radp_dlev_sel_mux</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_force_freqlock" type="string">
          <ipxact:name>pma_adapt_adp_force_freqlock</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_force_freqlock</ipxact:displayName>
          <ipxact:value>radp_force_freqlock_use</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_frame_capture" type="string">
          <ipxact:name>pma_adapt_adp_frame_capture</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_frame_capture</ipxact:displayName>
          <ipxact:value>radp_frame_capture_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_frame_en" type="string">
          <ipxact:name>pma_adapt_adp_frame_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_frame_en</ipxact:displayName>
          <ipxact:value>radp_frame_en_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_frame_odi_sel" type="string">
          <ipxact:name>pma_adapt_adp_frame_odi_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_frame_odi_sel</ipxact:displayName>
          <ipxact:value>radp_frame_odi_sel_deser_err</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_frame_out_sel" type="string">
          <ipxact:name>pma_adapt_adp_frame_out_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_frame_out_sel</ipxact:displayName>
          <ipxact:value>radp_frame_out_sel_select_a</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_load_sig_sel" type="string">
          <ipxact:name>pma_adapt_adp_load_sig_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_load_sig_sel</ipxact:displayName>
          <ipxact:value>radp_load_sig_sel_from_interanl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_oc_accum_depth" type="int">
          <ipxact:name>pma_adapt_adp_oc_accum_depth</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_oc_accum_depth</ipxact:displayName>
          <ipxact:value>11</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_oc_bypass" type="string">
          <ipxact:name>pma_adapt_adp_oc_bypass</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_oc_bypass</ipxact:displayName>
          <ipxact:value>radp_oc_bypass_bypass</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_oc_en" type="string">
          <ipxact:name>pma_adapt_adp_oc_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_oc_en</ipxact:displayName>
          <ipxact:value>radp_oc_en_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_oc_hold_en" type="string">
          <ipxact:name>pma_adapt_adp_oc_hold_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_oc_hold_en</ipxact:displayName>
          <ipxact:value>radp_oc_hold_en_not_hold</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_oc_initial_load" type="string">
          <ipxact:name>pma_adapt_adp_oc_initial_load</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_oc_initial_load</ipxact:displayName>
          <ipxact:value>radp_oc_initial_load_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_oc_initial_sign" type="string">
          <ipxact:name>pma_adapt_adp_oc_initial_sign</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_oc_initial_sign</ipxact:displayName>
          <ipxact:value>radp_oc_initial_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_oc_initial_value" type="int">
          <ipxact:name>pma_adapt_adp_oc_initial_value</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_oc_initial_value</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_oc_onetime" type="string">
          <ipxact:name>pma_adapt_adp_oc_onetime</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_oc_onetime</ipxact:displayName>
          <ipxact:value>radp_oc_onetime_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_oc_onetime_threshold" type="string">
          <ipxact:name>pma_adapt_adp_oc_onetime_threshold</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_oc_onetime_threshold</ipxact:displayName>
          <ipxact:value>radp_oc_onetime_threshold_1024</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_odi_bit_sel" type="string">
          <ipxact:name>pma_adapt_adp_odi_bit_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_odi_bit_sel</ipxact:displayName>
          <ipxact:value>radp_odi_bit_sel_all_bits</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_odi_control_sel" type="string">
          <ipxact:name>pma_adapt_adp_odi_control_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_odi_control_sel</ipxact:displayName>
          <ipxact:value>radp_odi_control_sel_from_cram</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_odi_count_threshold" type="string">
          <ipxact:name>pma_adapt_adp_odi_count_threshold</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_odi_count_threshold</ipxact:displayName>
          <ipxact:value>radp_odi_count_threshold_1e6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_odi_dfe_spec_en" type="string">
          <ipxact:name>pma_adapt_adp_odi_dfe_spec_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_odi_dfe_spec_en</ipxact:displayName>
          <ipxact:value>radp_odi_dfe_spec_en_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_odi_dlev_sel" type="string">
          <ipxact:name>pma_adapt_adp_odi_dlev_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_odi_dlev_sel</ipxact:displayName>
          <ipxact:value>radp_odi_dlev_sel_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_odi_en" type="string">
          <ipxact:name>pma_adapt_adp_odi_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_odi_en</ipxact:displayName>
          <ipxact:value>radp_odi_en_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_odi_mode" type="string">
          <ipxact:name>pma_adapt_adp_odi_mode</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_odi_mode</ipxact:displayName>
          <ipxact:value>radp_odi_mode_detect_errdata</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_odi_rstn" type="string">
          <ipxact:name>pma_adapt_adp_odi_rstn</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_odi_rstn</ipxact:displayName>
          <ipxact:value>radp_odi_rstn_1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_odi_spec_sel" type="string">
          <ipxact:name>pma_adapt_adp_odi_spec_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_odi_spec_sel</ipxact:displayName>
          <ipxact:value>radp_odi_spec_sel_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_odi_start" type="string">
          <ipxact:name>pma_adapt_adp_odi_start</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_odi_start</ipxact:displayName>
          <ipxact:value>radp_odi_start_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pat_dlev_sign_avg_win" type="string">
          <ipxact:name>pma_adapt_adp_pat_dlev_sign_avg_win</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pat_dlev_sign_avg_win</ipxact:displayName>
          <ipxact:value>radp_pat_dlev_sign_avg_win_2x</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pat_dlev_sign_force" type="string">
          <ipxact:name>pma_adapt_adp_pat_dlev_sign_force</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pat_dlev_sign_force</ipxact:displayName>
          <ipxact:value>radp_pat_dlev_sign_force_determined_by_cram</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pat_dlev_sign_value" type="string">
          <ipxact:name>pma_adapt_adp_pat_dlev_sign_value</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pat_dlev_sign_value</ipxact:displayName>
          <ipxact:value>radp_pat_dlev_sign_value_1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pat_spec_sign_avg_win" type="string">
          <ipxact:name>pma_adapt_adp_pat_spec_sign_avg_win</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pat_spec_sign_avg_win</ipxact:displayName>
          <ipxact:value>radp_pat_spec_sign_avg_win_256</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pat_spec_sign_force" type="string">
          <ipxact:name>pma_adapt_adp_pat_spec_sign_force</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pat_spec_sign_force</ipxact:displayName>
          <ipxact:value>radp_pat_spec_sign_force_generated_internally</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pat_spec_sign_value" type="string">
          <ipxact:name>pma_adapt_adp_pat_spec_sign_value</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pat_spec_sign_value</ipxact:displayName>
          <ipxact:value>radp_pat_spec_sign_value_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pat_trans_filter" type="string">
          <ipxact:name>pma_adapt_adp_pat_trans_filter</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pat_trans_filter</ipxact:displayName>
          <ipxact:value>radp_pat_trans_filter_5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pat_trans_only_en" type="string">
          <ipxact:name>pma_adapt_adp_pat_trans_only_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pat_trans_only_en</ipxact:displayName>
          <ipxact:value>radp_pat_trans_only_en_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pcie_adp_bypass" type="string">
          <ipxact:name>pma_adapt_adp_pcie_adp_bypass</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pcie_adp_bypass</ipxact:displayName>
          <ipxact:value>radp_pcie_adp_bypass_no</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pcie_eqz" type="string">
          <ipxact:name>pma_adapt_adp_pcie_eqz</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pcie_eqz</ipxact:displayName>
          <ipxact:value>radp_pcie_eqz_non_pcie_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pcie_hold_sel" type="int">
          <ipxact:name>pma_adapt_adp_pcie_hold_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pcie_hold_sel</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_pcs_option" type="string">
          <ipxact:name>pma_adapt_adp_pcs_option</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_pcs_option</ipxact:displayName>
          <ipxact:value>radp_pcs_option_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_po_actslp_ratio" type="string">
          <ipxact:name>pma_adapt_adp_po_actslp_ratio</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_po_actslp_ratio</ipxact:displayName>
          <ipxact:value>radp_po_actslp_ratio_10_percent</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_po_en" type="string">
          <ipxact:name>pma_adapt_adp_po_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_po_en</ipxact:displayName>
          <ipxact:value>radp_po_en_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_po_gb_act2slp" type="string">
          <ipxact:name>pma_adapt_adp_po_gb_act2slp</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_po_gb_act2slp</ipxact:displayName>
          <ipxact:value>radp_po_gb_act2slp_288ns</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_po_gb_slp2act" type="string">
          <ipxact:name>pma_adapt_adp_po_gb_slp2act</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_po_gb_slp2act</ipxact:displayName>
          <ipxact:value>radp_po_gb_slp2act_288ns</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_po_initwait" type="string">
          <ipxact:name>pma_adapt_adp_po_initwait</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_po_initwait</ipxact:displayName>
          <ipxact:value>radp_po_initwait_10sec</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_po_sleep_win" type="string">
          <ipxact:name>pma_adapt_adp_po_sleep_win</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_po_sleep_win</ipxact:displayName>
          <ipxact:value>radp_po_sleep_win_2_sec</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_po_startpos" type="string">
          <ipxact:name>pma_adapt_adp_po_startpos</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_po_startpos</ipxact:displayName>
          <ipxact:value>radp_po_startpos_6ov7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_reserved" type="int">
          <ipxact:name>pma_adapt_adp_reserved</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_reserved</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_rstn" type="string">
          <ipxact:name>pma_adapt_adp_rstn</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_rstn</ipxact:displayName>
          <ipxact:value>radp_rstn_1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_status_sel" type="string">
          <ipxact:name>pma_adapt_adp_status_sel</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_status_sel</ipxact:displayName>
          <ipxact:value>radp_status_sel_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_tx_accum_depth" type="int">
          <ipxact:name>pma_adapt_adp_tx_accum_depth</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_tx_accum_depth</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_tx_adp_accumulate" type="string">
          <ipxact:name>pma_adapt_adp_tx_adp_accumulate</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_tx_adp_accumulate</ipxact:displayName>
          <ipxact:value>radp_tx_adp_accumulate_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_tx_adp_en" type="string">
          <ipxact:name>pma_adapt_adp_tx_adp_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_tx_adp_en</ipxact:displayName>
          <ipxact:value>radp_tx_adp_en_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_tx_up_dn_flip" type="string">
          <ipxact:name>pma_adapt_adp_tx_up_dn_flip</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_tx_up_dn_flip</ipxact:displayName>
          <ipxact:value>radp_tx_up_dn_flip_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_vga_accum_depth" type="int">
          <ipxact:name>pma_adapt_adp_vga_accum_depth</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_vga_accum_depth</ipxact:displayName>
          <ipxact:value>9</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_vga_bypass" type="string">
          <ipxact:name>pma_adapt_adp_vga_bypass</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_vga_bypass</ipxact:displayName>
          <ipxact:value>radp_vga_bypass_bypass</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_vga_ctle_low_limit" type="string">
          <ipxact:name>pma_adapt_adp_vga_ctle_low_limit</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_vga_ctle_low_limit</ipxact:displayName>
          <ipxact:value>radp_vga_ctle_low_limit_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_vga_dlev_offset" type="int">
          <ipxact:name>pma_adapt_adp_vga_dlev_offset</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_vga_dlev_offset</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_vga_dlev_target" type="int">
          <ipxact:name>pma_adapt_adp_vga_dlev_target</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_vga_dlev_target</ipxact:displayName>
          <ipxact:value>15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_vga_en" type="string">
          <ipxact:name>pma_adapt_adp_vga_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_vga_en</ipxact:displayName>
          <ipxact:value>radp_vga_en_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_vga_hold_en" type="string">
          <ipxact:name>pma_adapt_adp_vga_hold_en</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_vga_hold_en</ipxact:displayName>
          <ipxact:value>radp_vga_hold_en_not_hold</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_vga_initial_load" type="string">
          <ipxact:name>pma_adapt_adp_vga_initial_load</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_vga_initial_load</ipxact:displayName>
          <ipxact:value>radp_vga_initial_load_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_vga_initial_value" type="string">
          <ipxact:name>pma_adapt_adp_vga_initial_value</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_vga_initial_value</ipxact:displayName>
          <ipxact:value>radp_vga_initial_value_4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_vga_onetime" type="string">
          <ipxact:name>pma_adapt_adp_vga_onetime</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_vga_onetime</ipxact:displayName>
          <ipxact:value>radp_vga_onetime_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_adp_vga_onetime_threshold" type="string">
          <ipxact:name>pma_adapt_adp_vga_onetime_threshold</ipxact:name>
          <ipxact:displayName>pma_adapt_adp_vga_onetime_threshold</ipxact:displayName>
          <ipxact:value>radp_vga_onetime_threshold_512</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_advanced_mode" type="string">
          <ipxact:name>pma_adapt_advanced_mode</ipxact:name>
          <ipxact:displayName>pma_adapt_advanced_mode</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_datarate_bps" type="string">
          <ipxact:name>pma_adapt_datarate_bps</ipxact:name>
          <ipxact:displayName>pma_adapt_datarate_bps</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_initial_settings" type="string">
          <ipxact:name>pma_adapt_initial_settings</ipxact:name>
          <ipxact:displayName>pma_adapt_initial_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_odi_mode" type="string">
          <ipxact:name>pma_adapt_odi_mode</ipxact:name>
          <ipxact:displayName>pma_adapt_odi_mode</ipxact:displayName>
          <ipxact:value>odi_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_offset_mode" type="string">
          <ipxact:name>pma_adapt_offset_mode</ipxact:name>
          <ipxact:displayName>pma_adapt_offset_mode</ipxact:displayName>
          <ipxact:value>offset_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_optimal" type="string">
          <ipxact:name>pma_adapt_optimal</ipxact:name>
          <ipxact:displayName>pma_adapt_optimal</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_power_mode" type="string">
          <ipxact:name>pma_adapt_power_mode</ipxact:name>
          <ipxact:displayName>pma_adapt_power_mode</ipxact:displayName>
          <ipxact:value>powsav_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_powermode_ac_adaptation" type="string">
          <ipxact:name>pma_adapt_powermode_ac_adaptation</ipxact:name>
          <ipxact:displayName>pma_adapt_powermode_ac_adaptation</ipxact:displayName>
          <ipxact:value>adapt_ac_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_powermode_ac_deser_adapt" type="string">
          <ipxact:name>pma_adapt_powermode_ac_deser_adapt</ipxact:name>
          <ipxact:displayName>pma_adapt_powermode_ac_deser_adapt</ipxact:displayName>
          <ipxact:value>adapt_deser_ac_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_powermode_ac_dfe_adapt" type="string">
          <ipxact:name>pma_adapt_powermode_ac_dfe_adapt</ipxact:name>
          <ipxact:displayName>pma_adapt_powermode_ac_dfe_adapt</ipxact:displayName>
          <ipxact:value>adapt_dfe_ac_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_powermode_dc_adaptation" type="string">
          <ipxact:name>pma_adapt_powermode_dc_adaptation</ipxact:name>
          <ipxact:displayName>pma_adapt_powermode_dc_adaptation</ipxact:displayName>
          <ipxact:value>powerdown_adapt</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_powermode_dc_deser_adapt" type="string">
          <ipxact:name>pma_adapt_powermode_dc_deser_adapt</ipxact:name>
          <ipxact:displayName>pma_adapt_powermode_dc_deser_adapt</ipxact:displayName>
          <ipxact:value>powerdown_adapt_deser</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_powermode_dc_dfe_adapt" type="string">
          <ipxact:name>pma_adapt_powermode_dc_dfe_adapt</ipxact:name>
          <ipxact:displayName>pma_adapt_powermode_dc_dfe_adapt</ipxact:displayName>
          <ipxact:value>powerdown_adapt_dfe</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_prot_mode" type="string">
          <ipxact:name>pma_adapt_prot_mode</ipxact:name>
          <ipxact:displayName>pma_adapt_prot_mode</ipxact:displayName>
          <ipxact:value>basic_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_sup_mode" type="string">
          <ipxact:name>pma_adapt_sup_mode</ipxact:name>
          <ipxact:displayName>pma_adapt_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_adapt_silicon_rev" type="string">
          <ipxact:name>pma_adapt_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_adapt_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_analog_mode" type="string">
          <ipxact:name>cdr_pll_analog_mode</ipxact:name>
          <ipxact:displayName>cdr_pll_analog_mode</ipxact:displayName>
          <ipxact:value>user_custom</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_atb_select_control" type="string">
          <ipxact:name>cdr_pll_atb_select_control</ipxact:name>
          <ipxact:displayName>cdr_pll_atb_select_control</ipxact:displayName>
          <ipxact:value>atb_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_auto_reset_on" type="string">
          <ipxact:name>cdr_pll_auto_reset_on</ipxact:name>
          <ipxact:displayName>cdr_pll_auto_reset_on</ipxact:displayName>
          <ipxact:value>auto_reset_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_bandwidth_range_high" type="string">
          <ipxact:name>cdr_pll_bandwidth_range_high</ipxact:name>
          <ipxact:displayName>cdr_pll_bandwidth_range_high</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_bandwidth_range_low" type="string">
          <ipxact:name>cdr_pll_bandwidth_range_low</ipxact:name>
          <ipxact:displayName>cdr_pll_bandwidth_range_low</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_bbpd_data_pattern_filter_select" type="string">
          <ipxact:name>cdr_pll_bbpd_data_pattern_filter_select</ipxact:name>
          <ipxact:displayName>cdr_pll_bbpd_data_pattern_filter_select</ipxact:displayName>
          <ipxact:value>bbpd_data_pat_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_bti_protected" type="string">
          <ipxact:name>cdr_pll_bti_protected</ipxact:name>
          <ipxact:displayName>cdr_pll_bti_protected</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_bw_mode" type="string">
          <ipxact:name>cdr_pll_bw_mode</ipxact:name>
          <ipxact:displayName>cdr_pll_bw_mode</ipxact:displayName>
          <ipxact:value>mid_bw</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_bypass_a_edge" type="string">
          <ipxact:name>cdr_pll_bypass_a_edge</ipxact:name>
          <ipxact:displayName>cdr_pll_bypass_a_edge</ipxact:displayName>
          <ipxact:value>bypass_a_edge_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_cal_vco_count_length" type="string">
          <ipxact:name>cdr_pll_cal_vco_count_length</ipxact:name>
          <ipxact:displayName>cdr_pll_cal_vco_count_length</ipxact:displayName>
          <ipxact:value>sel_8b_count</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_pm_cr2_rx_path_cdr_clock_enable" type="string">
          <ipxact:name>cdr_pll_pm_cr2_rx_path_cdr_clock_enable</ipxact:name>
          <ipxact:displayName>cdr_pll_pm_cr2_rx_path_cdr_clock_enable</ipxact:displayName>
          <ipxact:value>cdr_clock_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_cdr_d2a_enb" type="string">
          <ipxact:name>cdr_pll_cdr_d2a_enb</ipxact:name>
          <ipxact:displayName>cdr_pll_cdr_d2a_enb</ipxact:displayName>
          <ipxact:value>bti_d2a_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_cdr_odi_select" type="string">
          <ipxact:name>cdr_pll_cdr_odi_select</ipxact:name>
          <ipxact:displayName>cdr_pll_cdr_odi_select</ipxact:displayName>
          <ipxact:value>sel_cdr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_cdr_phaselock_mode" type="string">
          <ipxact:name>cdr_pll_cdr_phaselock_mode</ipxact:name>
          <ipxact:displayName>cdr_pll_cdr_phaselock_mode</ipxact:displayName>
          <ipxact:value>no_ignore_lock</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_cdr_powerdown_mode" type="string">
          <ipxact:name>cdr_pll_cdr_powerdown_mode</ipxact:name>
          <ipxact:displayName>cdr_pll_cdr_powerdown_mode</ipxact:displayName>
          <ipxact:value>power_up</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_chgpmp_current_dn_pd" type="string">
          <ipxact:name>cdr_pll_chgpmp_current_dn_pd</ipxact:name>
          <ipxact:displayName>cdr_pll_chgpmp_current_dn_pd</ipxact:displayName>
          <ipxact:value>cp_current_pd_dn_setting3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_chgpmp_current_dn_trim" type="string">
          <ipxact:name>cdr_pll_chgpmp_current_dn_trim</ipxact:name>
          <ipxact:displayName>cdr_pll_chgpmp_current_dn_trim</ipxact:displayName>
          <ipxact:value>cp_current_trimming_dn_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_chgpmp_current_pfd" type="string">
          <ipxact:name>cdr_pll_chgpmp_current_pfd</ipxact:name>
          <ipxact:displayName>cdr_pll_chgpmp_current_pfd</ipxact:displayName>
          <ipxact:value>cp_current_pfd_setting2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_chgpmp_current_up_pd" type="string">
          <ipxact:name>cdr_pll_chgpmp_current_up_pd</ipxact:name>
          <ipxact:displayName>cdr_pll_chgpmp_current_up_pd</ipxact:displayName>
          <ipxact:value>cp_current_pd_up_setting3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_chgpmp_current_up_trim" type="string">
          <ipxact:name>cdr_pll_chgpmp_current_up_trim</ipxact:name>
          <ipxact:displayName>cdr_pll_chgpmp_current_up_trim</ipxact:displayName>
          <ipxact:value>cp_current_trimming_up_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_chgpmp_dn_pd_trim_double" type="string">
          <ipxact:name>cdr_pll_chgpmp_dn_pd_trim_double</ipxact:name>
          <ipxact:displayName>cdr_pll_chgpmp_dn_pd_trim_double</ipxact:displayName>
          <ipxact:value>normal_dn_trim_current</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_chgpmp_replicate" type="string">
          <ipxact:name>cdr_pll_chgpmp_replicate</ipxact:name>
          <ipxact:displayName>cdr_pll_chgpmp_replicate</ipxact:displayName>
          <ipxact:value>disable_replica_bias_ctrl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_chgpmp_testmode" type="string">
          <ipxact:name>cdr_pll_chgpmp_testmode</ipxact:name>
          <ipxact:displayName>cdr_pll_chgpmp_testmode</ipxact:displayName>
          <ipxact:value>cp_test_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_chgpmp_up_pd_trim_double" type="string">
          <ipxact:name>cdr_pll_chgpmp_up_pd_trim_double</ipxact:name>
          <ipxact:displayName>cdr_pll_chgpmp_up_pd_trim_double</ipxact:displayName>
          <ipxact:value>normal_up_trim_current</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_chgpmp_vccreg" type="string">
          <ipxact:name>cdr_pll_chgpmp_vccreg</ipxact:name>
          <ipxact:displayName>cdr_pll_chgpmp_vccreg</ipxact:displayName>
          <ipxact:value>vreg_fw0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_clk0_dfe_tfall_adj" type="string">
          <ipxact:name>cdr_pll_clk0_dfe_tfall_adj</ipxact:name>
          <ipxact:displayName>cdr_pll_clk0_dfe_tfall_adj</ipxact:displayName>
          <ipxact:value>clk0_dfe_tf0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_clk0_dfe_trise_adj" type="string">
          <ipxact:name>cdr_pll_clk0_dfe_trise_adj</ipxact:name>
          <ipxact:displayName>cdr_pll_clk0_dfe_trise_adj</ipxact:displayName>
          <ipxact:value>clk0_dfe_tr0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_clk180_dfe_tfall_adj" type="string">
          <ipxact:name>cdr_pll_clk180_dfe_tfall_adj</ipxact:name>
          <ipxact:displayName>cdr_pll_clk180_dfe_tfall_adj</ipxact:displayName>
          <ipxact:value>clk180_dfe_tf0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_clk180_dfe_trise_adj" type="string">
          <ipxact:name>cdr_pll_clk180_dfe_trise_adj</ipxact:name>
          <ipxact:displayName>cdr_pll_clk180_dfe_trise_adj</ipxact:displayName>
          <ipxact:value>clk180_dfe_tr0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_clk270_dfe_tfall_adj" type="string">
          <ipxact:name>cdr_pll_clk270_dfe_tfall_adj</ipxact:name>
          <ipxact:displayName>cdr_pll_clk270_dfe_tfall_adj</ipxact:displayName>
          <ipxact:value>clk270_dfe_tf0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_clk270_dfe_trise_adj" type="string">
          <ipxact:name>cdr_pll_clk270_dfe_trise_adj</ipxact:name>
          <ipxact:displayName>cdr_pll_clk270_dfe_trise_adj</ipxact:displayName>
          <ipxact:value>clk270_dfe_tr0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_clk90_dfe_tfall_adj" type="string">
          <ipxact:name>cdr_pll_clk90_dfe_tfall_adj</ipxact:name>
          <ipxact:displayName>cdr_pll_clk90_dfe_tfall_adj</ipxact:displayName>
          <ipxact:value>clk90_dfe_tf0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_clk90_dfe_trise_adj" type="string">
          <ipxact:name>cdr_pll_clk90_dfe_trise_adj</ipxact:name>
          <ipxact:displayName>cdr_pll_clk90_dfe_trise_adj</ipxact:displayName>
          <ipxact:value>clk90_dfe_tr0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_clklow_mux_select" type="string">
          <ipxact:name>cdr_pll_clklow_mux_select</ipxact:name>
          <ipxact:displayName>cdr_pll_clklow_mux_select</ipxact:displayName>
          <ipxact:value>clklow_mux_cdr_fbclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_datarate_bps" type="string">
          <ipxact:name>cdr_pll_datarate_bps</ipxact:name>
          <ipxact:displayName>cdr_pll_datarate_bps</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_diag_loopback_enable" type="string">
          <ipxact:name>cdr_pll_diag_loopback_enable</ipxact:name>
          <ipxact:displayName>cdr_pll_diag_loopback_enable</ipxact:displayName>
          <ipxact:value>no_diag_rev_loopback</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_disable_up_dn" type="string">
          <ipxact:name>cdr_pll_disable_up_dn</ipxact:name>
          <ipxact:displayName>cdr_pll_disable_up_dn</ipxact:displayName>
          <ipxact:value>normal_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_enable_idle_rx_channel_support" type="string">
          <ipxact:name>cdr_pll_enable_idle_rx_channel_support</ipxact:name>
          <ipxact:displayName>cdr_pll_enable_idle_rx_channel_support</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_f_max_cmu_out_freq" type="string">
          <ipxact:name>cdr_pll_f_max_cmu_out_freq</ipxact:name>
          <ipxact:displayName>cdr_pll_f_max_cmu_out_freq</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_f_max_m_counter" type="string">
          <ipxact:name>cdr_pll_f_max_m_counter</ipxact:name>
          <ipxact:displayName>cdr_pll_f_max_m_counter</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_f_max_pfd" type="string">
          <ipxact:name>cdr_pll_f_max_pfd</ipxact:name>
          <ipxact:displayName>cdr_pll_f_max_pfd</ipxact:displayName>
          <ipxact:value>350000000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_f_max_ref" type="string">
          <ipxact:name>cdr_pll_f_max_ref</ipxact:name>
          <ipxact:displayName>cdr_pll_f_max_ref</ipxact:displayName>
          <ipxact:value>800000000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_f_max_vco" type="string">
          <ipxact:name>cdr_pll_f_max_vco</ipxact:name>
          <ipxact:displayName>cdr_pll_f_max_vco</ipxact:displayName>
          <ipxact:value>14150000000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_f_min_gt_channel" type="string">
          <ipxact:name>cdr_pll_f_min_gt_channel</ipxact:name>
          <ipxact:displayName>cdr_pll_f_min_gt_channel</ipxact:displayName>
          <ipxact:value>8700000000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_f_min_pfd" type="string">
          <ipxact:name>cdr_pll_f_min_pfd</ipxact:name>
          <ipxact:displayName>cdr_pll_f_min_pfd</ipxact:displayName>
          <ipxact:value>25000000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_f_min_ref" type="string">
          <ipxact:name>cdr_pll_f_min_ref</ipxact:name>
          <ipxact:displayName>cdr_pll_f_min_ref</ipxact:displayName>
          <ipxact:value>25000000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_f_min_vco" type="string">
          <ipxact:name>cdr_pll_f_min_vco</ipxact:name>
          <ipxact:displayName>cdr_pll_f_min_vco</ipxact:displayName>
          <ipxact:value>7000000000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_fref_clklow_div" type="int">
          <ipxact:name>cdr_pll_fref_clklow_div</ipxact:name>
          <ipxact:displayName>cdr_pll_fref_clklow_div</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_fref_mux_select" type="string">
          <ipxact:name>cdr_pll_fref_mux_select</ipxact:name>
          <ipxact:displayName>cdr_pll_fref_mux_select</ipxact:displayName>
          <ipxact:value>fref_mux_cdr_refclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_gpon_lck2ref_control" type="string">
          <ipxact:name>cdr_pll_gpon_lck2ref_control</ipxact:name>
          <ipxact:displayName>cdr_pll_gpon_lck2ref_control</ipxact:displayName>
          <ipxact:value>gpon_lck2ref_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_initial_settings" type="string">
          <ipxact:name>cdr_pll_initial_settings</ipxact:name>
          <ipxact:displayName>cdr_pll_initial_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_lck2ref_delay_control" type="string">
          <ipxact:name>cdr_pll_lck2ref_delay_control</ipxact:name>
          <ipxact:displayName>cdr_pll_lck2ref_delay_control</ipxact:displayName>
          <ipxact:value>lck2ref_delay_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_lf_resistor_pd" type="string">
          <ipxact:name>cdr_pll_lf_resistor_pd</ipxact:name>
          <ipxact:displayName>cdr_pll_lf_resistor_pd</ipxact:displayName>
          <ipxact:value>lf_pd_setting3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_lf_resistor_pfd" type="string">
          <ipxact:name>cdr_pll_lf_resistor_pfd</ipxact:name>
          <ipxact:displayName>cdr_pll_lf_resistor_pfd</ipxact:displayName>
          <ipxact:value>lf_pfd_setting2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_lf_ripple_cap" type="string">
          <ipxact:name>cdr_pll_lf_ripple_cap</ipxact:name>
          <ipxact:displayName>cdr_pll_lf_ripple_cap</ipxact:displayName>
          <ipxact:value>lf_no_ripple</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_loop_filter_bias_select" type="string">
          <ipxact:name>cdr_pll_loop_filter_bias_select</ipxact:name>
          <ipxact:displayName>cdr_pll_loop_filter_bias_select</ipxact:displayName>
          <ipxact:value>lpflt_bias_7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_loopback_mode" type="string">
          <ipxact:name>cdr_pll_loopback_mode</ipxact:name>
          <ipxact:displayName>cdr_pll_loopback_mode</ipxact:displayName>
          <ipxact:value>loopback_disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_lpd_counter" type="int">
          <ipxact:name>cdr_pll_lpd_counter</ipxact:name>
          <ipxact:displayName>cdr_pll_lpd_counter</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_lpfd_counter" type="int">
          <ipxact:name>cdr_pll_lpfd_counter</ipxact:name>
          <ipxact:displayName>cdr_pll_lpfd_counter</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_ltd_ltr_micro_controller_select" type="string">
          <ipxact:name>cdr_pll_ltd_ltr_micro_controller_select</ipxact:name>
          <ipxact:displayName>cdr_pll_ltd_ltr_micro_controller_select</ipxact:displayName>
          <ipxact:value>ltd_ltr_pcs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_mcnt_div" type="int">
          <ipxact:name>cdr_pll_mcnt_div</ipxact:name>
          <ipxact:displayName>cdr_pll_mcnt_div</ipxact:displayName>
          <ipxact:value>16</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_n_counter" type="int">
          <ipxact:name>cdr_pll_n_counter</ipxact:name>
          <ipxact:displayName>cdr_pll_n_counter</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_ncnt_div" type="int">
          <ipxact:name>cdr_pll_ncnt_div</ipxact:name>
          <ipxact:displayName>cdr_pll_ncnt_div</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_optimal" type="string">
          <ipxact:name>cdr_pll_optimal</ipxact:name>
          <ipxact:displayName>cdr_pll_optimal</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_out_freq" type="string">
          <ipxact:name>cdr_pll_out_freq</ipxact:name>
          <ipxact:displayName>cdr_pll_out_freq</ipxact:displayName>
          <ipxact:value>5156250000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_pcie_gen" type="string">
          <ipxact:name>cdr_pll_pcie_gen</ipxact:name>
          <ipxact:displayName>cdr_pll_pcie_gen</ipxact:displayName>
          <ipxact:value>non_pcie</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_pd_fastlock_mode" type="string">
          <ipxact:name>cdr_pll_pd_fastlock_mode</ipxact:name>
          <ipxact:displayName>cdr_pll_pd_fastlock_mode</ipxact:displayName>
          <ipxact:value>fast_lock_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_pd_l_counter" type="int">
          <ipxact:name>cdr_pll_pd_l_counter</ipxact:name>
          <ipxact:displayName>cdr_pll_pd_l_counter</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_pfd_l_counter" type="int">
          <ipxact:name>cdr_pll_pfd_l_counter</ipxact:name>
          <ipxact:displayName>cdr_pll_pfd_l_counter</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_position" type="string">
          <ipxact:name>cdr_pll_position</ipxact:name>
          <ipxact:displayName>cdr_pll_position</ipxact:displayName>
          <ipxact:value>position0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_power_mode" type="string">
          <ipxact:name>cdr_pll_power_mode</ipxact:name>
          <ipxact:displayName>cdr_pll_power_mode</ipxact:displayName>
          <ipxact:value>mid_power</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_powermode_ac_bbpd" type="string">
          <ipxact:name>cdr_pll_powermode_ac_bbpd</ipxact:name>
          <ipxact:displayName>cdr_pll_powermode_ac_bbpd</ipxact:displayName>
          <ipxact:value>bbpd_ac_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_powermode_ac_rvcotop" type="string">
          <ipxact:name>cdr_pll_powermode_ac_rvcotop</ipxact:name>
          <ipxact:displayName>cdr_pll_powermode_ac_rvcotop</ipxact:displayName>
          <ipxact:value>rvcotop_ac_div2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_powermode_ac_txpll" type="string">
          <ipxact:name>cdr_pll_powermode_ac_txpll</ipxact:name>
          <ipxact:displayName>cdr_pll_powermode_ac_txpll</ipxact:displayName>
          <ipxact:value>txpll_ac_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_powermode_dc_bbpd" type="string">
          <ipxact:name>cdr_pll_powermode_dc_bbpd</ipxact:name>
          <ipxact:displayName>cdr_pll_powermode_dc_bbpd</ipxact:displayName>
          <ipxact:value>bbpd_dc_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_powermode_dc_rvcotop" type="string">
          <ipxact:name>cdr_pll_powermode_dc_rvcotop</ipxact:name>
          <ipxact:displayName>cdr_pll_powermode_dc_rvcotop</ipxact:displayName>
          <ipxact:value>rvcotop_dc_div2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_powermode_dc_txpll" type="string">
          <ipxact:name>cdr_pll_powermode_dc_txpll</ipxact:name>
          <ipxact:displayName>cdr_pll_powermode_dc_txpll</ipxact:displayName>
          <ipxact:value>powerdown_txpll</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_primary_use" type="string">
          <ipxact:name>cdr_pll_primary_use</ipxact:name>
          <ipxact:displayName>cdr_pll_primary_use</ipxact:displayName>
          <ipxact:value>cdr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_prot_mode" type="string">
          <ipxact:name>cdr_pll_prot_mode</ipxact:name>
          <ipxact:displayName>cdr_pll_prot_mode</ipxact:displayName>
          <ipxact:value>basic_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_reference_clock_frequency" type="string">
          <ipxact:name>cdr_pll_reference_clock_frequency</ipxact:name>
          <ipxact:displayName>cdr_pll_reference_clock_frequency</ipxact:displayName>
          <ipxact:value>644531250</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_requires_gt_capable_channel" type="string">
          <ipxact:name>cdr_pll_requires_gt_capable_channel</ipxact:name>
          <ipxact:displayName>cdr_pll_requires_gt_capable_channel</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_reverse_serial_loopback" type="string">
          <ipxact:name>cdr_pll_reverse_serial_loopback</ipxact:name>
          <ipxact:displayName>cdr_pll_reverse_serial_loopback</ipxact:displayName>
          <ipxact:value>no_loopback</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_rx_pin_as_refclk_mode" type="string">
          <ipxact:name>cdr_pll_rx_pin_as_refclk_mode</ipxact:name>
          <ipxact:displayName>cdr_pll_rx_pin_as_refclk_mode</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_set_cdr_input_freq_range" type="int">
          <ipxact:name>cdr_pll_set_cdr_input_freq_range</ipxact:name>
          <ipxact:displayName>cdr_pll_set_cdr_input_freq_range</ipxact:displayName>
          <ipxact:value>149</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_set_cdr_v2i_enable" type="string">
          <ipxact:name>cdr_pll_set_cdr_v2i_enable</ipxact:name>
          <ipxact:displayName>cdr_pll_set_cdr_v2i_enable</ipxact:displayName>
          <ipxact:value>enable_v2i_bias</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_set_cdr_vco_reset" type="string">
          <ipxact:name>cdr_pll_set_cdr_vco_reset</ipxact:name>
          <ipxact:displayName>cdr_pll_set_cdr_vco_reset</ipxact:displayName>
          <ipxact:value>vco_normal</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_set_cdr_vco_speed" type="int">
          <ipxact:name>cdr_pll_set_cdr_vco_speed</ipxact:name>
          <ipxact:displayName>cdr_pll_set_cdr_vco_speed</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_set_cdr_vco_speed_fix" type="int">
          <ipxact:name>cdr_pll_set_cdr_vco_speed_fix</ipxact:name>
          <ipxact:displayName>cdr_pll_set_cdr_vco_speed_fix</ipxact:displayName>
          <ipxact:value>92</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_set_cdr_vco_speed_pciegen3" type="string">
          <ipxact:name>cdr_pll_set_cdr_vco_speed_pciegen3</ipxact:name>
          <ipxact:displayName>cdr_pll_set_cdr_vco_speed_pciegen3</ipxact:displayName>
          <ipxact:value>cdr_vco_max_speedbin_pciegen3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_side" type="string">
          <ipxact:name>cdr_pll_side</ipxact:name>
          <ipxact:displayName>cdr_pll_side</ipxact:displayName>
          <ipxact:value>side_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_speed_grade" type="string">
          <ipxact:name>cdr_pll_speed_grade</ipxact:name>
          <ipxact:displayName>cdr_pll_speed_grade</ipxact:displayName>
          <ipxact:value>e2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_sup_mode" type="string">
          <ipxact:name>cdr_pll_sup_mode</ipxact:name>
          <ipxact:displayName>cdr_pll_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_top_or_bottom" type="string">
          <ipxact:name>cdr_pll_top_or_bottom</ipxact:name>
          <ipxact:displayName>cdr_pll_top_or_bottom</ipxact:displayName>
          <ipxact:value>top_or_bot_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_tx_pll_prot_mode" type="string">
          <ipxact:name>cdr_pll_tx_pll_prot_mode</ipxact:name>
          <ipxact:displayName>cdr_pll_tx_pll_prot_mode</ipxact:displayName>
          <ipxact:value>txpll_unused</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_txpll_hclk_driver_enable" type="string">
          <ipxact:name>cdr_pll_txpll_hclk_driver_enable</ipxact:name>
          <ipxact:displayName>cdr_pll_txpll_hclk_driver_enable</ipxact:displayName>
          <ipxact:value>hclk_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_rstb" type="string">
          <ipxact:name>cdr_pll_rstb</ipxact:name>
          <ipxact:displayName>cdr_pll_rstb</ipxact:displayName>
          <ipxact:value>cdr_lf_reset_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_pm_cr2_tx_rx_uc_dyn_reconfig" type="string">
          <ipxact:name>cdr_pll_pm_cr2_tx_rx_uc_dyn_reconfig</ipxact:name>
          <ipxact:displayName>cdr_pll_pm_cr2_tx_rx_uc_dyn_reconfig</ipxact:displayName>
          <ipxact:value>uc_dyn_reconfig_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_uc_ro_cal" type="string">
          <ipxact:name>cdr_pll_uc_ro_cal</ipxact:name>
          <ipxact:displayName>cdr_pll_uc_ro_cal</ipxact:displayName>
          <ipxact:value>uc_ro_cal_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_uc_ro_cal_status" type="string">
          <ipxact:name>cdr_pll_uc_ro_cal_status</ipxact:name>
          <ipxact:displayName>cdr_pll_uc_ro_cal_status</ipxact:displayName>
          <ipxact:value>uc_ro_sta_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_vco_bypass" type="string">
          <ipxact:name>cdr_pll_vco_bypass</ipxact:name>
          <ipxact:displayName>cdr_pll_vco_bypass</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_vco_freq" type="string">
          <ipxact:name>cdr_pll_vco_freq</ipxact:name>
          <ipxact:displayName>cdr_pll_vco_freq</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_vco_overrange_voltage" type="string">
          <ipxact:name>cdr_pll_vco_overrange_voltage</ipxact:name>
          <ipxact:displayName>cdr_pll_vco_overrange_voltage</ipxact:displayName>
          <ipxact:value>vco_overrange_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_vco_underrange_voltage" type="string">
          <ipxact:name>cdr_pll_vco_underrange_voltage</ipxact:name>
          <ipxact:displayName>cdr_pll_vco_underrange_voltage</ipxact:displayName>
          <ipxact:value>vco_underange_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_vreg_output" type="string">
          <ipxact:name>cdr_pll_vreg_output</ipxact:name>
          <ipxact:displayName>cdr_pll_vreg_output</ipxact:displayName>
          <ipxact:value>vccdreg_nominal</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_direct_fb" type="string">
          <ipxact:name>cdr_pll_direct_fb</ipxact:name>
          <ipxact:displayName>cdr_pll_direct_fb</ipxact:displayName>
          <ipxact:value>direct_fb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_iqclk_sel" type="string">
          <ipxact:name>cdr_pll_iqclk_sel</ipxact:name>
          <ipxact:displayName>cdr_pll_iqclk_sel</ipxact:displayName>
          <ipxact:value>power_down</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_silicon_rev" type="string">
          <ipxact:name>cdr_pll_silicon_rev</ipxact:name>
          <ipxact:displayName>cdr_pll_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_pma_width" type="int">
          <ipxact:name>cdr_pll_pma_width</ipxact:name>
          <ipxact:displayName>cdr_pll_pma_width</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_cgb_div" type="int">
          <ipxact:name>cdr_pll_cgb_div</ipxact:name>
          <ipxact:displayName>cdr_pll_cgb_div</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cdr_pll_is_cascaded_pll" type="string">
          <ipxact:name>cdr_pll_is_cascaded_pll</ipxact:name>
          <ipxact:displayName>cdr_pll_is_cascaded_pll</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_act_isource_disable" type="string">
          <ipxact:name>pma_rx_buf_act_isource_disable</ipxact:name>
          <ipxact:displayName>pma_rx_buf_act_isource_disable</ipxact:displayName>
          <ipxact:value>isrc_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_advanced_mode" type="string">
          <ipxact:name>pma_rx_buf_advanced_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_advanced_mode</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_analog_mode" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_analog_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_analog_mode</ipxact:displayName>
          <ipxact:value>user_custom</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_bodybias_enable" type="string">
          <ipxact:name>pma_rx_buf_bodybias_enable</ipxact:name>
          <ipxact:displayName>pma_rx_buf_bodybias_enable</ipxact:displayName>
          <ipxact:value>bodybias_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_bodybias_select" type="string">
          <ipxact:name>pma_rx_buf_bodybias_select</ipxact:name>
          <ipxact:displayName>pma_rx_buf_bodybias_select</ipxact:displayName>
          <ipxact:value>bodybias_sel1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_bti_protected" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_bti_protected</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_bti_protected</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_bypass_ctle_rf_cal" type="string">
          <ipxact:name>pma_rx_buf_bypass_ctle_rf_cal</ipxact:name>
          <ipxact:displayName>pma_rx_buf_bypass_ctle_rf_cal</ipxact:displayName>
          <ipxact:value>use_dprio_rfcal</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_xrx_path_xcdr_deser_xcdr_cdr_d2a_enb" type="string">
          <ipxact:name>pma_rx_buf_xrx_path_xcdr_deser_xcdr_cdr_d2a_enb</ipxact:name>
          <ipxact:displayName>pma_rx_buf_xrx_path_xcdr_deser_xcdr_cdr_d2a_enb</ipxact:displayName>
          <ipxact:value>bti_d2a_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_clk_divrx_en" type="string">
          <ipxact:name>pma_rx_buf_clk_divrx_en</ipxact:name>
          <ipxact:displayName>pma_rx_buf_clk_divrx_en</ipxact:displayName>
          <ipxact:value>normal_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_const_gm_en" type="string">
          <ipxact:name>pma_rx_buf_const_gm_en</ipxact:name>
          <ipxact:displayName>pma_rx_buf_const_gm_en</ipxact:displayName>
          <ipxact:value>cgm_en_3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_ctle_ac_gain" type="int">
          <ipxact:name>pma_rx_buf_ctle_ac_gain</ipxact:name>
          <ipxact:displayName>pma_rx_buf_ctle_ac_gain</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_ctle_eq_gain" type="int">
          <ipxact:name>pma_rx_buf_ctle_eq_gain</ipxact:name>
          <ipxact:displayName>pma_rx_buf_ctle_eq_gain</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_ctle_hires_bypass" type="string">
          <ipxact:name>pma_rx_buf_ctle_hires_bypass</ipxact:name>
          <ipxact:displayName>pma_rx_buf_ctle_hires_bypass</ipxact:displayName>
          <ipxact:value>ctle_hires_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_ctle_oc_coeff" type="int">
          <ipxact:name>pma_rx_buf_ctle_oc_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_buf_ctle_oc_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_ctle_oc_ib_sel" type="string">
          <ipxact:name>pma_rx_buf_ctle_oc_ib_sel</ipxact:name>
          <ipxact:displayName>pma_rx_buf_ctle_oc_ib_sel</ipxact:displayName>
          <ipxact:value>ib_oc_bw3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_ctle_oc_sign" type="string">
          <ipxact:name>pma_rx_buf_ctle_oc_sign</ipxact:name>
          <ipxact:displayName>pma_rx_buf_ctle_oc_sign</ipxact:displayName>
          <ipxact:value>add_i_2_p_eq</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_ctle_rf_cal" type="int">
          <ipxact:name>pma_rx_buf_ctle_rf_cal</ipxact:name>
          <ipxact:displayName>pma_rx_buf_ctle_rf_cal</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_ctle_tia_isel" type="string">
          <ipxact:name>pma_rx_buf_ctle_tia_isel</ipxact:name>
          <ipxact:displayName>pma_rx_buf_ctle_tia_isel</ipxact:displayName>
          <ipxact:value>ib_tia_bw1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_tx_rx_cvp_mode" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_tx_rx_cvp_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_tx_rx_cvp_mode</ipxact:displayName>
          <ipxact:value>cvp_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_datarate_bps" type="string">
          <ipxact:name>pma_rx_buf_datarate_bps</ipxact:name>
          <ipxact:displayName>pma_rx_buf_datarate_bps</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_datarate_bps" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_datarate_bps</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_datarate_bps</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_datawidth" type="int">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_datawidth</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_datawidth</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_dfe_err_cal_en" type="string">
          <ipxact:name>pma_rx_buf_dfe_err_cal_en</ipxact:name>
          <ipxact:displayName>pma_rx_buf_dfe_err_cal_en</ipxact:displayName>
          <ipxact:value>dfe_err_cal_enb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_dfe_err_sw_togg" type="string">
          <ipxact:name>pma_rx_buf_dfe_err_sw_togg</ipxact:name>
          <ipxact:displayName>pma_rx_buf_dfe_err_sw_togg</ipxact:displayName>
          <ipxact:value>dfe_err_tog_a</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_dfe_h1_cal_en" type="string">
          <ipxact:name>pma_rx_buf_dfe_h1_cal_en</ipxact:name>
          <ipxact:displayName>pma_rx_buf_dfe_h1_cal_en</ipxact:displayName>
          <ipxact:value>dfe_h1_cal_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_dfe_h1_sw_togg" type="string">
          <ipxact:name>pma_rx_buf_dfe_h1_sw_togg</ipxact:name>
          <ipxact:displayName>pma_rx_buf_dfe_h1_sw_togg</ipxact:displayName>
          <ipxact:value>dfe_h1_tog_neg</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_diag_lp_en" type="string">
          <ipxact:name>pma_rx_buf_diag_lp_en</ipxact:name>
          <ipxact:displayName>pma_rx_buf_diag_lp_en</ipxact:displayName>
          <ipxact:value>dlp_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_eq_bw_sel" type="string">
          <ipxact:name>pma_rx_buf_eq_bw_sel</ipxact:name>
          <ipxact:displayName>pma_rx_buf_eq_bw_sel</ipxact:displayName>
          <ipxact:value>eq_bw_1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_eq_cdgen_sel" type="string">
          <ipxact:name>pma_rx_buf_eq_cdgen_sel</ipxact:name>
          <ipxact:displayName>pma_rx_buf_eq_cdgen_sel</ipxact:displayName>
          <ipxact:value>eq_cdgen_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_eq_isel" type="string">
          <ipxact:name>pma_rx_buf_eq_isel</ipxact:name>
          <ipxact:displayName>pma_rx_buf_eq_isel</ipxact:displayName>
          <ipxact:value>eq_isel_1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_eq_sel" type="string">
          <ipxact:name>pma_rx_buf_eq_sel</ipxact:name>
          <ipxact:displayName>pma_rx_buf_eq_sel</ipxact:displayName>
          <ipxact:value>eq_sel_1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_gt_enabled" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_gt_enabled</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_gt_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_initial_settings" type="string">
          <ipxact:name>pma_rx_buf_initial_settings</ipxact:name>
          <ipxact:displayName>pma_rx_buf_initial_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_initial_settings" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_initial_settings</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_initial_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_io_std" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_io_std</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_io_std</ipxact:displayName>
          <ipxact:value>io_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_jtag_hys" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_jtag_hys</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_jtag_hys</ipxact:displayName>
          <ipxact:value>hys_increase_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_jtag_lp" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_jtag_lp</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_jtag_lp</ipxact:displayName>
          <ipxact:value>lp_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_link" type="string">
          <ipxact:name>pma_rx_buf_link</ipxact:name>
          <ipxact:displayName>pma_rx_buf_link</ipxact:displayName>
          <ipxact:value>link_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_link" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_link</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_link</ipxact:displayName>
          <ipxact:value>sr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_xrx_path_xcdr_deser_xcdr_loopback_mode" type="string">
          <ipxact:name>pma_rx_buf_xrx_path_xcdr_deser_xcdr_loopback_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_xrx_path_xcdr_deser_xcdr_loopback_mode</ipxact:displayName>
          <ipxact:value>loopback_disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_loopback_modes" type="string">
          <ipxact:name>pma_rx_buf_loopback_modes</ipxact:name>
          <ipxact:displayName>pma_rx_buf_loopback_modes</ipxact:displayName>
          <ipxact:value>lpbk_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_offset_cancellation_coarse" type="string">
          <ipxact:name>pma_rx_buf_offset_cancellation_coarse</ipxact:name>
          <ipxact:displayName>pma_rx_buf_offset_cancellation_coarse</ipxact:displayName>
          <ipxact:value>coarse_setting_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_offset_rx_cal_en" type="string">
          <ipxact:name>pma_rx_buf_offset_rx_cal_en</ipxact:name>
          <ipxact:displayName>pma_rx_buf_offset_rx_cal_en</ipxact:displayName>
          <ipxact:value>rx_oc_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_optimal" type="string">
          <ipxact:name>pma_rx_buf_optimal</ipxact:name>
          <ipxact:displayName>pma_rx_buf_optimal</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_optimal" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_optimal</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_optimal</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_tx_rx_pcie_gen" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_tx_rx_pcie_gen</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_tx_rx_pcie_gen</ipxact:displayName>
          <ipxact:value>non_pcie</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_tx_rx_pcie_gen_bitwidth" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_tx_rx_pcie_gen_bitwidth</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_tx_rx_pcie_gen_bitwidth</ipxact:displayName>
          <ipxact:value>pcie_gen3_32b</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pdb_rx" type="string">
          <ipxact:name>pma_rx_buf_pdb_rx</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pdb_rx</ipxact:displayName>
          <ipxact:value>normal_rx_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_pma_rx_divclk_hz" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_pma_rx_divclk_hz</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_pma_rx_divclk_hz</ipxact:displayName>
          <ipxact:value>322265625</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_power_mode" type="string">
          <ipxact:name>pma_rx_buf_power_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_power_mode</ipxact:displayName>
          <ipxact:value>mid_power</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_power_mode" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_power_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_power_mode</ipxact:displayName>
          <ipxact:value>mid_power</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_power_rail_eht" type="int">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_power_rail_eht</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_power_rail_eht</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_power_rail_er" type="int">
          <ipxact:name>pma_rx_buf_power_rail_er</ipxact:name>
          <ipxact:displayName>pma_rx_buf_power_rail_er</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_power_rail_er" type="int">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_power_rail_er</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_power_rail_er</ipxact:displayName>
          <ipxact:value>1030</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_powermode_ac_aoc" type="string">
          <ipxact:name>pma_rx_buf_powermode_ac_aoc</ipxact:name>
          <ipxact:displayName>pma_rx_buf_powermode_ac_aoc</ipxact:displayName>
          <ipxact:value>aoc_pwr_ac_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_powermode_ac_ctle" type="string">
          <ipxact:name>pma_rx_buf_powermode_ac_ctle</ipxact:name>
          <ipxact:displayName>pma_rx_buf_powermode_ac_ctle</ipxact:displayName>
          <ipxact:value>ctle_pwr_ac2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_powermode_ac_vcm" type="string">
          <ipxact:name>pma_rx_buf_powermode_ac_vcm</ipxact:name>
          <ipxact:displayName>pma_rx_buf_powermode_ac_vcm</ipxact:displayName>
          <ipxact:value>vcm_pwr_ac3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_powermode_ac_vga" type="string">
          <ipxact:name>pma_rx_buf_powermode_ac_vga</ipxact:name>
          <ipxact:displayName>pma_rx_buf_powermode_ac_vga</ipxact:displayName>
          <ipxact:value>vga_pwr_ac_half</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_powermode_dc_aoc" type="string">
          <ipxact:name>pma_rx_buf_powermode_dc_aoc</ipxact:name>
          <ipxact:displayName>pma_rx_buf_powermode_dc_aoc</ipxact:displayName>
          <ipxact:value>powerdown_aoc</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_powermode_dc_ctle" type="string">
          <ipxact:name>pma_rx_buf_powermode_dc_ctle</ipxact:name>
          <ipxact:displayName>pma_rx_buf_powermode_dc_ctle</ipxact:displayName>
          <ipxact:value>ctle_pwr_dc1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_powermode_dc_vcm" type="string">
          <ipxact:name>pma_rx_buf_powermode_dc_vcm</ipxact:name>
          <ipxact:displayName>pma_rx_buf_powermode_dc_vcm</ipxact:displayName>
          <ipxact:value>vcm_pwr_dc3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_powermode_dc_vga" type="string">
          <ipxact:name>pma_rx_buf_powermode_dc_vga</ipxact:name>
          <ipxact:displayName>pma_rx_buf_powermode_dc_vga</ipxact:displayName>
          <ipxact:value>vga_pwr_dc_half</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_prot_mode" type="string">
          <ipxact:name>pma_rx_buf_prot_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_prot_mode</ipxact:displayName>
          <ipxact:value>basic_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_prot_mode" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_prot_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_prot_mode</ipxact:displayName>
          <ipxact:value>basic_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_qpi_afe_en" type="string">
          <ipxact:name>pma_rx_buf_qpi_afe_en</ipxact:name>
          <ipxact:displayName>pma_rx_buf_qpi_afe_en</ipxact:displayName>
          <ipxact:value>ctle_mode_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_qpi_enable" type="string">
          <ipxact:name>pma_rx_buf_qpi_enable</ipxact:name>
          <ipxact:displayName>pma_rx_buf_qpi_enable</ipxact:displayName>
          <ipxact:value>non_qpi_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_refclk_en" type="string">
          <ipxact:name>pma_rx_buf_refclk_en</ipxact:name>
          <ipxact:displayName>pma_rx_buf_refclk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_reserve_rx_channel" type="string">
          <ipxact:name>pma_rx_buf_reserve_rx_channel</ipxact:name>
          <ipxact:displayName>pma_rx_buf_reserve_rx_channel</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_rx_afe_oc_mode" type="string">
          <ipxact:name>pma_rx_buf_rx_afe_oc_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_rx_afe_oc_mode</ipxact:displayName>
          <ipxact:value>normal_op</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_rx_aoc_doc" type="string">
          <ipxact:name>pma_rx_buf_rx_aoc_doc</ipxact:name>
          <ipxact:displayName>pma_rx_buf_rx_aoc_doc</ipxact:displayName>
          <ipxact:value>lower_dac_l0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_rx_atb_select" type="string">
          <ipxact:name>pma_rx_buf_rx_atb_select</ipxact:name>
          <ipxact:displayName>pma_rx_buf_rx_atb_select</ipxact:displayName>
          <ipxact:value>atb_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_rx_lfeq_enable" type="string">
          <ipxact:name>pma_rx_buf_rx_lfeq_enable</ipxact:name>
          <ipxact:displayName>pma_rx_buf_rx_lfeq_enable</ipxact:displayName>
          <ipxact:value>rx_lfeq_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_rx_ltr_load_init" type="string">
          <ipxact:name>pma_rx_buf_rx_ltr_load_init</ipxact:name>
          <ipxact:displayName>pma_rx_buf_rx_ltr_load_init</ipxact:displayName>
          <ipxact:value>rx_load_original</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_rx_oc_or_lfeq_coeff" type="int">
          <ipxact:name>pma_rx_buf_rx_oc_or_lfeq_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_buf_rx_oc_or_lfeq_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_rx_pin_as_refclk_mode" type="string">
          <ipxact:name>pma_rx_buf_rx_pin_as_refclk_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_rx_pin_as_refclk_mode</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_rx_refclk_divider" type="string">
          <ipxact:name>pma_rx_buf_rx_refclk_divider</ipxact:name>
          <ipxact:displayName>pma_rx_buf_rx_refclk_divider</ipxact:displayName>
          <ipxact:value>bypass_divider</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_rx_vga_oc_en" type="string">
          <ipxact:name>pma_rx_buf_rx_vga_oc_en</ipxact:name>
          <ipxact:displayName>pma_rx_buf_rx_vga_oc_en</ipxact:displayName>
          <ipxact:value>vga_cal_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_sel_vcm_ctle" type="string">
          <ipxact:name>pma_rx_buf_sel_vcm_ctle</ipxact:name>
          <ipxact:displayName>pma_rx_buf_sel_vcm_ctle</ipxact:displayName>
          <ipxact:value>vocm_eq_gndref</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_sel_vcm_tia" type="string">
          <ipxact:name>pma_rx_buf_sel_vcm_tia</ipxact:name>
          <ipxact:displayName>pma_rx_buf_sel_vcm_tia</ipxact:displayName>
          <ipxact:value>vocm_tia_fixed</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_speed_grade" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_speed_grade</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_speed_grade</ipxact:displayName>
          <ipxact:value>e2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_sup_mode" type="string">
          <ipxact:name>pma_rx_buf_sup_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_sup_mode" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_sup_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_term_sel" type="string">
          <ipxact:name>pma_rx_buf_term_sel</ipxact:name>
          <ipxact:displayName>pma_rx_buf_term_sel</ipxact:displayName>
          <ipxact:value>r_r4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_term_sync_bypass" type="string">
          <ipxact:name>pma_rx_buf_term_sync_bypass</ipxact:name>
          <ipxact:displayName>pma_rx_buf_term_sync_bypass</ipxact:displayName>
          <ipxact:value>bypass_termsync</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_term_tri_enable" type="string">
          <ipxact:name>pma_rx_buf_term_tri_enable</ipxact:name>
          <ipxact:displayName>pma_rx_buf_term_tri_enable</ipxact:displayName>
          <ipxact:value>disable_tri</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_tx_rx_testmux_select" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_tx_rx_testmux_select</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_tx_rx_testmux_select</ipxact:displayName>
          <ipxact:value>setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_tia_sel" type="string">
          <ipxact:name>pma_rx_buf_tia_sel</ipxact:name>
          <ipxact:displayName>pma_rx_buf_tia_sel</ipxact:displayName>
          <ipxact:value>tia_sel_1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_tile_type" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_tile_type</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_tile_type</ipxact:displayName>
          <ipxact:value>h</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_uc_cal_clk_bypass" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_uc_cal_clk_bypass</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_uc_cal_clk_bypass</ipxact:displayName>
          <ipxact:value>cal_clk_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_uc_cal_enable" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_uc_cal_enable</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_uc_cal_enable</ipxact:displayName>
          <ipxact:value>rx_cal_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_uc_cru_rstb" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_uc_cru_rstb</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_uc_cru_rstb</ipxact:displayName>
          <ipxact:value>cdr_lf_reset_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_tx_rx_uc_odi_eye_left" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_tx_rx_uc_odi_eye_left</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_tx_rx_uc_odi_eye_left</ipxact:displayName>
          <ipxact:value>uc_odi_eye_left_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_tx_rx_uc_odi_eye_right" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_tx_rx_uc_odi_eye_right</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_tx_rx_uc_odi_eye_right</ipxact:displayName>
          <ipxact:value>uc_odi_eye_right_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_uc_pcie_sw" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_uc_pcie_sw</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_uc_pcie_sw</ipxact:displayName>
          <ipxact:value>uc_pcie_gen1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_tx_rx_uc_rx_cal" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_tx_rx_uc_rx_cal</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_tx_rx_uc_rx_cal</ipxact:displayName>
          <ipxact:value>uc_rx_cal_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_pm_cr2_rx_path_uc_rx_rstb" type="string">
          <ipxact:name>pma_rx_buf_pm_cr2_rx_path_uc_rx_rstb</ipxact:name>
          <ipxact:displayName>pma_rx_buf_pm_cr2_rx_path_uc_rx_rstb</ipxact:displayName>
          <ipxact:value>rx_reset_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_vcm_cal_i" type="int">
          <ipxact:name>pma_rx_buf_vcm_cal_i</ipxact:name>
          <ipxact:displayName>pma_rx_buf_vcm_cal_i</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_vcm_current_add" type="string">
          <ipxact:name>pma_rx_buf_vcm_current_add</ipxact:name>
          <ipxact:displayName>pma_rx_buf_vcm_current_add</ipxact:displayName>
          <ipxact:value>vcm_current_3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_vcm_sel" type="string">
          <ipxact:name>pma_rx_buf_vcm_sel</ipxact:name>
          <ipxact:displayName>pma_rx_buf_vcm_sel</ipxact:displayName>
          <ipxact:value>vcm_l1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_vcm_sel_vccref" type="int">
          <ipxact:name>pma_rx_buf_vcm_sel_vccref</ipxact:name>
          <ipxact:displayName>pma_rx_buf_vcm_sel_vccref</ipxact:displayName>
          <ipxact:value>5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_vga_dc_gain" type="int">
          <ipxact:name>pma_rx_buf_vga_dc_gain</ipxact:name>
          <ipxact:displayName>pma_rx_buf_vga_dc_gain</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_vga_halfbw_en" type="string">
          <ipxact:name>pma_rx_buf_vga_halfbw_en</ipxact:name>
          <ipxact:displayName>pma_rx_buf_vga_halfbw_en</ipxact:displayName>
          <ipxact:value>vga_half_bw_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_vga_ib_max_en" type="string">
          <ipxact:name>pma_rx_buf_vga_ib_max_en</ipxact:name>
          <ipxact:displayName>pma_rx_buf_vga_ib_max_en</ipxact:displayName>
          <ipxact:value>vga_ib_max_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_vga_mode" type="string">
          <ipxact:name>pma_rx_buf_vga_mode</ipxact:name>
          <ipxact:displayName>pma_rx_buf_vga_mode</ipxact:displayName>
          <ipxact:value>vga_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_buf_silicon_rev" type="string">
          <ipxact:name>pma_rx_buf_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_rx_buf_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_bitslip_bypass" type="string">
          <ipxact:name>pma_rx_deser_bitslip_bypass</ipxact:name>
          <ipxact:displayName>pma_rx_deser_bitslip_bypass</ipxact:displayName>
          <ipxact:value>bs_bypass_yes</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_bti_protected" type="string">
          <ipxact:name>pma_rx_deser_bti_protected</ipxact:name>
          <ipxact:displayName>pma_rx_deser_bti_protected</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_clkdiv_source" type="string">
          <ipxact:name>pma_rx_deser_clkdiv_source</ipxact:name>
          <ipxact:displayName>pma_rx_deser_clkdiv_source</ipxact:displayName>
          <ipxact:value>vco_bypass_normal</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_clkdivrx_user_mode" type="string">
          <ipxact:name>pma_rx_deser_clkdivrx_user_mode</ipxact:name>
          <ipxact:displayName>pma_rx_deser_clkdivrx_user_mode</ipxact:displayName>
          <ipxact:value>clkdivrx_user_div33</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_datarate_bps" type="string">
          <ipxact:name>pma_rx_deser_datarate_bps</ipxact:name>
          <ipxact:displayName>pma_rx_deser_datarate_bps</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_deser_aib_dftppm_en" type="string">
          <ipxact:name>pma_rx_deser_deser_aib_dftppm_en</ipxact:name>
          <ipxact:displayName>pma_rx_deser_deser_aib_dftppm_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_deser_aibck_en" type="string">
          <ipxact:name>pma_rx_deser_deser_aibck_en</ipxact:name>
          <ipxact:displayName>pma_rx_deser_deser_aibck_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_deser_aibck_x1" type="string">
          <ipxact:name>pma_rx_deser_deser_aibck_x1</ipxact:name>
          <ipxact:displayName>pma_rx_deser_deser_aibck_x1</ipxact:displayName>
          <ipxact:value>normal</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_deser_factor" type="string">
          <ipxact:name>pma_rx_deser_deser_factor</ipxact:name>
          <ipxact:displayName>pma_rx_deser_deser_factor</ipxact:displayName>
          <ipxact:value>deser_32b</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_deser_powerdown" type="string">
          <ipxact:name>pma_rx_deser_deser_powerdown</ipxact:name>
          <ipxact:displayName>pma_rx_deser_deser_powerdown</ipxact:displayName>
          <ipxact:value>deser_power_up</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_force_adaptation_outputs" type="string">
          <ipxact:name>pma_rx_deser_force_adaptation_outputs</ipxact:name>
          <ipxact:displayName>pma_rx_deser_force_adaptation_outputs</ipxact:displayName>
          <ipxact:value>normal_outputs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_force_clkdiv_for_testing" type="string">
          <ipxact:name>pma_rx_deser_force_clkdiv_for_testing</ipxact:name>
          <ipxact:displayName>pma_rx_deser_force_clkdiv_for_testing</ipxact:displayName>
          <ipxact:value>normal_clkdiv</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_odi_adapt_bti_en" type="string">
          <ipxact:name>pma_rx_deser_odi_adapt_bti_en</ipxact:name>
          <ipxact:displayName>pma_rx_deser_odi_adapt_bti_en</ipxact:displayName>
          <ipxact:value>deser_bti_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_optimal" type="string">
          <ipxact:name>pma_rx_deser_optimal</ipxact:name>
          <ipxact:displayName>pma_rx_deser_optimal</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_pcie_g3_hclk_en" type="string">
          <ipxact:name>pma_rx_deser_pcie_g3_hclk_en</ipxact:name>
          <ipxact:displayName>pma_rx_deser_pcie_g3_hclk_en</ipxact:displayName>
          <ipxact:value>disable_hclk_div2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_pm_cr2_tx_rx_pcie_gen" type="string">
          <ipxact:name>pma_rx_deser_pm_cr2_tx_rx_pcie_gen</ipxact:name>
          <ipxact:displayName>pma_rx_deser_pm_cr2_tx_rx_pcie_gen</ipxact:displayName>
          <ipxact:value>non_pcie</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_pm_cr2_tx_rx_pcie_gen_bitwidth" type="string">
          <ipxact:name>pma_rx_deser_pm_cr2_tx_rx_pcie_gen_bitwidth</ipxact:name>
          <ipxact:displayName>pma_rx_deser_pm_cr2_tx_rx_pcie_gen_bitwidth</ipxact:displayName>
          <ipxact:value>pcie_gen3_32b</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_powermode_ac_deser" type="string">
          <ipxact:name>pma_rx_deser_powermode_ac_deser</ipxact:name>
          <ipxact:displayName>pma_rx_deser_powermode_ac_deser</ipxact:displayName>
          <ipxact:value>deser_ac_32b_nobs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_powermode_ac_deser_bs" type="string">
          <ipxact:name>pma_rx_deser_powermode_ac_deser_bs</ipxact:name>
          <ipxact:displayName>pma_rx_deser_powermode_ac_deser_bs</ipxact:displayName>
          <ipxact:value>deser_ac_bs_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_powermode_dc_deser" type="string">
          <ipxact:name>pma_rx_deser_powermode_dc_deser</ipxact:name>
          <ipxact:displayName>pma_rx_deser_powermode_dc_deser</ipxact:displayName>
          <ipxact:value>deser_dc_32b_nobs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_powermode_dc_deser_bs" type="string">
          <ipxact:name>pma_rx_deser_powermode_dc_deser_bs</ipxact:name>
          <ipxact:displayName>pma_rx_deser_powermode_dc_deser_bs</ipxact:displayName>
          <ipxact:value>powerdown_deser_bs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_prot_mode" type="string">
          <ipxact:name>pma_rx_deser_prot_mode</ipxact:name>
          <ipxact:displayName>pma_rx_deser_prot_mode</ipxact:displayName>
          <ipxact:value>basic_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_rst_n_adapt_odi" type="string">
          <ipxact:name>pma_rx_deser_rst_n_adapt_odi</ipxact:name>
          <ipxact:displayName>pma_rx_deser_rst_n_adapt_odi</ipxact:displayName>
          <ipxact:value>no_rst_adapt_odi</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_sd_clk" type="string">
          <ipxact:name>pma_rx_deser_sd_clk</ipxact:name>
          <ipxact:displayName>pma_rx_deser_sd_clk</ipxact:displayName>
          <ipxact:value>sd_clk_disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_sup_mode" type="string">
          <ipxact:name>pma_rx_deser_sup_mode</ipxact:name>
          <ipxact:displayName>pma_rx_deser_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_tdr_mode" type="string">
          <ipxact:name>pma_rx_deser_tdr_mode</ipxact:name>
          <ipxact:displayName>pma_rx_deser_tdr_mode</ipxact:displayName>
          <ipxact:value>select_bbpd_data</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_deser_silicon_rev" type="string">
          <ipxact:name>pma_rx_deser_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_rx_deser_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_adapt_bti_en" type="string">
          <ipxact:name>pma_rx_dfe_adapt_bti_en</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_adapt_bti_en</ipxact:displayName>
          <ipxact:value>adapt_bti_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_atb_select" type="string">
          <ipxact:name>pma_rx_dfe_atb_select</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_atb_select</ipxact:displayName>
          <ipxact:value>atb_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_bti_protected" type="string">
          <ipxact:name>pma_rx_dfe_bti_protected</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_bti_protected</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_xrx_path_xcdr_deser_xcdr_cdr_d2a_enb" type="string">
          <ipxact:name>pma_rx_dfe_xrx_path_xcdr_deser_xcdr_cdr_d2a_enb</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_xrx_path_xcdr_deser_xcdr_cdr_d2a_enb</ipxact:displayName>
          <ipxact:value>bti_d2a_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_datarate_bps" type="string">
          <ipxact:name>pma_rx_dfe_datarate_bps</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_datarate_bps</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_dfe_bti_en" type="string">
          <ipxact:name>pma_rx_dfe_dfe_bti_en</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_dfe_bti_en</ipxact:displayName>
          <ipxact:value>dfe_bti_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_dfe_mode" type="string">
          <ipxact:name>pma_rx_dfe_dfe_mode</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_dfe_mode</ipxact:displayName>
          <ipxact:value>cdr_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_dft_en" type="string">
          <ipxact:name>pma_rx_dfe_dft_en</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_dft_en</ipxact:displayName>
          <ipxact:value>dft_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_dft_hilospeed_sel" type="string">
          <ipxact:name>pma_rx_dfe_dft_hilospeed_sel</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_dft_hilospeed_sel</ipxact:displayName>
          <ipxact:value>dft_osc_lospeed_path</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_dft_osc_sel" type="string">
          <ipxact:name>pma_rx_dfe_dft_osc_sel</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_dft_osc_sel</ipxact:displayName>
          <ipxact:value>dft_osc_even</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_h1edge_bti_en" type="string">
          <ipxact:name>pma_rx_dfe_h1edge_bti_en</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_h1edge_bti_en</ipxact:displayName>
          <ipxact:value>h1edge_bti_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_initial_settings" type="string">
          <ipxact:name>pma_rx_dfe_initial_settings</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_initial_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_latch_xcouple_disable" type="string">
          <ipxact:name>pma_rx_dfe_latch_xcouple_disable</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_latch_xcouple_disable</ipxact:displayName>
          <ipxact:value>latch_xcouple_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdr0e" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_cdr0e</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdr0e</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdr0e_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_cdr0e_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdr0e_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_cdr0e_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdr0o" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_cdr0o</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdr0o</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdr0o_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_cdr0o_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdr0o_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_cdr0o_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdrne" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_cdrne</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdrne</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdrne_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_cdrne_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdrne_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_cdrne_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdrno" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_cdrno</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdrno</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdrno_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_cdrno_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdrno_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_cdrno_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdrpe" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_cdrpe</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdrpe</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdrpe_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_cdrpe_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdrpe_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_cdrpe_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdrpo" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_cdrpo</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdrpo</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_cdrpo_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_cdrpo_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_cdrpo_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_cdrpo_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_dne" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_dne</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_dne</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_dne_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_dne_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_dne_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_dne_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_dno" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_dno</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_dno</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_dno_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_dno_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_dno_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_dno_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_dpe" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_dpe</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_dpe</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_dpe_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_dpe_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_dpe_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_dpe_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_dpo" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_dpo</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_dpo</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_dpo_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_dpo_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_dpo_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_dpo_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_odie" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_odie</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_odie</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_odie_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_odie_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_odie_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_odie_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_odio" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_odio</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_odio</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_odio_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_odio_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_odio_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_odio_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_vrefe" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_vrefe</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_vrefe</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_vrefe_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_vrefe_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_vrefe_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_vrefe_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_vrefo" type="int">
          <ipxact:name>pma_rx_dfe_oc_sa_vrefo</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_vrefo</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_oc_sa_vrefo_sgn" type="string">
          <ipxact:name>pma_rx_dfe_oc_sa_vrefo_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_oc_sa_vrefo_sgn</ipxact:displayName>
          <ipxact:value>oc_sa_vrefo_sgn_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_odi_bti_en" type="string">
          <ipxact:name>pma_rx_dfe_odi_bti_en</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_odi_bti_en</ipxact:displayName>
          <ipxact:value>odi_bti_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_odi_dlev_sign" type="string">
          <ipxact:name>pma_rx_dfe_odi_dlev_sign</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_odi_dlev_sign</ipxact:displayName>
          <ipxact:value>odi_dlev_pos</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_odi_h1_sign" type="string">
          <ipxact:name>pma_rx_dfe_odi_h1_sign</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_odi_h1_sign</ipxact:displayName>
          <ipxact:value>odi_h1_pos</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_optimal" type="string">
          <ipxact:name>pma_rx_dfe_optimal</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_optimal</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_pdb" type="string">
          <ipxact:name>pma_rx_dfe_pdb</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_pdb</ipxact:displayName>
          <ipxact:value>dfe_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_pdb_edge_pre_h1" type="string">
          <ipxact:name>pma_rx_dfe_pdb_edge_pre_h1</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_pdb_edge_pre_h1</ipxact:displayName>
          <ipxact:value>cdr_pre_h1_enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_pdb_edge_pst_h1" type="string">
          <ipxact:name>pma_rx_dfe_pdb_edge_pst_h1</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_pdb_edge_pst_h1</ipxact:displayName>
          <ipxact:value>cdr_pst_h1_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_pdb_tap_10t15" type="string">
          <ipxact:name>pma_rx_dfe_pdb_tap_10t15</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_pdb_tap_10t15</ipxact:displayName>
          <ipxact:value>tap10t15_dfe_powerdown</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_pdb_tap_4t9" type="string">
          <ipxact:name>pma_rx_dfe_pdb_tap_4t9</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_pdb_tap_4t9</ipxact:displayName>
          <ipxact:value>tap4t9_dfe_powerdown</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_pdb_tapsum" type="string">
          <ipxact:name>pma_rx_dfe_pdb_tapsum</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_pdb_tapsum</ipxact:displayName>
          <ipxact:value>tapsum_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_power_mode" type="string">
          <ipxact:name>pma_rx_dfe_power_mode</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_power_mode</ipxact:displayName>
          <ipxact:value>mid_power</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_powermode_ac_dfe" type="string">
          <ipxact:name>pma_rx_dfe_powermode_ac_dfe</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_powermode_ac_dfe</ipxact:displayName>
          <ipxact:value>ac_cdr_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_powermode_dc_dfe" type="string">
          <ipxact:name>pma_rx_dfe_powermode_dc_dfe</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_powermode_dc_dfe</ipxact:displayName>
          <ipxact:value>powerdown_dfe</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_prot_mode" type="string">
          <ipxact:name>pma_rx_dfe_prot_mode</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_prot_mode</ipxact:displayName>
          <ipxact:value>basic_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_sel_oc_en" type="string">
          <ipxact:name>pma_rx_dfe_sel_oc_en</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_sel_oc_en</ipxact:displayName>
          <ipxact:value>off_canc_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_sel_probe_tstmx" type="string">
          <ipxact:name>pma_rx_dfe_sel_probe_tstmx</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_sel_probe_tstmx</ipxact:displayName>
          <ipxact:value>probe_tstmx_none</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_sup_mode" type="string">
          <ipxact:name>pma_rx_dfe_sup_mode</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap10_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap10_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap10_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap10_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap10_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap10_sgn</ipxact:displayName>
          <ipxact:value>tap10_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap11_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap11_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap11_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap11_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap11_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap11_sgn</ipxact:displayName>
          <ipxact:value>tap11_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap12_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap12_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap12_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap12_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap12_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap12_sgn</ipxact:displayName>
          <ipxact:value>tap12_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap13_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap13_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap13_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap13_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap13_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap13_sgn</ipxact:displayName>
          <ipxact:value>tap13_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap14_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap14_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap14_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap14_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap14_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap14_sgn</ipxact:displayName>
          <ipxact:value>tap14_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap15_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap15_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap15_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap15_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap15_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap15_sgn</ipxact:displayName>
          <ipxact:value>tap15_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap1_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap1_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap1_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap1_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap1_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap1_sgn</ipxact:displayName>
          <ipxact:value>tap1_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap2_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap2_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap2_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap2_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap2_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap2_sgn</ipxact:displayName>
          <ipxact:value>tap2_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap3_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap3_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap3_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap3_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap3_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap3_sgn</ipxact:displayName>
          <ipxact:value>tap3_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap4_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap4_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap4_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap4_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap4_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap4_sgn</ipxact:displayName>
          <ipxact:value>tap4_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap5_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap5_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap5_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap5_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap5_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap5_sgn</ipxact:displayName>
          <ipxact:value>tap5_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap6_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap6_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap6_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap6_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap6_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap6_sgn</ipxact:displayName>
          <ipxact:value>tap6_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap7_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap7_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap7_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap7_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap7_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap7_sgn</ipxact:displayName>
          <ipxact:value>tap7_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap8_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap8_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap8_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap8_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap8_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap8_sgn</ipxact:displayName>
          <ipxact:value>tap8_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap9_coeff" type="int">
          <ipxact:name>pma_rx_dfe_tap9_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap9_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tap9_sgn" type="string">
          <ipxact:name>pma_rx_dfe_tap9_sgn</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tap9_sgn</ipxact:displayName>
          <ipxact:value>tap9_sign_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_tapsum_bw_sel" type="string">
          <ipxact:name>pma_rx_dfe_tapsum_bw_sel</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_tapsum_bw_sel</ipxact:displayName>
          <ipxact:value>tapsum_medbw</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_vref_coeff" type="int">
          <ipxact:name>pma_rx_dfe_vref_coeff</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_vref_coeff</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_dfe_silicon_rev" type="string">
          <ipxact:name>pma_rx_dfe_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_rx_dfe_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_datarate_bps" type="string">
          <ipxact:name>pma_rx_odi_datarate_bps</ipxact:name>
          <ipxact:displayName>pma_rx_odi_datarate_bps</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_enable_cdr_lpbk" type="string">
          <ipxact:name>pma_rx_odi_enable_cdr_lpbk</ipxact:name>
          <ipxact:displayName>pma_rx_odi_enable_cdr_lpbk</ipxact:displayName>
          <ipxact:value>disable_lpbk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_initial_settings" type="string">
          <ipxact:name>pma_rx_odi_initial_settings</ipxact:name>
          <ipxact:displayName>pma_rx_odi_initial_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_monitor_bw_sel" type="string">
          <ipxact:name>pma_rx_odi_monitor_bw_sel</ipxact:name>
          <ipxact:displayName>pma_rx_odi_monitor_bw_sel</ipxact:displayName>
          <ipxact:value>bw_4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_optimal" type="string">
          <ipxact:name>pma_rx_odi_optimal</ipxact:name>
          <ipxact:displayName>pma_rx_odi_optimal</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_phase_steps_64_vs_128" type="string">
          <ipxact:name>pma_rx_odi_phase_steps_64_vs_128</ipxact:name>
          <ipxact:displayName>pma_rx_odi_phase_steps_64_vs_128</ipxact:displayName>
          <ipxact:value>phase_steps_64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_phase_steps_sel" type="string">
          <ipxact:name>pma_rx_odi_phase_steps_sel</ipxact:name>
          <ipxact:displayName>pma_rx_odi_phase_steps_sel</ipxact:displayName>
          <ipxact:value>step33</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_power_mode" type="string">
          <ipxact:name>pma_rx_odi_power_mode</ipxact:name>
          <ipxact:displayName>pma_rx_odi_power_mode</ipxact:displayName>
          <ipxact:value>mid_power</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_prot_mode" type="string">
          <ipxact:name>pma_rx_odi_prot_mode</ipxact:name>
          <ipxact:displayName>pma_rx_odi_prot_mode</ipxact:displayName>
          <ipxact:value>basic_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_xrx_path_x119_rx_path_rstn_overrideb" type="string">
          <ipxact:name>pma_rx_odi_xrx_path_x119_rx_path_rstn_overrideb</ipxact:name>
          <ipxact:displayName>pma_rx_odi_xrx_path_x119_rx_path_rstn_overrideb</ipxact:displayName>
          <ipxact:value>use_sequencer</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_step_ctrl_sel" type="string">
          <ipxact:name>pma_rx_odi_step_ctrl_sel</ipxact:name>
          <ipxact:displayName>pma_rx_odi_step_ctrl_sel</ipxact:displayName>
          <ipxact:value>dprio_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_sup_mode" type="string">
          <ipxact:name>pma_rx_odi_sup_mode</ipxact:name>
          <ipxact:displayName>pma_rx_odi_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_vert_threshold" type="string">
          <ipxact:name>pma_rx_odi_vert_threshold</ipxact:name>
          <ipxact:displayName>pma_rx_odi_vert_threshold</ipxact:displayName>
          <ipxact:value>vert_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_vreg_voltage_sel" type="string">
          <ipxact:name>pma_rx_odi_vreg_voltage_sel</ipxact:name>
          <ipxact:displayName>pma_rx_odi_vreg_voltage_sel</ipxact:displayName>
          <ipxact:value>vreg0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_odi_silicon_rev" type="string">
          <ipxact:name>pma_rx_odi_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_rx_odi_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_link" type="string">
          <ipxact:name>pma_rx_sd_link</ipxact:name>
          <ipxact:displayName>pma_rx_sd_link</ipxact:displayName>
          <ipxact:value>sr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_optimal" type="string">
          <ipxact:name>pma_rx_sd_optimal</ipxact:name>
          <ipxact:displayName>pma_rx_sd_optimal</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_power_mode" type="string">
          <ipxact:name>pma_rx_sd_power_mode</ipxact:name>
          <ipxact:displayName>pma_rx_sd_power_mode</ipxact:displayName>
          <ipxact:value>mid_power</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_powermode_ac_sd" type="string">
          <ipxact:name>pma_rx_sd_powermode_ac_sd</ipxact:name>
          <ipxact:displayName>pma_rx_sd_powermode_ac_sd</ipxact:displayName>
          <ipxact:value>ac_off_sd</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_powermode_dc_sd" type="string">
          <ipxact:name>pma_rx_sd_powermode_dc_sd</ipxact:name>
          <ipxact:displayName>pma_rx_sd_powermode_dc_sd</ipxact:displayName>
          <ipxact:value>powerdown_sd</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_prot_mode" type="string">
          <ipxact:name>pma_rx_sd_prot_mode</ipxact:name>
          <ipxact:displayName>pma_rx_sd_prot_mode</ipxact:displayName>
          <ipxact:value>basic_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_sd_output_off" type="string">
          <ipxact:name>pma_rx_sd_sd_output_off</ipxact:name>
          <ipxact:displayName>pma_rx_sd_sd_output_off</ipxact:displayName>
          <ipxact:value>clk_divrx_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_sd_output_on" type="string">
          <ipxact:name>pma_rx_sd_sd_output_on</ipxact:name>
          <ipxact:displayName>pma_rx_sd_sd_output_on</ipxact:displayName>
          <ipxact:value>force_sd_output_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_sd_pdb" type="string">
          <ipxact:name>pma_rx_sd_sd_pdb</ipxact:name>
          <ipxact:displayName>pma_rx_sd_sd_pdb</ipxact:displayName>
          <ipxact:value>sd_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_sd_threshold" type="string">
          <ipxact:name>pma_rx_sd_sd_threshold</ipxact:name>
          <ipxact:displayName>pma_rx_sd_sd_threshold</ipxact:displayName>
          <ipxact:value>sdlv_3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_sup_mode" type="string">
          <ipxact:name>pma_rx_sd_sup_mode</ipxact:name>
          <ipxact:displayName>pma_rx_sd_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_rx_sd_silicon_rev" type="string">
          <ipxact:name>pma_rx_sd_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_rx_sd_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_analog_mode" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_analog_mode</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_analog_mode</ipxact:displayName>
          <ipxact:value>user_custom</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_bonding_mode" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_bonding_mode</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_bonding_mode</ipxact:displayName>
          <ipxact:value>x1_non_bonded</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_bti_protected" type="string">
          <ipxact:name>pma_tx_buf_bti_protected</ipxact:name>
          <ipxact:displayName>pma_tx_buf_bti_protected</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_calibration_en" type="string">
          <ipxact:name>pma_tx_buf_calibration_en</ipxact:name>
          <ipxact:displayName>pma_tx_buf_calibration_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_calibration_en" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_calibration_en</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_calibration_en</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_calibration_resistor_value" type="string">
          <ipxact:name>pma_tx_buf_calibration_resistor_value</ipxact:name>
          <ipxact:displayName>pma_tx_buf_calibration_resistor_value</ipxact:displayName>
          <ipxact:value>res_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_cdr_cp_calibration_en" type="string">
          <ipxact:name>pma_tx_buf_cdr_cp_calibration_en</ipxact:name>
          <ipxact:displayName>pma_tx_buf_cdr_cp_calibration_en</ipxact:displayName>
          <ipxact:value>cdr_cp_cal_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_chgpmp_current_dn_trim" type="string">
          <ipxact:name>pma_tx_buf_chgpmp_current_dn_trim</ipxact:name>
          <ipxact:displayName>pma_tx_buf_chgpmp_current_dn_trim</ipxact:displayName>
          <ipxact:value>cp_current_trimming_dn_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_chgpmp_current_up_trim" type="string">
          <ipxact:name>pma_tx_buf_chgpmp_current_up_trim</ipxact:name>
          <ipxact:displayName>pma_tx_buf_chgpmp_current_up_trim</ipxact:displayName>
          <ipxact:value>cp_current_trimming_up_setting0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_chgpmp_dn_trim_double" type="string">
          <ipxact:name>pma_tx_buf_chgpmp_dn_trim_double</ipxact:name>
          <ipxact:displayName>pma_tx_buf_chgpmp_dn_trim_double</ipxact:displayName>
          <ipxact:value>normal_dn_trim_current</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_chgpmp_up_trim_double" type="string">
          <ipxact:name>pma_tx_buf_chgpmp_up_trim_double</ipxact:name>
          <ipxact:displayName>pma_tx_buf_chgpmp_up_trim_double</ipxact:displayName>
          <ipxact:value>normal_up_trim_current</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_clock_divider_ratio" type="int">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_clock_divider_ratio</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_clock_divider_ratio</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_compensation_en" type="string">
          <ipxact:name>pma_tx_buf_compensation_en</ipxact:name>
          <ipxact:displayName>pma_tx_buf_compensation_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_compensation_posttap_en" type="string">
          <ipxact:name>pma_tx_buf_compensation_posttap_en</ipxact:name>
          <ipxact:displayName>pma_tx_buf_compensation_posttap_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_cpen_ctrl" type="string">
          <ipxact:name>pma_tx_buf_cpen_ctrl</ipxact:name>
          <ipxact:displayName>pma_tx_buf_cpen_ctrl</ipxact:displayName>
          <ipxact:value>cp_l1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_data_dcc_setting" type="string">
          <ipxact:name>pma_tx_buf_data_dcc_setting</ipxact:name>
          <ipxact:displayName>pma_tx_buf_data_dcc_setting</ipxact:displayName>
          <ipxact:value>ddcc_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_datarate_bps" type="string">
          <ipxact:name>pma_tx_buf_datarate_bps</ipxact:name>
          <ipxact:displayName>pma_tx_buf_datarate_bps</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_datarate_bps" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_datarate_bps</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_datarate_bps</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_datawidth" type="int">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_datawidth</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_datawidth</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_dcc_finestep_enin" type="string">
          <ipxact:name>pma_tx_buf_dcc_finestep_enin</ipxact:name>
          <ipxact:displayName>pma_tx_buf_dcc_finestep_enin</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_dcd_clk_div_ctrl" type="string">
          <ipxact:name>pma_tx_buf_dcd_clk_div_ctrl</ipxact:name>
          <ipxact:displayName>pma_tx_buf_dcd_clk_div_ctrl</ipxact:displayName>
          <ipxact:value>dcd_ck_div128</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_dcd_detection_en" type="string">
          <ipxact:name>pma_tx_buf_dcd_detection_en</ipxact:name>
          <ipxact:displayName>pma_tx_buf_dcd_detection_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_dft_sel" type="string">
          <ipxact:name>pma_tx_buf_dft_sel</ipxact:name>
          <ipxact:displayName>pma_tx_buf_dft_sel</ipxact:displayName>
          <ipxact:value>dft_disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_duty_cycle_correction_bandwidth" type="string">
          <ipxact:name>pma_tx_buf_duty_cycle_correction_bandwidth</ipxact:name>
          <ipxact:displayName>pma_tx_buf_duty_cycle_correction_bandwidth</ipxact:displayName>
          <ipxact:value>dcc_bw_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_duty_cycle_correction_bandwidth_dn" type="string">
          <ipxact:name>pma_tx_buf_duty_cycle_correction_bandwidth_dn</ipxact:name>
          <ipxact:displayName>pma_tx_buf_duty_cycle_correction_bandwidth_dn</ipxact:displayName>
          <ipxact:value>dcd_bw_dn_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_duty_cycle_correction_reference1" type="string">
          <ipxact:name>pma_tx_buf_duty_cycle_correction_reference1</ipxact:name>
          <ipxact:displayName>pma_tx_buf_duty_cycle_correction_reference1</ipxact:displayName>
          <ipxact:value>dcc_ref1_4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_duty_cycle_correction_reference2" type="string">
          <ipxact:name>pma_tx_buf_duty_cycle_correction_reference2</ipxact:name>
          <ipxact:displayName>pma_tx_buf_duty_cycle_correction_reference2</ipxact:displayName>
          <ipxact:value>dcc_ref2_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_duty_cycle_correction_reset_n" type="string">
          <ipxact:name>pma_tx_buf_duty_cycle_correction_reset_n</ipxact:name>
          <ipxact:displayName>pma_tx_buf_duty_cycle_correction_reset_n</ipxact:displayName>
          <ipxact:value>reset</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_duty_cycle_cp_comp_en" type="string">
          <ipxact:name>pma_tx_buf_duty_cycle_cp_comp_en</ipxact:name>
          <ipxact:displayName>pma_tx_buf_duty_cycle_cp_comp_en</ipxact:displayName>
          <ipxact:value>cp_comp_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_duty_cycle_detector_cp_cal" type="string">
          <ipxact:name>pma_tx_buf_duty_cycle_detector_cp_cal</ipxact:name>
          <ipxact:displayName>pma_tx_buf_duty_cycle_detector_cp_cal</ipxact:displayName>
          <ipxact:value>dcd_cp_cal_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_duty_cycle_detector_sa_cal" type="string">
          <ipxact:name>pma_tx_buf_duty_cycle_detector_sa_cal</ipxact:name>
          <ipxact:displayName>pma_tx_buf_duty_cycle_detector_sa_cal</ipxact:displayName>
          <ipxact:value>dcd_sa_cal_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_duty_cycle_input_polarity" type="string">
          <ipxact:name>pma_tx_buf_duty_cycle_input_polarity</ipxact:name>
          <ipxact:displayName>pma_tx_buf_duty_cycle_input_polarity</ipxact:displayName>
          <ipxact:value>dcc_input_pos</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_duty_cycle_setting" type="string">
          <ipxact:name>pma_tx_buf_duty_cycle_setting</ipxact:name>
          <ipxact:displayName>pma_tx_buf_duty_cycle_setting</ipxact:displayName>
          <ipxact:value>dcc_t32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_duty_cycle_setting_aux" type="string">
          <ipxact:name>pma_tx_buf_duty_cycle_setting_aux</ipxact:name>
          <ipxact:displayName>pma_tx_buf_duty_cycle_setting_aux</ipxact:displayName>
          <ipxact:value>dcc2_t32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_enable_idle_tx_channel_support" type="string">
          <ipxact:name>pma_tx_buf_enable_idle_tx_channel_support</ipxact:name>
          <ipxact:displayName>pma_tx_buf_enable_idle_tx_channel_support</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_gt_enabled" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_gt_enabled</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_gt_enabled</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_idle_ctrl" type="string">
          <ipxact:name>pma_tx_buf_idle_ctrl</ipxact:name>
          <ipxact:displayName>pma_tx_buf_idle_ctrl</ipxact:displayName>
          <ipxact:value>id_cpen_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_initial_settings" type="string">
          <ipxact:name>pma_tx_buf_initial_settings</ipxact:name>
          <ipxact:displayName>pma_tx_buf_initial_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_initial_settings" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_initial_settings</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_initial_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_jtag_drv_sel" type="string">
          <ipxact:name>pma_tx_buf_jtag_drv_sel</ipxact:name>
          <ipxact:displayName>pma_tx_buf_jtag_drv_sel</ipxact:displayName>
          <ipxact:value>drv1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_jtag_lp" type="string">
          <ipxact:name>pma_tx_buf_jtag_lp</ipxact:name>
          <ipxact:displayName>pma_tx_buf_jtag_lp</ipxact:displayName>
          <ipxact:value>lp_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_link" type="string">
          <ipxact:name>pma_tx_buf_link</ipxact:name>
          <ipxact:displayName>pma_tx_buf_link</ipxact:displayName>
          <ipxact:value>link_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_link" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_link</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_link</ipxact:displayName>
          <ipxact:value>sr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_low_power_en" type="string">
          <ipxact:name>pma_tx_buf_low_power_en</ipxact:name>
          <ipxact:displayName>pma_tx_buf_low_power_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_lst" type="string">
          <ipxact:name>pma_tx_buf_lst</ipxact:name>
          <ipxact:displayName>pma_tx_buf_lst</ipxact:displayName>
          <ipxact:value>atb_disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_rx_mcgb_location_for_pcie" type="int">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_rx_mcgb_location_for_pcie</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_rx_mcgb_location_for_pcie</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_optimal" type="string">
          <ipxact:name>pma_tx_buf_optimal</ipxact:name>
          <ipxact:displayName>pma_tx_buf_optimal</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_optimal" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_optimal</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_optimal</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pcie_gen" type="string">
          <ipxact:name>pma_tx_buf_pcie_gen</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pcie_gen</ipxact:displayName>
          <ipxact:value>non_pcie</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_pma_tx_divclk_hz" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_pma_tx_divclk_hz</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_pma_tx_divclk_hz</ipxact:displayName>
          <ipxact:value>322265625</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_power_mode" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_power_mode</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_power_mode</ipxact:displayName>
          <ipxact:value>mid_power</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_power_rail_eht" type="int">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_power_rail_eht</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_power_rail_eht</ipxact:displayName>
          <ipxact:value>1800</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_power_rail_er" type="int">
          <ipxact:name>pma_tx_buf_power_rail_er</ipxact:name>
          <ipxact:displayName>pma_tx_buf_power_rail_er</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_power_rail_et" type="int">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_power_rail_et</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_power_rail_et</ipxact:displayName>
          <ipxact:value>1030</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_powermode_ac_post_tap" type="string">
          <ipxact:name>pma_tx_buf_powermode_ac_post_tap</ipxact:name>
          <ipxact:displayName>pma_tx_buf_powermode_ac_post_tap</ipxact:displayName>
          <ipxact:value>tx_post_tap_ac_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_powermode_ac_pre_tap" type="string">
          <ipxact:name>pma_tx_buf_powermode_ac_pre_tap</ipxact:name>
          <ipxact:displayName>pma_tx_buf_powermode_ac_pre_tap</ipxact:displayName>
          <ipxact:value>tx_pre_tap_ac_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_powermode_ac_tx_vod_no_jitcomp" type="string">
          <ipxact:name>pma_tx_buf_powermode_ac_tx_vod_no_jitcomp</ipxact:name>
          <ipxact:displayName>pma_tx_buf_powermode_ac_tx_vod_no_jitcomp</ipxact:displayName>
          <ipxact:value>tx_vod_no_jitcomp_ac_l0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_powermode_ac_tx_vod_w_jitcomp" type="string">
          <ipxact:name>pma_tx_buf_powermode_ac_tx_vod_w_jitcomp</ipxact:name>
          <ipxact:displayName>pma_tx_buf_powermode_ac_tx_vod_w_jitcomp</ipxact:displayName>
          <ipxact:value>tx_vod_w_jitcomp_ac_l31</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_powermode_dc_post_tap" type="string">
          <ipxact:name>pma_tx_buf_powermode_dc_post_tap</ipxact:name>
          <ipxact:displayName>pma_tx_buf_powermode_dc_post_tap</ipxact:displayName>
          <ipxact:value>powerdown_tx_post_tap</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_powermode_dc_pre_tap" type="string">
          <ipxact:name>pma_tx_buf_powermode_dc_pre_tap</ipxact:name>
          <ipxact:displayName>pma_tx_buf_powermode_dc_pre_tap</ipxact:displayName>
          <ipxact:value>powerdown_tx_pre_tap</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_powermode_dc_tx_vod_no_jitcomp" type="string">
          <ipxact:name>pma_tx_buf_powermode_dc_tx_vod_no_jitcomp</ipxact:name>
          <ipxact:displayName>pma_tx_buf_powermode_dc_tx_vod_no_jitcomp</ipxact:displayName>
          <ipxact:value>powerdown_tx_vod_no_jitcomp</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_powermode_dc_tx_vod_w_jitcomp" type="string">
          <ipxact:name>pma_tx_buf_powermode_dc_tx_vod_w_jitcomp</ipxact:name>
          <ipxact:displayName>pma_tx_buf_powermode_dc_tx_vod_w_jitcomp</ipxact:displayName>
          <ipxact:value>tx_vod_w_jitcomp_dc_l31</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pre_emp_sign_1st_post_tap" type="string">
          <ipxact:name>pma_tx_buf_pre_emp_sign_1st_post_tap</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pre_emp_sign_1st_post_tap</ipxact:displayName>
          <ipxact:value>fir_post_1t_neg</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pre_emp_sign_pre_tap_1t" type="string">
          <ipxact:name>pma_tx_buf_pre_emp_sign_pre_tap_1t</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pre_emp_sign_pre_tap_1t</ipxact:displayName>
          <ipxact:value>fir_pre_1t_neg</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pre_emp_switching_ctrl_1st_post_tap" type="int">
          <ipxact:name>pma_tx_buf_pre_emp_switching_ctrl_1st_post_tap</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pre_emp_switching_ctrl_1st_post_tap</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pre_emp_switching_ctrl_pre_tap_1t" type="int">
          <ipxact:name>pma_tx_buf_pre_emp_switching_ctrl_pre_tap_1t</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pre_emp_switching_ctrl_pre_tap_1t</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_prot_mode" type="string">
          <ipxact:name>pma_tx_buf_prot_mode</ipxact:name>
          <ipxact:displayName>pma_tx_buf_prot_mode</ipxact:displayName>
          <ipxact:value>basic_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_prot_mode" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_prot_mode</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_prot_mode</ipxact:displayName>
          <ipxact:value>basic_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_res_cal_local" type="string">
          <ipxact:name>pma_tx_buf_res_cal_local</ipxact:name>
          <ipxact:displayName>pma_tx_buf_res_cal_local</ipxact:displayName>
          <ipxact:value>non_local</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_reserve_tx_channel" type="string">
          <ipxact:name>pma_tx_buf_reserve_tx_channel</ipxact:name>
          <ipxact:displayName>pma_tx_buf_reserve_tx_channel</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_rx_det" type="string">
          <ipxact:name>pma_tx_buf_rx_det</ipxact:name>
          <ipxact:displayName>pma_tx_buf_rx_det</ipxact:displayName>
          <ipxact:value>mode_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_rx_det_output_sel" type="string">
          <ipxact:name>pma_tx_buf_rx_det_output_sel</ipxact:name>
          <ipxact:displayName>pma_tx_buf_rx_det_output_sel</ipxact:displayName>
          <ipxact:value>rx_det_pcie_out</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_rx_det_pdb" type="string">
          <ipxact:name>pma_tx_buf_rx_det_pdb</ipxact:name>
          <ipxact:displayName>pma_tx_buf_rx_det_pdb</ipxact:displayName>
          <ipxact:value>rx_det_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_sense_amp_offset_cal_curr_n" type="string">
          <ipxact:name>pma_tx_buf_sense_amp_offset_cal_curr_n</ipxact:name>
          <ipxact:displayName>pma_tx_buf_sense_amp_offset_cal_curr_n</ipxact:displayName>
          <ipxact:value>sa_os_cal_in_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_sense_amp_offset_cal_curr_p" type="int">
          <ipxact:name>pma_tx_buf_sense_amp_offset_cal_curr_p</ipxact:name>
          <ipxact:displayName>pma_tx_buf_sense_amp_offset_cal_curr_p</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_ser_powerdown" type="string">
          <ipxact:name>pma_tx_buf_ser_powerdown</ipxact:name>
          <ipxact:displayName>pma_tx_buf_ser_powerdown</ipxact:displayName>
          <ipxact:value>normal_ser_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_slew_rate_ctrl" type="string">
          <ipxact:name>pma_tx_buf_slew_rate_ctrl</ipxact:name>
          <ipxact:displayName>pma_tx_buf_slew_rate_ctrl</ipxact:displayName>
          <ipxact:value>slew_r5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_speed_grade" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_speed_grade</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_speed_grade</ipxact:displayName>
          <ipxact:value>e2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_sup_mode" type="string">
          <ipxact:name>pma_tx_buf_sup_mode</ipxact:name>
          <ipxact:displayName>pma_tx_buf_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_sup_mode" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_sup_mode</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_swing_level" type="string">
          <ipxact:name>pma_tx_buf_swing_level</ipxact:name>
          <ipxact:displayName>pma_tx_buf_swing_level</ipxact:displayName>
          <ipxact:value>hv</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_swing_level" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_swing_level</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_swing_level</ipxact:displayName>
          <ipxact:value>hv</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_term_code" type="string">
          <ipxact:name>pma_tx_buf_term_code</ipxact:name>
          <ipxact:displayName>pma_tx_buf_term_code</ipxact:displayName>
          <ipxact:value>rterm_code0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_term_n_tune" type="string">
          <ipxact:name>pma_tx_buf_term_n_tune</ipxact:name>
          <ipxact:displayName>pma_tx_buf_term_n_tune</ipxact:displayName>
          <ipxact:value>rterm_n7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_term_p_tune" type="string">
          <ipxact:name>pma_tx_buf_term_p_tune</ipxact:name>
          <ipxact:displayName>pma_tx_buf_term_p_tune</ipxact:displayName>
          <ipxact:value>rterm_p7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_term_sel" type="string">
          <ipxact:name>pma_tx_buf_term_sel</ipxact:name>
          <ipxact:displayName>pma_tx_buf_term_sel</ipxact:displayName>
          <ipxact:value>r_r1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_tile_type" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_tile_type</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_tile_type</ipxact:displayName>
          <ipxact:value>h</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_tri_driver" type="string">
          <ipxact:name>pma_tx_buf_tri_driver</ipxact:name>
          <ipxact:displayName>pma_tx_buf_tri_driver</ipxact:displayName>
          <ipxact:value>tri_driver_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_pm_cr2_tx_path_tx_pll_clk_hz" type="string">
          <ipxact:name>pma_tx_buf_pm_cr2_tx_path_tx_pll_clk_hz</ipxact:name>
          <ipxact:displayName>pma_tx_buf_pm_cr2_tx_path_tx_pll_clk_hz</ipxact:displayName>
          <ipxact:value>5156250000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_tx_powerdown" type="string">
          <ipxact:name>pma_tx_buf_tx_powerdown</ipxact:name>
          <ipxact:displayName>pma_tx_buf_tx_powerdown</ipxact:displayName>
          <ipxact:value>normal_tx_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_tx_rst_enable" type="string">
          <ipxact:name>pma_tx_buf_tx_rst_enable</ipxact:name>
          <ipxact:displayName>pma_tx_buf_tx_rst_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_xtx_path_xcgb_tx_ucontrol_en" type="string">
          <ipxact:name>pma_tx_buf_xtx_path_xcgb_tx_ucontrol_en</ipxact:name>
          <ipxact:displayName>pma_tx_buf_xtx_path_xcgb_tx_ucontrol_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_uc_gen3" type="string">
          <ipxact:name>pma_tx_buf_uc_gen3</ipxact:name>
          <ipxact:displayName>pma_tx_buf_uc_gen3</ipxact:displayName>
          <ipxact:value>gen3_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_uc_gen4" type="string">
          <ipxact:name>pma_tx_buf_uc_gen4</ipxact:name>
          <ipxact:displayName>pma_tx_buf_uc_gen4</ipxact:displayName>
          <ipxact:value>gen4_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_uc_tx_cal" type="string">
          <ipxact:name>pma_tx_buf_uc_tx_cal</ipxact:name>
          <ipxact:displayName>pma_tx_buf_uc_tx_cal</ipxact:displayName>
          <ipxact:value>uc_tx_cal_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_uc_vcc_setting" type="string">
          <ipxact:name>pma_tx_buf_uc_vcc_setting</ipxact:name>
          <ipxact:displayName>pma_tx_buf_uc_vcc_setting</ipxact:displayName>
          <ipxact:value>vcc_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_user_fir_coeff_ctrl_sel" type="string">
          <ipxact:name>pma_tx_buf_user_fir_coeff_ctrl_sel</ipxact:name>
          <ipxact:displayName>pma_tx_buf_user_fir_coeff_ctrl_sel</ipxact:displayName>
          <ipxact:value>ram_ctl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_vod_output_swing_ctrl" type="int">
          <ipxact:name>pma_tx_buf_vod_output_swing_ctrl</ipxact:name>
          <ipxact:displayName>pma_tx_buf_vod_output_swing_ctrl</ipxact:displayName>
          <ipxact:value>31</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_vreg_output" type="string">
          <ipxact:name>pma_tx_buf_vreg_output</ipxact:name>
          <ipxact:displayName>pma_tx_buf_vreg_output</ipxact:displayName>
          <ipxact:value>vccdreg_nominal</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_buf_silicon_rev" type="string">
          <ipxact:name>pma_tx_buf_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_tx_buf_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_bitslip_enable" type="string">
          <ipxact:name>pma_cgb_bitslip_enable</ipxact:name>
          <ipxact:displayName>pma_cgb_bitslip_enable</ipxact:displayName>
          <ipxact:value>disable_bitslip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_bonding_mode" type="string">
          <ipxact:name>pma_cgb_bonding_mode</ipxact:name>
          <ipxact:displayName>pma_cgb_bonding_mode</ipxact:displayName>
          <ipxact:value>bond_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_bti_protected" type="string">
          <ipxact:name>pma_cgb_bti_protected</ipxact:name>
          <ipxact:displayName>pma_cgb_bti_protected</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_cgb_bti_en" type="string">
          <ipxact:name>pma_cgb_cgb_bti_en</ipxact:name>
          <ipxact:displayName>pma_cgb_cgb_bti_en</ipxact:displayName>
          <ipxact:value>cgb_bti_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_cgb_power_down" type="string">
          <ipxact:name>pma_cgb_cgb_power_down</ipxact:name>
          <ipxact:displayName>pma_cgb_cgb_power_down</ipxact:displayName>
          <ipxact:value>normal_cgb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_datarate_bps" type="string">
          <ipxact:name>pma_cgb_datarate_bps</ipxact:name>
          <ipxact:displayName>pma_cgb_datarate_bps</ipxact:displayName>
          <ipxact:value>10312500000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_initial_settings" type="string">
          <ipxact:name>pma_cgb_initial_settings</ipxact:name>
          <ipxact:displayName>pma_cgb_initial_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_observe_cgb_clocks" type="string">
          <ipxact:name>pma_cgb_observe_cgb_clocks</ipxact:name>
          <ipxact:displayName>pma_cgb_observe_cgb_clocks</ipxact:displayName>
          <ipxact:value>observe_nothing</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_pcie_gen" type="string">
          <ipxact:name>pma_cgb_pcie_gen</ipxact:name>
          <ipxact:displayName>pma_cgb_pcie_gen</ipxact:displayName>
          <ipxact:value>non_pcie</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_pcie_gen3_bitwidth" type="string">
          <ipxact:name>pma_cgb_pcie_gen3_bitwidth</ipxact:name>
          <ipxact:displayName>pma_cgb_pcie_gen3_bitwidth</ipxact:displayName>
          <ipxact:value>pciegen3_wide</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_power_rail_er" type="int">
          <ipxact:name>pma_cgb_power_rail_er</ipxact:name>
          <ipxact:displayName>pma_cgb_power_rail_er</ipxact:displayName>
          <ipxact:value>1030</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_powermode_ac_cgb" type="string">
          <ipxact:name>pma_cgb_powermode_ac_cgb</ipxact:name>
          <ipxact:displayName>pma_cgb_powermode_ac_cgb</ipxact:displayName>
          <ipxact:value>cgb_ac_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_powermode_dc_cgb" type="string">
          <ipxact:name>pma_cgb_powermode_dc_cgb</ipxact:name>
          <ipxact:displayName>pma_cgb_powermode_dc_cgb</ipxact:displayName>
          <ipxact:value>powerdown_cgb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_prot_mode" type="string">
          <ipxact:name>pma_cgb_prot_mode</ipxact:name>
          <ipxact:displayName>pma_cgb_prot_mode</ipxact:displayName>
          <ipxact:value>basic_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_scratch0_x1_clock_src" type="string">
          <ipxact:name>pma_cgb_scratch0_x1_clock_src</ipxact:name>
          <ipxact:displayName>pma_cgb_scratch0_x1_clock_src</ipxact:displayName>
          <ipxact:value>not_used</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_scratch1_x1_clock_src" type="string">
          <ipxact:name>pma_cgb_scratch1_x1_clock_src</ipxact:name>
          <ipxact:displayName>pma_cgb_scratch1_x1_clock_src</ipxact:displayName>
          <ipxact:value>not_used</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_scratch2_x1_clock_src" type="string">
          <ipxact:name>pma_cgb_scratch2_x1_clock_src</ipxact:name>
          <ipxact:displayName>pma_cgb_scratch2_x1_clock_src</ipxact:displayName>
          <ipxact:value>not_used</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_scratch3_x1_clock_src" type="string">
          <ipxact:name>pma_cgb_scratch3_x1_clock_src</ipxact:name>
          <ipxact:displayName>pma_cgb_scratch3_x1_clock_src</ipxact:displayName>
          <ipxact:value>not_used</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_select_done_master_or_slave" type="string">
          <ipxact:name>pma_cgb_select_done_master_or_slave</ipxact:name>
          <ipxact:displayName>pma_cgb_select_done_master_or_slave</ipxact:displayName>
          <ipxact:value>choose_slave_pcie_sw_done</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_ser_mode" type="string">
          <ipxact:name>pma_cgb_ser_mode</ipxact:name>
          <ipxact:displayName>pma_cgb_ser_mode</ipxact:displayName>
          <ipxact:value>thirty_two_bit</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_ser_powerdown" type="string">
          <ipxact:name>pma_cgb_ser_powerdown</ipxact:name>
          <ipxact:displayName>pma_cgb_ser_powerdown</ipxact:displayName>
          <ipxact:value>normal_poweron_ser</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_sup_mode" type="string">
          <ipxact:name>pma_cgb_sup_mode</ipxact:name>
          <ipxact:displayName>pma_cgb_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_tx_ucontrol_en" type="string">
          <ipxact:name>pma_cgb_tx_ucontrol_en</ipxact:name>
          <ipxact:displayName>pma_cgb_tx_ucontrol_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_tx_ucontrol_pcie" type="string">
          <ipxact:name>pma_cgb_tx_ucontrol_pcie</ipxact:name>
          <ipxact:displayName>pma_cgb_tx_ucontrol_pcie</ipxact:displayName>
          <ipxact:value>gen1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_tx_ucontrol_reset" type="string">
          <ipxact:name>pma_cgb_tx_ucontrol_reset</ipxact:name>
          <ipxact:displayName>pma_cgb_tx_ucontrol_reset</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_uc_cgb_vreg_boost" type="string">
          <ipxact:name>pma_cgb_uc_cgb_vreg_boost</ipxact:name>
          <ipxact:displayName>pma_cgb_uc_cgb_vreg_boost</ipxact:displayName>
          <ipxact:value>no_voltage_boost</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_uc_vcc_setting" type="string">
          <ipxact:name>pma_cgb_uc_vcc_setting</ipxact:name>
          <ipxact:displayName>pma_cgb_uc_vcc_setting</ipxact:displayName>
          <ipxact:value>vcc_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_vccdreg_output" type="string">
          <ipxact:name>pma_cgb_vccdreg_output</ipxact:name>
          <ipxact:displayName>pma_cgb_vccdreg_output</ipxact:displayName>
          <ipxact:value>vccdreg_nominal</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_vreg_sel_ref" type="string">
          <ipxact:name>pma_cgb_vreg_sel_ref</ipxact:name>
          <ipxact:displayName>pma_cgb_vreg_sel_ref</ipxact:displayName>
          <ipxact:value>sel_vccer_4ref</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_x1_clock_source_sel" type="string">
          <ipxact:name>pma_cgb_x1_clock_source_sel</ipxact:name>
          <ipxact:displayName>pma_cgb_x1_clock_source_sel</ipxact:displayName>
          <ipxact:value>lcpll_top</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_x1_div_m_sel" type="string">
          <ipxact:name>pma_cgb_x1_div_m_sel</ipxact:name>
          <ipxact:displayName>pma_cgb_x1_div_m_sel</ipxact:displayName>
          <ipxact:value>divbypass</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_xn_clock_source_sel" type="string">
          <ipxact:name>pma_cgb_xn_clock_source_sel</ipxact:name>
          <ipxact:displayName>pma_cgb_xn_clock_source_sel</ipxact:displayName>
          <ipxact:value>sel_cgb_loc</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_silicon_rev" type="string">
          <ipxact:name>pma_cgb_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_cgb_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_input_select_x1" type="string">
          <ipxact:name>pma_cgb_input_select_x1</ipxact:name>
          <ipxact:displayName>pma_cgb_input_select_x1</ipxact:displayName>
          <ipxact:value>fpll_bot</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_input_select_gen3" type="string">
          <ipxact:name>pma_cgb_input_select_gen3</ipxact:name>
          <ipxact:displayName>pma_cgb_input_select_gen3</ipxact:displayName>
          <ipxact:value>not_used</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cgb_input_select_xn" type="string">
          <ipxact:name>pma_cgb_input_select_xn</ipxact:name>
          <ipxact:displayName>pma_cgb_input_select_xn</ipxact:displayName>
          <ipxact:value>not_used</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_bonding_mode" type="string">
          <ipxact:name>pma_tx_ser_bonding_mode</ipxact:name>
          <ipxact:displayName>pma_tx_ser_bonding_mode</ipxact:displayName>
          <ipxact:value>bond_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_bti_protected" type="string">
          <ipxact:name>pma_tx_ser_bti_protected</ipxact:name>
          <ipxact:displayName>pma_tx_ser_bti_protected</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_clk_divtx_deskew" type="string">
          <ipxact:name>pma_tx_ser_clk_divtx_deskew</ipxact:name>
          <ipxact:displayName>pma_tx_ser_clk_divtx_deskew</ipxact:displayName>
          <ipxact:value>deskew_delay0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_control_clks_divtx_aibtx" type="string">
          <ipxact:name>pma_tx_ser_control_clks_divtx_aibtx</ipxact:name>
          <ipxact:displayName>pma_tx_ser_control_clks_divtx_aibtx</ipxact:displayName>
          <ipxact:value>no_dft_control_clkdivtx_clkaibtx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_datarate_bps" type="string">
          <ipxact:name>pma_tx_ser_datarate_bps</ipxact:name>
          <ipxact:displayName>pma_tx_ser_datarate_bps</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_duty_cycle_correction_mode_ctrl" type="string">
          <ipxact:name>pma_tx_ser_duty_cycle_correction_mode_ctrl</ipxact:name>
          <ipxact:displayName>pma_tx_ser_duty_cycle_correction_mode_ctrl</ipxact:displayName>
          <ipxact:value>dcc_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_xtx_path_xtx_idle_ctrl" type="string">
          <ipxact:name>pma_tx_ser_xtx_path_xtx_idle_ctrl</ipxact:name>
          <ipxact:displayName>pma_tx_ser_xtx_path_xtx_idle_ctrl</ipxact:displayName>
          <ipxact:value>id_cpen_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_initial_settings" type="string">
          <ipxact:name>pma_tx_ser_initial_settings</ipxact:name>
          <ipxact:displayName>pma_tx_ser_initial_settings</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_pcie_gen" type="string">
          <ipxact:name>pma_tx_ser_pcie_gen</ipxact:name>
          <ipxact:displayName>pma_tx_ser_pcie_gen</ipxact:displayName>
          <ipxact:value>non_pcie</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_power_rail_er" type="int">
          <ipxact:name>pma_tx_ser_power_rail_er</ipxact:name>
          <ipxact:displayName>pma_tx_ser_power_rail_er</ipxact:displayName>
          <ipxact:value>1030</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_powermode_ac_ser" type="string">
          <ipxact:name>pma_tx_ser_powermode_ac_ser</ipxact:name>
          <ipxact:displayName>pma_tx_ser_powermode_ac_ser</ipxact:displayName>
          <ipxact:value>ac_clk_divtx_user_0_jitcomp1p0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_powermode_dc_ser" type="string">
          <ipxact:name>pma_tx_ser_powermode_dc_ser</ipxact:name>
          <ipxact:displayName>pma_tx_ser_powermode_dc_ser</ipxact:displayName>
          <ipxact:value>dc_clk_divtx_user_0_jitcomp1p0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_prot_mode" type="string">
          <ipxact:name>pma_tx_ser_prot_mode</ipxact:name>
          <ipxact:displayName>pma_tx_ser_prot_mode</ipxact:displayName>
          <ipxact:value>basic_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_ser_clk_divtx_user_sel" type="string">
          <ipxact:name>pma_tx_ser_ser_clk_divtx_user_sel</ipxact:name>
          <ipxact:displayName>pma_tx_ser_ser_clk_divtx_user_sel</ipxact:displayName>
          <ipxact:value>divtx_user_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_ser_aibck_enable" type="string">
          <ipxact:name>pma_tx_ser_ser_aibck_enable</ipxact:name>
          <ipxact:displayName>pma_tx_ser_ser_aibck_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_ser_aibck_x1_override" type="string">
          <ipxact:name>pma_tx_ser_ser_aibck_x1_override</ipxact:name>
          <ipxact:displayName>pma_tx_ser_ser_aibck_x1_override</ipxact:displayName>
          <ipxact:value>normal</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_ser_clk_mon" type="string">
          <ipxact:name>pma_tx_ser_ser_clk_mon</ipxact:name>
          <ipxact:displayName>pma_tx_ser_ser_clk_mon</ipxact:displayName>
          <ipxact:value>disable_clk_mon</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_ser_dftppm_clkselect" type="string">
          <ipxact:name>pma_tx_ser_ser_dftppm_clkselect</ipxact:name>
          <ipxact:displayName>pma_tx_ser_ser_dftppm_clkselect</ipxact:displayName>
          <ipxact:value>aib_dftppm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_ser_in_jitcomp" type="string">
          <ipxact:name>pma_tx_ser_ser_in_jitcomp</ipxact:name>
          <ipxact:displayName>pma_tx_ser_ser_in_jitcomp</ipxact:displayName>
          <ipxact:value>jitcomp_on</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_ser_powerdown" type="string">
          <ipxact:name>pma_tx_ser_ser_powerdown</ipxact:name>
          <ipxact:displayName>pma_tx_ser_ser_powerdown</ipxact:displayName>
          <ipxact:value>normal_poweron_ser</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_ser_preset_bti_en" type="string">
          <ipxact:name>pma_tx_ser_ser_preset_bti_en</ipxact:name>
          <ipxact:displayName>pma_tx_ser_ser_preset_bti_en</ipxact:displayName>
          <ipxact:value>ser_preset_bti_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_sup_mode" type="string">
          <ipxact:name>pma_tx_ser_sup_mode</ipxact:name>
          <ipxact:displayName>pma_tx_ser_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_uc_vcc_setting" type="string">
          <ipxact:name>pma_tx_ser_uc_vcc_setting</ipxact:name>
          <ipxact:displayName>pma_tx_ser_uc_vcc_setting</ipxact:displayName>
          <ipxact:value>vcc_setting1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_silicon_rev" type="string">
          <ipxact:name>pma_tx_ser_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_tx_ser_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_ser_xtx_path_xchnseq_txpath_chnseq_idle_direct_on" type="string">
          <ipxact:name>pma_tx_ser_xtx_path_xchnseq_txpath_chnseq_idle_direct_on</ipxact:name>
          <ipxact:displayName>pma_tx_ser_xtx_path_xchnseq_txpath_chnseq_idle_direct_on</ipxact:displayName>
          <ipxact:value>cgb_idle_direct_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_reset_sequencer_rx_path_rstn_overrideb" type="string">
          <ipxact:name>pma_reset_sequencer_rx_path_rstn_overrideb</ipxact:name>
          <ipxact:displayName>pma_reset_sequencer_rx_path_rstn_overrideb</ipxact:displayName>
          <ipxact:value>use_sequencer</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_reset_sequencer_xrx_path_uc_cal_clk_bypass" type="string">
          <ipxact:name>pma_reset_sequencer_xrx_path_uc_cal_clk_bypass</ipxact:name>
          <ipxact:displayName>pma_reset_sequencer_xrx_path_uc_cal_clk_bypass</ipxact:displayName>
          <ipxact:value>cal_clk_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_reset_sequencer_xrx_path_uc_cal_enable" type="string">
          <ipxact:name>pma_reset_sequencer_xrx_path_uc_cal_enable</ipxact:name>
          <ipxact:displayName>pma_reset_sequencer_xrx_path_uc_cal_enable</ipxact:displayName>
          <ipxact:value>rx_cal_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_reset_sequencer_silicon_rev" type="string">
          <ipxact:name>pma_reset_sequencer_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_reset_sequencer_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_sequencer_tx_path_rstn_overrideb" type="string">
          <ipxact:name>pma_tx_sequencer_tx_path_rstn_overrideb</ipxact:name>
          <ipxact:displayName>pma_tx_sequencer_tx_path_rstn_overrideb</ipxact:displayName>
          <ipxact:value>use_sequencer</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_sequencer_xtx_path_xcgb_tx_ucontrol_en" type="string">
          <ipxact:name>pma_tx_sequencer_xtx_path_xcgb_tx_ucontrol_en</ipxact:name>
          <ipxact:displayName>pma_tx_sequencer_xtx_path_xcgb_tx_ucontrol_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_sequencer_xrx_path_uc_cal_clk_bypass" type="string">
          <ipxact:name>pma_tx_sequencer_xrx_path_uc_cal_clk_bypass</ipxact:name>
          <ipxact:displayName>pma_tx_sequencer_xrx_path_uc_cal_clk_bypass</ipxact:displayName>
          <ipxact:value>cal_clk_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_tx_sequencer_silicon_rev" type="string">
          <ipxact:name>pma_tx_sequencer_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_tx_sequencer_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_txpath_chnsequencer_pcie_gen" type="string">
          <ipxact:name>pma_txpath_chnsequencer_pcie_gen</ipxact:name>
          <ipxact:displayName>pma_txpath_chnsequencer_pcie_gen</ipxact:displayName>
          <ipxact:value>non_pcie</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_txpath_chnsequencer_prot_mode" type="string">
          <ipxact:name>pma_txpath_chnsequencer_prot_mode</ipxact:name>
          <ipxact:displayName>pma_txpath_chnsequencer_prot_mode</ipxact:displayName>
          <ipxact:value>basic_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_txpath_chnsequencer_sup_mode" type="string">
          <ipxact:name>pma_txpath_chnsequencer_sup_mode</ipxact:name>
          <ipxact:displayName>pma_txpath_chnsequencer_sup_mode</ipxact:displayName>
          <ipxact:value>sup_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_txpath_chnsequencer_txpath_chnseq_enable" type="string">
          <ipxact:name>pma_txpath_chnsequencer_txpath_chnseq_enable</ipxact:name>
          <ipxact:displayName>pma_txpath_chnsequencer_txpath_chnseq_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_txpath_chnsequencer_txpath_chnseq_idle_direct_on" type="string">
          <ipxact:name>pma_txpath_chnsequencer_txpath_chnseq_idle_direct_on</ipxact:name>
          <ipxact:displayName>pma_txpath_chnsequencer_txpath_chnseq_idle_direct_on</ipxact:displayName>
          <ipxact:value>cgb_idle_direct_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_txpath_chnsequencer_txpath_chnseq_stage_select" type="int">
          <ipxact:name>pma_txpath_chnsequencer_txpath_chnseq_stage_select</ipxact:name>
          <ipxact:displayName>pma_txpath_chnsequencer_txpath_chnseq_stage_select</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_txpath_chnsequencer_txpath_chnseq_wakeup_bypass" type="string">
          <ipxact:name>pma_txpath_chnsequencer_txpath_chnseq_wakeup_bypass</ipxact:name>
          <ipxact:displayName>pma_txpath_chnsequencer_txpath_chnseq_wakeup_bypass</ipxact:displayName>
          <ipxact:value>bypass_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_txpath_chnsequencer_silicon_rev" type="string">
          <ipxact:name>pma_txpath_chnsequencer_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_txpath_chnsequencer_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2ea</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_fifo_rx_pcs_double_read_mode" type="string">
          <ipxact:name>hssi_fifo_rx_pcs_double_read_mode</ipxact:name>
          <ipxact:displayName>hssi_fifo_rx_pcs_double_read_mode</ipxact:displayName>
          <ipxact:value>double_read_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_fifo_rx_pcs_prot_mode" type="string">
          <ipxact:name>hssi_fifo_rx_pcs_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_fifo_rx_pcs_prot_mode</ipxact:displayName>
          <ipxact:value>teng_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_fifo_rx_pcs_silicon_rev" type="string">
          <ipxact:name>hssi_fifo_rx_pcs_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_fifo_rx_pcs_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_fifo_tx_pcs_double_write_mode" type="string">
          <ipxact:name>hssi_fifo_tx_pcs_double_write_mode</ipxact:name>
          <ipxact:displayName>hssi_fifo_tx_pcs_double_write_mode</ipxact:displayName>
          <ipxact:value>double_write_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_fifo_tx_pcs_prot_mode" type="string">
          <ipxact:name>hssi_fifo_tx_pcs_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_fifo_tx_pcs_prot_mode</ipxact:displayName>
          <ipxact:value>teng_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_fifo_tx_pcs_silicon_rev" type="string">
          <ipxact:name>hssi_fifo_tx_pcs_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_fifo_tx_pcs_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_block_sync" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_block_sync</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_block_sync</ipxact:displayName>
          <ipxact:value>bypass_block_sync</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_block_sync_sm" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_block_sync_sm</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_block_sync_sm</ipxact:displayName>
          <ipxact:value>disable_blk_sync_sm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_cdr_ctrl_force_unalgn" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_cdr_ctrl_force_unalgn</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_cdr_ctrl_force_unalgn</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_lpbk_force" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_lpbk_force</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_lpbk_force</ipxact:displayName>
          <ipxact:value>lpbk_frce_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_mode" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_mode</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_mode</ipxact:displayName>
          <ipxact:value>disable_pcs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_rate_match_fifo" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_rate_match_fifo</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_rate_match_fifo</ipxact:displayName>
          <ipxact:value>bypass_rm_fifo</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_rate_match_fifo_latency" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_rate_match_fifo_latency</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_rate_match_fifo_latency</ipxact:displayName>
          <ipxact:value>low_latency</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_reverse_lpbk" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_reverse_lpbk</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_reverse_lpbk</ipxact:displayName>
          <ipxact:value>rev_lpbk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_rx_b4gb_par_lpbk" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_rx_b4gb_par_lpbk</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_rx_b4gb_par_lpbk</ipxact:displayName>
          <ipxact:value>b4gb_par_lpbk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_rx_force_balign" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_rx_force_balign</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_rx_force_balign</ipxact:displayName>
          <ipxact:value>dis_force_balign</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_rx_ins_del_one_skip" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_rx_ins_del_one_skip</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_rx_ins_del_one_skip</ipxact:displayName>
          <ipxact:value>ins_del_one_skip_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_rx_num_fixed_pat" type="int">
          <ipxact:name>hssi_gen3_rx_pcs_rx_num_fixed_pat</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_rx_num_fixed_pat</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_rx_test_out_sel" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_rx_test_out_sel</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_rx_test_out_sel</ipxact:displayName>
          <ipxact:value>rx_test_out0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_sup_mode" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_silicon_rev" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_rx_pcs_reconfig_settings" type="string">
          <ipxact:name>hssi_gen3_rx_pcs_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_gen3_rx_pcs_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_tx_pcs_mode" type="string">
          <ipxact:name>hssi_gen3_tx_pcs_mode</ipxact:name>
          <ipxact:displayName>hssi_gen3_tx_pcs_mode</ipxact:displayName>
          <ipxact:value>disable_pcs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_tx_pcs_reverse_lpbk" type="string">
          <ipxact:name>hssi_gen3_tx_pcs_reverse_lpbk</ipxact:name>
          <ipxact:displayName>hssi_gen3_tx_pcs_reverse_lpbk</ipxact:displayName>
          <ipxact:value>rev_lpbk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_tx_pcs_sup_mode" type="string">
          <ipxact:name>hssi_gen3_tx_pcs_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_gen3_tx_pcs_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_tx_pcs_tx_bitslip" type="int">
          <ipxact:name>hssi_gen3_tx_pcs_tx_bitslip</ipxact:name>
          <ipxact:displayName>hssi_gen3_tx_pcs_tx_bitslip</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_tx_pcs_tx_gbox_byp" type="string">
          <ipxact:name>hssi_gen3_tx_pcs_tx_gbox_byp</ipxact:name>
          <ipxact:displayName>hssi_gen3_tx_pcs_tx_gbox_byp</ipxact:displayName>
          <ipxact:value>bypass_gbox</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_tx_pcs_silicon_rev" type="string">
          <ipxact:name>hssi_gen3_tx_pcs_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_gen3_tx_pcs_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_gen3_tx_pcs_reconfig_settings" type="string">
          <ipxact:name>hssi_gen3_tx_pcs_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_gen3_tx_pcs_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_blksync_cor_en" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_blksync_cor_en</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_blksync_cor_en</ipxact:displayName>
          <ipxact:value>detect</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_bypass_gb" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_bypass_gb</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_bypass_gb</ipxact:displayName>
          <ipxact:value>bypass_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_clr_ctrl" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_clr_ctrl</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_clr_ctrl</ipxact:displayName>
          <ipxact:value>both_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_ctrl_bit_reverse" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_ctrl_bit_reverse</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_ctrl_bit_reverse</ipxact:displayName>
          <ipxact:value>ctrl_bit_reverse_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_data_bit_reverse" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_data_bit_reverse</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_data_bit_reverse</ipxact:displayName>
          <ipxact:value>data_bit_reverse_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_dv_start" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_dv_start</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_dv_start</ipxact:displayName>
          <ipxact:value>with_blklock</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_err_mark_type" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_err_mark_type</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_err_mark_type</ipxact:displayName>
          <ipxact:value>err_mark_10g</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_error_marking_en" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_error_marking_en</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_error_marking_en</ipxact:displayName>
          <ipxact:value>err_mark_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_low_latency_en" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_low_latency_en</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_low_latency_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_lpbk_mode" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_lpbk_mode</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_lpbk_mode</ipxact:displayName>
          <ipxact:value>lpbk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_parity_invalid_enum" type="int">
          <ipxact:name>hssi_krfec_rx_pcs_parity_invalid_enum</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_parity_invalid_enum</ipxact:displayName>
          <ipxact:value>8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_parity_valid_num" type="int">
          <ipxact:name>hssi_krfec_rx_pcs_parity_valid_num</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_parity_valid_num</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_pipeln_blksync" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_pipeln_blksync</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_pipeln_blksync</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_pipeln_descrm" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_pipeln_descrm</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_pipeln_descrm</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_pipeln_errcorrect" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_pipeln_errcorrect</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_pipeln_errcorrect</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_pipeln_errtrap_ind" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_pipeln_errtrap_ind</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_pipeln_errtrap_ind</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_pipeln_errtrap_lfsr" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_pipeln_errtrap_lfsr</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_pipeln_errtrap_lfsr</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_pipeln_errtrap_loc" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_pipeln_errtrap_loc</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_pipeln_errtrap_loc</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_pipeln_errtrap_pat" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_pipeln_errtrap_pat</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_pipeln_errtrap_pat</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_pipeln_gearbox" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_pipeln_gearbox</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_pipeln_gearbox</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_pipeln_syndrm" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_pipeln_syndrm</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_pipeln_syndrm</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_pipeln_trans_dec" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_pipeln_trans_dec</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_pipeln_trans_dec</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_prot_mode" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_prot_mode</ipxact:displayName>
          <ipxact:value>disable_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_receive_order" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_receive_order</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_receive_order</ipxact:displayName>
          <ipxact:value>receive_lsb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_rx_testbus_sel" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_rx_testbus_sel</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_rx_testbus_sel</ipxact:displayName>
          <ipxact:value>overall</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_signal_ok_en" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_signal_ok_en</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_signal_ok_en</ipxact:displayName>
          <ipxact:value>sig_ok_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_sup_mode" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_silicon_rev" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_rx_pcs_reconfig_settings" type="string">
          <ipxact:name>hssi_krfec_rx_pcs_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_krfec_rx_pcs_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_burst_err" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_burst_err</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_burst_err</ipxact:displayName>
          <ipxact:value>burst_err_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_burst_err_len" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_burst_err_len</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_burst_err_len</ipxact:displayName>
          <ipxact:value>burst_err_len1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_ctrl_bit_reverse" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_ctrl_bit_reverse</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_ctrl_bit_reverse</ipxact:displayName>
          <ipxact:value>ctrl_bit_reverse_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_data_bit_reverse" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_data_bit_reverse</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_data_bit_reverse</ipxact:displayName>
          <ipxact:value>data_bit_reverse_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_enc_frame_query" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_enc_frame_query</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_enc_frame_query</ipxact:displayName>
          <ipxact:value>enc_query_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_low_latency_en" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_low_latency_en</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_low_latency_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_pipeln_encoder" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_pipeln_encoder</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_pipeln_encoder</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_pipeln_scrambler" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_pipeln_scrambler</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_pipeln_scrambler</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_prot_mode" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_prot_mode</ipxact:displayName>
          <ipxact:value>disable_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_sup_mode" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_transcode_err" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_transcode_err</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_transcode_err</ipxact:displayName>
          <ipxact:value>trans_err_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_transmit_order" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_transmit_order</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_transmit_order</ipxact:displayName>
          <ipxact:value>transmit_lsb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_tx_testbus_sel" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_tx_testbus_sel</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_tx_testbus_sel</ipxact:displayName>
          <ipxact:value>overall</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_krfec_tx_pcs_silicon_rev" type="string">
          <ipxact:name>hssi_krfec_tx_pcs_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_krfec_tx_pcs_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_elec_idle_delay_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_elec_idle_delay_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_elec_idle_delay_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_error_replace_pad" type="string">
          <ipxact:name>hssi_pipe_gen1_2_error_replace_pad</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_error_replace_pad</ipxact:displayName>
          <ipxact:value>replace_edb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_hip_mode" type="string">
          <ipxact:name>hssi_pipe_gen1_2_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_hip_mode</ipxact:displayName>
          <ipxact:value>dis_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_ind_error_reporting" type="string">
          <ipxact:name>hssi_pipe_gen1_2_ind_error_reporting</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_ind_error_reporting</ipxact:displayName>
          <ipxact:value>dis_ind_error_reporting</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_phystatus_delay_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_phystatus_delay_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_phystatus_delay_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_phystatus_rst_toggle" type="string">
          <ipxact:name>hssi_pipe_gen1_2_phystatus_rst_toggle</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_phystatus_rst_toggle</ipxact:displayName>
          <ipxact:value>dis_phystatus_rst_toggle</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_pipe_byte_de_serializer_en" type="string">
          <ipxact:name>hssi_pipe_gen1_2_pipe_byte_de_serializer_en</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_pipe_byte_de_serializer_en</ipxact:displayName>
          <ipxact:value>dont_care_bds</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_prot_mode" type="string">
          <ipxact:name>hssi_pipe_gen1_2_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_prot_mode</ipxact:displayName>
          <ipxact:value>disabled_prot_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rpre_emph_a_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_rpre_emph_a_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rpre_emph_a_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rpre_emph_b_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_rpre_emph_b_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rpre_emph_b_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rpre_emph_c_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_rpre_emph_c_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rpre_emph_c_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rpre_emph_d_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_rpre_emph_d_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rpre_emph_d_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rpre_emph_e_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_rpre_emph_e_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rpre_emph_e_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rvod_sel_a_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_rvod_sel_a_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rvod_sel_a_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rvod_sel_b_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_rvod_sel_b_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rvod_sel_b_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rvod_sel_c_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_rvod_sel_c_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rvod_sel_c_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rvod_sel_d_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_rvod_sel_d_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rvod_sel_d_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rvod_sel_e_val" type="int">
          <ipxact:name>hssi_pipe_gen1_2_rvod_sel_e_val</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rvod_sel_e_val</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rx_pipe_enable" type="string">
          <ipxact:name>hssi_pipe_gen1_2_rx_pipe_enable</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rx_pipe_enable</ipxact:displayName>
          <ipxact:value>dis_pipe_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_rxdetect_bypass" type="string">
          <ipxact:name>hssi_pipe_gen1_2_rxdetect_bypass</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_rxdetect_bypass</ipxact:displayName>
          <ipxact:value>dis_rxdetect_bypass</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_sup_mode" type="string">
          <ipxact:name>hssi_pipe_gen1_2_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_tx_pipe_enable" type="string">
          <ipxact:name>hssi_pipe_gen1_2_tx_pipe_enable</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_tx_pipe_enable</ipxact:displayName>
          <ipxact:value>dis_pipe_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_txswing" type="string">
          <ipxact:name>hssi_pipe_gen1_2_txswing</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_txswing</ipxact:displayName>
          <ipxact:value>dis_txswing</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_silicon_rev" type="string">
          <ipxact:name>hssi_pipe_gen1_2_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen1_2_reconfig_settings" type="string">
          <ipxact:name>hssi_pipe_gen1_2_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen1_2_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_bypass_rx_detection_enable" type="string">
          <ipxact:name>hssi_pipe_gen3_bypass_rx_detection_enable</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_bypass_rx_detection_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_bypass_rx_preset" type="int">
          <ipxact:name>hssi_pipe_gen3_bypass_rx_preset</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_bypass_rx_preset</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_bypass_rx_preset_enable" type="string">
          <ipxact:name>hssi_pipe_gen3_bypass_rx_preset_enable</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_bypass_rx_preset_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_bypass_tx_coefficent" type="int">
          <ipxact:name>hssi_pipe_gen3_bypass_tx_coefficent</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_bypass_tx_coefficent</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_bypass_tx_coefficent_enable" type="string">
          <ipxact:name>hssi_pipe_gen3_bypass_tx_coefficent_enable</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_bypass_tx_coefficent_enable</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_elecidle_delay_g3" type="int">
          <ipxact:name>hssi_pipe_gen3_elecidle_delay_g3</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_elecidle_delay_g3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_ind_error_reporting" type="string">
          <ipxact:name>hssi_pipe_gen3_ind_error_reporting</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_ind_error_reporting</ipxact:displayName>
          <ipxact:value>dis_ind_error_reporting</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_mode" type="string">
          <ipxact:name>hssi_pipe_gen3_mode</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_mode</ipxact:displayName>
          <ipxact:value>disable_pcs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_phy_status_delay_g12" type="int">
          <ipxact:name>hssi_pipe_gen3_phy_status_delay_g12</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_phy_status_delay_g12</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_phy_status_delay_g3" type="int">
          <ipxact:name>hssi_pipe_gen3_phy_status_delay_g3</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_phy_status_delay_g3</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_phystatus_rst_toggle_g12" type="string">
          <ipxact:name>hssi_pipe_gen3_phystatus_rst_toggle_g12</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_phystatus_rst_toggle_g12</ipxact:displayName>
          <ipxact:value>dis_phystatus_rst_toggle</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_phystatus_rst_toggle_g3" type="string">
          <ipxact:name>hssi_pipe_gen3_phystatus_rst_toggle_g3</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_phystatus_rst_toggle_g3</ipxact:displayName>
          <ipxact:value>dis_phystatus_rst_toggle_g3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_rate_match_pad_insertion" type="string">
          <ipxact:name>hssi_pipe_gen3_rate_match_pad_insertion</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_rate_match_pad_insertion</ipxact:displayName>
          <ipxact:value>dis_rm_fifo_pad_ins</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_sup_mode" type="string">
          <ipxact:name>hssi_pipe_gen3_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_test_out_sel" type="string">
          <ipxact:name>hssi_pipe_gen3_test_out_sel</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_test_out_sel</ipxact:displayName>
          <ipxact:value>disable_test_out</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_silicon_rev" type="string">
          <ipxact:name>hssi_pipe_gen3_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pipe_gen3_reconfig_settings" type="string">
          <ipxact:name>hssi_pipe_gen3_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_pipe_gen3_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_aib_clk1_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_aib_clk1_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_aib_clk1_sel</ipxact:displayName>
          <ipxact:value>aib_clk1_pld_pcs_rx_clk_out</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_aib_clk2_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_aib_clk2_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_aib_clk2_sel</ipxact:displayName>
          <ipxact:value>aib_clk2_pld_pma_clkdiv_rx_user</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_aib_fabric_pld_pma_hclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_aib_fabric_pld_pma_hclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_aib_fabric_pld_pma_hclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_aib_fabric_rx_sr_clk_in_hz" type="int">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_aib_fabric_rx_sr_clk_in_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_aib_fabric_rx_sr_clk_in_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_aib_fabric_rx_transfer_clk_hz" type="int">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_aib_fabric_rx_transfer_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_aib_fabric_rx_transfer_clk_hz</ipxact:displayName>
          <ipxact:value>644531250</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_asn_bypass_pma_pcie_sw_done" type="string">
          <ipxact:name>hssi_pldadapt_rx_asn_bypass_pma_pcie_sw_done</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_asn_bypass_pma_pcie_sw_done</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_asn_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_asn_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_asn_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_asn_wait_for_dll_reset_cnt" type="int">
          <ipxact:name>hssi_pldadapt_rx_asn_wait_for_dll_reset_cnt</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_asn_wait_for_dll_reset_cnt</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_asn_wait_for_fifo_flush_cnt" type="int">
          <ipxact:name>hssi_pldadapt_rx_asn_wait_for_fifo_flush_cnt</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_asn_wait_for_fifo_flush_cnt</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_asn_wait_for_pma_pcie_sw_done_cnt" type="int">
          <ipxact:name>hssi_pldadapt_rx_asn_wait_for_pma_pcie_sw_done_cnt</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_asn_wait_for_pma_pcie_sw_done_cnt</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_bonding_dft_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_bonding_dft_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_bonding_dft_en</ipxact:displayName>
          <ipxact:value>dft_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_bonding_dft_val" type="string">
          <ipxact:name>hssi_pldadapt_rx_bonding_dft_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_bonding_dft_val</ipxact:displayName>
          <ipxact:value>dft_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_chnl_bonding" type="string">
          <ipxact:name>hssi_pldadapt_rx_chnl_bonding</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_chnl_bonding</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_clock_del_measure_enable" type="string">
          <ipxact:name>hssi_pldadapt_rx_clock_del_measure_enable</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_clock_del_measure_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_comp_cnt" type="int">
          <ipxact:name>hssi_pldadapt_rx_comp_cnt</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_comp_cnt</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_compin_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_compin_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_compin_sel</ipxact:displayName>
          <ipxact:value>compin_master</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_csr_clk_hz" type="int">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_csr_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_csr_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_ctrl_plane_bonding" type="string">
          <ipxact:name>hssi_pldadapt_rx_ctrl_plane_bonding</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_ctrl_plane_bonding</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_ds_bypass_pipeln" type="string">
          <ipxact:name>hssi_pldadapt_rx_ds_bypass_pipeln</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_ds_bypass_pipeln</ipxact:displayName>
          <ipxact:value>ds_bypass_pipeln_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_ds_last_chnl" type="string">
          <ipxact:name>hssi_pldadapt_rx_ds_last_chnl</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_ds_last_chnl</ipxact:displayName>
          <ipxact:value>ds_last_chnl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_ds_master" type="string">
          <ipxact:name>hssi_pldadapt_rx_ds_master</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_ds_master</ipxact:displayName>
          <ipxact:value>ds_master_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_duplex_mode" type="string">
          <ipxact:name>hssi_pldadapt_rx_duplex_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_duplex_mode</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_dv_mode" type="string">
          <ipxact:name>hssi_pldadapt_rx_dv_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_dv_mode</ipxact:displayName>
          <ipxact:value>dv_mode_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fifo_double_read" type="string">
          <ipxact:name>hssi_pldadapt_rx_fifo_double_read</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fifo_double_read</ipxact:displayName>
          <ipxact:value>fifo_double_read_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fifo_mode" type="string">
          <ipxact:name>hssi_pldadapt_rx_fifo_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fifo_mode</ipxact:displayName>
          <ipxact:value>phase_comp</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fifo_rd_clk_ins_sm_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_fifo_rd_clk_ins_sm_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fifo_rd_clk_ins_sm_scg_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fifo_rd_clk_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_fifo_rd_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fifo_rd_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fifo_rd_clk_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_fifo_rd_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fifo_rd_clk_sel</ipxact:displayName>
          <ipxact:value>fifo_rd_clk_pld_rx_clk1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fifo_stop_rd" type="string">
          <ipxact:name>hssi_pldadapt_rx_fifo_stop_rd</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fifo_stop_rd</ipxact:displayName>
          <ipxact:value>rd_empty</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fifo_stop_wr" type="string">
          <ipxact:name>hssi_pldadapt_rx_fifo_stop_wr</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fifo_stop_wr</ipxact:displayName>
          <ipxact:value>n_wr_full</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fifo_width" type="string">
          <ipxact:name>hssi_pldadapt_rx_fifo_width</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fifo_width</ipxact:displayName>
          <ipxact:value>fifo_double_width</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fifo_wr_clk_del_sm_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_fifo_wr_clk_del_sm_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fifo_wr_clk_del_sm_scg_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fifo_wr_clk_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_fifo_wr_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fifo_wr_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fifo_wr_clk_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_fifo_wr_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fifo_wr_clk_sel</ipxact:displayName>
          <ipxact:value>fifo_wr_clk_rx_transfer_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_free_run_div_clk" type="string">
          <ipxact:name>hssi_pldadapt_rx_free_run_div_clk</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_free_run_div_clk</ipxact:displayName>
          <ipxact:value>out_of_reset_sync</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fsr_pld_10g_rx_crc32_err_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_rx_fsr_pld_10g_rx_crc32_err_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fsr_pld_10g_rx_crc32_err_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_crc32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fsr_pld_8g_sigdet_out_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_rx_fsr_pld_8g_sigdet_out_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fsr_pld_8g_sigdet_out_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_sigdet</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fsr_pld_ltd_b_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_rx_fsr_pld_ltd_b_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fsr_pld_ltd_b_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_ltdb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fsr_pld_ltr_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_rx_fsr_pld_ltr_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fsr_pld_ltr_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_ltr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_fsr_pld_rx_fifo_align_clr_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_rx_fsr_pld_rx_fifo_align_clr_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_fsr_pld_rx_fifo_align_clr_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_alignclr</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_gb_rx_idwidth" type="string">
          <ipxact:name>hssi_pldadapt_rx_gb_rx_idwidth</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_gb_rx_idwidth</ipxact:displayName>
          <ipxact:value>idwidth_32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_gb_rx_odwidth" type="string">
          <ipxact:name>hssi_pldadapt_rx_gb_rx_odwidth</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_gb_rx_odwidth</ipxact:displayName>
          <ipxact:value>odwidth_66</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hip_mode" type="string">
          <ipxact:name>hssi_pldadapt_rx_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hip_mode</ipxact:displayName>
          <ipxact:value>disable_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hrdrst_align_bypass" type="string">
          <ipxact:name>hssi_pldadapt_rx_hrdrst_align_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hrdrst_align_bypass</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hrdrst_dll_lock_bypass" type="string">
          <ipxact:name>hssi_pldadapt_rx_hrdrst_dll_lock_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hrdrst_dll_lock_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hrdrst_rst_sm_dis" type="string">
          <ipxact:name>hssi_pldadapt_rx_hrdrst_rst_sm_dis</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hrdrst_rst_sm_dis</ipxact:displayName>
          <ipxact:value>enable_rx_rst_sm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hrdrst_rx_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_hrdrst_rx_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hrdrst_rx_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hrdrst_user_ctl_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_hrdrst_user_ctl_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hrdrst_user_ctl_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_indv" type="string">
          <ipxact:name>hssi_pldadapt_rx_indv</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_indv</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_internal_clk1_sel1" type="string">
          <ipxact:name>hssi_pldadapt_rx_internal_clk1_sel1</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_internal_clk1_sel1</ipxact:displayName>
          <ipxact:value>pma_clks_or_txfiford_post_ct_mux_clk1_mux1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_internal_clk1_sel2" type="string">
          <ipxact:name>hssi_pldadapt_rx_internal_clk1_sel2</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_internal_clk1_sel2</ipxact:displayName>
          <ipxact:value>pma_clks_clk1_mux2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_internal_clk2_sel1" type="string">
          <ipxact:name>hssi_pldadapt_rx_internal_clk2_sel1</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_internal_clk2_sel1</ipxact:displayName>
          <ipxact:value>pma_clks_or_rxfifowr_post_ct_mux_clk2_mux1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_internal_clk2_sel2" type="string">
          <ipxact:name>hssi_pldadapt_rx_internal_clk2_sel2</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_internal_clk2_sel2</ipxact:displayName>
          <ipxact:value>pma_clks_clk2_mux2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_loopback_mode" type="string">
          <ipxact:name>hssi_pldadapt_rx_loopback_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_loopback_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_low_latency_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_low_latency_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_low_latency_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_lpbk_mode" type="string">
          <ipxact:name>hssi_pldadapt_rx_lpbk_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_lpbk_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_phcomp_rd_del" type="string">
          <ipxact:name>hssi_pldadapt_rx_phcomp_rd_del</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_phcomp_rd_del</ipxact:displayName>
          <ipxact:value>phcomp_rd_del2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_pipe_enable" type="string">
          <ipxact:name>hssi_pldadapt_rx_pipe_enable</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_pipe_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_pipe_mode" type="string">
          <ipxact:name>hssi_pldadapt_rx_pipe_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_pipe_mode</ipxact:displayName>
          <ipxact:value>disable_pipe</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_pld_avmm1_clk_rowclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_pld_avmm1_clk_rowclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_pld_avmm1_clk_rowclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_pld_avmm2_clk_rowclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_pld_avmm2_clk_rowclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_pld_avmm2_clk_rowclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_pld_clk1_delay_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_pld_clk1_delay_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_pld_clk1_delay_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_pld_clk1_delay_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_pld_clk1_delay_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_pld_clk1_delay_sel</ipxact:displayName>
          <ipxact:value>delay_path13</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_pld_clk1_inv_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_pld_clk1_inv_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_pld_clk1_inv_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_pld_clk1_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_pld_clk1_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_pld_clk1_sel</ipxact:displayName>
          <ipxact:value>pld_clk1_dcm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_pld_rx_clk1_dcm_hz" type="int">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_pld_rx_clk1_dcm_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_pld_rx_clk1_dcm_hz</ipxact:displayName>
          <ipxact:value>156250000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_pld_rx_clk1_rowclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_pld_rx_clk1_rowclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_pld_rx_clk1_rowclk_hz</ipxact:displayName>
          <ipxact:value>156250000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_pld_sclk1_rowclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_pld_sclk1_rowclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_pld_sclk1_rowclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_pld_sclk2_rowclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_pld_sclk2_rowclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_pld_sclk2_rowclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_pma_hclk_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_rx_pma_hclk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_pma_hclk_scg_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_powerdown_mode" type="string">
          <ipxact:name>hssi_pldadapt_rx_powerdown_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_powerdown_mode</ipxact:displayName>
          <ipxact:value>powerup</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_powermode_dc" type="string">
          <ipxact:name>hssi_pldadapt_rx_powermode_dc</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_powermode_dc</ipxact:displayName>
          <ipxact:value>powerdown</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_datapath_tb_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_datapath_tb_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_datapath_tb_sel</ipxact:displayName>
          <ipxact:value>cp_bond</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_fastbond_rden" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_fastbond_rden</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_fastbond_rden</ipxact:displayName>
          <ipxact:value>rden_ds_fast_us_fast</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_fastbond_wren" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_fastbond_wren</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_fastbond_wren</ipxact:displayName>
          <ipxact:value>wren_ds_del_us_del</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_fifo_power_mode" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_fifo_power_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_fifo_power_mode</ipxact:displayName>
          <ipxact:value>full_width_ps_dw</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_fifo_read_latency_adjust" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_fifo_read_latency_adjust</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_fifo_read_latency_adjust</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_fifo_write_ctrl" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_fifo_write_ctrl</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_fifo_write_ctrl</ipxact:displayName>
          <ipxact:value>blklock_ignore</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_fifo_write_latency_adjust" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_fifo_write_latency_adjust</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_fifo_write_latency_adjust</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_osc_clock_setting" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_osc_clock_setting</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_osc_clock_setting</ipxact:displayName>
          <ipxact:value>osc_clk_div_by1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_pld_8g_eidleinfersel_polling_bypass" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_pld_8g_eidleinfersel_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_pld_8g_eidleinfersel_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_pld_pma_eye_monitor_polling_bypass" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_pld_pma_eye_monitor_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_pld_pma_eye_monitor_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_pld_pma_pcie_switch_polling_bypass" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_pld_pma_pcie_switch_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_pld_pma_pcie_switch_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_pld_pma_reser_out_polling_bypass" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_pld_pma_reser_out_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_pld_pma_reser_out_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_prbs_flags_sr_enable" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_prbs_flags_sr_enable</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_prbs_flags_sr_enable</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_true_b2b" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_true_b2b</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_true_b2b</ipxact:displayName>
          <ipxact:value>b2b</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rx_usertest_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_rx_usertest_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rx_usertest_sel</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rxfifo_empty" type="string">
          <ipxact:name>hssi_pldadapt_rx_rxfifo_empty</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rxfifo_empty</ipxact:displayName>
          <ipxact:value>empty_dw</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rxfifo_full" type="string">
          <ipxact:name>hssi_pldadapt_rx_rxfifo_full</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rxfifo_full</ipxact:displayName>
          <ipxact:value>full_pc_dw</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rxfifo_mode" type="string">
          <ipxact:name>hssi_pldadapt_rx_rxfifo_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rxfifo_mode</ipxact:displayName>
          <ipxact:value>rxphase_comp</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rxfifo_pempty" type="int">
          <ipxact:name>hssi_pldadapt_rx_rxfifo_pempty</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rxfifo_pempty</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rxfifo_pfull" type="int">
          <ipxact:name>hssi_pldadapt_rx_rxfifo_pfull</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rxfifo_pfull</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rxfiford_post_ct_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_rxfiford_post_ct_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rxfiford_post_ct_sel</ipxact:displayName>
          <ipxact:value>rxfiford_sclk_post_ct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_rxfifowr_post_ct_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_rxfifowr_post_ct_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_rxfifowr_post_ct_sel</ipxact:displayName>
          <ipxact:value>rxfifowr_sclk_post_ct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_sclk_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_sclk_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_sclk_sel</ipxact:displayName>
          <ipxact:value>sclk1_rowclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_speed_grade" type="string">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_speed_grade</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_speed_grade</ipxact:displayName>
          <ipxact:value>dash_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_hdpldadapt_sr_sr_testbus_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_hdpldadapt_sr_sr_testbus_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_hdpldadapt_sr_sr_testbus_sel</ipxact:displayName>
          <ipxact:value>ssr_testbus</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_stretch_num_stages" type="string">
          <ipxact:name>hssi_pldadapt_rx_stretch_num_stages</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_stretch_num_stages</ipxact:displayName>
          <ipxact:value>four_stage</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_sup_mode" type="string">
          <ipxact:name>hssi_pldadapt_rx_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_txfiford_post_ct_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_txfiford_post_ct_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_txfiford_post_ct_sel</ipxact:displayName>
          <ipxact:value>txfiford_sclk_post_ct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_txfifowr_post_ct_sel" type="string">
          <ipxact:name>hssi_pldadapt_rx_txfifowr_post_ct_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_txfifowr_post_ct_sel</ipxact:displayName>
          <ipxact:value>txfifowr_sclk_post_ct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_us_bypass_pipeln" type="string">
          <ipxact:name>hssi_pldadapt_rx_us_bypass_pipeln</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_us_bypass_pipeln</ipxact:displayName>
          <ipxact:value>us_bypass_pipeln_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_us_last_chnl" type="string">
          <ipxact:name>hssi_pldadapt_rx_us_last_chnl</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_us_last_chnl</ipxact:displayName>
          <ipxact:value>us_last_chnl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_us_master" type="string">
          <ipxact:name>hssi_pldadapt_rx_us_master</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_us_master</ipxact:displayName>
          <ipxact:value>us_master_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_word_align" type="string">
          <ipxact:name>hssi_pldadapt_rx_word_align</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_word_align</ipxact:displayName>
          <ipxact:value>wa_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_word_align_enable" type="string">
          <ipxact:name>hssi_pldadapt_rx_word_align_enable</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_word_align_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_silicon_rev" type="string">
          <ipxact:name>hssi_pldadapt_rx_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_rx_reconfig_settings" type="string">
          <ipxact:name>hssi_pldadapt_rx_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_rx_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_aib_clk1_sel" type="string">
          <ipxact:name>hssi_pldadapt_tx_aib_clk1_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_aib_clk1_sel</ipxact:displayName>
          <ipxact:value>aib_clk1_pld_pcs_tx_clk_out</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_aib_clk2_sel" type="string">
          <ipxact:name>hssi_pldadapt_tx_aib_clk2_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_aib_clk2_sel</ipxact:displayName>
          <ipxact:value>aib_clk2_pld_pcs_tx_clk_out</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_aib_fabric_pld_pma_hclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_aib_fabric_pld_pma_hclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_aib_fabric_pld_pma_hclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_aib_fabric_pma_aib_tx_clk_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_aib_fabric_pma_aib_tx_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_aib_fabric_pma_aib_tx_clk_hz</ipxact:displayName>
          <ipxact:value>644531250</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_aib_fabric_tx_sr_clk_in_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_aib_fabric_tx_sr_clk_in_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_aib_fabric_tx_sr_clk_in_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_bonding_dft_en" type="string">
          <ipxact:name>hssi_pldadapt_tx_bonding_dft_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_bonding_dft_en</ipxact:displayName>
          <ipxact:value>dft_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_bonding_dft_val" type="string">
          <ipxact:name>hssi_pldadapt_tx_bonding_dft_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_bonding_dft_val</ipxact:displayName>
          <ipxact:value>dft_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_chnl_bonding" type="string">
          <ipxact:name>hssi_pldadapt_tx_chnl_bonding</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_chnl_bonding</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_comp_cnt" type="int">
          <ipxact:name>hssi_pldadapt_tx_comp_cnt</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_comp_cnt</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_compin_sel" type="string">
          <ipxact:name>hssi_pldadapt_tx_compin_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_compin_sel</ipxact:displayName>
          <ipxact:value>compin_master</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_csr_clk_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_csr_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_csr_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_ctrl_plane_bonding" type="string">
          <ipxact:name>hssi_pldadapt_tx_ctrl_plane_bonding</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_ctrl_plane_bonding</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_ds_bypass_pipeln" type="string">
          <ipxact:name>hssi_pldadapt_tx_ds_bypass_pipeln</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_ds_bypass_pipeln</ipxact:displayName>
          <ipxact:value>ds_bypass_pipeln_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_ds_last_chnl" type="string">
          <ipxact:name>hssi_pldadapt_tx_ds_last_chnl</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_ds_last_chnl</ipxact:displayName>
          <ipxact:value>ds_last_chnl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_ds_master" type="string">
          <ipxact:name>hssi_pldadapt_tx_ds_master</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_ds_master</ipxact:displayName>
          <ipxact:value>ds_master_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_duplex_mode" type="string">
          <ipxact:name>hssi_pldadapt_tx_duplex_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_duplex_mode</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_dv_bond" type="string">
          <ipxact:name>hssi_pldadapt_tx_dv_bond</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_dv_bond</ipxact:displayName>
          <ipxact:value>dv_bond_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_dv_gen" type="string">
          <ipxact:name>hssi_pldadapt_tx_dv_gen</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_dv_gen</ipxact:displayName>
          <ipxact:value>dv_gen_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fifo_double_write" type="string">
          <ipxact:name>hssi_pldadapt_tx_fifo_double_write</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fifo_double_write</ipxact:displayName>
          <ipxact:value>fifo_double_write_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fifo_mode" type="string">
          <ipxact:name>hssi_pldadapt_tx_fifo_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fifo_mode</ipxact:displayName>
          <ipxact:value>phase_comp</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fifo_rd_clk_frm_gen_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_tx_fifo_rd_clk_frm_gen_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fifo_rd_clk_frm_gen_scg_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fifo_rd_clk_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_tx_fifo_rd_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fifo_rd_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fifo_rd_clk_sel" type="string">
          <ipxact:name>hssi_pldadapt_tx_fifo_rd_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fifo_rd_clk_sel</ipxact:displayName>
          <ipxact:value>fifo_rd_pma_aib_tx_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fifo_stop_rd" type="string">
          <ipxact:name>hssi_pldadapt_tx_fifo_stop_rd</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fifo_stop_rd</ipxact:displayName>
          <ipxact:value>rd_empty</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fifo_stop_wr" type="string">
          <ipxact:name>hssi_pldadapt_tx_fifo_stop_wr</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fifo_stop_wr</ipxact:displayName>
          <ipxact:value>wr_full</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fifo_width" type="string">
          <ipxact:name>hssi_pldadapt_tx_fifo_width</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fifo_width</ipxact:displayName>
          <ipxact:value>fifo_double_width</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fifo_wr_clk_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_tx_fifo_wr_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fifo_wr_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fpll_shared_direct_async_in_sel" type="string">
          <ipxact:name>hssi_pldadapt_tx_fpll_shared_direct_async_in_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fpll_shared_direct_async_in_sel</ipxact:displayName>
          <ipxact:value>fpll_shared_direct_async_in_rowclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_frmgen_burst" type="string">
          <ipxact:name>hssi_pldadapt_tx_frmgen_burst</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_frmgen_burst</ipxact:displayName>
          <ipxact:value>frmgen_burst_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_frmgen_bypass" type="string">
          <ipxact:name>hssi_pldadapt_tx_frmgen_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_frmgen_bypass</ipxact:displayName>
          <ipxact:value>frmgen_bypass_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_frmgen_mfrm_length" type="int">
          <ipxact:name>hssi_pldadapt_tx_frmgen_mfrm_length</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_frmgen_mfrm_length</ipxact:displayName>
          <ipxact:value>2048</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_frmgen_pipeln" type="string">
          <ipxact:name>hssi_pldadapt_tx_frmgen_pipeln</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_frmgen_pipeln</ipxact:displayName>
          <ipxact:value>frmgen_pipeln_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_frmgen_pyld_ins" type="string">
          <ipxact:name>hssi_pldadapt_tx_frmgen_pyld_ins</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_frmgen_pyld_ins</ipxact:displayName>
          <ipxact:value>frmgen_pyld_ins_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_frmgen_wordslip" type="string">
          <ipxact:name>hssi_pldadapt_tx_frmgen_wordslip</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_frmgen_wordslip</ipxact:displayName>
          <ipxact:value>frmgen_wordslip_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fsr_hip_fsr_in_bit0_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_tx_fsr_hip_fsr_in_bit0_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fsr_hip_fsr_in_bit0_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_hfsrin0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fsr_hip_fsr_in_bit1_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_tx_fsr_hip_fsr_in_bit1_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fsr_hip_fsr_in_bit1_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_hfsrin1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fsr_hip_fsr_in_bit2_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_tx_fsr_hip_fsr_in_bit2_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fsr_hip_fsr_in_bit2_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_hfsrin2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fsr_hip_fsr_in_bit3_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_tx_fsr_hip_fsr_in_bit3_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fsr_hip_fsr_in_bit3_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_hfsrin3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fsr_hip_fsr_out_bit0_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_tx_fsr_hip_fsr_out_bit0_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fsr_hip_fsr_out_bit0_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_hfsrout0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fsr_hip_fsr_out_bit1_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_tx_fsr_hip_fsr_out_bit1_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fsr_hip_fsr_out_bit1_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_one_hfsrout1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fsr_hip_fsr_out_bit2_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_tx_fsr_hip_fsr_out_bit2_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fsr_hip_fsr_out_bit2_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_hfsrout2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fsr_hip_fsr_out_bit3_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_tx_fsr_hip_fsr_out_bit3_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fsr_hip_fsr_out_bit3_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_hfsrout3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fsr_mask_tx_pll_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_tx_fsr_mask_tx_pll_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fsr_mask_tx_pll_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_maskpll</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_fsr_pld_txelecidle_rst_val" type="string">
          <ipxact:name>hssi_pldadapt_tx_fsr_pld_txelecidle_rst_val</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_fsr_pld_txelecidle_rst_val</ipxact:displayName>
          <ipxact:value>reset_to_zero_txelec</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_gb_tx_idwidth" type="string">
          <ipxact:name>hssi_pldadapt_tx_gb_tx_idwidth</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_gb_tx_idwidth</ipxact:displayName>
          <ipxact:value>idwidth_66</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_gb_tx_odwidth" type="string">
          <ipxact:name>hssi_pldadapt_tx_gb_tx_odwidth</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_gb_tx_odwidth</ipxact:displayName>
          <ipxact:value>odwidth_32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hip_mode" type="string">
          <ipxact:name>hssi_pldadapt_tx_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hip_mode</ipxact:displayName>
          <ipxact:value>disable_hip</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hip_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_tx_hip_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hip_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hrdrst_dcd_cal_done_bypass" type="string">
          <ipxact:name>hssi_pldadapt_tx_hrdrst_dcd_cal_done_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hrdrst_dcd_cal_done_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hrdrst_rst_sm_dis" type="string">
          <ipxact:name>hssi_pldadapt_tx_hrdrst_rst_sm_dis</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hrdrst_rst_sm_dis</ipxact:displayName>
          <ipxact:value>enable_tx_rst_sm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hrdrst_rx_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_tx_hrdrst_rx_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hrdrst_rx_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hrdrst_user_ctl_en" type="string">
          <ipxact:name>hssi_pldadapt_tx_hrdrst_user_ctl_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hrdrst_user_ctl_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_indv" type="string">
          <ipxact:name>hssi_pldadapt_tx_indv</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_indv</ipxact:displayName>
          <ipxact:value>indv_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_loopback_mode" type="string">
          <ipxact:name>hssi_pldadapt_tx_loopback_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_loopback_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_low_latency_en" type="string">
          <ipxact:name>hssi_pldadapt_tx_low_latency_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_low_latency_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_osc_clk_scg_en" type="string">
          <ipxact:name>hssi_pldadapt_tx_osc_clk_scg_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_osc_clk_scg_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_phcomp_rd_del" type="string">
          <ipxact:name>hssi_pldadapt_tx_phcomp_rd_del</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_phcomp_rd_del</ipxact:displayName>
          <ipxact:value>phcomp_rd_del3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_pipe_mode" type="string">
          <ipxact:name>hssi_pldadapt_tx_pipe_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_pipe_mode</ipxact:displayName>
          <ipxact:value>disable_pipe</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_pld_avmm1_clk_rowclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_pld_avmm1_clk_rowclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_pld_avmm1_clk_rowclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_pld_avmm2_clk_rowclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_pld_avmm2_clk_rowclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_pld_avmm2_clk_rowclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_pld_clk1_delay_en" type="string">
          <ipxact:name>hssi_pldadapt_tx_pld_clk1_delay_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_pld_clk1_delay_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_pld_clk1_delay_sel" type="string">
          <ipxact:name>hssi_pldadapt_tx_pld_clk1_delay_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_pld_clk1_delay_sel</ipxact:displayName>
          <ipxact:value>delay_path15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_pld_clk1_inv_en" type="string">
          <ipxact:name>hssi_pldadapt_tx_pld_clk1_inv_en</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_pld_clk1_inv_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_pld_clk1_sel" type="string">
          <ipxact:name>hssi_pldadapt_tx_pld_clk1_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_pld_clk1_sel</ipxact:displayName>
          <ipxact:value>pld_clk1_dcm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_pld_clk2_sel" type="string">
          <ipxact:name>hssi_pldadapt_tx_pld_clk2_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_pld_clk2_sel</ipxact:displayName>
          <ipxact:value>pld_clk2_dcm</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_pld_sclk1_rowclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_pld_sclk1_rowclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_pld_sclk1_rowclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_pld_sclk2_rowclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_pld_sclk2_rowclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_pld_sclk2_rowclk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_pld_tx_clk1_dcm_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_pld_tx_clk1_dcm_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_pld_tx_clk1_dcm_hz</ipxact:displayName>
          <ipxact:value>156250000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_pld_tx_clk1_rowclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_pld_tx_clk1_rowclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_pld_tx_clk1_rowclk_hz</ipxact:displayName>
          <ipxact:value>156250000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_pld_tx_clk2_dcm_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_pld_tx_clk2_dcm_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_pld_tx_clk2_dcm_hz</ipxact:displayName>
          <ipxact:value>644531250</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_pld_tx_clk2_rowclk_hz" type="int">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_pld_tx_clk2_rowclk_hz</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_pld_tx_clk2_rowclk_hz</ipxact:displayName>
          <ipxact:value>644531250</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_pma_aib_tx_clk_expected_setting" type="string">
          <ipxact:name>hssi_pldadapt_tx_pma_aib_tx_clk_expected_setting</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_pma_aib_tx_clk_expected_setting</ipxact:displayName>
          <ipxact:value>x2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_powerdown_mode" type="string">
          <ipxact:name>hssi_pldadapt_tx_powerdown_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_powerdown_mode</ipxact:displayName>
          <ipxact:value>powerup</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_powermode_dc" type="string">
          <ipxact:name>hssi_pldadapt_tx_powermode_dc</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_powermode_dc</ipxact:displayName>
          <ipxact:value>powerdown</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_sh_err" type="string">
          <ipxact:name>hssi_pldadapt_tx_sh_err</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_sh_err</ipxact:displayName>
          <ipxact:value>sh_err_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_speed_grade" type="string">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_speed_grade</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_speed_grade</ipxact:displayName>
          <ipxact:value>dash_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_hdpldadapt_sr_sr_testbus_sel" type="string">
          <ipxact:name>hssi_pldadapt_tx_hdpldadapt_sr_sr_testbus_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_hdpldadapt_sr_sr_testbus_sel</ipxact:displayName>
          <ipxact:value>ssr_testbus</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_stretch_num_stages" type="string">
          <ipxact:name>hssi_pldadapt_tx_stretch_num_stages</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_stretch_num_stages</ipxact:displayName>
          <ipxact:value>four_stage</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_sup_mode" type="string">
          <ipxact:name>hssi_pldadapt_tx_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_datapath_tb_sel" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_datapath_tb_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_datapath_tb_sel</ipxact:displayName>
          <ipxact:value>cp_bond</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_fastbond_rden" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_fastbond_rden</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_fastbond_rden</ipxact:displayName>
          <ipxact:value>rden_ds_fast_us_fast</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_fastbond_wren" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_fastbond_wren</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_fastbond_wren</ipxact:displayName>
          <ipxact:value>wren_ds_fast_us_fast</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_fifo_power_mode" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_fifo_power_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_fifo_power_mode</ipxact:displayName>
          <ipxact:value>full_width_ps_dw</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_fifo_read_latency_adjust" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_fifo_read_latency_adjust</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_fifo_read_latency_adjust</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_fifo_write_latency_adjust" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_fifo_write_latency_adjust</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_fifo_write_latency_adjust</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_hip_aib_ssr_in_polling_bypass" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_hip_aib_ssr_in_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_hip_aib_ssr_in_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_osc_clock_setting" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_osc_clock_setting</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_osc_clock_setting</ipxact:displayName>
          <ipxact:value>osc_clk_div_by1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_pld_10g_tx_bitslip_polling_bypass" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_pld_10g_tx_bitslip_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_pld_10g_tx_bitslip_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_pld_8g_tx_boundary_sel_polling_bypass" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_pld_8g_tx_boundary_sel_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_pld_8g_tx_boundary_sel_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_pld_pma_fpll_cnt_sel_polling_bypass" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_pld_pma_fpll_cnt_sel_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_pld_pma_fpll_cnt_sel_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_pld_pma_fpll_num_phase_shifts_polling_bypass" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_pld_pma_fpll_num_phase_shifts_polling_bypass</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_pld_pma_fpll_num_phase_shifts_polling_bypass</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_tx_usertest_sel" type="string">
          <ipxact:name>hssi_pldadapt_tx_tx_usertest_sel</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_tx_usertest_sel</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_txfifo_empty" type="string">
          <ipxact:name>hssi_pldadapt_tx_txfifo_empty</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_txfifo_empty</ipxact:displayName>
          <ipxact:value>empty_default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_txfifo_full" type="string">
          <ipxact:name>hssi_pldadapt_tx_txfifo_full</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_txfifo_full</ipxact:displayName>
          <ipxact:value>full_pc_dw</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_txfifo_mode" type="string">
          <ipxact:name>hssi_pldadapt_tx_txfifo_mode</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_txfifo_mode</ipxact:displayName>
          <ipxact:value>txphase_comp</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_txfifo_pempty" type="int">
          <ipxact:name>hssi_pldadapt_tx_txfifo_pempty</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_txfifo_pempty</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_txfifo_pfull" type="int">
          <ipxact:name>hssi_pldadapt_tx_txfifo_pfull</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_txfifo_pfull</ipxact:displayName>
          <ipxact:value>10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_us_bypass_pipeln" type="string">
          <ipxact:name>hssi_pldadapt_tx_us_bypass_pipeln</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_us_bypass_pipeln</ipxact:displayName>
          <ipxact:value>us_bypass_pipeln_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_us_last_chnl" type="string">
          <ipxact:name>hssi_pldadapt_tx_us_last_chnl</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_us_last_chnl</ipxact:displayName>
          <ipxact:value>us_last_chnl</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_us_master" type="string">
          <ipxact:name>hssi_pldadapt_tx_us_master</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_us_master</ipxact:displayName>
          <ipxact:value>us_master_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_word_align_enable" type="string">
          <ipxact:name>hssi_pldadapt_tx_word_align_enable</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_word_align_enable</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_word_mark" type="string">
          <ipxact:name>hssi_pldadapt_tx_word_mark</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_word_mark</ipxact:displayName>
          <ipxact:value>wm_en</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_silicon_rev" type="string">
          <ipxact:name>hssi_pldadapt_tx_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_pldadapt_tx_reconfig_settings" type="string">
          <ipxact:name>hssi_pldadapt_tx_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_pldadapt_tx_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch0_src" type="string">
          <ipxact:name>pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch0_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch0_src</ipxact:displayName>
          <ipxact:value>cdr_clkin_scratch0_src_refclk_iqclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch1_src" type="string">
          <ipxact:name>pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch1_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch1_src</ipxact:displayName>
          <ipxact:value>cdr_clkin_scratch1_src_refclk_iqclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch2_src" type="string">
          <ipxact:name>pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch2_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch2_src</ipxact:displayName>
          <ipxact:value>cdr_clkin_scratch2_src_refclk_iqclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch3_src" type="string">
          <ipxact:name>pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch3_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch3_src</ipxact:displayName>
          <ipxact:value>cdr_clkin_scratch3_src_refclk_iqclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch4_src" type="string">
          <ipxact:name>pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch4_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_pm_cr_tx_rx_cdr_clkin_scratch4_src</ipxact:displayName>
          <ipxact:value>cdr_clkin_scratch4_src_refclk_iqclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_powerdown_mode" type="string">
          <ipxact:name>pma_cdr_refclk_powerdown_mode</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_powerdown_mode</ipxact:displayName>
          <ipxact:value>powerup</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_receiver_detect_src" type="string">
          <ipxact:name>pma_cdr_refclk_receiver_detect_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_receiver_detect_src</ipxact:displayName>
          <ipxact:value>iqclk_src</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_pm_cr_tx_rx_scratch0_src" type="string">
          <ipxact:name>pma_cdr_refclk_pm_cr_tx_rx_scratch0_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_pm_cr_tx_rx_scratch0_src</ipxact:displayName>
          <ipxact:value>scratch0_power_down</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_pm_cr_tx_rx_scratch1_src" type="string">
          <ipxact:name>pma_cdr_refclk_pm_cr_tx_rx_scratch1_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_pm_cr_tx_rx_scratch1_src</ipxact:displayName>
          <ipxact:value>scratch1_power_down</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_pm_cr_tx_rx_scratch2_src" type="string">
          <ipxact:name>pma_cdr_refclk_pm_cr_tx_rx_scratch2_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_pm_cr_tx_rx_scratch2_src</ipxact:displayName>
          <ipxact:value>scratch2_power_down</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_pm_cr_tx_rx_scratch3_src" type="string">
          <ipxact:name>pma_cdr_refclk_pm_cr_tx_rx_scratch3_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_pm_cr_tx_rx_scratch3_src</ipxact:displayName>
          <ipxact:value>scratch3_power_down</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_pm_cr_tx_rx_scratch4_src" type="string">
          <ipxact:name>pma_cdr_refclk_pm_cr_tx_rx_scratch4_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_pm_cr_tx_rx_scratch4_src</ipxact:displayName>
          <ipxact:value>scratch4_power_down</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_xmux_refclk_src" type="string">
          <ipxact:name>pma_cdr_refclk_xmux_refclk_src</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_xmux_refclk_src</ipxact:displayName>
          <ipxact:value>refclk_iqclk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_xpm_iqref_mux_iqclk_sel" type="string">
          <ipxact:name>pma_cdr_refclk_xpm_iqref_mux_iqclk_sel</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_xpm_iqref_mux_iqclk_sel</ipxact:displayName>
          <ipxact:value>power_down</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_silicon_rev" type="string">
          <ipxact:name>pma_cdr_refclk_silicon_rev</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_refclk_select" type="string">
          <ipxact:name>pma_cdr_refclk_refclk_select</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_refclk_select</ipxact:displayName>
          <ipxact:value>ref_iqclk0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_inclk0_logical_to_physical_mapping" type="string">
          <ipxact:name>pma_cdr_refclk_inclk0_logical_to_physical_mapping</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_inclk0_logical_to_physical_mapping</ipxact:displayName>
          <ipxact:value>ref_iqclk0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_inclk1_logical_to_physical_mapping" type="string">
          <ipxact:name>pma_cdr_refclk_inclk1_logical_to_physical_mapping</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_inclk1_logical_to_physical_mapping</ipxact:displayName>
          <ipxact:value>ref_iqclk0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_inclk2_logical_to_physical_mapping" type="string">
          <ipxact:name>pma_cdr_refclk_inclk2_logical_to_physical_mapping</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_inclk2_logical_to_physical_mapping</ipxact:displayName>
          <ipxact:value>ref_iqclk0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_inclk3_logical_to_physical_mapping" type="string">
          <ipxact:name>pma_cdr_refclk_inclk3_logical_to_physical_mapping</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_inclk3_logical_to_physical_mapping</ipxact:displayName>
          <ipxact:value>ref_iqclk0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="pma_cdr_refclk_inclk4_logical_to_physical_mapping" type="string">
          <ipxact:name>pma_cdr_refclk_inclk4_logical_to_physical_mapping</ipxact:name>
          <ipxact:displayName>pma_cdr_refclk_inclk4_logical_to_physical_mapping</ipxact:displayName>
          <ipxact:value>ref_iqclk0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_block_sel" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_block_sel</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_block_sel</ipxact:displayName>
          <ipxact:value>ten_g_pcs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_channel_operation_mode" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_clkslip_sel" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_clkslip_sel</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_clkslip_sel</ipxact:displayName>
          <ipxact:value>pld</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_lpbk_en" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_master_clk_sel" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_master_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_master_clk_sel</ipxact:displayName>
          <ipxact:value>master_rx_pma_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_pldif_datawidth_mode" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_pldif_datawidth_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_pldif_datawidth_mode</ipxact:displayName>
          <ipxact:value>pldif_data_10bit</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_pma_dw_rx" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_pma_dw_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_pma_dw_rx</ipxact:displayName>
          <ipxact:value>pma_32b_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_pma_if_dft_en" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_pma_if_dft_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_pma_if_dft_en</ipxact:displayName>
          <ipxact:value>dft_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_pma_if_dft_val" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_pma_if_dft_val</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_pma_if_dft_val</ipxact:displayName>
          <ipxact:value>dft_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_prbs9_dwidth" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_prbs9_dwidth</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_prbs9_dwidth</ipxact:displayName>
          <ipxact:value>prbs9_64b</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_prbs_clken" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_prbs_clken</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_prbs_clken</ipxact:displayName>
          <ipxact:value>prbs_clk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_prbs_ver" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_prbs_ver</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_prbs_ver</ipxact:displayName>
          <ipxact:value>prbs_off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_prot_mode_rx" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_prot_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_prot_mode_rx</ipxact:displayName>
          <ipxact:value>teng_krfec_mode_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_rx_dyn_polarity_inversion" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_rx_dyn_polarity_inversion</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_rx_dyn_polarity_inversion</ipxact:displayName>
          <ipxact:value>rx_dyn_polinv_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_rx_lpbk_en" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_rx_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_rx_lpbk_en</ipxact:displayName>
          <ipxact:value>lpbk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_rx_prbs_force_signal_ok" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_rx_prbs_force_signal_ok</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_rx_prbs_force_signal_ok</ipxact:displayName>
          <ipxact:value>force_sig_ok</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_rx_prbs_mask" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_rx_prbs_mask</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_rx_prbs_mask</ipxact:displayName>
          <ipxact:value>prbsmask128</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_rx_prbs_mode" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_rx_prbs_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_rx_prbs_mode</ipxact:displayName>
          <ipxact:value>teng_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_rx_signalok_signaldet_sel" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_rx_signalok_signaldet_sel</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_rx_signalok_signaldet_sel</ipxact:displayName>
          <ipxact:value>sel_sig_det</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_rx_static_polarity_inversion" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_rx_static_polarity_inversion</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_rx_static_polarity_inversion</ipxact:displayName>
          <ipxact:value>rx_stat_polinv_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_rx_uhsif_lpbk_en" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_rx_uhsif_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_rx_uhsif_lpbk_en</ipxact:displayName>
          <ipxact:value>uhsif_lpbk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_sup_mode" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_silicon_rev" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pcs_pma_interface_reconfig_settings" type="string">
          <ipxact:name>hssi_rx_pcs_pma_interface_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_rx_pcs_pma_interface_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs10g_advanced_user_mode_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs10g_advanced_user_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs10g_advanced_user_mode_rx</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_krfec_channel_operation_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_krfec_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_krfec_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs10g_channel_operation_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs10g_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs10g_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs8g_channel_operation_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs8g_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs8g_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_channel_operation_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_channel_operation_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_channel_operation_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_clklow_clk_hz" type="int">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_clklow_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_clklow_clk_hz</ipxact:displayName>
          <ipxact:value>322265625</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs10g_ctrl_plane_bonding_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs10g_ctrl_plane_bonding_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs10g_ctrl_plane_bonding_rx</ipxact:displayName>
          <ipxact:value>individual_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs8g_ctrl_plane_bonding_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs8g_ctrl_plane_bonding_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs8g_ctrl_plane_bonding_rx</ipxact:displayName>
          <ipxact:value>individual_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_ctrl_plane_bonding_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_ctrl_plane_bonding_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_ctrl_plane_bonding_rx</ipxact:displayName>
          <ipxact:value>individual_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs10g_fifo_mode_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs10g_fifo_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs10g_fifo_mode_rx</ipxact:displayName>
          <ipxact:value>reg_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs8g_fifo_mode_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs8g_fifo_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs8g_fifo_mode_rx</ipxact:displayName>
          <ipxact:value>reg_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_fref_clk_hz" type="int">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_fref_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_fref_clk_hz</ipxact:displayName>
          <ipxact:value>322265625</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_frequency_rules_en" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_frequency_rules_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_frequency_rules_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_func_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_func_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_func_mode</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_hclk_clk_hz" type="int">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_hclk_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_hclk_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_hip_en" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_hip_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_hip_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs8g_hip_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs8g_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs8g_hip_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_hrdrstctl_en" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_hrdrstctl_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_hrdrstctl_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_if_hrdrstctl_en" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_if_hrdrstctl_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_if_hrdrstctl_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_krfec_low_latency_en_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_krfec_low_latency_en_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_krfec_low_latency_en_rx</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs10g_low_latency_en_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs10g_low_latency_en_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs10g_low_latency_en_rx</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_low_latency_en_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_low_latency_en_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_low_latency_en_rx</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_krfec_lpbk_en" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_krfec_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_krfec_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs10g_lpbk_en" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs10g_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs10g_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs8g_lpbk_en" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs8g_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs8g_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_lpbk_en" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_lpbk_en" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_operating_voltage" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_operating_voltage</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_operating_voltage</ipxact:displayName>
          <ipxact:value>standard</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_ac_pwr_rules_en" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_ac_pwr_rules_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_ac_pwr_rules_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_pair_ac_pwr_uw_per_mhz" type="int">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_pair_ac_pwr_uw_per_mhz</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_pair_ac_pwr_uw_per_mhz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_rx_ac_pwr_uw_per_mhz" type="int">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_rx_ac_pwr_uw_per_mhz</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_rx_ac_pwr_uw_per_mhz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_pcs_rx_block_sel" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_pcs_rx_block_sel</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_pcs_rx_block_sel</ipxact:displayName>
          <ipxact:value>teng</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_pcs_rx_clk_out_sel" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_pcs_rx_clk_out_sel</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_pcs_rx_clk_out_sel</ipxact:displayName>
          <ipxact:value>teng_clk_out</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_pcs_rx_clk_sel" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_pcs_rx_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_pcs_rx_clk_sel</ipxact:displayName>
          <ipxact:value>pcs_rx_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_pcs_rx_hip_clk_en" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_pcs_rx_hip_clk_en</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_pcs_rx_hip_clk_en</ipxact:displayName>
          <ipxact:value>hip_rx_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_pcs_rx_output_sel" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_pcs_rx_output_sel</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_pcs_rx_output_sel</ipxact:displayName>
          <ipxact:value>teng_output</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_rx_pwr_scaling_clk" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_rx_pwr_scaling_clk</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pcs_rx_pwr_scaling_clk</ipxact:displayName>
          <ipxact:value>pma_rx_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_8g_refclk_dig_nonatpg_mode_clk_hz" type="int">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_8g_refclk_dig_nonatpg_mode_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_8g_refclk_dig_nonatpg_mode_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_fifo_mode_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_fifo_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_fifo_mode_rx</ipxact:displayName>
          <ipxact:value>reg_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_pcs_refclk_dig_nonatpg_mode_clk_hz" type="int">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_pcs_refclk_dig_nonatpg_mode_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_pcs_refclk_dig_nonatpg_mode_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_rx_clk_hz" type="int">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_rx_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_rx_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs10g_pma_dw_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs10g_pma_dw_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs10g_pma_dw_rx</ipxact:displayName>
          <ipxact:value>pma_32b_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs8g_pma_dw_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs8g_pma_dw_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs8g_pma_dw_rx</ipxact:displayName>
          <ipxact:value>pma_10b_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_dw_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_dw_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_dw_rx</ipxact:displayName>
          <ipxact:value>pma_32b_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_pma_dw_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_pma_dw_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_pma_dw_rx</ipxact:displayName>
          <ipxact:value>pma_32b_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_rx_clk_hz" type="int">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_rx_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_rx_clk_hz</ipxact:displayName>
          <ipxact:value>322265625</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_g3pcs_prot_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_g3pcs_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_g3pcs_prot_mode</ipxact:displayName>
          <ipxact:value>disabled_prot_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_krfec_prot_mode_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_krfec_prot_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_krfec_prot_mode_rx</ipxact:displayName>
          <ipxact:value>disabled_prot_mode_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs10g_prot_mode_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs10g_prot_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs10g_prot_mode_rx</ipxact:displayName>
          <ipxact:value>teng_1588_mode_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs8g_prot_mode_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs8g_prot_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs8g_prot_mode_rx</ipxact:displayName>
          <ipxact:value>disabled_prot_mode_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_prot_mode_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_prot_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_prot_mode_rx</ipxact:displayName>
          <ipxact:value>teng_1588_baser_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_if_prot_mode_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_if_prot_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_if_prot_mode_rx</ipxact:displayName>
          <ipxact:value>teng_reg_mode_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_prot_mode_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_prot_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_prot_mode_rx</ipxact:displayName>
          <ipxact:value>teng_krfec_mode_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_prot_mode_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_prot_mode_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_prot_mode_rx</ipxact:displayName>
          <ipxact:value>teng_mode_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs10g_shared_fifo_width_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs10g_shared_fifo_width_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs10g_shared_fifo_width_rx</ipxact:displayName>
          <ipxact:value>single_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_shared_fifo_width_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_shared_fifo_width_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_shared_fifo_width_rx</ipxact:displayName>
          <ipxact:value>single_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_shared_fifo_width_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_shared_fifo_width_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_shared_fifo_width_rx</ipxact:displayName>
          <ipxact:value>single_rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_sim_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_sim_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_sim_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_speed_grade" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_speed_grade</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_speed_grade</ipxact:displayName>
          <ipxact:value>e2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_g3pcs_sup_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_g3pcs_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_g3pcs_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_krfec_sup_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_krfec_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_krfec_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs10g_sup_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs10g_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs10g_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs8g_sup_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs8g_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs8g_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_sup_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_if_sup_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_if_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pld_if_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_sup_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_pma_if_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_sup_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_krfec_test_bus_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_krfec_test_bus_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_krfec_test_bus_mode</ipxact:displayName>
          <ipxact:value>tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs10g_test_bus_mode" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs10g_test_bus_mode</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs10g_test_bus_mode</ipxact:displayName>
          <ipxact:value>rx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_hd_pcs_channel_transparent_pcs_rx" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_hd_pcs_channel_transparent_pcs_rx</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_hd_pcs_channel_transparent_pcs_rx</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_silicon_rev" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_rx_pld_pcs_interface_reconfig_settings" type="string">
          <ipxact:name>hssi_rx_pld_pcs_interface_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_rx_pld_pcs_interface_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_bypass_pma_txelecidle" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_bypass_pma_txelecidle</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_bypass_pma_txelecidle</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_channel_operation_mode" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_lpbk_en" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_master_clk_sel" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_master_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_master_clk_sel</ipxact:displayName>
          <ipxact:value>master_tx_pma_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_pcie_sub_prot_mode_tx" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_pcie_sub_prot_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_pcie_sub_prot_mode_tx</ipxact:displayName>
          <ipxact:value>other_prot_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_pldif_datawidth_mode" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_pldif_datawidth_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_pldif_datawidth_mode</ipxact:displayName>
          <ipxact:value>pldif_data_10bit</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_pma_dw_tx" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_pma_dw_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_pma_dw_tx</ipxact:displayName>
          <ipxact:value>pma_32b_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_pma_if_dft_en" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_pma_if_dft_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_pma_if_dft_en</ipxact:displayName>
          <ipxact:value>dft_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_pmagate_en" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_pmagate_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_pmagate_en</ipxact:displayName>
          <ipxact:value>pmagate_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_prbs9_dwidth" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_prbs9_dwidth</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_prbs9_dwidth</ipxact:displayName>
          <ipxact:value>prbs9_64b</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_prbs_clken" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_prbs_clken</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_prbs_clken</ipxact:displayName>
          <ipxact:value>prbs_clk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_prbs_gen_pat" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_prbs_gen_pat</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_prbs_gen_pat</ipxact:displayName>
          <ipxact:value>prbs_gen_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_prot_mode_tx" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_prot_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_prot_mode_tx</ipxact:displayName>
          <ipxact:value>teng_krfec_mode_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_sq_wave_num" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_sq_wave_num</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_sq_wave_num</ipxact:displayName>
          <ipxact:value>sq_wave_default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_sqwgen_clken" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_sqwgen_clken</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_sqwgen_clken</ipxact:displayName>
          <ipxact:value>sqwgen_clk_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_sup_mode" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_tx_dyn_polarity_inversion" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_tx_dyn_polarity_inversion</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_tx_dyn_polarity_inversion</ipxact:displayName>
          <ipxact:value>tx_dyn_polinv_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_tx_pma_data_sel" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_tx_pma_data_sel</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_tx_pma_data_sel</ipxact:displayName>
          <ipxact:value>ten_g_pcs</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_tx_static_polarity_inversion" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_tx_static_polarity_inversion</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_tx_static_polarity_inversion</ipxact:displayName>
          <ipxact:value>tx_stat_polinv_dis</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_cnt_step_filt_before_lock" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_cnt_step_filt_before_lock</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_cnt_step_filt_before_lock</ipxact:displayName>
          <ipxact:value>uhsif_filt_stepsz_b4lock_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_cnt_thresh_filt_after_lock_value" type="int">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_cnt_thresh_filt_after_lock_value</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_cnt_thresh_filt_after_lock_value</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_cnt_thresh_filt_before_lock" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_cnt_thresh_filt_before_lock</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_cnt_thresh_filt_before_lock</ipxact:displayName>
          <ipxact:value>uhsif_filt_cntthr_b4lock_8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_dcn_test_update_period" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_dcn_test_update_period</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_dcn_test_update_period</ipxact:displayName>
          <ipxact:value>uhsif_dcn_test_period_4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_dcn_testmode_enable" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_dcn_testmode_enable</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_dcn_testmode_enable</ipxact:displayName>
          <ipxact:value>uhsif_dcn_test_mode_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_dead_zone_count_thresh" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_dead_zone_count_thresh</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_dead_zone_count_thresh</ipxact:displayName>
          <ipxact:value>uhsif_dzt_cnt_thr_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_dead_zone_detection_enable" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_dead_zone_detection_enable</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_dead_zone_detection_enable</ipxact:displayName>
          <ipxact:value>uhsif_dzt_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_dead_zone_obser_window" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_dead_zone_obser_window</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_dead_zone_obser_window</ipxact:displayName>
          <ipxact:value>uhsif_dzt_obr_win_16</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_dead_zone_skip_size" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_dead_zone_skip_size</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_dead_zone_skip_size</ipxact:displayName>
          <ipxact:value>uhsif_dzt_skipsz_4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_delay_cell_index_sel" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_delay_cell_index_sel</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_delay_cell_index_sel</ipxact:displayName>
          <ipxact:value>uhsif_index_cram</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_delay_cell_margin" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_delay_cell_margin</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_delay_cell_margin</ipxact:displayName>
          <ipxact:value>uhsif_dcn_margin_2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_delay_cell_static_index_value" type="int">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_delay_cell_static_index_value</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_delay_cell_static_index_value</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_dft_dead_zone_control" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_dft_dead_zone_control</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_dft_dead_zone_control</ipxact:displayName>
          <ipxact:value>uhsif_dft_dz_det_val_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_dft_up_filt_control" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_dft_up_filt_control</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_dft_up_filt_control</ipxact:displayName>
          <ipxact:value>uhsif_dft_up_val_0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_enable" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_enable</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_enable</ipxact:displayName>
          <ipxact:value>uhsif_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_lock_det_segsz_after_lock" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_lock_det_segsz_after_lock</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_lock_det_segsz_after_lock</ipxact:displayName>
          <ipxact:value>uhsif_lkd_segsz_aflock_512</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_lock_det_segsz_before_lock" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_lock_det_segsz_before_lock</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_lock_det_segsz_before_lock</ipxact:displayName>
          <ipxact:value>uhsif_lkd_segsz_b4lock_16</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_cnt_after_lock_value" type="int">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_cnt_after_lock_value</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_cnt_after_lock_value</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_cnt_before_lock_value" type="int">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_cnt_before_lock_value</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_cnt_before_lock_value</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_diff_after_lock_value" type="int">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_diff_after_lock_value</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_diff_after_lock_value</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_diff_before_lock_value" type="int">
          <ipxact:name>hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_diff_before_lock_value</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_uhsif_lock_det_thresh_diff_before_lock_value</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_silicon_rev" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pcs_pma_interface_reconfig_settings" type="string">
          <ipxact:name>hssi_tx_pcs_pma_interface_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_tx_pcs_pma_interface_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs10g_advanced_user_mode_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs10g_advanced_user_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs10g_advanced_user_mode_tx</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_krfec_channel_operation_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_krfec_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_krfec_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs10g_channel_operation_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs10g_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs10g_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs8g_channel_operation_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs8g_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs8g_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_channel_operation_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_channel_operation_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_channel_operation_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_channel_operation_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_channel_operation_mode</ipxact:displayName>
          <ipxact:value>tx_rx_pair_enabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_ctrl_plane_bonding" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_ctrl_plane_bonding</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_ctrl_plane_bonding</ipxact:displayName>
          <ipxact:value>individual</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs10g_ctrl_plane_bonding_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs10g_ctrl_plane_bonding_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs10g_ctrl_plane_bonding_tx</ipxact:displayName>
          <ipxact:value>individual_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs8g_ctrl_plane_bonding_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs8g_ctrl_plane_bonding_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs8g_ctrl_plane_bonding_tx</ipxact:displayName>
          <ipxact:value>individual_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_ctrl_plane_bonding_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_ctrl_plane_bonding_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_ctrl_plane_bonding_tx</ipxact:displayName>
          <ipxact:value>individual_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs10g_fifo_mode_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs10g_fifo_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs10g_fifo_mode_tx</ipxact:displayName>
          <ipxact:value>reg_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs8g_fifo_mode_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs8g_fifo_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs8g_fifo_mode_tx</ipxact:displayName>
          <ipxact:value>reg_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_frequency_rules_en" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_frequency_rules_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_frequency_rules_en</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_func_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_func_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_func_mode</ipxact:displayName>
          <ipxact:value>enable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_hclk_clk_hz" type="int">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_hclk_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_hclk_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_hip_en" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_hip_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_hip_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs8g_hip_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs8g_hip_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs8g_hip_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_hrdrstctl_en" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_hrdrstctl_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_hrdrstctl_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_if_hrdrstctl_en" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_if_hrdrstctl_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_if_hrdrstctl_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_krfec_low_latency_en_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_krfec_low_latency_en_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_krfec_low_latency_en_tx</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs10g_low_latency_en_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs10g_low_latency_en_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs10g_low_latency_en_tx</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_low_latency_en_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_low_latency_en_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_low_latency_en_tx</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_krfec_lpbk_en" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_krfec_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_krfec_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs10g_lpbk_en" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs10g_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs10g_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs8g_lpbk_en" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs8g_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs8g_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_lpbk_en" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_lpbk_en" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_lpbk_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_lpbk_en</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pcs_tx_ac_pwr_uw_per_mhz" type="int">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pcs_tx_ac_pwr_uw_per_mhz</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pcs_tx_ac_pwr_uw_per_mhz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_pcs_tx_clk_out_sel" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_pcs_tx_clk_out_sel</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_pcs_tx_clk_out_sel</ipxact:displayName>
          <ipxact:value>teng_clk_out</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_pcs_tx_clk_source" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_pcs_tx_clk_source</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_pcs_tx_clk_source</ipxact:displayName>
          <ipxact:value>teng</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_pcs_tx_data_source" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_pcs_tx_data_source</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_pcs_tx_data_source</ipxact:displayName>
          <ipxact:value>hip_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_pcs_tx_delay1_clk_en" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_pcs_tx_delay1_clk_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_pcs_tx_delay1_clk_en</ipxact:displayName>
          <ipxact:value>delay1_clk_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_pcs_tx_delay1_clk_sel" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_pcs_tx_delay1_clk_sel</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_pcs_tx_delay1_clk_sel</ipxact:displayName>
          <ipxact:value>pcs_tx_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_pcs_tx_delay1_ctrl" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_pcs_tx_delay1_ctrl</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_pcs_tx_delay1_ctrl</ipxact:displayName>
          <ipxact:value>delay1_path0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_pcs_tx_delay1_data_sel" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_pcs_tx_delay1_data_sel</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_pcs_tx_delay1_data_sel</ipxact:displayName>
          <ipxact:value>one_ff_delay</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_pcs_tx_delay2_clk_en" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_pcs_tx_delay2_clk_en</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_pcs_tx_delay2_clk_en</ipxact:displayName>
          <ipxact:value>delay2_clk_disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_pcs_tx_delay2_ctrl" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_pcs_tx_delay2_ctrl</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_pcs_tx_delay2_ctrl</ipxact:displayName>
          <ipxact:value>delay2_path0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_pcs_tx_output_sel" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_pcs_tx_output_sel</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_pcs_tx_output_sel</ipxact:displayName>
          <ipxact:value>teng_output</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pcs_tx_pwr_scaling_clk" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pcs_tx_pwr_scaling_clk</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pcs_tx_pwr_scaling_clk</ipxact:displayName>
          <ipxact:value>pma_tx_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_8g_refclk_dig_nonatpg_mode_clk_hz" type="int">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_8g_refclk_dig_nonatpg_mode_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_8g_refclk_dig_nonatpg_mode_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_fifo_mode_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_fifo_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_fifo_mode_tx</ipxact:displayName>
          <ipxact:value>reg_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_pcs_refclk_dig_nonatpg_mode_clk_hz" type="int">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_pcs_refclk_dig_nonatpg_mode_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_pcs_refclk_dig_nonatpg_mode_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_tx_clk_hz" type="int">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_tx_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_tx_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_uhsif_tx_clk_hz" type="int">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_uhsif_tx_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_uhsif_tx_clk_hz</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs10g_pma_dw_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs10g_pma_dw_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs10g_pma_dw_tx</ipxact:displayName>
          <ipxact:value>pma_32b_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs8g_pma_dw_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs8g_pma_dw_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs8g_pma_dw_tx</ipxact:displayName>
          <ipxact:value>pma_10b_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_dw_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_dw_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_dw_tx</ipxact:displayName>
          <ipxact:value>pma_32b_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_pma_dw_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_pma_dw_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_pma_dw_tx</ipxact:displayName>
          <ipxact:value>pma_32b_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_tx_clk_hz" type="int">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_tx_clk_hz</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_tx_clk_hz</ipxact:displayName>
          <ipxact:value>322265625</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_g3pcs_prot_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_g3pcs_prot_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_g3pcs_prot_mode</ipxact:displayName>
          <ipxact:value>disabled_prot_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_krfec_prot_mode_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_krfec_prot_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_krfec_prot_mode_tx</ipxact:displayName>
          <ipxact:value>disabled_prot_mode_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs10g_prot_mode_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs10g_prot_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs10g_prot_mode_tx</ipxact:displayName>
          <ipxact:value>teng_1588_mode_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs8g_prot_mode_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs8g_prot_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs8g_prot_mode_tx</ipxact:displayName>
          <ipxact:value>disabled_prot_mode_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_prot_mode_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_prot_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_prot_mode_tx</ipxact:displayName>
          <ipxact:value>teng_1588_baser_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_if_prot_mode_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_if_prot_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_if_prot_mode_tx</ipxact:displayName>
          <ipxact:value>teng_reg_mode_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_prot_mode_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_prot_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_prot_mode_tx</ipxact:displayName>
          <ipxact:value>teng_krfec_mode_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_prot_mode_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_prot_mode_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_prot_mode_tx</ipxact:displayName>
          <ipxact:value>teng_mode_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs10g_shared_fifo_width_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs10g_shared_fifo_width_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs10g_shared_fifo_width_tx</ipxact:displayName>
          <ipxact:value>single_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_shared_fifo_width_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_shared_fifo_width_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_shared_fifo_width_tx</ipxact:displayName>
          <ipxact:value>single_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_shared_fifo_width_tx" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_shared_fifo_width_tx</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_shared_fifo_width_tx</ipxact:displayName>
          <ipxact:value>single_tx</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_sim_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_sim_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_sim_mode</ipxact:displayName>
          <ipxact:value>disable</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_speed_grade" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_speed_grade</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_speed_grade</ipxact:displayName>
          <ipxact:value>e2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_g3pcs_sup_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_g3pcs_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_g3pcs_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_krfec_sup_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_krfec_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_krfec_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs10g_sup_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs10g_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs10g_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs8g_sup_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs8g_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs8g_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_sup_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_if_sup_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_if_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pld_if_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_sup_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_pma_if_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_sup_mode" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_sup_mode</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_hd_pcs_channel_share_fifo_mem_sup_mode</ipxact:displayName>
          <ipxact:value>user_mode</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_silicon_rev" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_silicon_rev</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_silicon_rev</ipxact:displayName>
          <ipxact:value>14nm5bcr2eb</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hssi_tx_pld_pcs_interface_reconfig_settings" type="string">
          <ipxact:name>hssi_tx_pld_pcs_interface_reconfig_settings</ipxact:name>
          <ipxact:displayName>hssi_tx_pld_pcs_interface_reconfig_settings</ipxact:displayName>
          <ipxact:value>{}</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </altera:altera_module_parameters>
    <altera:altera_system_parameters>
      <ipxact:parameters>
        <ipxact:parameter parameterId="device" type="string">
          <ipxact:name>device</ipxact:name>
          <ipxact:displayName>Device</ipxact:displayName>
          <ipxact:value>1SG165HU2F50E2VG</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="deviceFamily" type="string">
          <ipxact:name>deviceFamily</ipxact:name>
          <ipxact:displayName>Device family</ipxact:displayName>
          <ipxact:value>Stratix 10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="deviceSpeedGrade" type="string">
          <ipxact:name>deviceSpeedGrade</ipxact:name>
          <ipxact:displayName>Device Speed Grade</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="generationId" type="int">
          <ipxact:name>generationId</ipxact:name>
          <ipxact:displayName>Generation Id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bonusData" type="string">
          <ipxact:name>bonusData</ipxact:name>
          <ipxact:displayName>bonusData</ipxact:displayName>
          <ipxact:value>bonusData 
{
}
</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hideFromIPCatalog" type="bit">
          <ipxact:name>hideFromIPCatalog</ipxact:name>
          <ipxact:displayName>Hide from IP Catalog</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="lockedInterfaceDefinition" type="string">
          <ipxact:name>lockedInterfaceDefinition</ipxact:name>
          <ipxact:displayName>lockedInterfaceDefinition</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="systemInfos" type="string">
          <ipxact:name>systemInfos</ipxact:name>
          <ipxact:displayName>systemInfos</ipxact:displayName>
          <ipxact:value>&lt;systemInfosDefinition&gt;
    &lt;connPtSystemInfos&gt;
        &lt;entry&gt;
            &lt;key&gt;reconfig_avmm&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;reconfig_avmm&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos/&gt;
                &lt;consumedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_MAP&lt;/key&gt;
                        &lt;value&gt;&amp;lt;address-map&amp;gt;&amp;lt;slave name='reconfig_avmm' start='0x0' end='0x2000' datawidth='32' /&amp;gt;&amp;lt;/address-map&amp;gt;&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_WIDTH&lt;/key&gt;
                        &lt;value&gt;13&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;MAX_SLAVE_DATA_WIDTH&lt;/key&gt;
                        &lt;value&gt;32&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/consumedSystemInfos&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
        &lt;entry&gt;
            &lt;key&gt;rx_clkout&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;rx_clkout&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos/&gt;
                &lt;consumedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;CLOCK_RATE&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/consumedSystemInfos&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
        &lt;entry&gt;
            &lt;key&gt;rx_clkout2&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;rx_clkout2&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos/&gt;
                &lt;consumedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;CLOCK_RATE&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/consumedSystemInfos&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
        &lt;entry&gt;
            &lt;key&gt;tx_clkout&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;tx_clkout&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos/&gt;
                &lt;consumedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;CLOCK_RATE&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/consumedSystemInfos&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
    &lt;/connPtSystemInfos&gt;
&lt;/systemInfosDefinition&gt;</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </altera:altera_system_parameters>
    <altera:altera_interface_boundary>
      <altera:interface_mapping altera:name="latency_sclk" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.latency_sclk" altera:type="clock" altera:dir="end">
        <altera:port_mapping altera:name="latency_sclk" altera:internal="latency_sclk"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="reconfig_avmm" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.reconfig_avmm" altera:type="avalon" altera:dir="end">
        <altera:port_mapping altera:name="reconfig_address" altera:internal="reconfig_address"></altera:port_mapping>
        <altera:port_mapping altera:name="reconfig_read" altera:internal="reconfig_read"></altera:port_mapping>
        <altera:port_mapping altera:name="reconfig_readdata" altera:internal="reconfig_readdata"></altera:port_mapping>
        <altera:port_mapping altera:name="reconfig_waitrequest" altera:internal="reconfig_waitrequest"></altera:port_mapping>
        <altera:port_mapping altera:name="reconfig_write" altera:internal="reconfig_write"></altera:port_mapping>
        <altera:port_mapping altera:name="reconfig_writedata" altera:internal="reconfig_writedata"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="reconfig_clk" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.reconfig_clk" altera:type="clock" altera:dir="end">
        <altera:port_mapping altera:name="reconfig_clk" altera:internal="reconfig_clk"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="reconfig_reset" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.reconfig_reset" altera:type="reset" altera:dir="end">
        <altera:port_mapping altera:name="reconfig_reset" altera:internal="reconfig_reset"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_analogreset" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_analogreset" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_analogreset" altera:internal="rx_analogreset"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_analogreset_stat" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_analogreset_stat" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_analogreset_stat" altera:internal="rx_analogreset_stat"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_cal_busy" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_cal_busy" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_cal_busy" altera:internal="rx_cal_busy"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_cdr_refclk0" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_cdr_refclk0" altera:type="clock" altera:dir="end">
        <altera:port_mapping altera:name="rx_cdr_refclk0" altera:internal="rx_cdr_refclk0"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_clkout" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_clkout" altera:type="clock" altera:dir="start">
        <altera:port_mapping altera:name="rx_clkout" altera:internal="rx_clkout"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_clkout2" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_clkout2" altera:type="clock" altera:dir="start">
        <altera:port_mapping altera:name="rx_clkout2" altera:internal="rx_clkout2"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_coreclkin" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_coreclkin" altera:type="clock" altera:dir="end">
        <altera:port_mapping altera:name="rx_coreclkin" altera:internal="rx_coreclkin"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_digitalreset" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_digitalreset" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_digitalreset" altera:internal="rx_digitalreset"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_digitalreset_stat" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_digitalreset_stat" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_digitalreset_stat" altera:internal="rx_digitalreset_stat"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_enh_blk_lock" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_enh_blk_lock" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_enh_blk_lock" altera:internal="rx_enh_blk_lock"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_enh_clr_errblk_count" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_enh_clr_errblk_count" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_enh_clr_errblk_count" altera:internal="rx_enh_clr_errblk_count"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_enh_highber" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_enh_highber" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_enh_highber" altera:internal="rx_enh_highber"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_enh_highber_clr_cnt" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_enh_highber_clr_cnt" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_enh_highber_clr_cnt" altera:internal="rx_enh_highber_clr_cnt"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_fifo_latency_pulse" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_fifo_latency_pulse" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_fifo_latency_pulse" altera:internal="rx_fifo_latency_pulse"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_is_lockedtodata" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_is_lockedtodata" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_is_lockedtodata" altera:internal="rx_is_lockedtodata"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_parallel_data" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_parallel_data" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_parallel_data" altera:internal="rx_parallel_data"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_pcs_fifo_latency_pulse" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_pcs_fifo_latency_pulse" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_pcs_fifo_latency_pulse" altera:internal="rx_pcs_fifo_latency_pulse"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_serial_data" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_serial_data" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_serial_data" altera:internal="rx_serial_data"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="rx_seriallpbken" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.rx_seriallpbken" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="rx_seriallpbken" altera:internal="rx_seriallpbken"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_analogreset" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_analogreset" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="tx_analogreset" altera:internal="tx_analogreset"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_analogreset_stat" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_analogreset_stat" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="tx_analogreset_stat" altera:internal="tx_analogreset_stat"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_cal_busy" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_cal_busy" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="tx_cal_busy" altera:internal="tx_cal_busy"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_clkout" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_clkout" altera:type="clock" altera:dir="start">
        <altera:port_mapping altera:name="tx_clkout" altera:internal="tx_clkout"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_coreclkin" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_coreclkin" altera:type="clock" altera:dir="end">
        <altera:port_mapping altera:name="tx_coreclkin" altera:internal="tx_coreclkin"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_digitalreset" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_digitalreset" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="tx_digitalreset" altera:internal="tx_digitalreset"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_digitalreset_stat" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_digitalreset_stat" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="tx_digitalreset_stat" altera:internal="tx_digitalreset_stat"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_fifo_latency_pulse" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_fifo_latency_pulse" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="tx_fifo_latency_pulse" altera:internal="tx_fifo_latency_pulse"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_parallel_data" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_parallel_data" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="tx_parallel_data" altera:internal="tx_parallel_data"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_pcs_fifo_latency_pulse" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_pcs_fifo_latency_pulse" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="tx_pcs_fifo_latency_pulse" altera:internal="tx_pcs_fifo_latency_pulse"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_serial_clk0" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_serial_clk0" altera:type="hssi_serial_clock" altera:dir="end">
        <altera:port_mapping altera:name="tx_serial_clk0" altera:internal="tx_serial_clk0"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="tx_serial_data" altera:internal="alt_usxgmii_phy_altera_xcvr_native_s10_htile_1921_x6s27ia.tx_serial_data" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="tx_serial_data" altera:internal="tx_serial_data"></altera:port_mapping>
      </altera:interface_mapping>
    </altera:altera_interface_boundary>
    <altera:altera_has_warnings>false</altera:altera_has_warnings>
    <altera:altera_has_errors>false</altera:altera_has_errors>
  </ipxact:vendorExtensions>
</ipxact:component>