gflish_onchip_memory2_0 |

2020.02.21.15:03:01 | Datasheet

Overview

All Components
onchip_memory2_0 altera_avalon_onchip_memory2 18.0
Memory Map

onchip_memory2_0
s1

## onchip_memory2_0

altera_avalon_onchip_memory2 v18.0

## Parameters

allowInSystemMemoryContentEditor | false
blockType | AUTO
dataWidth | 32
dualPort | false
enableDiffWidth | false
initMemContent | true
initializationFileName | onchip_mem.hex
enPRInitMode | false
instanceID | NONE
memorySize | 102400
readDuringWriteMode | DONT_CARE
singleClockOperation | false
slave1Latency | 1
slave2Latency | 1
useNonDefaultInitFile | false
useShallowMemBlocks | false
writable | true
ecc_enabled | false
resetrequest_enabled | true
generateLegacySim | false

## Software Assignments

ALLOW_IN_SYSTEM_MEMORY_CONTENT_EDITOR | 0
ALLOW_MRAM_SIM_CONTENTS_ONLY_FILE | 0
CONTENTS_INFO | ""
DUAL_PORT | 0
GUI_RAM_BLOCK_TYPE | AUTO
INIT_CONTENTS_FILE | gflish_onchip_memory2_0_onchip_memory2_0
INIT_MEM_CONTENT | 1
INSTANCE_ID | NONE
NON_DEFAULT_INIT_FILE_ENABLED | 0
RAM_BLOCK_TYPE | AUTO
READ_DURING_WRITE_MODE | DONT_CARE
SINGLE_CLOCK_OP | 0
SIZE_MULTIPLE | 1
SIZE_VALUE | 102400
WRITABLE | 1

generation took 0.00 seconds | rendering took 0.00 seconds